{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":10,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data","index":0,"n_rows":556,"n_cols":679,"rows_kept":139,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":62,"rows_last":15,"rows_between":62,"halvings":5}}
["rtu","workbook","dnv_gl_id","Test_Type","Economizer_opening","Compressor_1_on_off","Compressor_2_on_off","Motor_sheave_setting","Cabinet_sealing","Ductwork_Sealing","Fan_Speed","Pulley_Diameter","Air_Discharge_Configuration","condenser_blockage","evaporator_blockage","Customer","Date","Time","Psy_Room","Average_time","Conditions","Engineer","Tech","OD_Unit_Model","OD_Unit_Serial","Unit_capacity","Refrigerant_type","ID_Unit_type","Refrigerant_charge","Volt_min_max_phs","TU_ID_Tag","Test_Standard","conditions_indoor_dry_bulb","conditions_indoor_wet_bulb","conditions_outdoor_dry_bulb","conditions_outdoor_wet_bulb","refrig_charge_ck_1","refrig_charge_ck_2","refrig_charge_factory_ck_1","refrig_charge_factory_ck_2","Total_Volts_mean","Total_Volts_std","Total_Amps_mean","Total_Amps_std","Net_Sensible_Capacity_mean","Net_Sensible_Capacity_std","Sensible_ViaGrids_mean","Sensible_ViaGrids_std","Net_Latent_Enthalpy_mean","Net_Latent_Enthalpy_std","Air_Side_Only_Cap_mean","Air_Side_Only_Cap_std","Air_Side_Only_EER_mean","ID_Blower_Motor_mean","ID_Blower_Power_mean","Code_tester_spd_mean","Air_Side_Only_EERs_mean","Enthalpy_evap_out_1_mean","Enthalpy_evap_out_1_std","Total_meas_heat_bal_mean","Cycle_number","Fan_on_time_min","OD_Outdoor_Dry_Air_mean","Cycle_total_time","OD_Outdoor_Wet_Air_mean","Nozzle_Area_mean","ID_Calc_Power_From_CFM_mean","C_test_SCFM_mean","C_test_Spec_vol_mix","Qss_mean","C_test_Spec_heat","Qcyc_mean","C_test_Hum_ratio","Delta_T_mean","C_Net_mean","OD_Off_Watt_hours","D_Net_mean","OD_On_Watt_hours","Integrated_EER_mean","Off_Watt_hours","EER_from_B_sensible_only_mean","ID_Off_Watt_hours","ID_On_Watt_hours","CLF_mean","Cyclic_Watt_hours","CD_mean","OD_SS_Watt_hours","ID_SS_Watt_hours","SEER_mean","Steady_Watt_hours","Watt_hour_ratio","Average_air_side_EER_mean","comments1","comments2","In_Dry_Bulb_avg","In_Dry_Bulb_std","In_Wet_Bulb_avg","In_Wet_Bulb_std","OD_Dry_Bulb_avg","OD_Dry_Bulb_std","OD_Wet_Bulb_avg","OD_Wet_Bulb_std","Inlet_Grid_avg","Inlet_Grid_std","Outlet_Grid_avg","Outlet_Grid_std","Nozzle_Temp_avg","Nozzle_Temp_std","B4Nozzle_avg","B4Nozzle_std","Nozzle_Delta_avg","Nozzle_delta_std","Net_Sensible_avg","Net_Sensible_std","Net_Latent_Enthalpy_avg","Net_Latent_Enthalpy_std","Air_Side_Only_EER_avg","Air_Side_Only_EER_std","Ref_Only_Cap_avg","Ref_Only_Cap_std","Meas_Refr_Only_EER_avg","Meas_Refr_Only_EER_std","Total_meas_heat_bal_avg","Total_meas_heat_bal_std","Tu_Total_V1_avg","Tu_Total_V1_std","Tu_Total_V2_avg","Tu_Total_V2_std","Tu_Total_V3_avg","Tu_Total_V3_std","Tu_Total_A1_avg","Tu_Total_A1_std","Tu_Total_A2_avg","Tu_Total_A2_std","Tu_Total_A3_avg","Tu_Total_A3_std","Tu_Total_W1_avg","Tu_Total_W1_std","Tu_Total_W2_avg","Tu_Total_W2_std","Tu_Total_W3_avg","Tu_Total_W3_std","ID_Blower_V1_avg","ID_Blower_V1_std","ID_Blower_V2_avg","ID_Blower_V2_std","ID_Blower_V3_avg","ID_Blower_V3_std","ID_Blower_A1_avg","ID_Blower_A1_std","ID_Blower_A2_avg","ID_Blower_A2_std","ID_Blower_A3_avg","ID_Blower_A3_std","ID_Blower_PF_avg","Comp_1_V1_avg","Comp_1_V1_std","Comp_1_V2_avg","Comp_1_V2_std","Comp_1_V3_avg","Comp_1_V3_std","Comp_1_A1_avg","Comp_1_A1_std","Comp_1_A2_avg","Comp_1_A2_std","Comp_1_A3_avg","Comp_1_A3_std","Comp_1_W_avg","Comp_1_W_std","Comp_1_PF_avg","Comp_2_V1_avg","Comp_2_V2_avg","Comp_2_V3_avg","Comp_2_A1_avg","Comp_2_A2_avg","Comp_2_A3_avg","Comp_2_W_avg","Comp_2_PF_avg","OD_Fan_Volts_avg","OD_Fan_Volts_std","OD_Fan_Amps_avg","OD_Fan_Amps_std","OD_Fan_Watts_avg","OD_Fan_Watts_std","Control_Watts_avg","Control_Watts_std","Total_Power_Individual_avg","Code_Tester_L1_V_avg","Code_Tester_L2_V_avg","Code_Tester_L3_V_avg","Code_Tester_L1_A_avg","Code_Tester_L2_A_avg","Code_Tester_L3_A_avg","Code_Tester_Watts_avg","Code_Tester_PF_avg","Code_Speed_avg","Code_Hz_avg","Control_Volts_avg","Control_Volts_std","Control_Amps_avg","Control_Amps_std","Liq_OD_PSIG_avg","Liq_OD_PSIG_std","Liq_OD_Temp_avg","Liq_OD_Temp_std","Sat_Liq_OD_avg","Sat_Liq_OD_std","SC_Liq_OD_avg","SC_Liq_OD_std","Discharge_PSIG_avg","Discharge_PSIG_std","Discharge_temp_avg","Discharge_temp_std","Sat_Compr_disch_avg","Sat_Compr_disch_std","SH_Compr_disch_avg","SH_Compr_disch_std","Liq_ID_PSIG_avg","Liq_ID_PSIG_std","Liq_ID_temp_avg","Liq_ID_temp_std","Sat_Liq_ID_avg","Sat_Liq_ID_std","SC_Liq_ID_avg","SC_Liq_ID_std","Gas_ID_PSIG_avg","Gas_ID_PSIG_std","Gas_ID_temp_avg","Gas_ID_temp_std","Sat_Gas_ID_avg","Sat_Gas_ID_std","SH_Gas_ID_avg","SH_Gas_ID_std","Suction_PSIG_avg","Suction_PSIG_std","Suction_temp_avg","Suction_temp_std","Sat_Suction_avg","Sat_Suction_std","SH_Suction_avg","SH_Suction_std","Flow_rate_lbs_hr_avg","Flow_rate_lbs_hr_std","Enthalpy_evap_In_1_mean","Enthalpy_evap_In_1_std","Meas_Refr_Only_Cap_mean","Meas_Refr_Only_Cap_std","Gross_ref_meas_cap_avg","Gross_ref_meas_cap_std","Liq_OD_BR_PSIG_avg","Liq_OD_BR_PSIG_std","Liq_OD_BR_temp_avg","Liq_OD_BR_temp_std","Sat_Liq_OD_BR_avg","Sat_Liq_OD_BR_std","SC_Liq_OD_BR_avg","SC_Liq_OD_BR_std","Liq_OD_AR_PSIG_avg","Liq_OD_AR_PSIG_std","Sat_Liq_OD_AR_avg","Sat_Liq_OD_AR_std","SC_Liq_OD_AR_avg","SC_Liq_OD_AR_std","Sat_ID_Gas_avg","Sat_ID_Gas_std","SH_ID_Gas_avg","SH_ID_Gas_std","Cond_Outlet_Sat_Liq_ID_avg","Cond_Outlet_Sat_Liq_ID_std","Liq_1_After_Restriction_avg","Liq_1_After_Restriction_std","Liq_Bef_Drier_PSIG_avg","Liq_Bef_Drier_PSIG_std","Liq_Bef_Drier_temp_avg","Liq_Bef_Drier_temp_std","Sat_Liq_Bef_Drier_avg","Sat_Liq_Bef_Drier_std","SC_Liq_Bef_Drier_avg","SC_Liq_Bef_Drier_std","Liq_After_Restriction__PSIG_avg","Liq_After_Restriction__PSIG_std","Sat_Liq_After_Restriction_avg","Sat_Liq_After_Restriction_std","SC_Liq_After_Restriction_avg","SC_Liq_After_Restriction_std","Gas_SH_ID_avg","Gas_SH_ID_std","Discharge_PSIG_avg_c2","Discharge_PSIG_std_c2","Discharge_temp_avg_c2","Discharge_temp_std_c2","Sat_Compr_disch_avg_c2","Sat_Compr_disch_std_c2","SH_Compr_disch_avg_c2","SH_Compr_disch_std_c2","liq_od_psig_avg_c2","liq_od_psig_std_c2","Sat_Liq_OD_avg_c2","Sat_Liq_OD_std_c2","SC_Liq_OD_avg_c2","SC_Liq_OD_std_c2","liq_id_psig_avg_c2","liq_id_psig_std_c2","liq_id_temp_avg_c2","liq_id_temp_std_c2","sat_liq_id_avg_c2","sat_liq_id_std_c2","sc_liq_id_avg_c2","sc_liq_id_std_c2","gas_id_psig_avg_c2","gas_id_psig_std_c2","sat_gas_id_avg_c2","sat_gas_id_std_c2","sh_gas_id_avg_c2","sh_gas_id_std_c2","suction_psig_avg_c2","suction_psig_std_c2","suction_temp_avg_c2","suction_temp_std_c2","sat_suction_avg_c2","sat_suction_std_c2","sh_suction_avg_c2","sh_suction_std_c2","liquid_bef_filter_temp_avg_c2","liquid_bef_filter_temp_std_c2","Flow_rate_lbs_hr_avg_c2","Flow_rate_lbs_hr_std_c2","Enthalpy_Evap_In_avg_c2","Enthalpy_Evap_In_std_c2","Enthalpy_Evap_Out_avg_c2","Enthalpy_Evap_Out_std_c2","Meas_ref_only_cap_avg_c2","Meas_ref_only_cap_std_c2","Gross_ref_meas_cap_avg_c2","Gross_ref_meas_cap_std_c2","liq_od_br_psig_avg_c2","liq_od_br_psig_std_c2","liq_od_br_temp_avg_c2","liq_od_br_temp_std_c2","sat_liq_od_br_avg_c2","sat_liq_od_br_std_c2","sc_liq_od_br_avg_c2","sc_liq_od_br_std_c2","liq_od_ar_psig_avg_c2","liq_od_ar_psig_std_c2","sat_liq_od_ar_avg_c2","sat_liq_od_ar_std_c2","sc_liq_od_ar_avg_c2","sc_liq_od_ar_std_c2","Cond_Outlet_Liq_ID_temp_avg_c2","Cond_Outlet_Liq_ID_temp_std_c2","Cond_Outlet_Sat_Liq_ID_avg_c2","Cond_Outlet_Sat_Liq_ID_std_c2","Bef_FD_CK1_avg","Bef_FD_CK1_std","Aft_FD_CK1_avg","Aft_FD_CK1_std","Bef_FD_CK2_avg","Bef_FD_CK2_std","Aft_FD_CK2_avg","Aft_FD_CK2_std","Inside_Supply_Duct_1_avg","Inside_Supply_Duct_1_std","Inside_Supply_Duct_2_avg","Inside_Supply_Duct_2_std","Inside_Supply_Duct_3_avg","Inside_Supply_Duct_3_std","Inside_Supply_Duct_4_avg","Inside_Supply_Duct_4_std","Inside_Supply_Duct_5_avg","Inside_Supply_Duct_5_std","Inside_Supply_Duct_6_avg","Inside_Supply_Duct_6_std","liq_od_backup_ck1_avg","liq_od_backup_ck1_std","liq_id_backup_ck1_avg","liq_id_backup_ck1_std","gas_id_backup_ck1_avg","gas_id_backup_ck1_std","suction_backup_ck1_avg","suction_backup_ck1_std","discharge_backup_ck2_avg","discharge_backup_ck2_std","liq_od_backup_ck2_avg","liq_od_backup_ck2_std","liq_id_backup_ck2_avg","liq_id_backup_ck2_std","gas_id_backup_ck2_avg","gas_id_backup_ck2_std","suction_backup_ck2_avg","suction_backup_ck2_std","Liq_ID_Temp_CK1_avg","Liq_ID_Temp_CK1_std","Liq_ID_Temp_CK2_avg","Liq_ID_Temp_CK2_std","OD_Inlet_Grid_Econo_avg","OD_Inlet_Grid_Econo_std","Liq_Upstream_CK1_avg","Liq_Upstream_CK1_std","Liq_Downstream_CK1_avg","Liq_Downstream_CK1_std","Liq_Upstream_CK2_avg","Liq_Upstream_CK2_std","Liq_Downstream_CK2_avg","Liq_Downstream_CK2_std","liq_aft_filter_temp_ck1_avg","liq_aft_filter_temp_ck1_std","liq_aft_filter_temp_ck2_avg","liq_aft_filter_temp_ck2_std","Economizer_Inlet_A1_temp_avg","Economizer_Inlet_A1_temp_std","Economizer_Inlet_A2_temp_avg","Economizer_Inlet_A2_temp_std","Economizer_Inlet_B1_temp_avg","Economizer_Inlet_B1_temp_std","Economizer_Inlet_B2_temp_avg","Economizer_Inlet_B2_temp_std","Economizer_Inlet_C1_temp_avg","Economizer_Inlet_C1_temp_std","Economizer_Inlet_C2_temp_avg","Economizer_Inlet_C2_temp_std","CK1_Liq_ID_Temp_avg","CK1_Liq_ID_Temp_std","Inside_Supply_Duct_6_avg","Inside_Supply_Duct_6_std","Liq_OD_Temp_CK1_avg","Liq_OD_Temp_CK1_std","Liq_OD_Temp_CK2_avg","Liq_OD_Temp_CK2_std","Liq_Bef_Filter_Temp_CK1_avg","Liq_Bef_Filter_Temp_CK1_std","Liq_Bef_Filter_Temp_CK2_avg","Liq_Bef_Filter_Temp_CK2_std","Liq_Aft_Restric_Temp_CK1_avg","Liq_Aft_Restric_Temp_CK1_std","Liq_Aft_Restric_Temp_CK2_avg","Liq_Aft_Restric_Temp_CK2_std","Suction_CK1_avg","Suction_CK1_std","Suction_CK2_avg","Suction_CK2_std","liq_od_backup_2_ck1_avg","liq_od_backup_2_ck1_std","liq_od_backup_2_ck2_avg","liq_od_backup_2_ck2_std","gas_id_ck1_avg","gas_id_ck1_std","Liq_OD_BR_1_avg","Liq_OD_BR_1_std","gas_id_ck2_avg","gas_id_ck2_std","Liq_OD_BR_2_avg","Liq_OD_BR_2_std","liq_aft_dryer_b4_restr_ck1_avg","liq_aft_dryer_b4_restr_ck1_std","liq_aft_dryer_b4_restr_ck2_avg","liq_aft_dryer_b4_restr_ck2_std","Liq_2_After_Restriction_avg","Liq_2_After_Restriction_std","Compressor_Top_avg","Compressor_Top_std","Compressor_Middle_avg","Compressor_Middle_std","discharge_backup_ck1_avg","discharge_backup_ck1_std","OD_Inlet_Grid_1_avg","OD_Inlet_Grid_1_std","OD_Inlet_Grid_2_avg","OD_Inlet_Grid_2_std","Inside_Return_Duct_1_avg","Inside_Return_Duct_1_std","Inside_Return_Duct_2_avg","Inside_Return_Duct_2_std","Inside_Return_Duct_3_avg","Inside_Return_Duct_3_std","Inside_Return_Duct_4_avg","Inside_Return_Duct_4_std","Inside_Return_Duct_5_avg","Inside_Return_Duct_5_std","Inside_Return_Duct_6_avg","Inside_Return_Duct_6_std","Inside_Return_Duct_7_avg","Inside_Return_Duct_7_std","Return_Coil_Face_A1_avg","Return_Coil_Face_A1_std","Return_Coil_Face_A2_avg","Return_Coil_Face_A2_std","Return_Coil_Face_A3_avg","Return_Coil_Face_A3_std","Return_Coil_Face_A4_avg","Return_Coil_Face_A4_std","Return_Coil_Face_B1_avg","Return_Coil_Face_B1_std","Return_Coil_Face_B2_avg","Return_Coil_Face_B2_std","Return_Coil_Face_B3_avg","Return_Coil_Face_B3_std","Return_Coil_Face_B4_avg","Return_Coil_Face_B4_std","Return_Coil_Face_C1_avg","Return_Coil_Face_C1_std","Return_Coil_Face_C2_avg","Return_Coil_Face_C2_std","Return_Coil_Face_C3_avg","Return_Coil_Face_C3_std","Return_Coil_Face_C4_avg","Return_Coil_Face_C4_std","Return_Coil_Face_D1_avg","Return_Coil_Face_D1_std","Return_Coil_Face_D2_avg","Return_Coil_Face_D2_std","Return_Coil_Face_D3_avg","Return_Coil_Face_D3_std","Return_Coil_Face_D4_avg","Return_Coil_Face_D4_std","Return_Coil_Face_E1_avg","Return_Coil_Face_E1_std","Return_Coil_Face_E2_avg","Return_Coil_Face_E2_std","Return_Coil_Face_E3_avg","Return_Coil_Face_E3_std","Return_Coil_Face_E4_avg","Return_Coil_Face_E4_std","Inside_Return_Duct_8_avg","Inside_Return_Duct_8_std","Inside_Return_Duct_9_avg","Inside_Return_Duct_9_std","Inside_Return_Duct_10_avg","Inside_Return_Duct_10_std","Inside_Return_Duct_11_avg","Inside_Return_Duct_11_std","Inside_Return_Duct_12_avg","Inside_Return_Duct_12_std","Inside_Return_Duct_13_avg","Inside_Return_Duct_13_std","Inside_Return_Duct_14_avg","Inside_Return_Duct_14_std","Inside_Return_Duct_15_avg","Inside_Return_Duct_15_std","Return_Coil_Face_A5_avg","Return_Coil_Face_A5_std","Return_Coil_Face_B5_avg","Return_Coil_Face_B5_std","Return_Coil_Face_C5_avg","Return_Coil_Face_C5_std","Economizer_1_avg","Economizer_1_std","Economizer_2_avg","Economizer_2_std","Economizer_3_avg","Economizer_3_std","Economizer_4_avg","Economizer_4_std","Economizer_5_avg","Economizer_5_std","Economizer_6_avg","Economizer_6_std","Return_Coil_Face_D5_avg","Return_Coil_Face_D5_std","OD_Inlet_Grid_3_avg","OD_Inlet_Grid_3_std","Return_Coil_Face_1_avg","Return_Coil_Face_1_std","Return_Coil_Face_2_avg","Return_Coil_Face_2_std","Return_Coil_Face_3_avg","Return_Coil_Face_3_std","Return_Coil_Face_4_avg","Return_Coil_Face_4_std","Return_Coil_Face_5_avg","Return_Coil_Face_5_std","Return_Coil_Face_6_avg","Return_Coil_Face_6_std","Return_Coil_Face_7_avg","Return_Coil_Face_7_std","Return_Coil_Face_8_avg","Return_Coil_Face_8_std","Return_Coil_Face_9_avg","Return_Coil_Face_9_std","Return_Coil_Face_10_avg","Return_Coil_Face_10_std","Return_Coil_Face_11_avg","Return_Coil_Face_11_std","Return_Coil_Face_12_avg","Return_Coil_Face_12_std","Return_Coil_Face_13_avg","Return_Coil_Face_13_std","Return_Coil_Face_14_avg","Return_Coil_Face_14_std","Return_Coil_Face_15_avg","Return_Coil_Face_15_std","Return_Coil_Face_16_avg","Return_Coil_Face_16_std","Economizer_grid_avg","Economizer_grid_std","Liq_Bef_FlowM_Ck1_avg","Liq_Bef_FlowM_Ck1_1std","Liq_After_FlowM_Ck1_avg","Liq_After_FlowM_Ck1_std","Liq_Bef_FlowM_Ck2_avg","Liq_Bef_FlowM_Ck2_std","Liq_After_FlowM_Ck2_avg","Liq_After_FlowM_Ck2_std","Inside_Supply_Duct_7_avg","Inside_Supply_Duct_7_std","Inside_Supply_Duct_8_avg","Inside_Supply_Duct_8_std","Comparison","ID_Inlet_Dry_Air_mean","ID_Inlet_Dry_Air_std","ID_Inlet_Wet_Air_mean","ID_Inlet_Wet_Air_std","ID_Outlet_Dry_Air_mean","ID_Outlet_Dry_Air_std","ID_Outlet_Wet_Air_mean","ID_Outlet_Wet_Air_std","OD_Inlet_Dry_Air_mean","OD_Inlet_Dry_Air_std","OD_Inlet_Wet_Air_mean","OD_Inlet_Wet_Air_std","Tot_Air_Flow_CFM_mean","Tot_Air_Flow_CFM_std","Tot_Air_Flow_SCFM_mean","Tot_Air_Flow_SCFM_std","Unit_Total_Static_mean","Unit_Total_Static_std","Unit_Inlet_Static_mean","Unit_Inlet_Static_std","B4_Nozzle_Static_mean","B4_Nozzle_Static_std","Nozzle_Delta_mean","Nozzle_Delta_std","Barometric_Pressure_mean","Barometric_Pressure_std","Total_Power_mean","Total_Power_std","ID_Blower_W_avg","ID_Blower_W_std","OA_Comp_Ratio","OA_Comp","Spec_Vol_Comp","Delta_P_Comp","Fan_Heat_DT","SA_Mass_Flow","Flow_Power","OA_Flow_Corrected","OA_Mass_Flow_Corrected","RA_Mass_Flow_Rate","MA_Hum_Ratio","MA_Enthalpy","Coil_Leaving_DB","OA_Spec_Vol","Coil_Out_Spec_Vol","OA_Hum_Ratio","OA_Enthalpy","RA_Hum_Ratio","RA_Enthalpy","Coil_Out_Hum_Ratio","SA_Enthalpy","MA_Dry_Bulb","MA_Wet_Bulb","Coil_Leaving_Enthalpy","Gross_Cooling_Capacity","Gross_Sensible_Capacity","Comp_Unit_Power","EIR","Net_Cooling_Capacity","Net_Sensible_Capacity","EER","Coil_Bypass_Factor","dh","dT","Ts","Gross_Coil_Capacity","Space_Load","Fan_Heat","OA_Load","Total load","Calibration"]
[5,"C-55-1ER-DM","30N0001","C-55-1ER-DM","1 Finger","Off","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","6:42:49","10 Ton","0:30:00","75/62  55/51","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.2,0.8,1.7,0,7597,27,6946,49,3193,71,10793,82,null,943,null,12.9,null,109.86,0.01,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28.781333332999999,"Econo 1F-open, no compressor, 55/51 ambient, 53.5% inlet 52% outlet Meriam, adjust code tester speed to match total static of run C-55-1E-DM-SPWCT-SSR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 1F: with flow meter: new filter drier: with isolation ball valves: with code",74.995999999999995,1.2E-2,62.002000000000002,3.1E-2,54.994,1.4E-2,50.997,1.7000000000000001E-2,74.36,0.04,68.97,0.03,71.69,0.02,6.0000000000000001E-3,6.0000000000000001E-3,1.1762999999999999,6.4000000000000003E-3,7597,27,3193,71,28.827000000000002,0.41899999999999998,null,null,null,null,null,null,230.2,0.8,230.2,0.8,230.2,0.8,0,0,0,0,0,0,0.3,0.2,0.3,0.2,0.3,0.2,229.8,0.8,229.8,0.8,229.8,0.8,1.7,0,1.7,0,1.7,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,23,null,397.1,476.6,477.8,478,0.9,0.9,1,500,0.64,12.9,18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-0.59,0.04,26.22,0.01,-1277,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68.86,0.35,69.81,0.22,69.38,0.02,69.7,0.2,69.180000000000007,0.17,69.150000000000006,0.17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.01,0.02,null,null,55.97,0.25,55.9,0.21,55.12,0.17,55.1,0.12,54.95,7.0000000000000007E-2,54.98,7.0000000000000007E-2,null,null,null,null,null,null,null,null,54.74,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.83,0.09,54.57,0.06,74.400000000000006,0.05,74.42,0.05,74.38,0.03,74.489999999999995,0.06,74.45,0.06,74.53,0.06,74.489999999999995,0.05,58.54,0.04,57.71,0.05,57.21,0.05,60.23,0.23,59.32,7.0000000000000007E-2,59.98,0.11,60.99,0.14000000000000001,62.25,0.11,59.85,7.0000000000000007E-2,74.25,0.06,73.45,0.1,74.55,0.06,67.72,0.15,73.95,0.04,74.48,0.03,73.349999999999994,0.05,72.459999999999994,0.14000000000000001,74.150000000000006,0.06,74.31,0.05,74.42,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.995999999999995,1.2E-2,62.002000000000002,3.1E-2,69.094999999999999,7.0000000000000001E-3,58.991,2.5999999999999999E-2,54.994,1.4E-2,50.997,1.7000000000000001E-2,1177.7,3.2,1144.0999999999999,3.1,0.56799999999999995,1.0999999999999999E-2,-0.13600000000000001,1E-3,6.0000000000000001E-3,6.0000000000000001E-3,1.1762999999999999,6.4000000000000003E-3,29.600999999999999,1E-3,375,5,374.1,4.7,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,{"$f":"(XM2-XU2)*3.412/XT2/0.24","v":0.8025309192016622},{"$f":"WW2*60/YC2","v":5274.6771734329113},{"$f":"XA2*WY2*746/6350","v":76.344441700787385},{"$f":"XP2*SQRT(-XC2*YB2/(XR2*XQ2))","v":291.77742921384669},{"$f":"XV2*60/YB2","v":1343.6317114105198},{"$f":"XT2-XW2","v":3931.0454620223918},{"$f":"(XW2*YD2+XX2*YF2)/XT2","v":8.323930046997146E-3},{"$f":"(XW2*YE2+XX2*YG2)/XT2","v":25.86927045497487},{"$f":"WO2-XS2","v":68.292469080798341},13.029348447315707,13.396459665039773,6.9811591442616814E-3,20.776031160556553,8.7828892687881119E-3,27.610140128423488,8.2502815653290856E-3,25.589452363726007,{"$f":"psych(\"tdb\",\"h\",\"w\",XZ2,XY2)","v":69.913305569535723},{"$f":"psych(\"Twb\",\"TDB\",\"W\",YJ2,XY2)","v":59.419136474295769},{"$f":"psych(\"H\",\"TDB\",\"w\",YA2,YH2)","v":25.393905172032166}]
[5,"C-55-2ER-DM","30N0002","C-55-2ER-DM","2 Finger","Off","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","9:20:19","10 Ton","0:30:00","75/62 55/51","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.2,0.8,1.7,0,9635,29,8894,53,4063,82,13702,85,null,942,null,13.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,36.344827586000001,"Econo 2F-open, no compressor, 55/51, 53.5% inlet 52% outlet Meriam, ambient--adjust code tester speed to match total static of run C-55-2E-DM-SPWCT-SSR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 1F: with flow meter: new filter drier: with isolation ball valves: with code",75,1.4E-2,62.000999999999998,2.9000000000000001E-2,55,1.6E-2,50.997999999999998,1.7999999999999999E-2,74.37,0.06,67.58,0.05,70.69,0.01,2.5000000000000001E-2,4.0000000000000001E-3,1.2104999999999999,4.7000000000000002E-3,9635,29,4063,82,36.343000000000004,0.51800000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,1.7,0,1.7,0,1.7,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,478,480,480,0.9,0.9,1.1000000000000001,510,0.64,13.8,18.399999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,66.83,0.21,69.040000000000006,0.16,67.989999999999995,0.08,68.89,0.13,67.33,0.1,68.12,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.14,0.03,null,null,55.04,0.18,55.27,0.19,54.58,0.11,54.89,0.12,54.82,0.1,54.82,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.22,0.1,54.95,0.1,74.680000000000007,0.09,74.64,7.0000000000000007E-2,74.47,0.03,74.849999999999994,0.1,74.790000000000006,0.1,74.849999999999994,0.1,74.75,0.08,59.12,7.0000000000000007E-2,58.71,7.0000000000000007E-2,57.59,7.0000000000000007E-2,58.85,0.12,60.43,0.09,59.03,0.13,58.94,0.1,59.74,0.1,60.27,0.09,73.41,7.0000000000000007E-2,68.900000000000006,0.15,70.64,0.12,64.849999999999994,0.15,73.3,0.04,73.73,0.04,72.75,0.05,70.62,0.15,73.23,0.05,73.84,0.04,72.84,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75,1.4E-2,62.000999999999998,2.9000000000000001E-2,67.638999999999996,8.0000000000000002E-3,58.203000000000003,2.5999999999999999E-2,55,1.6E-2,50.997999999999998,1.7999999999999999E-2,1192.7,2.4,1162.9000000000001,2.2999999999999998,0.53800000000000003,7.0000000000000001E-3,-0.108,2E-3,2.5000000000000001E-2,4.0000000000000001E-3,1.2104999999999999,4.7000000000000002E-3,29.645,1E-3,377,5,376.8,4.9000000000000004,0.32805000000000023,381.4893450000003,13.029,0.108,0.80490214861994736,5357.0601228673304,73.500407748031506,381.49656993496882,1756.7677651478721,3600.2923577194583,8.1906723247139081E-3,25.368637479749061,66.834097851380051,13.029493510869054,13.358446304257066,6.980280398114924E-3,20.7765359497219,8.7812847829730582E-3,27.609359938007415,8.1087436134834392E-3,25.080256459222877,68.455766242559491,58.650651841180498,24.884182068704337]
[5,"C-55-3ER-DM","30N0003","C-55-3ER-DM","3 Finger","Off","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","16:28:28","10 Ton","0:30:00","75/62 55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.2,0.8,1.7,0,13008,144,12228,143,5272,135,18284,260,null,942,null,14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48.498673740000001,"Econo 3F-open, no compressor, 55/51 ambient, 53.5% inlet 52% outlet Meriam,--adjust code tester speed to match total static of run C-55-3E-DM-SPWCT-SSR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 3F: with flow meter: new filter drier: with isolation ball valves: with code",75.001999999999995,1.7000000000000001E-2,62.003,3.1E-2,55,1.0999999999999999E-2,51.002000000000002,1.9E-2,74.38,0.05,65.03,0.03,69.010000000000005,0.03,1.6E-2,1.4E-2,1.2053,2.5100000000000001E-2,13008,144,5272,135,48.572000000000003,0.83799999999999997,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,1.7,0,1.7,0,1.7,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,482,482,482,0.9,0.9,1,500,0.63,14,18.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64.13,0.23,66.260000000000005,0.17,65.099999999999994,0.08,66.180000000000007,0.16,64.349999999999994,0.13,65.42,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.31,0.02,null,null,55.23,0.1,55.4,0.13,54.59,0.06,54.8,7.0000000000000007E-2,54.72,0.06,54.73,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.11,0.09,54.67,7.0000000000000007E-2,74.430000000000007,0.05,74.430000000000007,0.05,74.400000000000006,0.04,74.489999999999995,7.0000000000000007E-2,74.45,7.0000000000000007E-2,74.53,7.0000000000000007E-2,74.53,0.06,57.27,0.04,57.09,0.03,57.1,0.04,56.92,0.03,57.04,0.08,59.98,0.08,57.19,0.05,57.04,0.06,60.89,0.09,69.3,0.13,61.55,0.14000000000000001,65.53,0.15,67.150000000000006,0.09,72.69,0.06,71.5,0.05,69.75,0.06,69.75,0.1,72.47,0.06,72.67,0.04,69.27,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75.001999999999995,1.7000000000000001E-2,62.003,3.1E-2,65.039000000000001,7.0000000000000001E-3,56.87,2.3E-2,55,1.0999999999999999E-2,51.002000000000002,1.9E-2,1191.7,12.5,1159,12.3,0.497,4.0000000000000001E-3,-6.0999999999999999E-2,2E-3,1.6E-2,1.4E-2,1.2053,2.5100000000000001E-2,29.471,2E-3,377,5,376.1,5.3,0.45760423957604218,530.36331366863294,13.03,6.0999999999999999E-2,0.81506897760524311,5379.7006591538002,67.671363464566923,530.35334207753749,2442.2407618444154,2937.4598973093848,7.9651037375800503E-3,24.509259206400614,64.223931022394765,13.029510039223332,13.291074082037662,6.98240575763208E-3,20.77884285744901,8.7821310833522959E-3,27.610773843044818,7.9184305424591407E-3,24.239477826547791,65.937893257390456,57.30290098870946,24.040995666136137]
[5,"C-55-CE-DM","30N0004","C-55-CE-DM","closed","Off","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/12/2014","23:25:52","10 Ton","0:30:00","75/62 - 55/51","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.2,0.5,1.7,0,5340,17,4796,44,2236,49,7578,48,null,942,null,13.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.100795756,"Econo closed, no compressor, 55/51 ambient, 53.5% inlet 52% outlet Meriam,--adjust code tester speed to match total static of run C-55-CE-DM-SPWCT-SS","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo  fulley closed: with flow meter: new filter drier: with isolation ball valves: with code",74.995999999999995,0.01,62,2.8000000000000001E-2,54.981000000000002,1.2999999999999999E-2,51,1.7000000000000001E-2,74.36,0.03,70.67,0.05,72.83,0.01,3.3000000000000002E-2,4.0000000000000001E-3,1.1992,4.7000000000000002E-3,5340,17,2236,49,20.12,0.28799999999999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229.9,0.5,229.9,0.5,229.9,0.5,1.7,0,1.7,0,1.7,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,486,487,488,0.9,0.9,1.1000000000000001,510,0.62,13.8,18.399999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.73,0.04,71.62,0.03,71.38,0.03,71.34,0.03,71.33,0.03,70.900000000000006,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.99,0.03,null,null,54.32,0.1,54.41,0.11,54.01,0.08,54.24,0.09,54.33,7.0000000000000007E-2,54.36,7.0000000000000007E-2,null,null,null,null,null,null,null,null,54.19,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.67,0.11,54.29,7.0000000000000007E-2,74.5,0.06,74.52,0.05,74.45,0.03,74.61,0.06,74.58,7.0000000000000007E-2,74.63,7.0000000000000007E-2,74.569999999999993,0.06,64.16,0.08,65.540000000000006,0.14000000000000001,67.94,0.09,63.66,0.11,64.150000000000006,0.08,65.010000000000005,0.16,70.92,0.1,65.150000000000006,0.14000000000000001,58.35,7.0000000000000007E-2,72.28,0.11,74.930000000000007,7.0000000000000007E-2,74.91,0.06,67.61,0.21,74.78,0.05,74.87,0.04,74.28,0.05,73.84,0.06,74.28,0.06,74.38,0.04,74.5,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.995999999999995,0.01,62,2.8000000000000001E-2,70.879000000000005,8.9999999999999993E-3,59.927,2.5999999999999999E-2,54.981000000000002,1.2999999999999999E-2,51,1.7000000000000001E-2,1190.2,2.4,1153.9000000000001,2.2999999999999998,0.59899999999999998,7.0000000000000001E-3,-0.182,1E-3,3.3000000000000002E-2,4.0000000000000001E-3,1.1992,4.7000000000000002E-3,29.611000000000001,1E-3,377,5,376.3,4.8,0.16622533100174824,191.8074094429173,13.029,0.182,0.78975097583486553,5312.2156815735407,81.200760724409449,191.80781789362877,883.29265942010443,4428.9230221534362,8.4829787519141338E-3,26.472903895800144,70.089249024165142,13.029055490139832,13.442978275092724,6.9858082952810119E-3,20.777917107585136,8.7815704564052372E-3,27.60869695437512,8.4154184094527209E-3,26.204554472430296,71.677066195439608,60.330253900790645,26.012063376533916]
[5,"C-55-OER-DM","30N0005","C-55-OER-DM","Fully open","Off","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","18:30:01","10 Ton","0:30:00","75/62 - 55/51","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.2,0.6,1.7,0,16001,132,15186,132,6554,120,22562,221,null,943,null,12.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.650537634000003,"Econo fully open, no compressor, 55/51 ambient, 53.5% inlet 52% outlet Meriam,--adjust code tester speed to match total static of run C-55-OE-DM-SPWCT-SSR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo fully open: with flow meter: new filter drier: with isolation ball valves: with code",74.998000000000005,0.02,62.005000000000003,2.5000000000000001E-2,54.997999999999998,1.0999999999999999E-2,50.999000000000002,1.4999999999999999E-2,74.36,0.05,62.31,0.03,67.260000000000005,0.02,0.01,8.9999999999999993E-3,1.1154999999999999,1.78E-2,16001,132,6554,120,60.728999999999999,0.92800000000000005,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229.8,0.6,229.8,0.6,229.8,0.6,1.7,0,1.7,0,1.7,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,480,480,480,0.8,0.9,0.9,490,0.63,12.1,17.600000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.45,0.21,62.55,0.14000000000000001,62.33,0.05,62.46,0.13,62.26,0.14000000000000001,61.98,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.42,0.03,null,null,55.53,0.11,55.68,0.17,54.68,0.08,54.92,0.08,54.74,7.0000000000000007E-2,54.75,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.15,0.1,54.77,0.09,74.37,0.05,74.38,0.04,74.37,0.03,74.430000000000007,0.06,74.41,0.06,74.47,0.05,74.48,0.04,57.19,0.04,57.07,0.04,57.32,0.05,57.17,0.04,57.12,0.04,58.78,0.1,57.75,0.09,56.51,7.0000000000000007E-2,70.09,0.09,66.39,0.09,56.32,0.13,56.24,0.09,74,0.05,72.44,0.05,62.87,0.09,63.7,0.13,72.98,0.05,71.28,7.0000000000000007E-2,65.260000000000005,7.0000000000000007E-2,64.8,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.998000000000005,0.02,62.005000000000003,2.5000000000000001E-2,62.293999999999997,8.9999999999999993E-3,55.341000000000001,1.9E-2,54.997999999999998,1.0999999999999999E-2,50.999000000000002,1.4999999999999999E-2,1145.0999999999999,9.1,1116.2,8.8000000000000007,0.42499999999999999,3.0000000000000001E-3,-2.3E-2,1E-3,0.01,8.9999999999999993E-3,1.1154999999999999,1.78E-2,29.43,1E-3,372,5,371.2,5.0999999999999996,0.59220000000000017,661.01364000000024,13.029,2.3E-2,0.86293408498565971,5197.2904159905675,55.73089921259843,661.02507194202508,3043.9889857503217,2153.3014302402457,7.7283337958786828E-3,23.609018933338163,61.431065915014337,13.029450665619022,13.219580685468605,6.9812817427720121E-3,20.77713662986141,8.7843950558134602E-3,27.61227570903386,7.6693236722884259E-3,23.299834681183661,63.300207076470208,55.851323267363725,23.089792055149413]
[5,"C-MF-75629575-1E3J","30N0006","C-MF-75629575-1E3J","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/11/2014","18:53:52","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,1,15.2,0,17856,38,16991,73,-1179,73,16677,81,null,939,null,8.23,null,112.36,0.01,54.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9961054520000001,"Factory charge, 3 turns, Econo 1-F open unsealed cab, 53.5% inlet 52% outlet Meriam,--adjust code tester speed to match total static of run C-1E3J-SPWCT-SS","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 1F: with flow meter: new filter drier: with isolation ball valves: with code",74.998999999999995,2.1999999999999999E-2,62.000999999999998,2.9000000000000001E-2,94.998999999999995,0.01,75.001999999999995,1.2E-2,74.31,0.06,60.6,0.04,66.14,0.02,1.4E-2,3.0000000000000001E-3,0.81230000000000002,2.8E-3,17856,38,-1179,73,4.9969999999999999,2.7E-2,null,null,10.933792690000001,null,null,null,229.8,1,229.8,1,229.8,1,13.5,0,13.5,0,13.5,0,2974.4,5.6,2974.4,5.6,2974.4,5.6,230,1,230,1,230,1,1.7,0,1.7,0,1.7,0,null,227.8,1,227.8,1,227.8,1,12.8,0,12.8,0,12.8,0,2781.7,4.9000000000000004,null,null,null,null,null,null,null,null,null,228.3,1,0.7,0,169.1,0.9,23,null,3335.8,482,483,483,0.7,0.8,0.8,400,0.62,8.23,15.8,null,null,null,null,null,null,null,null,null,null,null,null,264.87,0.17,182.61,0.04,121.25,0.05,61.36,0.05,244.87,0.22,103.24,0.04,115.48,7.0000000000000007E-2,12.24,7.0000000000000007E-2,78.349999999999994,0.04,65.87,7.0000000000000007E-2,46.14,0.02,null,null,79.13,0.02,69.510000000000005,0.06,46.63,0.01,22.88,0.06,525.11,0.53,40.5,0.01,36497,47,37733,43,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,248.56,0.22,104.19,0.05,116.57,0.06,12.38,7.0000000000000007E-2,247.15,0.19,116.15,0.06,12.99,7.0000000000000007E-2,19.739999999999998,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.06,0.06,61.83,0.05,61.49,0.08,61.64,0.04,60.99,7.0000000000000007E-2,61,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.89,0.05,null,null,87.45,0.27,90.02,0.24,84.71,0.33,87.18,0.47,91.93,0.7,91.95,0.7,null,null,null,null,null,null,null,null,93.58,0.34,null,null,103.16,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.87,0.06,95.19,0.06,74.680000000000007,0.05,74.67,0.05,74.45,0.05,74.86,0.06,74.87,0.06,74.849999999999994,0.06,74.650000000000006,0.06,93.15,0.05,93.03,0.09,92.45,0.17,89.84,0.31,90.76,0.09,91.15,0.15,89.05,0.14000000000000001,87.32,0.1,91.63,0.06,76.2,0.1,76.89,0.12,75.59,7.0000000000000007E-2,82.46,0.16,75.77,0.06,75.3,0.06,75.37,0.05,76.650000000000006,0.12,74.819999999999993,0.04,74.86,0.04,75.010000000000005,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",74.998999999999995,2.1999999999999999E-2,62.000999999999998,2.9000000000000001E-2,60.591000000000001,1.2999999999999999E-2,57.182000000000002,2.1999999999999999E-2,94.998999999999995,0.01,75.001999999999995,1.2E-2,1160.9000000000001,2,1109.9000000000001,2,0.54,4.0000000000000001E-3,-0.13500000000000001,1E-3,1.4E-2,3.0000000000000001E-3,0.81230000000000002,2.8E-3,28.879000000000001,1E-3,3338,9,362,5.6,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.78488247323141469,5281.5786883055225,70.411356850393716,302.40979547537324,1286.8589410359762,3994.7197472695461,1.0034188705276472E-2,30.179813856459628,59.806117526768588,14.099904154153235,13.188102291125183,1.392277047341731E-2,38.159075749154418,8.7815210507553067E-3,27.609374586846183,9.1558588312692767E-3,24.502520833222476,79.906425616874913,65.527170339152875,24.310958334379862,{"$f":"(XZ7-YL7)*XT7","v":30996.822250160672},{"$f":"0.24*(YJ7-YA7)*XT7","v":25478.726120899351},{"$f":"XK7-XM7","v":2976},{"$f":"YO7*3.413/YM7","v":0.32768159000387048},{"$f":"YM7-(XM7-XU7)*3.413","v":30001.630211091066},{"$f":"YN7-(XM7-XU7)*3.413","v":24483.534081829745},{"$f":"YQ7/XK7","v":8.9879059949344118},{"$f":"(YA7-YW7)/(YJ7-YW7)","v":0.22534332360854581},{"$f":"-XZ7+YL7","v":-5.868855522079766},{"$f":"-YJ7+YA7","v":-20.100308090106324},{"$f":"(-(-0.0182984848494437-(YU7/YV7))+SQRT((-0.0182984848494437-(YU7/YV7))^2-4*0.00577826340327261*(6.76723916086377-XZ7+(YU7/YV7)*YJ7)))/(2*0.00577826340327261)","v":53.959049569283586},{"$f":"XT7*(XZ7-YL7)","v":30996.822250160672},{"$f":"XT7*(YG7-YI7)","v":16409.092572820984},{"$f":"XT7*(YI7-YL7)","v":1011.7524113657043},{"$f":"XW7*(YE7-YG7)","v":13575.977265973983},{"$f":"SUM(YY7:ZA7)","v":30996.822250160672},{"$f":"ZB7/YX7","v":1}]
[5,"C-MF-75629575-2E3J","30N0007","C-MF-75629575-2E3J","2 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/11/2014","21:36:24","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.8,15.2,0,16314,38,15548,72,-3297,77,13014,65,null,939,null,8.5,null,112.78,0.01,64.84,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.8929105590000002,"Factory charge, 3 turns, Econo 2-F open unsealed cab, 53.5% inlet 52% outlet--Meriam, adjust code tester speed to match total static of run C-2E3J-SPWCT-SS","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 2F: with flow meter: new filter drier: with isolation ball valves: with code",75.001999999999995,1.9E-2,61.996000000000002,2.9000000000000001E-2,95.001000000000005,1.2E-2,74.998000000000005,1.4999999999999999E-2,74.349999999999994,0.05,61.85,0.04,66.97,0.01,2.3E-2,3.0000000000000001E-3,0.82430000000000003,2.5000000000000001E-3,16314,38,-3297,77,3.8940000000000001,2.1999999999999999E-2,null,null,11.072988334,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,13.5,0,13.5,0,13.5,0,2977.9,6,2977.9,6,2977.9,6,230,0.8,230,0.8,230,0.8,1.7,0,1.7,0,1.7,0,null,227.8,0.9,227.8,0.9,227.8,0.9,12.8,0,12.8,0,12.8,0,2784.7,5.6,null,null,null,null,null,null,null,null,null,228.3,0.9,0.7,0,169.4,0.8,23,null,3340.7,486,487,488,0.7,0.7,0.8,410,0.62,8.5,15.9,null,null,null,null,null,null,null,null,null,null,null,null,265.77999999999997,0.19,183.77,0.04,121.52,0.05,62.25,0.06,245.68,0.23,103.04,0.06,115.74,7.0000000000000007E-2,12.7,0.09,79.34,0.05,68.53,0.04,46.81,0.03,null,null,79.959999999999994,0.03,71.36,0.05,47.2,0.02,24.16,0.06,528.88,0.52,40.44,0.02,37017,46,38259,42,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,249.41,0.22,103.93,0.05,116.84,0.06,12.91,7.0000000000000007E-2,247.94,0.22,116.41,7.0000000000000007E-2,13.51,0.08,21.72,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.5,0.05,62.89,0.04,62.76,0.05,62.65,0.04,62.45,0.05,62.11,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.67,0.06,null,null,94.4,0.1,94.28,0.11,94.78,0.09,94.84,0.09,94.91,0.08,94.94,7.0000000000000007E-2,null,null,null,null,null,null,null,null,94.76,0.08,null,null,102.89,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.7,0.09,95.04,0.08,74.59,0.06,74.63,0.06,74.489999999999995,0.04,74.72,7.0000000000000007E-2,74.73,7.0000000000000007E-2,74.709999999999994,0.08,74.569999999999993,7.0000000000000007E-2,91.72,0.08,91.58,0.08,92.44,0.09,90.63,0.14000000000000001,89.28,0.09,91.15,0.1,91.17,7.0000000000000007E-2,90.26,0.09,90.56,0.08,77.25,0.09,82.42,0.17,79.099999999999994,0.13,84.01,0.14000000000000001,75.75,0.06,75.459999999999994,0.05,75.180000000000007,0.09,77.849999999999994,0.15,75.099999999999994,0.08,75.010000000000005,0.06,75.27,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-2ER-DM",75.001999999999995,1.9E-2,61.996000000000002,2.9000000000000001E-2,61.89,1.4E-2,58.280999999999999,1.7000000000000001E-2,95.001000000000005,1.2E-2,74.998000000000005,1.4999999999999999E-2,1167.7,1.8,1119.5,1.7,0.50700000000000001,3.0000000000000001E-3,-0.107,1E-3,2.3E-2,3.0000000000000001E-3,0.82430000000000003,2.5000000000000001E-3,29.02,4.0000000000000001E-3,3343,9,363.6,5.6,0.32805000000000023,381.4893450000003,13.029,0.108,0.79673231851645698,5298.1523974482152,66.680240787401573,395.01650085314031,1680.9305724448534,3617.221825003362,1.0408672473942447E-2,30.952718391347705,61.093267681483546,14.09992205491044,13.223855175201157,1.3918785867587104E-2,38.155172373345664,8.7775154143059468E-3,27.605722912308682,9.5159398513504929E-3,25.211502216008508,81.387453346457505,66.537298225381051,25.016920203936202,31448.763397403025,25805.205224433837,2979.4,0.32334155945984538,30435.376259210425,24791.818086241237,9.1042106668293226,0.23139562728138224,-5.9357981874115033,-20.294185664973959,54.983510843252986,31448.763397403025,12684.946122122901,1030.9251537611872,17732.892121518944,31448.763397403032,1.0000000000000002]
[5,"C-MF-75629575-3E3J","30N0008","C-MF-75629575-3E3J","3 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/12/2014","5:25:29","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.8,15.2,0,13667,36,12957,60,-6980,61,6681,70,null,937,null,8.6,null,113.31,0.01,82.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.994328358,".","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 3F: with flow meter: new filter drier: with isolation ball valves: with code",75.001999999999995,1.2999999999999999E-2,62.006,1.7000000000000001E-2,94.997,1.0999999999999999E-2,75.001000000000005,1.4E-2,74.489999999999995,0.05,64.09,0.03,68.38,0.01,2.5999999999999999E-2,3.0000000000000001E-3,0.83950000000000002,2.8999999999999998E-3,13667,36,-6980,61,1.994,2.1999999999999999E-2,null,null,11.246268657,null,null,null,229.7,0.8,229.7,0.8,229.7,0.8,13.5,0,13.5,0,13.5,0,2982.8,5.5,2982.8,5.5,2982.8,5.5,230,0.8,230,0.8,230,0.8,1.7,0,1.7,0,1.7,0,null,227.8,0.8,227.8,0.8,227.8,0.8,12.8,0,12.8,0,12.8,0,2789.2,5.0999999999999996,null,null,null,null,null,null,null,null,null,228.3,0.8,0.7,0,170.3,0.8,23,null,3348.5,480,480,480,0.8,0.7,0.9,410,0.63,8.6,16,null,null,null,null,null,null,null,null,null,null,null,null,266.60000000000002,0.2,185.16,0.03,121.8,0.06,63.37,0.05,246.35,0.23,102.77,0.04,115.99,7.0000000000000007E-2,13.22,7.0000000000000007E-2,80.53,0.05,71.86,0.04,47.66,0.03,null,null,81.33,0.03,73.86,0.05,48.16,0.02,25.7,0.05,533.52,0.57999999999999996,40.35,0.01,37675,50,38923,47,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250.12,0.23,103.65,0.05,117.09,7.0000000000000007E-2,13.44,7.0000000000000007E-2,248.68,0.22,116.67,0.06,14.13,7.0000000000000007E-2,24.2,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.74,0.16,65.069999999999993,0.06,64.98,0.11,64.739999999999995,0.08,64.8,0.16,64.19,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.32,0.06,null,null,94.2,0.18,93.9,0.2,94.72,0.11,94.72,0.13,94.89,0.08,94.9,0.08,null,null,null,null,null,null,null,null,94.79,0.08,null,null,102.55,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.93,0.08,95.31,0.06,74.87,0.04,74.86,0.03,74.59,0.03,75.06,0.04,75.06,0.05,75.02,0.04,74.819999999999993,0.04,93.97,0.05,93.41,0.05,93.39,0.05,92.93,0.06,92.96,0.05,90.7,0.09,93.27,0.06,93.26,0.06,89.69,7.0000000000000007E-2,80.42,0.11,90.01,0.14000000000000001,85.57,0.17,84.07,0.11,75.650000000000006,0.03,76.16,0.04,76.010000000000005,0.04,80.83,0.11,75.760000000000005,0.04,75.98,0.03,77.02,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-3ER-DM",75.001999999999995,1.2999999999999999E-2,62.006,1.7000000000000001E-2,64.046999999999997,1.4999999999999999E-2,60.125,1.9E-2,94.997,1.0999999999999999E-2,75.001000000000005,1.4E-2,1173.2,2.1,1134.0999999999999,2,0.47299999999999998,5.0000000000000001E-3,-6.7000000000000004E-2,1E-3,2.5999999999999999E-2,3.0000000000000001E-3,0.83950000000000002,2.8999999999999998E-3,29.361999999999998,2E-3,3350,8,366,5.4,0.45760423957604218,530.36331366863294,13.03,6.0999999999999999E-2,0.8128390381741909,5299.1639501134141,63.019883118110222,578.20387516838696,2460.4681925564328,2838.6957575569813,1.1169869511535644E-2,32.509209987151664,63.234160961825808,14.099850026534137,13.283604859686111,1.3922372875947001E-2,38.15814476468654,8.7841094454878584E-3,27.61293876648655,1.0159014518218041E-2,26.43888495869399,84.332246791834535,68.505616862565788,26.24013719577832,33220.844536682496,26832.531803227415,2984,0.30656631828713393,32186.773397764606,25798.460664309525,9.6079920590342098,0.23708769008313801,-6.2690727913733433,-21.098085830008728,56.677579858608773,33220.844536682496,6221.5036137477209,1053.1969804084026,25946.143942526382,33220.844536682504,1.0000000000000002]
[5,"C-MF-75629575-E3J","30N0009","C-MF-75629575-E3J","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/11/2014","12:31:48","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,1,15,0,19926,38,19005,79,1249,73,21176,85,null,939,null,8.25,null,111.82,0.02,40.880000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.3668069750000003,"Factory charge, 3 turns, closed econo unsealed cab, return and supply Meriam's--set to same as run C-MF-NE3J-SPWCT-SS, adjust code tester speed to match--total static of run C-MF-E3J-SPWCT-SS","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: with economizer: with flow meter: new filter drier: with isolation ball valves: with code",75.001000000000005,1.9E-2,61.999000000000002,2.5000000000000001E-2,95,8.9999999999999993E-3,75.001000000000005,1.7999999999999999E-2,74.41,0.08,59.2,0.05,65.12,0.02,2.7E-2,3.0000000000000001E-3,0.81389999999999996,2.7000000000000001E-3,19926,38,1249,73,6.367,0.03,null,null,10.769993986999999,null,null,null,229.7,1,229.7,1,229.7,1,13.4,0,13.4,0,13.4,0,2962,6.3,2962,6.3,2962,6.3,229.9,1,229.9,1,229.9,1,1.6,0,1.6,0,1.6,0,null,227.8,1,227.8,1,227.8,1,12.7,0,12.7,0,12.7,0,2769.4,6,null,null,null,null,null,null,null,null,null,228.3,1,0.7,0,169.3,0.9,23,null,3324.8,475,478,478,0.7,0.7,0.8,400,0.62,8.25,15.8,null,null,null,null,null,null,null,null,null,null,null,null,263.3,0.2,180.58,0.05,120.82,0.06,59.77,0.06,243.42,0.22,103.44,0.06,115.06,7.0000000000000007E-2,11.62,0.08,76.92,0.04,62.46,0.11,45.26,0.03,null,null,77.53,0.02,66.739999999999995,0.1,45.64,0.01,21.09,0.1,520.11,0.55000000000000004,40.57,0.02,35821,50,37060,46,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,247.06,0.22,104.26,0.05,116.14,7.0000000000000007E-2,11.88,7.0000000000000007E-2,245.66,0.22,115.73,0.06,12.31,7.0000000000000007E-2,17.21,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.28,0.05,60.34,0.08,59.66,0.11,60.21,0.06,59.05,7.0000000000000007E-2,59.54,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.44,0.06,null,null,null,null,null,null,null,null,null,null,null,null,104.11,0.06,null,null,94.75,7.0000000000000007E-2,94.76,0.06,94.91,0.05,94.89,7.0000000000000007E-2,94.78,0.08,94.81,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,103.42,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.83,0.09,95.13,0.09,74.61,0.08,74.62,7.0000000000000007E-2,74.459999999999994,0.06,74.72,0.09,74.709999999999994,0.09,74.709999999999994,0.1,74.59,0.08,86.86,0.11,82.29,0.11,80.52,0.1,84.64,0.15,84.1,0.09,86.45,0.11,77.540000000000006,0.08,82.79,0.1,92.09,0.05,79.239999999999995,0.15,75,7.0000000000000007E-2,74.989999999999995,7.0000000000000007E-2,82.59,0.18,74.959999999999994,0.06,74.900000000000006,0.06,74.97,0.06,76.040000000000006,0.09,74.81,0.05,74.760000000000005,0.06,74.83,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.001000000000005,1.9E-2,61.999000000000002,2.5000000000000001E-2,59.058999999999997,1.2999999999999999E-2,55.828000000000003,1.7999999999999999E-2,95,8.9999999999999993E-3,75.001000000000005,1.7999999999999999E-2,1158.9000000000001,2,1114.7,1.9,0.56499999999999995,5.0000000000000001E-3,-0.17599999999999999,1E-3,2.7E-2,3.0000000000000001E-3,0.81389999999999996,2.7000000000000001E-3,28.974,2E-3,3326,9,363.1,5.7,0.16622533100174824,191.8074094429173,13.029,0.182,0.77705562905072711,5289.4334997055639,73.989748503936994,196.21798309058644,834.97485755236892,4454.4586421531949,9.59141929851773E-3,29.273324796924747,58.281944370949269,14.099920349633747,13.145831213091272,1.392165457242138E-2,38.15809089120382,8.7797297372362235E-3,27.607902149657605,8.7157318646476287E-3,23.65009713762937,78.182834462527424,64.31391801682571,23.46059674848021,30746.03846412068,25263.464333844484,2962.9,0.32890018373588892,29759.305175764617,24276.731045488421,8.9474759999292299,0.22116040710729296,-5.8127280484445372,-19.900890091578155,52.630859096632406,30746.03846412068,20934.546415924728,1002.3497065728066,8809.1423416231573,30746.038464120691,1.0000000000000004]
[5,"C-MF-75629575-OE3J","30N0011","C-MF-75629575-OE3J","Fully open","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/12/2014","7:42:47","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.9,15.1,0,10435,28,9786,47,-10648,115,-223,126,null,940,null,7.3,null,111.71,0.1,93.61,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-6.6726511000000002E-2,"Factory charge, 3 turns, Econo fully open unsealed cab, 53.5% inlet 52% outlet Meriam, CT-SS--adjust code tester speed to match total static of run C-OE3J-SPWCT-SS","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo Fully open: with flow meter: new filter drier: with isolation ball valves: with code",74.995999999999995,0.01,62.002000000000002,2.8000000000000001E-2,95,1.2E-2,74.998999999999995,1.7000000000000001E-2,74.5,0.04,66.19,0.05,69.989999999999995,0.03,1.4999999999999999E-2,3.0000000000000001E-3,0.77710000000000001,2.5999999999999999E-3,10435,28,-10648,115,5.0000000000000001E-3,4.0000000000000001E-3,null,null,11.080490724000001,null,null,null,229.8,0.9,229.8,0.9,229.8,0.9,13.5,0,13.5,0,13.5,0,2981.6,5.6,2981.6,5.6,2981.6,5.6,230,0.9,230,0.9,230,0.9,1.6,0,1.6,0,1.6,0,null,227.8,0.9,227.8,0.9,227.8,0.9,12.8,0,12.8,0,12.8,0,2788,5.3,null,null,null,null,null,null,null,null,null,228.3,0.9,0.8,0,170.6,0.8,23,null,3341,480,480,480,0.7,0.7,0.8,390,0.62,7.3,15.3,null,null,null,null,null,null,null,null,null,null,null,null,266.79000000000002,0.19,184.19,0.05,121.86,0.05,62.33,7.0000000000000007E-2,246.5,0.22,102.57,0.05,116.05,0.06,13.47,7.0000000000000007E-2,80.819999999999993,0.06,63.15,0.52,47.87,0.04,null,null,81.44,0.03,72.95,0.1,48.26,0.02,24.69,0.11,535.73,0.52,40.29,0.02,37031,73,38260,72,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250.3,0.21,103.53,0.05,117.16,0.06,13.64,7.0000000000000007E-2,248.89,0.21,116.75,0.06,14.41,0.08,15.28,0.54,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65.8,0.14000000000000001,67.489999999999995,0.06,67.14,0.14000000000000001,67.12,0.08,67.06,0.16,66.41,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.11,0.06,null,null,93.82,0.26,93.4,0.27,94.47,0.18,94.53,0.17,94.77,0.12,94.77,0.12,null,null,null,null,null,null,null,null,94.7,0.12,null,null,102.33,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.93,0.08,95.33,7.0000000000000007E-2,74.91,0.03,74.89,0.04,74.61,0.03,75.099999999999994,0.04,75.09,0.04,75.069999999999993,0.05,74.86,0.04,93.87,7.0000000000000007E-2,93.47,7.0000000000000007E-2,92.99,0.09,92.82,0.08,92.54,0.08,91.96,0.13,92.14,0.23,94.02,0.11,79.84,0.09,82.5,0.13,94.07,0.22,94.08,0.1,75.7,0.02,76.930000000000007,0.03,85.6,0.09,84.58,0.09,76.349999999999994,0.03,77.39,0.04,83.07,7.0000000000000007E-2,83.84,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-OER-DM",74.995999999999995,0.01,62.002000000000002,2.8000000000000001E-2,66.16,1.4E-2,62.017000000000003,2.1999999999999999E-2,95,1.2E-2,74.998999999999995,1.7000000000000001E-2,1128.5,1.9,1090,1.9,0.41299999999999998,4.0000000000000001E-3,-2.8000000000000001E-2,1E-3,1.4999999999999999E-2,3.0000000000000001E-3,0.77710000000000001,2.5999999999999999E-3,29.462,2E-3,3342,8,359.4,5.5,0.59220000000000017,661.01364000000024,13.029,2.3E-2,0.85871120246707189,5074.5882226513277,52.886113385826761,758.7139746663928,3228.5916611936696,1845.9965614576581,1.2051196918818976E-2,34.319804273706481,65.301288797532919,14.099905859000126,13.342954547083124,1.3919901703093901E-2,38.156157160819127,8.7828892687881119E-3,27.610140128423488,1.0888487816409873E-2,27.750935338357426,87.76613062110043,70.692672978660397,27.540693220254479,34401.197111892965,27359.957217984156,2982.6,0.29590870826064269,33355.065216878793,26313.825322969984,9.9805700828482333,0.23115127483004333,-6.7791110534520023,-22.464841823567511,58.547324517726089,34401.197111892965,-714.47771413648081,1066.8921764304844,34048.782649598972,34401.197111892972,1.0000000000000002]
[5,"C-95-3+10-C","30N0016","C-95-3+10-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","10:38:37","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","6.1 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,6.1,null,5.5,null,230.3,0.9,15.4,0,20231,42,19565,69,1542,116,21774,123,null,945,null,12.17,5.9415565350000001,109.77,0.01,42.85,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.3947136560000004,"Closed damper, +10% charge 95F Test, adjust code tester speed to match total--static of run C-95-FC3-EC-SPWCT-SS","R22 6.1  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75.001999999999995,1.7999999999999999E-2,62.002000000000002,0.04,94.995000000000005,8.0000000000000002E-3,74.998999999999995,1.4E-2,74.56,0.06,58.77,0.04,65.12,0.02,1.7999999999999999E-2,3.0000000000000001E-3,1.1047,3.3E-3,20231,42,1542,116,6.3940000000000001,3.9E-2,null,null,11.188839940999999,null,null,null,229.8,0.9,229.8,0.9,229.8,0.9,13.7,0,13.7,0,13.7,0,3036.9,4.9000000000000004,3036.9,4.9000000000000004,3036.9,4.9000000000000004,230,0.9,230,0.9,230,0.9,1.7,0,1.7,0,1.7,0,null,227.7,0.9,227.7,0.9,227.7,0.9,13,0,13,0,13,0,2843.1,4.5999999999999996,null,null,null,null,null,null,null,null,null,228.2,0.9,0.7,0,168.9,0.8,23,null,3402,480,480,480,0.8,0.8,1,490,0.65,12.17,17.600000000000001,null,null,null,null,null,null,null,null,null,null,null,null,273.51,0.15,161.58000000000001,0.08,123.66,0.04,37.92,0.08,252.77,0.24,101.43,0.05,117.81,7.0000000000000007E-2,16.38,0.08,78.8,0.04,51.81,0.04,46.46,0.03,null,null,79,0.04,51.97,0.05,46.59,0.03,5.39,0.04,563.47,0.45,39.93,0.01,38098,38,39351,34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,256.81,0.23,102.25,0.04,118.98,0.06,16.72,7.0000000000000007E-2,255.38,0.24,118.56,7.0000000000000007E-2,16.59,0.08,5.35,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.76,0.04,60.16,0.05,59.36,0.1,59.96,0.04,58.79,7.0000000000000007E-2,59.11,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102.04,0.04,null,null,null,null,95.06,0.16,95.19,0.13,95.29,0.11,95.27,0.08,95.3,0.08,null,null,null,null,null,null,null,null,null,null,null,null,101.98,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.87,0.09,95.35,0.08,75.03,7.0000000000000007E-2,74.97,0.06,74.739999999999995,0.04,75.209999999999994,7.0000000000000007E-2,75.17,0.08,75.150000000000006,0.08,74.97,0.06,91.9,0.11,84,0.13,81.05,0.08,86.69,0.14000000000000001,85.3,0.16,86.11,0.13,78.08,7.0000000000000007E-2,83.29,0.11,92.88,0.08,79.290000000000006,0.16,75.260000000000005,0.05,75.34,0.05,83.55,0.22,75.22,0.06,75.27,0.05,74.98,0.05,76.16,0.08,75.040000000000006,0.05,75.03,0.04,75.11,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.001999999999995,1.7999999999999999E-2,62.002000000000002,0.04,58.664999999999999,1.2E-2,55.579000000000001,1.7000000000000001E-2,94.995000000000005,8.0000000000000002E-3,74.998999999999995,1.4E-2,1146.4000000000001,1.7,1103.2,1.6,0.56899999999999995,4.0000000000000001E-3,-0.17699999999999999,1E-3,1.7999999999999999E-2,3.0000000000000001E-3,1.1047,3.3E-3,28.984999999999999,1E-3,3405,8,367,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,0.79616051392567244,5236.5205553227852,73.74483729133857,196.77371201265697,837.34749580660332,4399.1730595161816,9.6033253931568259E-3,29.296444875631597,57.868839486074329,14.099788653916594,13.135439701479426,1.3921098870557112E-2,38.1562469471817,8.7814716584099315E-3,27.61005223374482,8.6636396803538938E-3,23.497385776155976,78.224078440358738,64.345204467687623,23.303244697181565,31383.515926617772,25581.75052622817,3038,0.33038662794329693,30382.636056293111,24580.870655903509,8.9229474467821177,0.20979739176248913,-5.9932001784500315,-20.35523895428441,52.464559625702734,31383.515926617772,21536.062442350525,1016.623750682048,8830.8297335852094,31383.51592661778,1.0000000000000002]
[5,"C-95-3+40-C","30N0017","C-95-3+40-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","5:37:43","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","7.7 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,7.7,null,5.5,null,230.3,1,15.5,0,19797,34,19133,74,910,104,20707,111,null,943,null,12.3,5.7784588440000002,109.8,0.01,49.29,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.0440747229999996,"Closed Damper, +40% charge, 95F Test, adjust code tester speed to match total static--of run C-95-FC3-EC-SPWCT-SS","R22 7.7  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",74.998000000000005,1.2E-2,62.000999999999998,0.04,95,6.0000000000000001E-3,75.001999999999995,1.4999999999999999E-2,74.53,0.06,59.05,0.04,65.34,0.02,1.9E-2,3.0000000000000001E-3,1.1039000000000001,3.8E-3,19797,34,910,104,6.0430000000000001,3.4000000000000002E-2,null,null,11.918272036999999,null,null,null,229.7,1,229.7,1,229.7,1,13.8,0,13.8,0,13.8,0,3058.4,6,3058.4,6,3058.4,6,229.9,1,229.9,1,229.9,1,1.7,0,1.7,0,1.7,0,null,227.7,1,227.7,1,227.7,1,13.1,0,13.1,0,13.1,0,2864.4,5.5,null,null,null,null,null,null,null,null,null,228.2,1,0.7,0,168.9,0.9,23,null,3423.1,480,480,480,0.8,0.8,1,490,0.63,12.3,17.7,null,null,null,null,null,null,null,null,null,null,null,null,281.17,0.18,140.69999999999999,0.08,125.74,0.05,14.97,7.0000000000000007E-2,260.14,0.18,99.68,0.04,119.92,0.05,20.25,0.06,79.73,0.04,52.29,0.04,47.04,0.03,null,null,79.91,0.05,52.03,0.05,47.15,0.03,4.88,0.04,597.61,0.49,39.380000000000003,0.01,40832,41,42084,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,264.51,0.21,100.58,0.03,121.16,0.06,20.57,0.06,262.98,0.19,120.73,0.05,20.309999999999999,0.06,5.25,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.1,0.05,60.43,0.05,59.64,0.12,60.22,0.04,59.1,0.09,59.39,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100.42,0.04,null,null,null,null,95.03,0.08,95.21,7.0000000000000007E-2,95.25,7.0000000000000007E-2,95.24,7.0000000000000007E-2,95.28,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,100.42,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.84,7.0000000000000007E-2,95.3,7.0000000000000007E-2,74.98,0.05,74.94,0.04,74.709999999999994,0.03,75.13,0.06,75.099999999999994,0.06,75.09,0.05,74.92,0.04,91.96,0.09,84.4,0.11,80.930000000000007,0.09,86.66,0.14000000000000001,85.38,0.14000000000000001,86.12,0.11,78.069999999999993,0.06,83.19,0.09,93.06,0.05,79.27,0.15,75.23,0.04,75.3,0.04,83.63,0.21,75.2,0.05,75.28,0.05,74.989999999999995,0.05,76.2,0.08,75.05,0.04,75.03,0.04,75.11,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.998000000000005,1.2E-2,62.000999999999998,0.04,58.981000000000002,1.2E-2,55.905999999999999,0.02,95,6.0000000000000001E-3,75.001999999999995,1.4999999999999999E-2,1146.5999999999999,1.9,1102,1.9,0.56799999999999995,5.0000000000000001E-3,-0.17699999999999999,1E-3,1.9E-2,3.0000000000000001E-3,1.1039000000000001,3.8E-3,28.968,2E-3,3426,9,366.8,5.3,0.16622533100174824,191.8074094429173,13.029,0.182,0.79658821026768123,5233.8817521800547,73.53515842519684,196.77468152800697,837.34337016785651,4396.5383820121979,9.6042047861456606E-3,29.297179568106021,58.184411789732323,14.099927595191508,13.144355042286652,1.39225310385042E-2,38.159057791057066,8.7817573187407936E-3,27.609389235697552,8.7798253015200101E-3,23.700756881905104,78.22314139738009,64.346153189697162,23.506470417477271,30307.886955657879,25171.281895281078,3059.2,0.34449942403691269,29306.974051363075,24170.368990986273,8.5542831440055682,0.20762981215137369,-5.79070915062875,-20.038729607647767,52.933535711866909,30307.886955657879,20457.319552494871,1016.8723808644147,8833.6950222985979,30307.886955657883,1.0000000000000002]
[5,"C-95-3-10-C","30N0018","C-95-3+10-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","10:38:37","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","4.95 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,6.1,null,5.5,null,230.3,1,14.9,0,19376,34,18738,62,1101,97,20478,101,null,944,null,12.8,5.9037172460000003,112.55,0.01,41.7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.2394881169999996,"Closed Damper, -10% charge, 95F Test, adjust code tester speed to match total--static of run C-95-FC3-EC-SPWCT-SS","R22 4.95  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75.001999999999995,1.0999999999999999E-2,62.006999999999998,4.3999999999999997E-2,94.995999999999995,8.0000000000000002E-3,74.992000000000004,1.2E-2,74.59,0.05,59.64,0.05,65.67,0.02,3.5000000000000003E-2,3.0000000000000001E-3,1.1374,4.1999999999999997E-3,19376,34,1101,97,6.2389999999999999,3.5000000000000003E-2,null,null,10.702315661,null,null,null,229.8,1,229.8,1,229.8,1,13.2,0,13.2,0,13.2,0,2912.7,5.6,2912.7,5.6,2912.7,5.6,230,1,230,1,230,1,1.7,0,1.7,0,1.7,0,null,227.8,1,227.8,1,227.8,1,12.5,0,12.5,0,12.5,0,2720.9,5,null,null,null,null,null,null,null,null,null,228.3,1,0.7,0,168.8,0.9,23,null,3281.2,480,480,480,0.8,0.9,1,510,0.65,12.8,17.899999999999999,null,null,null,null,null,null,null,null,null,null,null,null,260.05,0.13,183.21,0.04,119.89,0.04,63.31,0.05,240.38,0.18,104.21,0.05,114.15,0.05,9.94,0.06,76.16,0.05,66.290000000000006,0.06,44.76,0.03,null,null,76.010000000000005,0.04,69.260000000000005,7.0000000000000007E-2,44.66,0.03,24.6,7.0000000000000007E-2,507.13,0.46,40.81,0.02,35125,42,36383,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243.88,0.19,104.72,0.05,115.2,0.06,10.47,7.0000000000000007E-2,242.53,0.19,114.79,0.06,10.119999999999999,0.08,21.53,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.68,0.05,60.83,7.0000000000000007E-2,60.05,7.0000000000000007E-2,60.69,0.06,59.47,0.06,59.96,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.59,0.04,null,null,null,null,95.09,7.0000000000000007E-2,95.22,0.06,95.26,0.08,96.07,0.08,96.09,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,104.67,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.7,0.09,95.18,0.09,74.89,0.08,74.88,0.06,74.72,0.04,75,0.09,74.98,0.1,75,0.09,74.87,7.0000000000000007E-2,91.72,0.09,83.9,0.12,81.17,0.11,86.97,0.15,85.25,0.15,85.91,0.13,78.19,0.06,83.6,0.11,92.99,0.06,79.489999999999995,0.15,75.45,0.05,75.489999999999995,0.04,83.76,0.2,75.41,0.04,75.37,0.04,74.849999999999994,0.06,76.03,0.09,74.94,0.06,75.010000000000005,0.04,75.099999999999994,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.001999999999995,1.0999999999999999E-2,62.006999999999998,4.3999999999999997E-2,59.543999999999997,1.7999999999999999E-2,56.076999999999998,0.03,94.995999999999995,8.0000000000000002E-3,74.992000000000004,1.2E-2,1164.8,2.1,1118,2.1,0.56799999999999995,4.0000000000000001E-3,-0.18,1E-3,3.5000000000000003E-2,3.0000000000000001E-3,1.1374,4.1999999999999997E-3,28.943999999999999,1E-3,3282,8,368.5,5.3,0.16622533100174824,191.8074094429173,13.029,0.182,0.78666997551412743,5311.2974679365198,74.602819527559049,198.43408720800869,844.41466128246338,4466.8828066540564,9.6003531009551321E-3,29.288690894292746,58.757330024485867,14.099761383107788,13.158366749726039,1.391472503662552E-2,38.149461653352873,8.784768928637306E-3,27.613660439482612,8.7470023529526795E-3,23.802378686081063,78.205667320648629,64.334622065090983,23.610522726125364,30158.440214105161,24791.017112804318,2913.5,0.32971783120763909,29155.36913715272,23787.946035851877,8.8834153373408657,0.23837034919243971,-5.6781681681673817,-19.448337296162762,52.670504298119795,30158.440214105161,20242.851126434303,1019.0040743212359,8896.5850133496224,30158.440214105161,1]
[5,"C-95-3-40-C","30N0019","C-95-3+40-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","5:37:43","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","3.3 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,7.7,null,5.5,null,230.3,1,14.1,0,14400,27,13831,58,-1373,72,13026,73,null,942,null,16.899999999999999,null,114.13,0.01,52.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.1763385700000004,"Closed Damper, -40% charge, 95F Test, adjust code tester speed--to match total static of run C-95-FC3-EC-SPWCT-SS","R22 3.3  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",74.998000000000005,1.7000000000000001E-2,61.999000000000002,3.9E-2,95.001000000000005,7.0000000000000001E-3,75.001999999999995,1.4999999999999999E-2,74.58,0.05,64.150000000000006,0.04,68.42,0.01,0.13900000000000001,2E-3,1.2959000000000001,2.7000000000000001E-3,14400,27,-1373,72,4.1769999999999996,2.5999999999999999E-2,null,null,8.7252324459999997,null,null,null,229.8,1,229.8,1,229.8,1,12.4,0,12.4,0,12.4,0,2739.1,6,2739.1,6,2739.1,6,229.9,1,229.9,1,229.9,1,1.7,0,1.7,0,1.7,0,null,227.9,1,227.9,1,227.9,1,11.7,0,11.7,0,11.7,0,2549.1999999999998,5.4,null,null,null,null,null,null,null,null,null,228.4,1,0.7,0,169.4,0.9,23,null,3120.2,478,478,479,1,1,1.2,600,0.64,16.899999999999999,19.899999999999999,null,null,null,null,null,null,null,null,null,null,null,null,239.37,0.14000000000000001,196.34,0.09,113.87,0.04,82.47,0.09,222.46,0.24,108.2,0.06,108.65,0.08,0.45,0.09,61.14,0.06,70.72,0.03,34.409999999999997,0.04,null,null,60.93,0.05,73.73,0.03,34.25,0.04,39.479999999999997,0.05,395.66,2.38,42.08,0.02,27214,175,28508,174,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,225.51,0.16,107.84,0.03,109.61,0.05,1.77,0.05,224.31,0.24,109.23,7.0000000000000007E-2,0.43,7.0000000000000007E-2,36.299999999999997,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.19,0.06,65.67,7.0000000000000007E-2,64.7,7.0000000000000007E-2,65.53,0.06,63.77,0.05,64.88,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,109,0.04,null,null,null,null,94.63,0.11,94.8,0.11,94.87,0.09,94.92,0.08,94.95,0.08,null,null,null,null,null,null,null,null,null,null,null,null,108.8,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.64,7.0000000000000007E-2,95.01,7.0000000000000007E-2,74.78,7.0000000000000007E-2,74.81,0.05,74.67,0.04,74.849999999999994,0.09,74.84,0.09,74.89,0.08,74.790000000000006,0.06,87.53,0.77,83.16,0.19,80.790000000000006,0.12,86.54,0.19,84.81,0.14000000000000001,85.46,0.17,78.34,0.08,83.59,0.12,92.9,0.06,78.28,0.37,75.52,0.05,75.540000000000006,0.05,84.57,0.28000000000000003,75.400000000000006,0.04,75.37,0.04,74.87,0.08,76.08,0.11,74.930000000000007,0.08,74.98,0.05,75.099999999999994,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.998000000000005,1.7000000000000001E-2,61.999000000000002,3.9E-2,64.144000000000005,1.2999999999999999E-2,58.517000000000003,2.9000000000000001E-2,95.001000000000005,7.0000000000000001E-3,75.001999999999995,1.4999999999999999E-2,1243.9000000000001,1.3,1193.0999999999999,1.3,0.54100000000000004,3.0000000000000001E-3,-0.19500000000000001,1E-3,0.13900000000000001,2E-3,1.2959000000000001,2.7000000000000001E-3,29.084,2E-3,3119,9,378.6,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,0.7657819504624005,5620.9012747345732,75.829678204724402,206.53813527589801,878.88873406138271,4742.0125406731904,9.5844229007407203E-3,29.257723766412717,63.378218049537608,14.099951036223416,13.277941801873103,1.392229160379788E-2,38.159039832975218,8.7804385375080674E-3,27.607946094565659,9.1272422656815105E-3,25.338507319471187,78.150348046487466,64.292701047453406,25.15161632340147,23080.024560619036,19927.844239296068,2740.4,0.40524156182913262,22046.66945233176,18894.489131008791,7.0685057557972941,0.39475633417329642,-4.106107443011247,-14.772129996949857,53.743434218198864,23080.024560619036,12756.291303860582,1050.4958380446885,9273.2374187137593,23080.024560619029,0.99999999999999967]
[5,"C-95-3-FC-C","30N0020","C-95-3-FC-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/17/2014","23:01:06","10 Ton","0:30:08","75/62 - 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.8,15.1,0,19903,39,19222,57,1384,112,21288,117,null,944,null,12.6,5.9661270980000003,111.39,0.05,40.85,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.3812949640000003,"Closed damper, 5.5 lbs factory charge 95F test, adjust code tester speed to match--total static of run C -95-FC3-EC-SPWCT-SS","R22 5.5  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",74.992000000000004,1.0999999999999999E-2,62.005000000000003,4.3999999999999997E-2,94.995999999999995,1.4E-2,75,1.4E-2,74.55,0.04,59.18,0.03,65.48,0.03,0.03,3.0000000000000001E-3,1.1257999999999999,3.5999999999999999E-3,19903,39,1384,112,6.383,3.6999999999999998E-2,null,null,10.790167866000001,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,13.4,0,13.4,0,13.4,0,2965.5,4.4000000000000004,2965.5,4.4000000000000004,2965.5,4.4000000000000004,230,0.8,230,0.8,230,0.8,1.7,0,1.7,0,1.7,0,null,227.8,0.8,227.8,0.8,227.8,0.8,12.7,0,12.7,0,12.7,0,2772.5,4,null,null,null,null,null,null,null,null,null,228.3,0.8,0.7,0,169.3,0.8,23,null,3334.4,489,490,491,0.8,0.8,1,490,0.63,12.6,17.899999999999999,null,null,null,null,null,null,null,null,null,null,null,null,264.19,0.15,178.57,7.0000000000000007E-2,121.08,0.04,57.49,7.0000000000000007E-2,244.25,0.21,103.13,0.02,115.32,0.06,12.19,0.06,77.42,0.05,60.24,0.28999999999999998,45.61,0.03,null,null,77.72,0.05,64.91,0.18,45.8,0.03,19.11,0.17,525.32000000000005,0.43,40.47,0.01,35996,51,37255,49,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,247.9,0.25,103.82,0.03,116.4,7.0000000000000007E-2,12.59,7.0000000000000007E-2,246.44,0.21,115.97,0.06,12.37,7.0000000000000007E-2,14.64,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.19,0.04,60.38,0.05,59.64,7.0000000000000007E-2,60.25,0.04,59.06,0.05,59.53,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.54,0.04,null,null,null,null,95.02,0.08,95.17,0.06,95.12,0.06,95.16,0.05,95.2,0.05,null,null,null,null,null,null,null,null,null,null,null,null,103.61,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.67,7.0000000000000007E-2,95.14,7.0000000000000007E-2,74.83,0.04,74.84,0.03,74.66,0.03,74.959999999999994,0.04,74.930000000000007,0.04,74.97,0.04,74.819999999999993,0.04,86.79,0.09,83.29,0.12,80.63,7.0000000000000007E-2,86.33,0.14000000000000001,84.49,0.08,86.11,0.12,78.12,0.06,83.37,0.1,93.01,0.05,79.150000000000006,0.16,75.38,0.04,75.45,0.04,83.12,0.2,75.38,0.04,75.41,0.03,74.92,0.05,75.98,0.08,75.02,0.04,75.09,0.04,75.180000000000007,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.992000000000004,1.0999999999999999E-2,62.005000000000003,4.3999999999999997E-2,59.082999999999998,1.7000000000000001E-2,55.792999999999999,2.1999999999999999E-2,94.995999999999995,1.4E-2,75,1.4E-2,1156,1.9,1115,1.8,0.57099999999999995,4.0000000000000001E-3,-0.18,1E-3,0.03,3.0000000000000001E-3,1.1257999999999999,3.5999999999999999E-3,29.07,1E-3,3336,7,369.6,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,0.79437222629433291,5276.035189513791,74.795604724409444,198.4344950389648,844.41292580578352,4431.6222637080073,9.607801117802444E-3,29.300031018275568,58.288627773705663,14.099819340136801,13.146235290062918,1.3921735863287198E-2,38.157195844658276,8.78581268029467E-3,27.612363608839818,8.6895992231823763E-3,23.627537746157557,78.218682476409612,64.349818616153101,23.433823579178366,30950.31687766442,25236.400785696202,2966.4,0.3271153326157481,29944.149476588827,24230.233384620609,8.9760639917832208,0.22537259874345683,-5.8662074390972023,-19.930054702703949,52.490113269620785,30950.31687766442,21024.081475596256,1022.0427616895638,8904.1926403786056,30950.316877664427,1.0000000000000002]
[5,"C-95-3+10-1","30N0039","C-95-3+10-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","11:54:44","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","6.1 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,6.1,null,5.5,null,230.3,1,15.5,0,18714,36,18080,63,-1097,109,17616,120,null,945,null,13.3,5.4591598599999998,109.98,0.01,54.29,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.138856476,"1 Finger Open, +10% charge 95F Test, adjust code tester speed to match total--static of run C-95-FC3-1F-SPWCT-SS","R22 6.1  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",74.995999999999995,1.6E-2,61.991999999999997,4.1000000000000002E-2,95,8.0000000000000002E-3,75.003,1.7000000000000001E-2,74.64,0.05,60.27,0.03,65.98,0.02,3.2000000000000001E-2,3.0000000000000001E-3,1.1537999999999999,3.5999999999999999E-3,18714,36,-1097,109,5.1390000000000002,3.6999999999999998E-2,null,null,11.240665111,null,null,null,229.7,1,229.7,1,229.7,1,13.8,0,13.8,0,13.8,0,3056.6,5.9,3056.6,5.9,3056.6,5.9,230,1,230,1,230,1,1.7,0,1.7,0,1.7,0,null,227.7,1,227.7,1,227.7,1,13.1,0,13.1,0,13.1,0,2862.5,5.5,null,null,null,null,null,null,null,null,null,228.2,1,0.7,0,168.8,0.9,23,null,3424.5,480,480,480,0.9,0.9,1,510,0.65,13.3,18.2,null,null,null,null,null,null,null,null,null,null,null,null,275.74,0.18,167.51,0.06,124.27,0.05,43.24,7.0000000000000007E-2,254.7,0.28000000000000003,101.63,0.04,118.37,0.08,16.739999999999998,0.08,80.58,0.05,53.55,0.05,47.58,0.03,null,null,81.28,0.05,53.97,0.06,48.01,0.03,5.95,0.05,568.64,0.47,39.99,0.01,38533,40,39795,35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,258.81,0.27,102.51,0.04,119.55,0.08,17.03,0.08,257.39999999999998,0.28000000000000003,119.14,0.08,17.02,0.08,5.97,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.47,0.06,61.19,0.05,60.71,0.09,61.02,0.05,60.36,0.08,60.39,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101.98,0.04,null,null,null,null,95.16,0.08,95.27,7.0000000000000007E-2,95.34,7.0000000000000007E-2,96.18,7.0000000000000007E-2,96.18,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,102.12,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.68,7.0000000000000007E-2,95.18,7.0000000000000007E-2,74.88,0.06,74.86,0.05,74.680000000000007,0.03,74.98,0.06,74.959999999999994,7.0000000000000007E-2,75,7.0000000000000007E-2,74.849999999999994,0.05,93.22,0.04,93.33,0.05,92.22,0.08,89.16,0.11,89.17,0.13,90.94,0.1,88.52,0.13,87.49,0.09,92.22,7.0000000000000007E-2,76.22,0.08,76.540000000000006,0.11,75.78,0.06,81.73,0.16,75.819999999999993,0.05,75.48,0.04,75.72,0.05,76.83,0.12,75.03,0.05,75.05,0.04,75.13,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",74.995999999999995,1.6E-2,61.991999999999997,4.1000000000000002E-2,60.12,0.01,56.953000000000003,2.1999999999999999E-2,95,8.0000000000000002E-3,75.003,1.7000000000000001E-2,1172.8,1.9,1125.9000000000001,1.8,0.54300000000000004,4.0000000000000001E-3,-0.14199999999999999,1E-3,3.2000000000000001E-2,3.0000000000000001E-3,1.1537999999999999,3.5999999999999999E-3,28.983000000000001,2E-3,3428,8,370.2,5.2,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.79427324784639586,5340.6349990013023,71.823200031496071,310.1513065335501,1319.7988928303528,4020.8361061709493,1.0048270445902056E-2,30.211837253799192,59.325726752153599,14.099934840909903,13.175961287966469,1.3923407525533815E-2,38.160024714018391,8.7762957888364405E-3,27.602924895022394,9.1300780100550556E-3,24.359524497412654,79.974260743349802,65.569593794566217,24.165679129068444,32290.323690433117,26466.307994748116,3057.8,0.32320120107969147,31271.963672140613,25447.947976455613,9.1225098226781256,0.20721643824800853,-6.0461581247307485,-20.648533991196203,53.928647555351162,32290.323690433117,17321.817679249318,1035.2573585733862,13933.248652610435,32290.323690433135,1.0000000000000007]
[5,"C-95-3+20-1","30N0040","C-95-3+20-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","8:44:20","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","6.6 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,6.6,null,5.5,null,230.3,1,15.7,0,18437,38,17795,65,-1220,117,17216,116,null,944,null,12.5,5.319388344,109.93,0.01,57.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.9671090590000002,"1 Finger Open, +20% charge 95F Test, adjust code tester speed to match total--static of run C-95-FC3-1F-SPWCT-SS","R22 6.6  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",74.998000000000005,0.02,62,4.2000000000000003E-2,94.998999999999995,8.9999999999999993E-3,75,1.9E-2,74.62,0.06,60.3,0.03,66.08,0.01,1.7000000000000001E-2,3.0000000000000001E-3,1.1261000000000001,3.5000000000000001E-3,18437,38,-1220,117,4.9669999999999996,3.5000000000000003E-2,null,null,11.616849394000001,null,null,null,229.8,1,229.8,1,229.8,1,14,0,14,0,14,0,3097,5.2,3097,5.2,3097,5.2,230,1,230,1,230,1,1.7,0,1.7,0,1.7,0,null,227.7,1,227.7,1,227.7,1,13.3,0,13.3,0,13.3,0,2902.5,4.8,null,null,null,null,null,null,null,null,null,228.2,1,0.7,0,168.9,0.9,23,null,3462.5,482,483,483,0.8,0.8,1,490,0.65,12.5,17.899999999999999,null,null,null,null,null,null,null,null,null,null,null,null,281.13,0.16,156.13999999999999,0.1,125.72,0.04,30.42,0.09,259.86,0.18,100.58,0.04,119.84,0.05,19.260000000000002,0.06,80.989999999999995,0.04,53.44,0.03,47.83,0.03,null,null,81.77,0.04,53.4,0.05,48.31,0.02,5.08,0.04,590.89,0.44,39.659999999999997,0.01,40264,37,41521,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,264.18,0.2,101.52,0.04,121.07,0.06,19.55,7.0000000000000007E-2,262.76,0.18,120.67,0.05,19.52,0.08,5.61,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.53,0.08,61.5,0.04,60.94,0.13,61.25,0.04,60.52,0.12,60.49,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101.21,0.04,null,null,null,null,95.09,0.1,95.3,0.08,95.36,7.0000000000000007E-2,95.41,0.06,95.42,0.06,null,null,null,null,null,null,null,null,null,null,null,null,101.15,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.91,0.06,95.4,7.0000000000000007E-2,75.08,0.04,75.02,0.03,74.75,0.04,75.27,0.04,75.23,0.04,75.239999999999995,0.04,75,0.04,93.56,0.04,93.43,0.06,92.43,0.08,89.58,0.1,89.3,0.15,90.49,0.11,88.4,0.14000000000000001,87.6,0.09,91.98,7.0000000000000007E-2,75.88,0.06,76.59,0.1,75.75,0.05,82.48,0.15,75.92,0.04,75.5,0.03,76.19,0.04,77.180000000000007,0.14000000000000001,75.23,0.03,75.13,0.03,75.260000000000005,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",74.998000000000005,0.02,62,4.2000000000000003E-2,60.156999999999996,7.0000000000000001E-3,57.018999999999998,1.7999999999999999E-2,94.998999999999995,8.9999999999999993E-3,75,1.9E-2,1158.9000000000001,1.8,1111.9000000000001,1.7,0.54100000000000004,5.0000000000000001E-3,-0.13700000000000001,1E-3,1.7000000000000001E-2,3.0000000000000001E-3,1.1261000000000001,3.5000000000000001E-3,28.972999999999999,1E-3,3466,8,368.1,5.3,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.80132399974450952,5276.8659708846571,70.668861952755904,304.64147581713468,1296.3568499905721,3980.5091208940848,1.0043811446385767E-2,30.200089726711401,59.355676000255485,14.099889663221212,13.17713968549835,1.3921017560975253E-2,38.157141971984878,8.7810979208495076E-3,27.608667657170663,9.1608283390836442E-3,24.402001917742794,79.946206209836632,65.553972363390415,24.206424846331203,31627.766248164724,26076.832364498703,3097.9,0.33429906548058957,30612.633774009479,25061.699890343458,8.8322659474926368,0.20457405839847187,-5.993664880380198,-20.590530209581146,54.060037387980358,31627.766248164724,16921.145320388609,1032.0339928171052,13674.586934959014,31627.766248164728,1.0000000000000002]
[5,"C-95-3+20-C","30N0041","C-95-3+20-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","9:50:45","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","6.6 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,6.6,null,5.5,null,230.3,0.8,15.5,0,20098,40,19432,66,1337,122,21436,128,null,945,null,12.17,5.8577674149999996,109.77,0.01,45.83,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.2477411829999996,"Closed damper, +20% charge 95F Test, adjust code tester speed to match total--static of run C-95-FC3-EC-SPWCT-SS","R22 6.6  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75.001000000000005,1.2E-2,62.000999999999998,4.3999999999999997E-2,95,8.9999999999999993E-3,74.998000000000005,1.4999999999999999E-2,74.58,0.06,58.87,0.04,65.22,0.02,1.9E-2,3.0000000000000001E-3,1.1034999999999999,3.3E-3,20098,40,1337,122,6.2480000000000002,3.9E-2,null,null,11.533080734,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,13.8,0,13.8,0,13.8,0,3062.9,5.2,3062.9,5.2,3062.9,5.2,230,0.8,230,0.8,230,0.8,1.7,0,1.7,0,1.7,0,null,227.7,0.8,227.7,0.8,227.7,0.8,13.1,0,13.1,0,13.1,0,2868.8,5,null,null,null,null,null,null,null,null,null,228.2,0.8,0.7,0,168.9,0.7,23,null,3427.4,482,482,482,0.8,0.8,1,490,0.64,12.17,17.7,null,null,null,null,null,null,null,null,null,null,null,null,277.95999999999998,0.16,151.43,0.1,124.87,0.04,26.56,0.1,257.01,0.24,100.59,0.05,119.03,7.0000000000000007E-2,18.440000000000001,0.08,79.349999999999994,0.05,52.02,0.04,46.8,0.03,null,null,79.569999999999993,0.06,52.01,0.06,46.94,0.04,5.07,0.05,582.27,0.48,39.67,0.01,39570,41,40821,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,261.25,0.22,101.43,0.04,120.24,0.06,18.82,7.0000000000000007E-2,259.83999999999997,0.23,119.84,7.0000000000000007E-2,18.690000000000001,0.17,5.22,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.86,0.05,60.3,0.06,59.5,0.12,60.08,0.04,58.93,0.09,59.21,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101.29,0.04,null,null,null,null,95.08,0.14000000000000001,95.25,0.13,95.33,0.12,95.31,0.11,95.33,0.11,null,null,null,null,null,null,null,null,null,null,null,null,101.15,0.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.93,0.06,95.42,0.08,75.08,0.04,75.010000000000005,0.03,74.75,0.03,75.27,0.04,75.239999999999995,0.04,75.22,0.04,75.010000000000005,0.04,92,0.11,84.05,0.11,81.069999999999993,0.08,86.65,0.14000000000000001,85.35,0.15,86.07,0.12,78.010000000000005,7.0000000000000007E-2,83.16,0.1,92.81,7.0000000000000007E-2,79.2,0.15,75.2,0.05,75.27,0.05,83.51,0.2,75.150000000000006,0.05,75.19,0.04,75.03,0.04,76.22,0.08,75.08,0.03,75.05,0.03,75.12,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.001000000000005,1.2E-2,62.000999999999998,4.3999999999999997E-2,58.753999999999998,1.2E-2,55.68,2.1999999999999999E-2,95,8.9999999999999993E-3,74.998000000000005,1.4999999999999999E-2,1146,1.7,1102.2,1.6,0.56799999999999995,5.0000000000000001E-3,-0.17699999999999999,2E-3,1.9E-2,3.0000000000000001E-3,1.1034999999999999,3.3E-3,28.975999999999999,1E-3,3431,8,366.7,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,0.79631144624617645,5233.6772483007162,73.548504188976366,196.77447930063641,837.34423071516233,4396.3330175855535,9.6030814788152959E-3,29.296591575920193,57.957688553753819,14.09989861392425,13.137990123927718,1.3919025299848052E-2,38.155190330286374,8.78104851539405E-3,27.609345289181249,8.7014285463010328E-3,23.560167904992756,78.225773185824934,64.34543169136407,23.365976660959021,31038.924348865174,25458.387217320957,3064.3,0.33694646703768188,30038.398293662151,24457.861162117933,8.7549980453693248,0.20840208758299486,-5.930614914961172,-20.268084632071115,52.621758427642867,31038.924348865174,21192.087549961125,1016.3342957185733,8830.5025031854802,31038.924348865177,1.0000000000000002]
[5,"C-95-3+30-1","30N0042","C-95-3+30-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","7:39:56","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","7.2 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,7.2,null,5.5,null,230.3,1,15.7,0,18262,41,17642,71,-1459,113,16802,117,null,944,null,12.5,5.2704184700000001,109.93,0.01,59.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.8490620489999996,"1 Finger Open, +30% charge 95F Test, adjust code tester speed to match total static--of run C-95-FC3-1F-SPWCT-SS","R22 7.2  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75,1.6E-2,61.997,3.9E-2,95.004000000000005,8.0000000000000002E-3,75.006,2.3E-2,74.56,0.05,60.35,0.03,66.150000000000006,0.02,1.4999999999999999E-2,4.0000000000000001E-3,1.1261000000000001,3.8E-3,18262,41,-1459,113,4.8490000000000002,3.5000000000000003E-2,null,null,11.920057720000001,null,null,null,229.7,1,229.7,1,229.7,1,14,0,14,0,14,0,3095.6,5.4,3095.6,5.4,3095.6,5.4,230,1,230,1,230,1,1.7,0,1.7,0,1.7,0,null,227.7,1,227.7,1,227.7,1,13.3,0,13.3,0,13.3,0,2901,5,null,null,null,null,null,null,null,null,null,228.2,1,0.7,0,168.9,0.9,23,null,3461,480,480,480,0.8,0.8,1,490,0.65,12.5,17.8,null,null,null,null,null,null,null,null,null,null,null,null,284.07,0.17,147.56,0.09,126.51,0.04,21.05,0.09,262.76,0.18,99.89,0.03,120.67,0.05,20.77,0.06,81.33,0.05,53.53,0.03,48.04,0.03,null,null,81.95,0.04,53.43,0.05,48.42,0.03,5.01,0.04,603.83000000000004,0.49,39.44,0.01,41303,41,42559,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,267.20999999999998,0.2,100.89,0.03,121.91,0.05,21.03,0.06,265.76,0.19,121.51,0.05,20.92,7.0000000000000007E-2,5.49,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.62,0.1,61.54,0.04,60.96,0.18,61.31,0.04,60.58,0.16,60.6,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100.58,0.04,null,null,null,null,94.81,0.15,95.06,0.14000000000000001,95.03,0.13,95.14,0.11,95.17,0.11,null,null,null,null,null,null,null,null,null,null,null,null,100.59,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.74,7.0000000000000007E-2,95.2,0.08,74.91,0.04,74.89,0.03,74.7,0.03,75.040000000000006,0.05,75.010000000000005,0.06,75.02,0.04,74.849999999999994,0.03,93.34,0.09,93.21,0.11,92.31,0.11,89.51,0.12,89.16,0.13,90.59,0.13,88.54,0.15,87.77,0.09,92.13,0.08,76.06,7.0000000000000007E-2,76.77,0.1,75.87,0.06,82.79,0.16,76.069999999999993,0.05,75.64,0.04,76.17,0.04,77.22,0.14000000000000001,75.22,0.03,75.14,0.03,75.3,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",75,1.6E-2,61.997,3.9E-2,60.289000000000001,1.2E-2,57.139000000000003,1.7000000000000001E-2,95.004000000000005,8.0000000000000002E-3,75.006,2.3E-2,1159.2,2,1111.5999999999999,1.9,0.54,6.0000000000000001E-3,-0.13500000000000001,1E-3,1.4999999999999999E-2,4.0000000000000001E-3,1.1261000000000001,3.8E-3,28.968,1E-3,3465,8,368.1,5.3,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.8017426185370703,5276.7644982965385,70.519203779527558,302.41136317807889,1286.8522699498692,3989.9122283466695,1.0033715195951693E-2,30.180873555250098,59.487257381462932,14.100050343301318,13.180804264138184,1.3925079364943216E-2,38.162853784759008,8.7786472828053005E-3,27.606473721573838,9.2015444538290584E-3,24.478508515140774,79.912884440621866,65.528658879572959,24.2828147786587,31122.667161183803,25867.493693091601,3096.9,0.33961484230318656,30107.02390368333,24851.850435591128,8.6888957874987973,0.205030621675342,-5.8980587765913981,-20.425627059158934,54.219282125769809,31122.667161183803,16505.535753212796,1032.6297612076057,13584.50164676338,31122.667161183781,0.99999999999999933]
[5,"C-95-3+30-C","30N0043","C-95-3+30-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","6:33:57","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","7.2 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,7.2,null,5.5,null,230.3,0.9,15.5,0,19903,34,19231,61,1135,128,21040,124,null,944,null,12.1,5.8195906429999997,109.77,0.01,47.85,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.1520467840000004,"Closed damper, +30% charge 95F Test, adjust code tester speed to match total--static of run C-95-FC3-EC-SPWCT-SS","R22 7.2  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75,1.4E-2,62,4.5999999999999999E-2,95.003,5.0000000000000001E-3,74.998000000000005,1.7000000000000001E-2,74.56,0.06,58.96,0.05,65.260000000000005,0.02,1.2999999999999999E-2,3.0000000000000001E-3,1.0965,3.0999999999999999E-3,19903,34,1135,128,6.1529999999999996,3.7999999999999999E-2,null,null,11.797076023000001,null,null,null,229.8,0.9,229.8,0.9,229.8,0.9,13.8,0,13.8,0,13.8,0,3052.6,5.6,3052.6,5.6,3052.6,5.6,230,0.9,230,0.9,230,0.9,1.7,0,1.7,0,1.7,0,null,227.7,0.9,227.7,0.9,227.7,0.9,13.1,0,13.1,0,13.1,0,2858.6,5.0999999999999996,null,null,null,null,null,null,null,null,null,228.2,0.9,0.7,0,168.9,0.8,23,null,3416.6,480,480,480,0.8,0.8,1,480,0.65,12.1,17.600000000000001,null,null,null,null,null,null,null,null,null,null,null,null,279.92,0.16,144.4,0.08,125.4,0.04,19,0.08,258.95999999999998,0.17,100.05,0.05,119.59,0.05,19.54,7.0000000000000007E-2,79.55,0.04,52.08,0.05,46.93,0.03,null,null,79.75,0.05,51.97,0.04,47.05,0.03,4.92,0.03,591.87,0.44,39.49,0.01,40346,38,41595,33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,263.27,0.19,100.86,0.03,120.81,0.05,19.95,0.06,261.83999999999997,0.17,120.41,0.05,19.670000000000002,0.06,5.16,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.98,0.05,60.34,0.04,59.58,0.08,60.14,0.04,59.02,7.0000000000000007E-2,59.3,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100.77,0.04,null,null,null,null,95.07,7.0000000000000007E-2,95.25,0.06,95.3,7.0000000000000007E-2,95.28,0.06,95.3,0.05,null,null,null,null,null,null,null,null,null,null,null,null,100.73,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.87,0.06,95.34,0.06,75.02,0.05,74.98,0.05,74.739999999999995,0.04,75.180000000000007,0.06,75.150000000000006,0.06,75.150000000000006,0.06,74.959999999999994,0.05,91.97,0.1,84.36,0.12,80.92,0.09,86.66,0.13,85.35,0.18,86.1,0.13,77.989999999999995,7.0000000000000007E-2,83.09,0.1,92.97,0.06,79.16,0.16,75.22,0.04,75.290000000000006,0.04,83.54,0.21,75.19,0.04,75.209999999999994,0.05,75.05,0.05,76.25,0.09,75.099999999999994,0.04,75.06,0.04,75.13,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75,1.4E-2,62,4.5999999999999999E-2,58.85,1.7000000000000001E-2,55.78,1.9E-2,95.003,5.0000000000000001E-3,74.998000000000005,1.7000000000000001E-2,1142.5999999999999,1.6,1098.4000000000001,1.5,0.56899999999999995,4.0000000000000001E-3,-0.17599999999999999,1E-3,1.2999999999999999E-2,3.0000000000000001E-3,1.0965,3.0999999999999999E-3,28.966000000000001,1E-3,3420,8,366.1,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,0.79755016147432811,5217.0730932769511,73.423975055118106,196.21832116625717,834.97341892684574,4382.0996743501055,9.60289249045603E-3,29.296566709571106,58.052449838525675,14.099968936863728,13.140701457364203,1.3918307003685576E-2,38.155136459510778,8.7806253861067458E-3,27.608638360016613,8.7370954670979856E-3,23.622353352888954,78.226519159547209,64.345413922188712,23.427847401411249,30617.537594595713,25259.902616785308,3053.9,0.3404245252511669,29618.634321458831,24260.999343648426,8.6604193922394241,0.2076164621215898,-5.8687193081598572,-20.174069321021534,52.766538788126105,30617.537594595713,20796.740252819029,1014.7517659365669,8806.045575840124,30617.53759459572,1.0000000000000002]
[5,"C-95-3+40-1","30N0044","C-95-3+40-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","3:01:30","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","7.7 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,7.7,null,5.5,null,230.3,0.7,15.7,0,18021,135,17406,129,-1789,112,16230,185,null,944,null,12.5,5.1888856900000002,109.94,0.01,61.21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.6731932049999996,"1 Finger Open, +40% charge, 95F Test, adjust code tester speed--to match total static of run C-95-FC3-1F-SPWCT-SS","R22 7.7  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",74.995999999999995,1.7999999999999999E-2,62.000999999999998,4.2000000000000003E-2,94.998000000000005,1.4E-2,75,1.4999999999999999E-2,74.55,0.05,60.54,0.04,66.31,0.02,1.7999999999999999E-2,1.0999999999999999E-2,1.1291,1.6500000000000001E-2,18021,135,-1789,112,4.673,5.2999999999999999E-2,null,null,12.045205874000001,null,null,null,229.7,0.8,229.7,0.8,229.7,0.8,14,0,14,0,14,0,3103.1,5.4,3103.1,5.4,3103.1,5.4,230,0.7,230,0.7,230,0.7,1.7,0,1.7,0,1.7,0,null,227.7,0.8,227.7,0.8,227.7,0.8,13.3,0,13.3,0,13.3,0,2908.1,4.9000000000000004,null,null,null,null,null,null,null,null,null,228.2,0.8,0.7,0,169,0.7,23,null,3468.5,489,489,490,0.8,0.9,1.1000000000000001,500,0.63,12.5,18,null,null,null,null,null,null,null,null,null,null,null,null,285.51,0.2,143.02000000000001,0.1,126.9,0.05,16.12,0.08,264.19,0.21,99.55,0.04,121.07,0.06,21.52,0.06,81.73,0.08,53.73,0.05,48.3,0.05,null,null,82.07,0.08,53.47,0.06,48.51,0.05,4.96,0.06,610.39,0.53,39.340000000000003,0.01,41833,44,43093,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,268.68,0.24,100.48,0.04,122.33,7.0000000000000007E-2,21.85,7.0000000000000007E-2,267.14,0.22,121.9,0.06,21.59,0.08,5.43,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.85,0.08,61.65,0.09,61.1,0.15,61.43,7.0000000000000007E-2,60.77,0.12,60.76,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100.18,0.04,null,null,null,null,95.04,0.11,95.22,0.08,95.15,0.1,95.21,0.09,95.25,0.09,null,null,null,null,null,null,null,null,null,null,null,null,100.3,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.62,0.1,95.11,0.11,74.81,0.09,74.819999999999993,7.0000000000000007E-2,74.67,0.04,74.91,0.11,74.88,0.11,74.930000000000007,0.1,74.790000000000006,7.0000000000000007E-2,93.56,7.0000000000000007E-2,93.33,0.08,92.39,0.1,89.55,0.09,89.53,0.12,90.84,0.12,88.6,0.14000000000000001,87.81,0.09,92.21,0.06,76.22,7.0000000000000007E-2,76.78,0.09,75.86,0.05,83.3,0.15,76.16,0.05,75.69,0.04,76.180000000000007,7.0000000000000007E-2,77.150000000000006,0.16,75.19,0.06,75.150000000000006,0.03,75.36,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",74.995999999999995,1.7999999999999999E-2,62.000999999999998,4.2000000000000003E-2,60.493000000000002,2.1000000000000001E-2,57.319000000000003,3.2000000000000001E-2,94.998000000000005,1.4E-2,75,1.4999999999999999E-2,1160.3,8.6,1113.3,8.3000000000000007,0.54,4.0000000000000001E-3,-0.13600000000000001,2E-3,1.7999999999999999E-2,1.0999999999999999E-2,1.1291,1.6500000000000001E-2,28.995999999999999,1E-3,3473,8,368.4,5.3,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.80184274583236848,5279.5124535680588,70.627050708661415,303.52735698058939,1291.618028982585,3987.8944245854736,1.0039478543197755E-2,30.1898941118274,59.691157254167635,14.099866222199436,13.186444887150515,1.3921256994872441E-2,38.157159929527168,8.7822298553215002E-3,27.609418533438092,9.2615190109259296E-3,24.593545809462817,79.923934024548387,65.54045178918912,24.39780628132862,30579.399833278305,25636.60726307705,3104.6,0.34650777509599151,29563.100757346965,24620.308187145711,8.5122662704713399,0.20621526834708706,-5.7920878304987795,-20.232776770380752,54.43493686501666,30579.399833278305,15922.337604603685,1033.4092764400305,13623.652952234592,30579.399833278309,1.0000000000000002]
[5,"C-95-3-10-1","30N0045","C-95-3+10-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","11:54:44","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler",4.95,"208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,6.1,null,5.5,null,230.3,0.9,14.9,0,17538,36,16911,62,-1648,100,15888,101,null,944,null,13.3,5.3209951459999996,112.93,0.01,55.49,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.82038835,"1 Finger Open, -10% charge, 95F Test, adjust code tester speed to match total--static of run C-95-FC3-1F-SPWCT-SS","R22 4.95  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",74.994,1.4E-2,62.003,4.2000000000000003E-2,94.998999999999995,8.0000000000000002E-3,75.001999999999995,1.4999999999999999E-2,74.63,0.04,61.18,0.04,66.58,0.02,3.1E-2,3.0000000000000001E-3,1.1604000000000001,3.5000000000000001E-3,17538,36,-1648,100,4.8220000000000001,3.2000000000000001E-2,null,null,10.83131068,null,null,null,229.7,0.9,229.7,0.9,229.7,0.9,13.2,0,13.2,0,13.2,0,2923.8,5.2,2923.8,5.2,2923.8,5.2,229.9,0.9,229.9,0.9,229.9,0.9,1.7,0,1.7,0,1.7,0,null,227.8,0.9,227.8,0.9,227.8,0.9,12.5,0,12.5,0,12.5,0,2731.7,4.8,null,null,null,null,null,null,null,null,null,228.3,0.9,0.7,0,168.8,0.8,23,null,3294.1,480,480,480,0.9,0.9,1,510,0.65,13.3,18.2,null,null,null,null,null,null,null,null,null,null,null,null,261.29000000000002,0.16,184.46,0.06,120.25,0.04,64.209999999999994,7.0000000000000007E-2,241.52,0.2,104.04,0.05,114.49,0.06,10.45,0.08,77.25,0.05,68.73,0.04,45.47,0.03,null,null,77.14,0.06,71.48,0.05,45.39,0.04,26.09,0.06,512.15,0.46,40.75,0.01,35700,40,36965,37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,245.06,0.21,104.52,0.04,115.55,0.06,11.02,7.0000000000000007E-2,243.72,0.19,115.15,0.06,10.74,7.0000000000000007E-2,23.27,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.55,0.08,62.25,0.04,61.87,0.1,62.06,0.03,61.42,0.09,61.43,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.3,0.04,null,null,null,null,95.09,0.09,95.25,0.08,95.35,7.0000000000000007E-2,96.22,7.0000000000000007E-2,96.23,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,104.41,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.81,0.06,95.31,0.06,75.010000000000005,0.04,74.97,0.03,74.73,0.04,75.16,0.04,75.14,0.05,75.180000000000007,0.05,74.97,0.04,93.43,0.05,93.4,7.0000000000000007E-2,92.26,0.08,89.12,0.09,89.42,0.11,91.01,0.11,88.49,0.13,87.48,0.09,92.31,7.0000000000000007E-2,76.319999999999993,7.0000000000000007E-2,76.62,0.09,75.84,0.05,81.89,0.16,75.900000000000006,0.04,75.53,0.03,75.63,0.04,76.72,0.13,74.930000000000007,0.05,75,0.04,75.13,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",74.994,1.4E-2,62.003,4.2000000000000003E-2,61.055999999999997,1.2E-2,57.488999999999997,2.1999999999999999E-2,94.998999999999995,8.0000000000000002E-3,75.001999999999995,1.4999999999999999E-2,1177.4000000000001,1.8,1127.9000000000001,1.7,0.54400000000000004,5.0000000000000001E-3,-0.14199999999999999,1E-3,3.1E-2,3.0000000000000001E-3,1.1604000000000001,3.5000000000000001E-3,28.960999999999999,2E-3,3296,8,370.6,5.2,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.79301382198987336,5351.6249617248159,72.083289700787404,310.15096903047078,1319.8003290218683,4031.8246327029474,1.0051322846971435E-2,30.212250018257073,60.262986178010124,14.099904154153235,13.20047658519621,1.392277047341731E-2,38.159075749154418,8.7840212362491604E-3,27.610891038194882,9.2307911174622018E-3,24.697545636643085,79.962258018881784,65.569883524233745,24.503972175010357,30548.562194379821,25301.54757873877,2925.4,0.32683666538770456,29529.72466212861,24282.710046487558,8.9592611232186314,0.23560707294547883,-5.7082778432467158,-19.69927184087166,54.191124948904296,30548.562194379821,15591.131973070807,1035.9325692011848,13921.497652107835,30548.562194379829,1.0000000000000002]
[5,"C-95-3-20-1","30N0046","C-95-3+20-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","8:44:20","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","4.4 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,6.6,null,5.5,null,230.3,0.9,14.7,0,16420,232,15827,76,-2510,113,13908,248,null,943,null,14.4,5.0647748300000002,113.54,0.01,58.73,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2899444789999999,"1-Finger Open, -20% charge, 95F Test, adjust code tester speed to match total--static of run C-95-FC3-1F-SPWCT-SS","R22 4.4  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75.004000000000005,1.7000000000000001E-2,61.997999999999998,3.7999999999999999E-2,95.001000000000005,8.0000000000000002E-3,75.001000000000005,1.4E-2,74.59,0.05,62.16,0.04,67.19,0.02,5.5E-2,5.0000000000000001E-3,1.1989000000000001,4.8999999999999998E-3,16420,232,-2510,113,4.29,7.3999999999999996E-2,null,null,10.402529303,null,null,null,229.8,0.9,229.8,0.9,229.8,0.9,13,0,13,0,13,0,2867.9,5.8,2867.9,5.8,2867.9,5.8,230,0.9,230,0.9,230,0.9,1.7,0,1.7,0,1.7,0,null,227.9,0.9,227.9,0.9,227.9,0.9,12.3,0,12.3,0,12.3,0,2676.6,5.3,null,null,null,null,null,null,null,null,null,228.3,0.9,0.7,0,168.7,0.8,23,null,3241.3,482,482,482,0.9,1,1,500,0.64,14.4,18.7,null,null,null,null,null,null,null,null,null,null,null,null,254.62,0.15,188.27,0.04,118.34,0.04,69.930000000000007,0.05,235.4,0.2,105.67,0.05,112.64,0.06,6.97,7.0000000000000007E-2,73.66,0.04,71.05,0.03,43.11,0.02,null,null,73.25,0.03,73.81,0.03,42.84,0.02,30.97,0.04,484.29,0.43,41.27,0.01,33725,38,34998,34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,238.7,0.21,105.98,0.03,113.64,0.06,7.66,7.0000000000000007E-2,237.41,0.22,113.25,7.0000000000000007E-2,7.28,0.08,27.94,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.46,0.16,62.98,0.05,62.6,0.18,62.83,0.05,62.24,0.19,62.37,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105.99,0.05,null,null,null,null,95.04,0.09,95.22,7.0000000000000007E-2,95.17,7.0000000000000007E-2,95.2,0.06,95.23,0.06,null,null,null,null,null,null,null,null,null,null,null,null,105.97,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.52,7.0000000000000007E-2,95.02,7.0000000000000007E-2,74.739999999999995,0.05,74.78,0.04,74.66,0.04,74.78,0.06,74.77,0.06,74.83,0.06,74.739999999999995,0.04,93.18,0.04,93.08,0.05,92.13,0.06,89.51,0.1,89.72,0.13,91.02,0.11,88.6,0.13,87.34,0.08,92.31,0.06,76.33,0.08,76.760000000000005,0.09,75.89,0.05,82.38,0.15,76.06,0.04,75.599999999999994,0.04,75.84,0.04,76.849999999999994,0.12,74.98,0.04,75.02,0.05,75.19,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",75.004000000000005,1.7000000000000001E-2,61.997999999999998,3.7999999999999999E-2,62.109000000000002,0.03,58.122999999999998,2.8000000000000001E-2,95.001000000000005,8.0000000000000002E-3,75.001000000000005,1.4E-2,1198.5,2.5,1144.9000000000001,2.4,0.53900000000000003,7.0000000000000001E-3,-0.14499999999999999,1E-3,5.5E-2,5.0000000000000001E-3,1.1989000000000001,4.8999999999999998E-3,28.92,1E-3,3242,8,373,5.2,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.78588507261508622,5436.0972612341393,72.497231590551195,313.41052849011936,1333.6671399974875,4102.4301212366518,1.0040134718331647E-2,30.195654916199317,61.323114927384914,14.09994379065423,13.228240140735544,1.3921415138326419E-2,38.158072933407261,8.778361573076392E-3,27.607136659787649,9.3671138781109952E-3,25.102979066355651,79.944556467222199,65.548252108796888,24.91109815404122,28727.36454160398,24294.712165185862,2869,0.34085608465124007,27701.74859302253,23269.096216604412,8.544647931222249,0.26446745582809511,-5.2845567621580969,-18.621441539837285,54.6276052495135,28727.36454160398,13612.844235354358,1043.0833019155884,14071.437004334017,28727.364541603965,0.99999999999999944]
[5,"C-95-3-20-C","30N0047","C-95-3+20-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","9:50:45","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","4.4 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,6.6,null,5.5,null,230.3,1,14.7,0,18445,39,17822,70,459,99,18904,102,null,944,null,12.8,5.706992574,113.23,0.01,43.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8490099009999996,"Closed Damper, -20% charge, 95F Test, adjust code tester speed to match total--static of run C-95-FC3-EC-SPWCT-SS","R22 4.4  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75.001999999999995,1.7000000000000001E-2,61.999000000000002,4.2999999999999997E-2,94.997,5.0000000000000001E-3,74.998000000000005,1.2999999999999999E-2,74.63,0.05,60.33,0.04,66.06,0.01,2.5999999999999999E-2,3.0000000000000001E-3,1.1282000000000001,3.5000000000000001E-3,18445,39,459,99,5.8479999999999999,3.5000000000000003E-2,null,null,10.309715346999999,null,null,null,229.8,1,229.8,1,229.8,1,13,0,13,0,13,0,2863.3,5.9,2863.3,5.9,2863.3,5.9,230,1,230,1,230,1,1.7,0,1.7,0,1.7,0,null,227.9,1,227.9,1,227.9,1,12.3,0,12.3,0,12.3,0,2671.8,5.0999999999999996,null,null,null,null,null,null,null,null,null,228.3,1,0.7,0,168.8,0.9,23,null,3231.6,480,480,480,0.9,1,0.9,500,0.64,12.8,17.899999999999999,null,null,null,null,null,null,null,null,null,null,null,null,253.89,0.14000000000000001,187.14,0.04,118.13,0.04,69.010000000000005,0.05,234.76,0.2,105.91,0.04,112.45,0.06,6.54,7.0000000000000007E-2,72.7,0.06,69.02,0.03,42.48,0.04,null,null,72.349999999999994,0.05,71.87,0.03,42.24,0.03,29.63,0.04,481.04,0.44,41.35,0.01,33321,39,34578,34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,238.05,0.21,106.23,0.04,113.44,0.06,7.21,7.0000000000000007E-2,236.72,0.2,113.04,0.06,6.8,7.0000000000000007E-2,26.54,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.35,0.05,61.43,0.08,60.67,0.11,61.3,0.06,60.1,0.08,60.61,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106.26,0.04,null,null,null,null,95.09,0.06,95.19,0.06,95.23,7.0000000000000007E-2,96.1,0.06,96.11,0.06,null,null,null,null,null,null,null,null,null,null,null,null,106.24,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.69,0.06,95.16,0.06,74.89,0.05,74.88,0.05,74.709999999999994,0.04,74.98,0.06,74.959999999999994,0.06,74.98,0.06,74.849999999999994,0.05,91.62,0.08,83.81,0.11,81.09,0.1,86.84,0.14000000000000001,85.19,0.16,85.84,0.13,78.12,0.06,83.53,0.09,92.91,0.06,79.510000000000005,0.16,75.42,0.04,75.459999999999994,0.04,83.76,0.18,75.36,0.04,75.319999999999993,0.04,74.88,0.06,76.08,0.09,74.959999999999994,0.06,75.010000000000005,0.05,75.099999999999994,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.001999999999995,1.7000000000000001E-2,61.999000000000002,4.2999999999999997E-2,60.195,1.7000000000000001E-2,56.518999999999998,0.03,94.997,5.0000000000000001E-3,74.998000000000005,1.2999999999999999E-2,1160.9000000000001,1.8,1112.4000000000001,1.8,0.57199999999999995,5.0000000000000001E-3,-0.17799999999999999,2E-3,2.5999999999999999E-2,3.0000000000000001E-3,1.1282000000000001,3.5000000000000001E-3,28.922000000000001,1E-3,3232,8,368,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,0.78860714075595861,5286.5496364484216,74.751878551181093,197.32906441907471,839.70837238938077,4446.8412640590404,9.5959638276653606E-3,29.283215330774588,59.406392859244043,14.099828290927508,13.175701504770991,1.3919743597871624E-2,38.155244201201548,8.7794934708854237E-3,27.607887501380119,8.8538839483910513E-3,24.077404906900295,78.202940174267539,64.32735405680333,23.885039080288188,28537.726694493387,23848.531289933526,2864,0.34252314855500182,27536.870855988567,22847.675451428706,8.5200714282142851,0.25258779440136231,-5.3981762504864008,-18.796547315023496,53.054103730034662,28537.726694493387,18664.071476334797,1016.9514907413361,8856.7037274172817,28537.726694493416,1.0000000000000011]
[5,"C-95-3-30-1","30N0048","C-95-3+30-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","7:39:56","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","3.85 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,7.2,null,5.5,null,230.3,1,14.4,0,14475,39,13929,61,-3287,92,11184,91,null,943,null,14.3,4.5619287740000001,113.93,0.01,63.68,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.5247399939999999,"1 Finger Open, -30% charge, 95F Test, adjust code tester speed to match total--static of run C-95-FC3-1F-SPWCT-SS","R22 3.85  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75.004000000000005,1.4999999999999999E-2,61.997,4.2000000000000003E-2,95.001999999999995,5.0000000000000001E-3,74.998000000000005,1.0999999999999999E-2,74.61,0.05,63.59,0.04,68.11,0.02,4.8000000000000001E-2,4.0000000000000001E-3,1.1908000000000001,4.1999999999999997E-3,14475,39,-3287,92,3.5249999999999999,0.03,null,null,9.7040655529999995,null,null,null,229.8,1,229.8,1,229.8,1,12.7,0,12.7,0,12.7,0,2799.9,5.9,2799.9,5.9,2799.9,5.9,230,1,230,1,230,1,1.7,0,1.7,0,1.7,0,null,227.9,1,227.9,1,227.9,1,12,0,12,0,12,0,2609.5,5.3,null,null,null,null,null,null,null,null,null,228.4,1,0.7,0,168.8,0.9,23,null,3173.3,482,482,482,0.9,1,1,530,0.64,14.3,18.7,null,null,null,null,null,null,null,null,null,null,null,null,246.55,0.12,192.14,0.03,115.98,0.04,76.150000000000006,0.05,228.31,0.17,108.57,0.04,110.46,0.05,1.88,7.0000000000000007E-2,67.66,0.05,71.5,0.03,39.04,0.03,null,null,67.430000000000007,0.05,74.31,0.03,38.880000000000003,0.03,35.43,0.05,446.93,0.32,42.2,0.01,30791,30,32060,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,231.31,0.18,108.12,0.03,111.39,0.05,3.27,0.06,230.03,0.19,110.99,0.06,2.2200000000000002,7.0000000000000007E-2,32.46,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.92,0.11,64.569999999999993,0.05,64.150000000000006,0.13,64.41,0.05,63.8,0.13,63.88,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,109.03,0.04,null,null,null,null,95,0.09,95.18,7.0000000000000007E-2,95.16,0.08,95.19,7.0000000000000007E-2,95.22,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,108.77,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.56,7.0000000000000007E-2,95.05,0.08,74.78,0.06,74.8,0.04,74.680000000000007,0.04,74.84,7.0000000000000007E-2,74.819999999999993,7.0000000000000007E-2,74.87,0.06,74.77,0.04,93.17,0.04,93.1,0.05,92.15,0.08,89.58,0.1,89.7,0.14000000000000001,90.93,0.12,88.58,0.15,87.31,0.09,92.24,0.08,76.33,7.0000000000000007E-2,76.72,0.09,75.87,0.06,82.27,0.15,76.06,0.04,75.62,0.04,75.87,0.05,76.849999999999994,0.13,74.989999999999995,0.06,75.05,0.05,75.2,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",75.004000000000005,1.4999999999999999E-2,61.997,4.2000000000000003E-2,63.555999999999997,2.1999999999999999E-2,58.884999999999998,2.5999999999999999E-2,95.001999999999995,5.0000000000000001E-3,74.998000000000005,1.0999999999999999E-2,1195.5,2.2000000000000002,1139.7,2.1,0.54,6.0000000000000001E-3,-0.14299999999999999,1E-3,4.8000000000000001E-2,4.0000000000000001E-3,1.1908000000000001,4.1999999999999997E-3,28.917000000000002,1E-3,3173,8,372,5.2,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.7879861382054808,5407.0858502033589,72.301850078740173,311.24159025827538,1324.4374186368034,4082.6484315665557,1.0036925143188704E-2,30.190273685240047,62.768013861794515,14.099945495890264,13.265925858621657,1.3918546435532947E-2,38.155154416420466,8.7777022219083078E-3,27.606415130633408,9.4943556714191506E-3,25.594871298835123,79.936939785174616,65.541198119553414,25.402432874892646,25888.266298655613,22280.125541639562,2801,0.36927204354725152,24865.396512974352,21257.2557559583,7.8365573630552641,0.31182244383241353,-4.7878408103474008,-17.168925923380101,54.988544171994974,25888.266298655613,10876.590189980352,1040.5310791348015,13971.145029540447,25888.266298655602,0.99999999999999956]
[5,"C-95-3-30-C","30N0049","C-95-3+30-C","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","6:33:57","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU5","RTU5","3","R22","PSC Air Handler","3.85 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,7.2,null,5.5,null,230.3,0.9,14.4,0,16722,41,16128,68,-480,83,16241,84,null,943,null,13.5,5.2817435250000004,113.68,0.01,46.96,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.1298168039999998,"Closed Damper, -30% charge, 95F Test, adjust code tester speed to--match total static of run C-95-FC3-EC-SPWCT-SS","R22 3.85  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75.001999999999995,1.2E-2,62.003999999999998,3.9E-2,95,6.0000000000000001E-3,75.001999999999995,1.4999999999999999E-2,74.599999999999994,0.05,61.81,0.06,67.040000000000006,0.01,3.5000000000000003E-2,5.0000000000000001E-3,1.1607000000000001,6.0000000000000001E-3,16722,41,-480,83,5.13,2.9000000000000001E-2,null,null,9.6724573589999991,null,null,null,229.8,0.9,229.8,0.9,229.8,0.9,12.7,0,12.7,0,12.7,0,2794.8,5.6,2794.8,5.6,2794.8,5.6,229.9,0.9,229.9,0.9,229.9,0.9,1.7,0,1.7,0,1.7,0,null,227.9,0.9,227.9,0.9,227.9,0.9,12,0,12,0,12,0,2604.1999999999998,5.2,null,null,null,null,null,null,null,null,null,228.3,0.9,0.7,0,169,0.8,23,null,3166.4,477,478,478,0.9,0.9,1,500,0.65,13.5,18.3,null,null,null,null,null,null,null,null,null,null,null,null,246.49,0.12,190.93,0.04,115.98,0.04,74.95,0.05,228.25,0.16,108.71,7.0000000000000007E-2,110.45,0.05,1.74,0.09,67.319999999999993,0.04,70,0.04,38.83,0.03,null,null,67.13,0.04,72.89,0.05,38.700000000000003,0.03,34.18,0.05,446.34,0.28999999999999998,42.25,0.02,30623,31,31886,25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,231.25,0.18,108.14,0.04,111.38,0.05,3.24,0.06,229.97,0.19,110.99,0.06,2.06,7.0000000000000007E-2,31.17,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.91,0.08,62.83,0.09,62.2,0.14000000000000001,62.69,7.0000000000000007E-2,61.68,0.1,62.14,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,109.22,0.04,null,null,null,null,94.7,0.09,94.87,0.08,94.9,0.08,94.96,7.0000000000000007E-2,94.98,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,108.92,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.62,0.06,95.01,7.0000000000000007E-2,74.790000000000006,0.08,74.819999999999993,0.05,74.72,0.05,74.83,0.1,74.819999999999993,0.1,74.87,0.09,74.8,0.06,91.23,7.0000000000000007E-2,83.71,0.12,81.02,0.09,86.88,0.13,85.07,0.17,86.07,0.14000000000000001,78.319999999999993,0.08,83.72,0.12,92.84,0.08,79.47,0.17,75.55,0.08,75.540000000000006,0.06,83.77,0.2,75.38,0.05,75.37,0.04,74.94,0.08,76.040000000000006,0.11,74.97,0.08,75,0.06,75.12,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.001999999999995,1.2E-2,62.003999999999998,3.9E-2,61.741,2.1999999999999999E-2,57.389000000000003,2.7E-2,95,6.0000000000000001E-3,75.001999999999995,1.4999999999999999E-2,1176.8,3,1128.9000000000001,3,0.57399999999999995,6.0000000000000001E-3,-0.17699999999999999,2E-3,3.5000000000000003E-2,5.0000000000000001E-3,1.1607000000000001,6.0000000000000001E-3,29.015999999999998,4.0000000000000001E-3,3166,8,370.2,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,0.782535062084452,5342.5764404153269,76.125904818897638,196.77468152800697,837.34337016785651,4505.2330702474701,9.588343366715853E-3,29.26461760529704,60.958464937915551,14.099927595191508,13.216095415288246,1.39225310385042E-2,38.159057791057066,8.782790522845807E-3,27.611495468268149,9.008233816928125E-3,24.622518829417125,78.160985149254785,64.302002991548193,24.431580543605573,25820.869941446948,22057.387007248675,2795.8,0.36954856368659134,24817.195054593845,21053.712120395572,7.8386592086525093,0.30163917103820159,-4.8330370616914671,-17.202520211339234,53.528274524701352,25820.869941446948,15968.836171677276,1020.1023873500824,8831.931382419576,25820.869941446937,0.99999999999999956]
[5,"C-95-3-40-1","30N0050","C-95-3+40-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","3:01:30","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","3.3 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,7.7,null,5.5,null,230.3,0.8,14.2,0,11858,29,11385,52,-3781,83,8073,93,null,943,null,13.7,3.8104113110000002,114.36,0.01,70.77,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.5941516710000001,"1 Finger Open, -40% charge, 95F Test, adjust code tester speed--to match total static of run C-95-FC3-1F-SPWCT-SS","R22 3.3  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75,1.7999999999999999E-2,61.994,4.7E-2,94.997,1.0999999999999999E-2,75.001000000000005,1.4999999999999999E-2,74.61,0.05,65.55,0.05,69.5,0.01,3.1E-2,4.0000000000000001E-3,1.1789000000000001,4.1000000000000003E-3,11858,29,-3781,83,2.5939999999999999,3.1E-2,null,null,8.8746786629999992,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,12.5,0,12.5,0,12.5,0,2738.7,5.8,2738.7,5.8,2738.7,5.8,229.9,0.8,229.9,0.8,229.9,0.8,1.7,0,1.7,0,1.7,0,null,228,0.8,228,0.8,228,0.8,11.7,0,11.7,0,11.7,0,2548.4,5.2,null,null,null,null,null,null,null,null,null,228.4,0.8,0.7,0,169.7,0.8,23,null,3113,482,483,484,0.9,0.9,1,510,0.64,13.7,18.399999999999999,null,null,null,null,null,null,null,null,null,null,null,null,239.2,0.16,197,0.08,113.83,0.05,83.16,0.1,222.27,0.27,108.15,0.06,108.6,0.09,0.46,0.1,61.63,0.05,72.180000000000007,0.04,34.82,0.04,null,null,61.43,0.06,75.260000000000005,0.04,34.67,0.05,40.58,0.06,399.59,2.5,42.06,0.02,27618,181,28885,180,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,225.29,0.17,107.71,0.03,109.56,0.05,1.85,0.05,224.1,0.23,109.18,7.0000000000000007E-2,0.45,7.0000000000000007E-2,37.369999999999997,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65.06,0.09,66.72,7.0000000000000007E-2,66.38,0.14000000000000001,66.569999999999993,0.05,65.77,0.12,66.099999999999994,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,108.93,0.05,null,null,null,null,94.98,0.09,95.33,0.06,95.23,0.08,95.25,7.0000000000000007E-2,95.27,0.06,null,null,null,null,null,null,null,null,null,null,null,null,108.73,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.62,7.0000000000000007E-2,95.1,7.0000000000000007E-2,74.86,0.06,74.88,0.05,74.73,0.04,74.95,7.0000000000000007E-2,74.930000000000007,7.0000000000000007E-2,74.989999999999995,7.0000000000000007E-2,74.849999999999994,0.05,93.47,0.05,93.37,0.06,92.51,0.08,89.72,0.1,89.68,0.1,91.08,0.11,88.9,0.12,87.7,0.1,91.93,0.08,76.319999999999993,7.0000000000000007E-2,76.97,0.1,75.98,7.0000000000000007E-2,82.82,0.14000000000000001,76.2,0.05,75.709999999999994,0.04,76.13,0.06,77.02,0.14000000000000001,75.12,7.0000000000000007E-2,75.08,0.05,75.3,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",75,1.7999999999999999E-2,61.994,4.7E-2,65.569000000000003,1.2E-2,59.741,3.1E-2,94.997,1.0999999999999999E-2,75.001000000000005,1.4999999999999999E-2,1185.2,2.1,1138,2,0.54700000000000004,5.0000000000000001E-3,-0.13900000000000001,1E-3,3.1E-2,4.0000000000000001E-3,1.1789000000000001,4.1000000000000003E-3,29.204000000000001,2E-3,3112,8,371.9,5.2,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.7954495452334146,5339.7674798134885,73.129851338582696,306.85664806961182,1305.7868594012548,4033.9806204122337,1.0034999775880803E-2,30.185144405897944,64.773550454766593,14.099850026534137,13.317433815017701,1.3922372875947001E-2,38.15814476468654,8.776669310441524E-3,27.604309226416159,9.5538943360705623E-3,26.151380938759349,79.924593452214751,65.534371922152843,25.957098807341584,22576.780390339805,19416.731203927091,2740.1,0.41422918318333529,21557.077872958387,18397.028686545673,6.9270815787141347,0.39287227062655605,-4.2280455985563599,-15.151042997448158,54.969312603678908,22576.780390339805,7758.2992209309332,1037.4214072534319,13781.059762155432,22576.780390339794,0.99999999999999956]
[5,"C-95-3-FC-1","30N0051","C-95-3-FC-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/18/2014","0:55:24","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.8,15.2,0,17780,138,17152,128,-1406,120,16373,179,null,944,null,12.6,5.3042959429999996,112.21,0.02,55.56,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.8845465389999996,"1 Finger Open, 5.5 lbs factory charge 95F test, adjust code tester speed to match--total static of run C -95-FC3-1F-SPWCT-SS","R22 5.5  LBS: Unsealed cab:Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. ID Pulley is 3 turns open from fully closed: with flow meter: new filter drier: with isolation ball valves: with code:",75,2.3E-2,62.008000000000003,4.4999999999999998E-2,95.001000000000005,1.0999999999999999E-2,75.001000000000005,1.9E-2,74.55,0.05,60.82,0.04,66.680000000000007,0.05,2.1000000000000001E-2,1.0999999999999999E-2,1.1375,1.66E-2,17780,138,-1406,120,4.8849999999999998,5.1999999999999998E-2,null,null,10.991348449,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,13.5,0,13.5,0,13.5,0,2980.9,4.8,2980.9,4.8,2980.9,4.8,230,0.8,230,0.8,230,0.8,1.7,0,1.7,0,1.7,0,null,227.8,0.9,227.8,0.9,227.8,0.9,12.8,0,12.8,0,12.8,0,2787.8,4.4000000000000004,null,null,null,null,null,null,null,null,null,228.3,0.9,0.7,0,169.2,0.8,23,null,3349.6,490,490,490,0.8,0.8,1,510,0.63,12.6,17.899999999999999,null,null,null,null,null,null,null,null,null,null,null,null,266,0.16,181.39,7.0000000000000007E-2,121.59,0.05,59.8,0.08,245.88,0.21,103.03,0.03,115.8,0.06,12.78,0.06,79.040000000000006,7.0000000000000007E-2,65.31,0.11,46.62,0.04,null,null,79.709999999999994,7.0000000000000007E-2,68.48,0.1,47.05,0.04,21.43,0.11,530.86,0.46,40.43,0.01,36843,43,38104,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,249.59,0.23,103.79,0.03,116.89,7.0000000000000007E-2,13.1,7.0000000000000007E-2,248.13,0.21,116.47,0.06,13,7.0000000000000007E-2,18.68,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.19,0.09,61.96,0.06,61.47,0.1,61.76,0.05,60.99,0.1,61.07,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.38,0.04,null,null,null,null,95.07,0.1,95.22,7.0000000000000007E-2,95.21,7.0000000000000007E-2,95.26,0.06,95.3,0.06,null,null,null,null,null,null,null,null,null,null,null,null,103.47,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.78,0.05,95.28,0.06,74.959999999999994,0.04,74.95,0.04,74.709999999999994,0.03,75.12,0.04,75.09,0.04,75.12,0.04,74.930000000000007,0.04,93.67,0.04,93.31,0.08,92.43,7.0000000000000007E-2,89.38,0.09,89.78,0.13,90.98,0.13,88.45,0.14000000000000001,87.8,0.09,92.25,0.06,76.260000000000005,0.06,76.69,0.09,75.84,0.05,83.35,0.14000000000000001,76.13,0.04,75.739999999999995,0.03,76.319999999999993,0.04,77.28,0.15,75.260000000000005,0.04,75.150000000000006,0.03,75.400000000000006,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-1ER-DM",75,2.3E-2,62.008000000000003,4.4999999999999998E-2,60.762,2.4E-2,57.302,3.2000000000000001E-2,95.001000000000005,1.0999999999999999E-2,75.001000000000005,1.9E-2,1164.2,8.6,1118.0999999999999,8.3000000000000007,0.54,5.0000000000000001E-3,-0.13700000000000001,2E-3,2.1000000000000001E-2,1.0999999999999999E-2,1.1375,1.66E-2,29.038,1E-3,3352,8,369.6,5.3,0.25502449755024487,291.77352764723514,13.029,0.13600000000000001,0.80193924895214264,5294.7522712713835,70.93155968503936,304.64206055381158,1296.3543617346988,3998.3979095366849,1.0043267857939802E-2,30.195896054303141,59.960060751047855,14.09994379065423,13.192685213812098,1.3921415138326419E-2,38.158072933407261,8.7859009684694879E-3,27.61441142979616,9.1875639648067269E-3,24.578750480823473,79.931489522438653,65.548300719389673,24.383013727618295,30777.771901847875,25378.504283485461,2982.4,0.33072345952985843,29758.416515052915,24359.148896690502,8.877809222867814,0.22797318926480287,-5.8128823266848464,-19.971428771390798,54.062661531384677,30777.771901847875,16073.072704382979,1036.3776186044045,13668.321578860485,30777.771901847867,0.99999999999999978]
[5,"C-55-T1ER-DM","30N0021","C-55-T1ER-DM","1 Finger","Off","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","4:49:30","10 Ton","0:30:00","75/62  55/51","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,0.8,1.7,0,6120,21,5475,38,2578,46,8700,56,null,942,null,13.7,null,110.12,0.01,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.2,"Econo 1F-open, tape around damper perimeter frame gaps, no compressor,--55/51 ambient, 53.5% inlet 52% outlet Meriam, adjust code tester speed to match--total static of run C-55-T1E-DM-SPWCT-SSR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 1F: with flow meter: new filter drier: with isolation ball valves: without code",74.991,1.2999999999999999E-2,61.997999999999998,2.5999999999999999E-2,54.991,1.2E-2,51.000999999999998,1.7999999999999999E-2,74.34,0.05,70.11,0.05,72.42,0.01,4.1000000000000002E-2,5.0000000000000001E-3,1.1912,5.1000000000000004E-3,6120,21,2578,46,23.204000000000001,0.33500000000000002,null,null,null,null,null,null,230.2,0.8,230.2,0.8,230.2,0.8,0,0,0,0,0,0,0.3,0.2,0.3,0.2,0.3,0.2,229.8,0.8,229.8,0.8,229.8,0.8,1.7,0,1.7,0,1.7,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,23,null,374.6,482,482,483,0.9,0.9,1.1000000000000001,510,0.63,13.7,18.399999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-0.6,0,26.2,0.01,-1278,16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69.680000000000007,0.24,71.349999999999994,0.14000000000000001,70.709999999999994,0.04,71.150000000000006,0.14000000000000001,70.19,0.14000000000000001,70.59,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.98,0.03,null,null,54.73,0.08,54.81,0.09,54.35,0.06,54.66,7.0000000000000007E-2,54.67,0.05,54.68,0.04,null,null,null,null,null,null,null,null,54.49,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.99,0.1,54.68,0.09,74.56,0.08,74.56,7.0000000000000007E-2,74.42,0.04,74.709999999999994,0.09,74.66,0.09,74.73,0.09,74.64,0.08,63.6,0.04,63.55,0.04,63.44,0.06,63.2,7.0000000000000007E-2,62.28,0.04,63.41,0.08,62.98,0.09,63.2,0.1,61.33,0.1,74.28,7.0000000000000007E-2,73.77,0.1,74.41,0.08,69.05,0.15,73.489999999999995,7.0000000000000007E-2,74.23,0.06,73.2,0.09,73.06,0.11,74.150000000000006,0.09,74.319999999999993,0.05,74.38,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.991,1.2999999999999999E-2,61.997999999999998,2.5999999999999999E-2,70.259,7.0000000000000001E-3,59.6,0.02,54.991,1.2E-2,51.000999999999998,1.7999999999999999E-2,1186.2,2.6,1150.2,2.5,0.56899999999999995,8.0000000000000002E-3,-0.16400000000000001,1E-3,4.1000000000000002E-2,5.0000000000000001E-3,1.1912,5.1000000000000004E-3,29.59,1E-3,375,5,374.6,4.8,0.19659999999999997,226.12931999999998,13.029,0.16400000000000001,0.79847116820592234,5300.7449093695886,76.886613354330706,226.13187571380993,1041.3390021417194,4259.4059072278687,8.4283226590937052E-3,26.265769373873013,69.460528831794079,13.029294509207377,13.426792123913845,6.9839895098535963E-3,20.77837398576321,8.7814330395431638E-3,27.607327084565657,8.3557221217261529E-3,25.988237889315805,71.072308327643654,60.019511897671258,25.793642528323925]
[5,"C-55-T2ER-DM","30N0022","C-55-T2ER-DM","2 Finger","Off","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","11:45:56","10 Ton","0:30:00","75/62 55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,0.8,1.7,0,8232,28,7564,44,3518,54,11753,65,null,943,null,13.55,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.341333333000001,"Econo 2F-open, tape around damper perimeter frame gaps, no compressor,--55/51, 53.5% inlet 52% outlet Meriam, ambient adjust code tester speed to match--otal static of run C-55-T2E-DM-SPWCT-SSR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 2F: with flow meter: new filter drier: with isolation ball valves: with code",74.997,8.9999999999999993E-3,62.000999999999998,2.7E-2,54.999000000000002,1.0999999999999999E-2,50.999000000000002,1.7000000000000001E-2,74.39,0.04,68.56,0.03,71.37,0.01,4.3999999999999997E-2,6.0000000000000001E-3,1.1904999999999999,6.1999999999999998E-3,8232,28,3518,54,31.359000000000002,0.436,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,1.7,0,1.7,0,1.7,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,480,481,482,0.9,0.9,1,520,0.64,13.55,18.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68.069999999999993,0.35,69.63,0.23,68.81,0.06,69.540000000000006,0.21,68.34,0.16,68.900000000000006,0.19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.96,0.02,null,null,55.18,0.14000000000000001,55.25,0.14000000000000001,54.51,7.0000000000000007E-2,54.71,0.08,54.68,0.04,54.69,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.18,0.06,54.92,0.05,74.64,0.03,74.62,0.03,74.459999999999994,0.03,74.78,0.04,74.709999999999994,0.04,74.77,0.04,74.7,0.04,61.33,0.03,61.56,0.04,61.31,0.05,60.53,7.0000000000000007E-2,60.26,0.03,62.43,0.09,60.77,7.0000000000000007E-2,60.94,7.0000000000000007E-2,61.59,7.0000000000000007E-2,73.819999999999993,0.05,70.33,0.13,71.36,0.11,66.42,0.13,73.38,0.04,74.02,0.03,72.92,0.05,71.37,0.14000000000000001,73.010000000000005,0.04,73.930000000000007,0.03,73.2,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.997,8.9999999999999993E-3,62.000999999999998,2.7E-2,68.647000000000006,0.01,58.731000000000002,0.02,54.999000000000002,1.0999999999999999E-2,50.999000000000002,1.7000000000000001E-2,1183.9000000000001,3.1,1152.0999999999999,3,0.53600000000000003,0.01,-0.126,1E-3,4.3999999999999997E-2,6.0000000000000001E-3,1.1904999999999999,6.1999999999999998E-3,29.629000000000001,1E-3,375,5,374.5,4.9000000000000004,0.27702770277027677,319.16361636163583,13.029,0.126,0.80886935301894081,5307.1162655650314,72.547101984251967,319.16942384504802,1469.7573519866196,3837.3589135784118,8.2832378130376933E-3,25.717266584127405,67.838130646981071,13.029474154232515,13.384670025207605,6.9810467322748938E-3,20.777124644561066,8.7819935869295259E-3,27.609403884561523,8.1951044438036465E-3,25.420066599506352,69.471877252942122,59.187085439370165,25.222994781421562]
[5,"C-55-T3ER-DM","30N0023","C-55-T3ER-DM","3 Finger","Off","N/A",null,"unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","14:38:07","10 Ton","0:30:00","75/62  55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.2,0.8,1.7,0,12185,55,11392,77,5034,101,17224,127,null,943,null,13.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,46.176943700000002,"Econo 3F-open, tape around damper perimeter frame gaps, no compressor,--55/51 ambient, 53.5% inlet 52% outlet Meriam, adjust code tester speed to match--match total static of run C-55-T3E-DM-SPWCT-SSR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 3F: with flow meter: new filter drier: with isolation ball valves: with code",75.007999999999996,1.2E-2,61.997999999999998,2.8000000000000001E-2,55.000999999999998,1.2999999999999999E-2,51.000999999999998,1.7999999999999999E-2,74.38,0.05,65.48,0.02,69.27,0.01,4.0000000000000001E-3,8.0000000000000002E-3,1.1559999999999999,9.4000000000000004E-3,12185,55,5034,101,46.183999999999997,0.67800000000000005,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,1.7,0,1.7,0,1.7,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,478,478,478,0.9,0.9,1,500,0.63,13.1,18.100000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65.03,0.42,66.27,0.28999999999999998,65.38,0.1,66.27,0.25,64.95,0.2,65.62,0.22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.21,0.03,null,null,55.39,0.15,55.69,0.21,54.66,0.1,55,0.12,54.83,7.0000000000000007E-2,54.83,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.03,7.0000000000000007E-2,54.8,0.09,74.44,7.0000000000000007E-2,74.42,0.06,74.37,0.03,74.5,0.08,74.45,0.08,74.53,7.0000000000000007E-2,74.52,0.06,57.92,0.04,58.22,0.04,58.08,0.06,57.19,0.05,57.99,0.05,60.03,0.08,57.61,0.05,57.5,0.06,62.46,0.11,69.02,0.14000000000000001,62.66,0.17,64.7,0.16,68.989999999999995,7.0000000000000007E-2,72.77,0.05,71.55,0.06,70.040000000000006,7.0000000000000007E-2,70.55,0.08,72.540000000000006,0.06,72.66,0.04,69.569999999999993,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75.007999999999996,1.2E-2,61.997999999999998,2.8000000000000001E-2,65.486000000000004,1.2E-2,57.066000000000003,2.1000000000000001E-2,55.000999999999998,1.2999999999999999E-2,51.000999999999998,1.7999999999999999E-2,1166.0999999999999,4.8,1135.8,4.7,0.49099999999999999,8.0000000000000002E-3,-6.3E-2,1E-3,4.0000000000000001E-3,8.0000000000000002E-3,1.1559999999999999,9.4000000000000004E-3,29.530999999999999,2E-3,373,5,372.6,4.9000000000000004,0.43444794321987268,493.4459739091314,13.03,6.3E-2,0.83004291182707213,5259.6178808932054,65.516163590551173,493.43706293720828,2272.2404529945247,2987.3774278986807,8.0016115946503902E-3,24.656915079774642,64.655957088172926,13.029529395630313,13.302487287939281,6.9816393907336169E-3,20.77825412733797,8.7774165133813614E-3,27.607078067976676,7.9298605673168102E-3,24.360788974928557,66.380722306759338,57.537269925444633,24.158656212787339]
[5,"C-55-TCE-DM","30N0024","C-55-TCE-DM","closed","Off","N/A",null,"unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","1:56:07","10 Ton","0:30:00","75/62 - 55/51","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,0.9,1.7,0,2635,13,2131,30,1266,35,3902,36,null,944,null,11.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.60326087,"Econo closed, tape around damper perimeter frame gaps, no compressor, 55/51 ambient,--53.5% inlet 52% outlet Meriam, adjust code tester speed to match total static of run C-55-TCE-DM-SPWCT-SS","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo  fulley closed: with flow meter: new filter drier: with isolation ball valves: with code",74.998999999999995,0.01,62,0.03,54.991,1.4E-2,50.994999999999997,1.4E-2,74.37,0.04,72.650000000000006,0.04,74.2,0,1.4E-2,5.0000000000000001E-3,1.0891999999999999,4.8999999999999998E-3,2635,13,1266,35,10.62,0.17199999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229.8,0.9,229.8,0.9,229.8,0.9,1.7,0,1.7,0,1.7,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,484,485,486,0.8,0.8,1,470,0.62,11.9,17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72.64,0.05,73.72,0.03,73.510000000000005,0.03,73.430000000000007,0.04,73.25,0.04,72.989999999999995,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.84,0.03,null,null,54.71,0.08,54.7,0.08,54.42,0.06,54.61,7.0000000000000007E-2,54.7,0.06,54.72,0.05,null,null,null,null,null,null,null,null,54.47,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.89,7.0000000000000007E-2,54.64,0.06,74.64,0.05,74.63,0.04,74.47,0.02,74.81,0.06,74.760000000000005,0.05,74.8,0.06,74.69,0.05,70.89,0.05,70.84,0.05,71.290000000000006,0.08,70.33,0.06,69.81,0.05,68.63,0.1,72.180000000000007,0.08,69.81,7.0000000000000007E-2,60.24,0.11,72.44,0.09,74.61,0.05,74.62,0.05,61.53,0.14000000000000001,74.489999999999995,0.04,74.62,0.04,74.34,0.06,73.739999999999995,0.08,74.36,0.06,74.41,0.03,74.510000000000005,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.998999999999995,0.01,62,0.03,72.866,5.0000000000000001E-3,60.908000000000001,2.5000000000000001E-2,54.991,1.4E-2,50.994999999999997,1.4E-2,1135.7,2.6,1097.5,2.5,0.59799999999999998,8.9999999999999993E-3,-0.20899999999999999,2E-3,1.4E-2,5.0000000000000001E-3,1.0891999999999999,4.8999999999999998E-3,29.600999999999999,0,368,5,367.1,4.9000000000000004,6.5623750499799877E-2,72.022066173530362,13.029,0.20899999999999999,0.81646221774571048,5049.5806883948972,77.102918110236217,72.022811646885714,331.66622476578885,4717.9144636291085,8.6626302263166886E-3,27.159799798582092,72.049537782254291,13.029269717966438,13.494585828998844,6.980801574107855E-3,20.774913749285059,8.7808616533765083E-3,27.608653008587336,8.5726272112408332E-3,26.860743427268702,73.688860241322146,61.346985172365741,26.661684838565922]
[5,"C-55-TOER-DM","30N0025","C-55-TOER-DM","Fully open","Off","N/A",null,"unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/13/2014","20:37:37","10 Ton","0:30:00","75/62 - 55/51","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,0.8,1.7,0,15988,116,15169,138,6508,111,22503,193,null,944,null,11.7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.491935484000003,"Econo fully-open, tape around damper perimeter frame gaps, no compressor,--55/51 ambient, 53.5% inlet 52% outlet Meriam, adjust code tester speed to match--match total static of run C-55-TOE-DM-SPWCT-SSR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo fully open: with flow meter: new filter drier: with isolation ball valves: with code",75.001999999999995,1.6E-2,62,2.5000000000000001E-2,54.991999999999997,8.9999999999999993E-3,50.997999999999998,1.4E-2,74.36,0.05,62.38,0.03,67.3,0.02,2.5000000000000001E-2,8.9999999999999993E-3,1.1268,1.6899999999999998E-2,15988,116,6508,111,60.512,0.90100000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229.8,0.8,229.8,0.8,229.8,0.8,1.7,0,1.7,0,1.7,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,481,481,481,0.8,0.8,1,470,0.63,11.7,17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.09,0.17,62.79,0.14000000000000001,62.39,0.06,62.65,0.14000000000000001,61.99,0.13,62.21,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.56,0.02,null,null,55.67,0.11,55.8,0.17,54.73,0.09,54.9,0.08,54.67,7.0000000000000007E-2,54.69,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.11,0.09,54.73,0.09,74.33,0.06,74.36,0.05,74.37,0.04,74.349999999999994,7.0000000000000007E-2,74.319999999999993,7.0000000000000007E-2,74.41,0.06,74.45,0.05,57.8,0.05,58.13,0.05,58.41,0.06,57.08,0.06,57.12,0.05,62.49,0.13,58.06,0.08,57.46,7.0000000000000007E-2,68.430000000000007,7.0000000000000007E-2,65.819999999999993,0.1,56.4,0.15,55.92,0.09,73.900000000000006,0.04,72.2,0.04,62,0.09,61.8,0.14000000000000001,72.88,0.05,71.2,0.06,64.89,7.0000000000000007E-2,63.28,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75.001999999999995,1.6E-2,62,2.5000000000000001E-2,62.366,1.9E-2,55.387999999999998,2.1999999999999999E-2,54.991999999999997,8.9999999999999993E-3,50.997999999999998,1.4E-2,1151.0999999999999,8.6999999999999993,1121.5999999999999,8.5,0.41599999999999998,4.0000000000000001E-3,-2.4E-2,1E-3,2.5000000000000001E-2,8.9999999999999993E-3,1.1268,1.6899999999999998E-2,29.416,1E-3,372,5,371.5,5.2,0.58850574712643666,660.06804597701125,13.029,2.4E-2,{"$f":"(XM34-XU34)*3.412/XT34/0.24","v":0.86186988072195658},5223.7704788745159,54.814623244094477,{"$f":"XP34*SQRT(-XC34*YB34/(XR34*XQ34))","v":660.07578704908326},3039.6514160521442,2184.1190628223717,7.7339219592447474E-3,23.633160801233227,61.504130119278045,13.02930560188471,13.221484419981746,6.9821604824847798E-3,20.776631830264595,8.7801528521769482E-3,27.608609062912965,7.679507295856855E-3,23.328446668398076,63.374378227109332,55.890867486105066,23.118659178224341]
[5,"C-75629575-T1E3","30N0026","C-75629575-T1E3","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/11/2014","16:39:59","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.9,15,0,19299,73,18440,105,1127,70,20427,101,null,939,null,7.38,null,112.07,0.01,43.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.8024654240000002,"1 Finger open damper, tape around damper perimiter frame gaps, unsealed cab,--53.5% inlet 52% outlet Meriam, adjust code tester speed to match total static--of run C-T1EM3-SPWCT-SR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: with economizer: with flow meter: new filter drier: with isolation ball valves: with code",74.995999999999995,0.01,61.999000000000002,2.1000000000000001E-2,95.001999999999995,1.4E-2,75,1.7999999999999999E-2,74.41,7.0000000000000007E-2,59.27,0.05,65.41,0.05,0.01,6.0000000000000001E-3,0.77549999999999997,5.8999999999999999E-3,19299,73,1127,70,6.1420000000000003,3.4000000000000002E-2,null,null,10.830426939000001,null,null,null,229.8,0.9,229.8,0.9,229.8,0.9,13.4,0,13.4,0,13.4,0,2966.3,5.7,2966.3,5.7,2966.3,5.7,230,0.9,230,0.9,230,0.9,1.6,0,1.6,0,1.6,0,null,227.8,0.9,227.8,0.9,227.8,0.9,12.7,0,12.7,0,12.7,0,2773.6,5.0999999999999996,null,null,null,null,null,null,null,null,null,228.3,0.9,0.7,0,168.9,0.8,23,null,3323.7,484,485,484,0.7,0.7,0.7,380,0.62,7.38,15.3,null,null,null,null,null,null,null,null,null,null,null,null,263.72000000000003,0.19,181.44,0.03,120.92,0.05,60.51,0.05,243.8,0.22,103.46,0.05,115.16,7.0000000000000007E-2,11.7,0.09,77.31,0.06,63.98,0.06,45.47,0.04,null,null,78.010000000000005,0.03,67.56,0.06,45.92,0.02,21.64,0.06,520.89,0.54,40.57,0.02,36022,46,37245,42,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,247.45,0.23,104.3,0.04,116.24,7.0000000000000007E-2,11.93,7.0000000000000007E-2,246.06,0.21,115.83,0.06,12.54,7.0000000000000007E-2,18.510000000000002,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.53,7.0000000000000007E-2,60.32,0.05,59.81,0.1,60.14,0.03,59.41,0.1,59.42,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.07,0.06,null,null,94.69,0.08,94.63,0.09,94.85,0.06,94.9,7.0000000000000007E-2,94.89,0.06,94.91,0.06,null,null,null,null,null,null,null,null,null,null,null,null,103.29,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.96,0.08,95.26,0.08,74.739999999999995,0.05,74.72,0.04,74.47,0.05,74.900000000000006,0.06,74.900000000000006,0.06,74.87,0.05,74.680000000000007,0.05,87.16,0.04,86.45,0.04,86.2,0.06,85.62,7.0000000000000007E-2,86.12,0.05,86.46,7.0000000000000007E-2,86.35,0.08,86.03,0.08,89.46,0.06,75.69,0.08,75.849999999999994,7.0000000000000007E-2,75.290000000000006,0.05,81.39,0.16,75.8,0.05,75.06,0.05,75.55,0.04,76.239999999999995,0.09,74.95,0.04,74.87,0.04,74.959999999999994,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-T1ER-DM",74.995999999999995,0.01,61.999000000000002,2.1000000000000001E-2,59.146000000000001,1.4999999999999999E-2,55.908000000000001,0.02,95.001999999999995,1.4E-2,75,1.7999999999999999E-2,1133.5,4.3,1085.3,4.2,0.54400000000000004,5.0000000000000001E-3,-0.159,2E-3,0.01,6.0000000000000001E-3,0.77549999999999997,5.8999999999999999E-3,28.861000000000001,1E-3,3326,9,358.2,5.6,0.19659999999999997,226.12931999999998,13.029,0.16400000000000001,0.79386904073909503,5172.5550077850567,69.360753889763771,231.62578967011956,985.64445528649753,4186.9105524985589,9.7602354995068134E-3,29.618137570929989,58.352130959260904,14.099959986248358,13.148241033230232,1.3920299260524417E-2,38.157088099451066,8.7809110720388339E-3,27.607975391234032,8.741976885038194E-3,23.699848991415578,78.837016589355898,64.77913337594795,23.50623906838527,{"$f":"(XZ35-YL35)*XT35","v":31614.131206411676},{"$f":"0.24*(YJ35-YA35)*XT35","v":25430.20745996448},{"$f":"XK35-XM35","v":2967.8},{"$f":"YO35*3.413/YM35","v":0.32039790478081248},{"$f":"YM35-(XM35-XU35)*3.413","v":30628.322859437438},{"$f":"YN35-(XM35-XU35)*3.413","v":24444.399112990242},{"$f":"YQ35/XK35","v":9.2087561212980873},{"$f":"(YA35-YW35)/(YJ35-YW35)","v":0.21941925987906663},{"$f":"-XZ35+YL35","v":-6.1118985025447188},{"$f":"-YJ35+YA35","v":-20.484885630094993},{"$f":"(-(-0.0182984848494437-(YU35/YV35))+SQRT((-0.0182984848494437-(YU35/YV35))^2-4*0.00577826340327261*(6.76723916086377-XZ35+(YU35/YV35)*YJ35)))/(2*0.00577826340327261)","v":52.593881731940222},{"$f":"XT35*(XZ35-YL35)","v":31614.131206411676},{"$f":"XT35*(YG35-YI35)","v":20214.998780437923},{"$f":"XT35*(YI35-YL35)","v":1001.4579769273018},{"$f":"XW35*(YE35-YG35)","v":10397.674449046448},{"$f":"SUM(YY35:ZA35)","v":31614.131206411672},{"$f":"ZB35/YX35","v":0.99999999999999989}]
[5,"C-75629575-T2E3-1","30N0027","C-75629575-T2E3-1","2 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/11/2014","23:42:30","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.9,15,0,17224,33,16415,67,-1803,74,15419,75,null,939,null,7.5,null,112.64,0.01,58.01,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.1723723719999999,"Factory charge, 3 turns, Econo 2 Fingers open damper, tape around damper perimiter frame gaps, unsealed cab,--cab, 53.5% inlet 52% outlet Meriam, adjust code tester speed to match total static of run C-T2EM3-SPWCT-SR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 2F: with flow meter: new filter drier: with isolation ball valves: with code",75.003,1.2999999999999999E-2,62,2.3E-2,94.998000000000005,7.0000000000000001E-3,75.001999999999995,2.5000000000000001E-2,74.41,0.05,61.02,0.03,66.44,0.02,8.0000000000000002E-3,2E-3,0.79079999999999995,2.3999999999999998E-3,17224,33,-1803,74,4.63,2.5000000000000001E-2,null,null,11.028228228,null,null,null,229.7,0.9,229.7,0.9,229.7,0.9,13.4,0,13.4,0,13.4,0,2967.8,5.0999999999999996,2967.8,5.0999999999999996,2967.8,5.0999999999999996,230,0.9,230,0.9,230,0.9,1.6,0,1.6,0,1.6,0,null,227.8,0.9,227.8,0.9,227.8,0.9,12.7,0,12.7,0,12.7,0,2774.8,4.5999999999999996,null,null,null,null,null,null,null,null,null,228.3,0.9,0.7,0,169.7,0.8,23,null,3328.5,487,488,489,0.7,0.7,0.8,380,0.63,7.5,15.4,null,null,null,null,null,null,null,null,null,null,null,null,264.75,0.17,182.86,0.04,121.25,0.05,61.61,0.06,244.71,0.22,103.14,0.04,115.47,7.0000000000000007E-2,12.33,0.08,78.55,0.04,67.55,0.04,46.35,0.03,null,null,79.31,0.02,70.180000000000007,0.04,46.83,0.01,23.35,0.04,525.9,0.51,40.47,0.01,36724,45,37956,41,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,248.41,0.21,103.98,0.04,116.56,0.06,12.59,7.0000000000000007E-2,247,0.2,116.15,0.06,13.13,7.0000000000000007E-2,21.2,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.61,0.06,61.97,7.0000000000000007E-2,61.76,0.09,61.74,0.06,61.49,0.06,61.12,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.7,0.05,null,null,94.67,0.08,94.64,0.08,94.86,0.06,94.91,0.08,94.89,0.08,94.91,7.0000000000000007E-2,null,null,null,null,null,null,null,null,94.85,7.0000000000000007E-2,null,null,103.02,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.79,0.09,95.12,0.08,74.650000000000006,7.0000000000000007E-2,74.680000000000007,0.05,74.5,0.05,74.78,0.09,74.8,0.09,74.790000000000006,0.09,74.650000000000006,0.06,89.75,7.0000000000000007E-2,88.87,0.05,88.99,0.05,89.26,0.06,88.87,0.03,87.94,0.08,89.83,7.0000000000000007E-2,89.49,0.08,88.79,0.08,76.150000000000006,0.06,80.099999999999994,0.14000000000000001,78.78,0.13,83.16,0.14000000000000001,75.83,0.04,75.63,0.04,75.78,0.06,77.62,0.14000000000000001,75.510000000000005,0.06,75.09,0.04,75.75,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-T2ER-DM",75.003,1.2999999999999999E-2,62,2.3E-2,60.959000000000003,7.0000000000000001E-3,57.484000000000002,1.2E-2,94.998000000000005,7.0000000000000001E-3,75.001999999999995,2.5000000000000001E-2,1140.3,1.7,1099.8,1.7,0.51600000000000001,3.0000000000000001E-3,-0.12,1E-3,8.0000000000000002E-3,2E-3,0.79079999999999995,2.3999999999999998E-3,29.15,3.0000000000000001E-3,3330,8,361,5.6,0.27702770277027677,319.16361636163583,13.029,0.126,0.80719083204574871,5183.898972865687,66.669702803149605,324.0193190450513,1378.8172778390044,3805.0816950266826,1.0147880346469341E-2,30.414824009325127,60.151809167954255,14.099880713108599,13.198173876096618,1.3923009908537207E-2,38.159093707267274,8.7799165855169062E-3,27.608594414380043,9.2507429262720948E-3,24.695576965665616,80.357743261311185,65.836679064551021,24.49853576696805,{"$f":"(XZ36-YL36)*XT36","v":30669.440542732191},{"$f":"0.24*(YJ36-YA36)*XT36","v":25138.925038162739},{"$f":"XK36-XM36","v":2969},{"$f":"YO36*3.413/YM36","v":0.3304004514161667},{"$f":"YM36-(XM36-XU36)*3.413","v":29664.891238399341},{"$f":"YN36-(XM36-XU36)*3.413","v":24134.375733829889},{"$f":"YQ36/XK36","v":8.908375747267069},{"$f":"(YA36-YW36)/(YJ36-YW36)","v":0.22697961734655722},{"$f":"-XZ36+YL36","v":-5.9162882423570764},{"$f":"-YJ36+YA36","v":-20.20593409335693},{"$f":"(-(-0.0182984848494437-(YU36/YV36))+SQRT((-0.0182984848494437-(YU36/YV36))^2-4*0.00577826340327261*(6.76723916086377-XZ36+(YU36/YV36)*YJ36)))/(2*0.00577826340327261)","v":54.218802365601881},{"$f":"XT36*(XZ36-YL36)","v":30669.440542732191},{"$f":"XT36*(YG36-YI36)","v":15100.788160330545},{"$f":"XT36*(YI36-YL36)","v":1021.4416675405337},{"$f":"XW36*(YE36-YG36)","v":14547.210714861114},{"$f":"SUM(YY36:ZA36)","v":30669.440542732191},{"$f":"ZB36/YX36","v":1}]
[5,"C-75629575-T3E3","30N0028","C-75629575-T3E3","3 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/12/2014","2:32:39","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.9,15.2,0,14084,30,13373,60,-6256,72,7822,80,null,939,null,8.3000000000000007,null,113.19,0.01,79.150000000000006,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2092050209999998,"Factory charge, 3 turns, Econo 3 Fingers open damper, tape around damper perimiter frame gaps, unsealed cab,--cab, 53.5% inlet 52% outlet Meriam, adjust code tester speed to match total static of run C-T3EM3-SPWCT-SR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo open 3F: with flow meter: new filter drier: with isolation ball valves: with code",74.994,7.0000000000000001E-3,61.999000000000002,2.1000000000000001E-2,95,8.0000000000000002E-3,75.001000000000005,1.2E-2,74.42,0.05,63.57,0.05,68.17,0.02,2.4E-2,5.0000000000000001E-3,0.81910000000000005,3.5000000000000001E-3,14084,30,-6256,72,2.3380000000000001,2.5000000000000001E-2,null,null,11.213389121000001,null,null,null,229.8,0.9,229.8,0.9,229.8,0.9,13.5,0,13.5,0,13.5,0,2981,6.4,2981,6.4,2981,6.4,230,0.9,230,0.9,230,0.9,1.7,0,1.7,0,1.7,0,null,227.8,1,227.8,1,227.8,1,12.8,0,12.8,0,12.8,0,2787.8,6.1,null,null,null,null,null,null,null,null,null,228.3,1,0.7,0,170.1,0.9,23,null,3344.8,488,489,490,0.8,0.7,0.9,410,0.62,8.3000000000000007,15.8,null,null,null,null,null,null,null,null,null,null,null,null,266.27,0.19,184.64,0.03,121.69,0.05,62.95,0.06,246.05,0.22,102.82,0.05,115.89,7.0000000000000007E-2,13.07,0.08,80.16,0.05,71.099999999999994,0.06,47.4,0.03,null,null,80.86,0.03,73.12,0.05,47.84,0.02,25.27,0.06,532.28,0.55000000000000004,40.369999999999997,0.02,37520,47,38762,43,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,249.83,0.21,103.73,0.06,117,0.06,13.27,0.06,248.39,0.22,116.58,0.06,13.91,7.0000000000000007E-2,23.7,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.18,0.28000000000000003,64.040000000000006,7.0000000000000007E-2,63.91,0.19,63.9,0.11,63.98,0.27,63.6,0.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.3,0.05,null,null,94.38,0.15,94.19,0.15,94.72,0.09,94.64,0.11,94.79,7.0000000000000007E-2,94.82,7.0000000000000007E-2,null,null,null,null,null,null,null,null,94.76,7.0000000000000007E-2,null,null,102.66,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.49,7.0000000000000007E-2,94.88,7.0000000000000007E-2,74.47,0.05,74.569999999999993,0.03,74.5,0.03,74.48,0.06,74.52,0.06,74.55,0.05,74.540000000000006,0.04,92.59,0.04,92.06,0.04,91.89,0.05,92.41,0.05,91.97,0.04,90.54,0.09,93.38,0.06,93.22,7.0000000000000007E-2,88.77,0.11,80.849999999999994,0.12,90.04,0.13,86.05,0.19,82.49,0.09,75.959999999999994,0.04,76.239999999999995,0.04,75.94,0.04,79.790000000000006,0.09,75.58,0.03,75.819999999999993,0.03,76.81,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-T3ER-DM",74.994,7.0000000000000001E-3,61.999000000000002,2.1000000000000001E-2,63.581000000000003,1.6E-2,59.76,1.6E-2,95,8.0000000000000002E-3,75.001000000000005,1.2E-2,1160,2.5,1119.0999999999999,2.4,0.46800000000000003,7.0000000000000001E-3,-7.0999999999999994E-2,1E-3,2.4E-2,5.0000000000000001E-3,0.81910000000000005,3.5000000000000001E-3,29.286000000000001,2E-3,3346,9,363.9,5.5,0.43444794321987268,493.4459739091314,13.03,6.3E-2,0.81964689047592776,5244.584928288592,61.528999181102357,544.92236309478835,2318.831665353101,2925.753262935491,1.105409407831714E-2,32.272601466307648,62.761353109524073,14.099920349633747,13.270830952624463,1.392165457242138E-2,38.15809089120382,8.7813836073825612E-3,27.608004687952807,1.0037573824976522E-2,26.19266617602652,83.885402512391323,68.211848010581193,25.992298016131233,{"$f":"(XZ37-YL37)*XT37","v":32937.584819874071},{"$f":"0.24*(YJ37-YA37)*XT37","v":26588.849069448293},{"$f":"XK37-XM37","v":2982.1},{"$f":"YO37*3.413/YM37","v":0.30900587750012543},{"$f":"YM37-(XM37-XU37)*3.413","v":31905.592594079175},{"$f":"YN37-(XM37-XU37)*3.413","v":25556.856843653397},{"$f":"YQ37/XK37","v":9.535443094464787},{"$f":"(YA37-YW37)/(YJ37-YW37)","v":0.23265804399324264},{"$f":"-XZ37+YL37","v":-6.2803034501764152},{"$f":"-YJ37+YA37","v":-21.12404940286725},{"$f":"(-(-0.0182984848494437-(YU37/YV37))+SQRT((-0.0182984848494437-(YU37/YV37))^2-4*0.00577826340327261*(6.76723916086377-XZ37+(YU37/YV37)*YJ37)))/(2*0.00577826340327261)","v":56.356542351014681},{"$f":"XT37*(XZ37-YL37)","v":32937.584819874071},{"$f":"XT37*(YG37-YI37)","v":7422.8630280750058},{"$f":"XT37*(YI37-YL37)","v":1050.8478314957426},{"$f":"XW37*(YE37-YG37)","v":24463.873960303321},{"$f":"SUM(YY37:ZA37)","v":32937.584819874071},{"$f":"ZB37/YX37","v":1}]
[5,"C-75629575-TE3","30N0029","C-75629575-TE3","closed","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/11/2014","14:48:22","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.9,15,0,21752,40,20819,88,4239,61,25995,73,null,940,null,7.5,null,111.06,0.06,25.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.8534743200000001,"Closed damper, tape around damper perimiter frame gaps, 53.5% inlet 52% outlet--Meriam, adjust code tester speed to match total static of run C-TEM3-SPWCT-SR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: with economizer: with flow meter: new filter drier: with isolation ball valves: with code",74.994,1.4999999999999999E-2,62,2.4E-2,95,1.4E-2,74.998999999999995,0.02,74.349999999999994,0.08,57.32,0.05,64,0.02,3.4000000000000002E-2,3.0000000000000001E-3,0.7712,2.5999999999999999E-3,21752,40,4239,61,7.8540000000000001,2.9000000000000001E-2,null,null,10.579154079,null,null,null,229.7,0.9,229.7,0.9,229.7,0.9,13.4,0,13.4,0,13.4,0,2950,5.7,2950,5.7,2950,5.7,230,0.9,230,0.9,230,0.9,1.6,0,1.6,0,1.6,0,null,227.8,1,227.8,1,227.8,1,12.7,0,12.7,0,12.7,0,2757.6,5.3,null,null,null,null,null,null,null,null,null,228.3,1,0.7,0,169,0.9,23,null,3308.3,482,482,482,0.7,0.7,0.8,380,0.62,7.5,15.4,null,null,null,null,null,null,null,null,null,null,null,null,261.77,0.19,178.19,0.04,120.37,0.06,57.81,7.0000000000000007E-2,242.05,0.23,103.59,0.06,114.64,7.0000000000000007E-2,11.05,0.09,75.3,0.05,57.72,0.3,44.18,0.03,null,null,75.88,0.02,63.2,0.15,44.55,0.02,18.64,0.15,514.42999999999995,0.54,40.61,0.02,35017,59,36240,56,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,245.65,0.22,104.38,0.05,115.71,7.0000000000000007E-2,11.33,7.0000000000000007E-2,244.23,0.22,115.29,7.0000000000000007E-2,11.68,0.08,13.54,0.31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.37,0.05,58.47,0.09,57.74,0.11,58.37,7.0000000000000007E-2,57.23,0.08,57.58,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.59,0.06,null,null,null,null,null,null,null,null,null,null,null,null,104.33,0.05,null,null,94.65,7.0000000000000007E-2,94.66,0.06,94.78,0.05,94.79,0.08,94.7,0.08,94.73,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,103.61,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.75,0.08,95.03,7.0000000000000007E-2,74.53,0.09,74.540000000000006,7.0000000000000007E-2,74.41,0.08,74.61,0.1,74.62,0.1,74.63,0.09,74.52,0.09,78.989999999999995,7.0000000000000007E-2,78.760000000000005,0.06,78.290000000000006,0.08,78.45,0.1,78.489999999999995,0.06,80.41,0.09,76.819999999999993,0.09,78.239999999999995,0.09,91.19,0.08,78.42,0.1,75.2,0.1,75.17,0.1,88.24,0.21,75.25,0.09,75.08,0.08,74.930000000000007,0.09,76.400000000000006,0.15,74.69,0.08,74.739999999999995,7.0000000000000007E-2,74.86,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-TCE-DM",74.994,1.4999999999999999E-2,62,2.4E-2,57.201000000000001,1.0999999999999999E-2,54.125,0.02,95,1.4E-2,74.998999999999995,0.02,1128.2,1.9,1085.0999999999999,1.8,0.57499999999999996,5.0000000000000001E-3,-0.215,2E-3,3.4000000000000002E-2,3.0000000000000001E-3,0.7712,2.5999999999999999E-3,28.884,1E-3,3310,8,358.7,5.6,6.5623750499799877E-2,72.022066173530362,13.029,0.20899999999999999,0.78488301759750445,5169.4833616371234,73.299786614173215,75.991361854190416,323.3696562832763,4846.1137053538469,9.1034344141135756E-3,28.268505743926468,56.4161169824025,14.099905859000126,13.09453871200054,1.3919901703093901E-2,38.156157160819127,8.7820429927739294E-3,27.608726251629978,8.175579176422176E-3,22.610166685368842,76.256413072110135,62.930783486042799,22.418945669420399,{"$f":"(XZ38-YL38)*XT38","v":30239.203478055937},{"$f":"0.24*(YJ38-YA38)*XT38","v":24615.379326167447},{"$f":"XK38-XM38","v":2951.3},{"$f":"YO38*3.413/YM38","v":0.3331035788462367},{"$f":"YM38-(XM38-XU38)*3.413","v":29265.132549770111},{"$f":"YN38-(XM38-XU38)*3.413","v":23641.308397881621},{"$f":"YQ38/XK38","v":8.8414297733444442},{"$f":"(YA38-YW38)/(YJ38-YW38)","v":0.2190688492490232},{"$f":"-XZ38+YL38","v":-5.8495600745060692},{"$f":"-YJ38+YA38","v":-19.840296089707635},{"$f":"(-(-0.0182984848494437-(YU38/YV38))+SQRT((-0.0182984848494437-(YU38/YV38))^2-4*0.00577826340327261*(6.76723916086377-XZ38+(YU38/YV38)*YJ38)))/(2*0.00577826340327261)","v":50.850465223022084},{"$f":"XT38*(XZ38-YL38)","v":30239.203478055937},{"$f":"XT38*(YG38-YI38)","v":25839.970509939019},{"$f":"XT38*(YI38-YL38)","v":988.51386034082361},{"$f":"XW38*(YE38-YG38)","v":3410.7191077760995},{"$f":"SUM(YY38:ZA38)","v":30239.203478055941},{"$f":"ZB38/YX38","v":1.0000000000000002}]
[5,"C-75629575-TOE3","30N0030","C-75629575-TOE3","Fully open","on","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 1","3/12/2014","10:06:20","10 Ton","0:30:00","75/62  95/75","ENG 1","TECH 4","RTU5","RTU5","3","R22","PSC Air Handler","5.5 LBS","208/230/1","TU1","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.3,0.9,15,0,10582,114,9950,69,-10102,216,470,182,null,939,null,7.3,null,111.11,0.13,98.38,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.1758703480000001,"Factory charge, 3 turns, Econo Fully open damper, tape around damper--perimiter frame gaps, unsealed cab, cab, 53.5% inlet 52% outlet Meriam,--adjust code tester speed to match total static of run C-TOEM3-SPWCT-SR","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: Econo Fully open: with flow meter: new filter drier: with isolation ball valves: with code",75.001000000000005,1.4999999999999999E-2,62.003999999999998,3.3000000000000002E-2,95.001000000000005,1.4999999999999999E-2,75,0.02,74.510000000000005,0.04,65.930000000000007,0.08,69.739999999999995,0.02,1E-3,1.2E-2,0.74750000000000005,1.6899999999999998E-2,10582,114,-10102,216,0.14899999999999999,5.0999999999999997E-2,null,null,10.979891957,null,null,null,229.7,0.9,229.7,0.9,229.7,0.9,13.4,0,13.4,0,13.4,0,2973.3,5.2,2973.3,5.2,2973.3,5.2,230,0.9,230,0.9,230,0.9,1.6,0,1.6,0,1.6,0,null,227.8,0.9,227.8,0.9,227.8,0.9,12.7,0,12.7,0,12.7,0,2779.4,4.8,null,null,null,null,null,null,null,null,null,228.3,0.9,0.8,0,170.9,0.9,23,null,3307.6,480,480,480,0.7,0.7,0.8,390,0.63,7.3,15.3,null,null,null,null,null,null,null,null,null,null,null,null,266.02999999999997,0.23,183.28,0.09,121.67,0.06,61.61,0.1,245.84,0.24,102.54,7.0000000000000007E-2,115.87,7.0000000000000007E-2,13.33,0.08,80.180000000000007,7.0000000000000007E-2,59.7,0.72,47.51,0.04,null,null,80.88,0.05,71.790000000000006,0.24,47.95,0.03,23.84,0.22,533.73,0.57999999999999996,40.28,0.02,36585,92,37805,94,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,249.59,0.24,103.53,0.06,116.97,7.0000000000000007E-2,13.44,7.0000000000000007E-2,248.17,0.24,116.55,7.0000000000000007E-2,14.22,7.0000000000000007E-2,12.19,0.7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65.239999999999995,0.35,67.260000000000005,0.1,66.45,0.38,67.02,0.08,66.36,0.46,66.42,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.09,0.06,null,null,93.8,0.25,93.43,0.26,94.46,0.16,94.55,0.17,94.79,0.12,94.78,0.12,null,null,null,null,null,null,null,null,94.72,0.11,null,null,102.33,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.93,0.09,95.35,0.09,74.89,0.04,74.86,0.03,74.599999999999994,0.03,75.09,0.06,75.08,0.06,75.05,0.06,74.84,0.04,93.35,0.08,92.63,0.08,92.1,0.09,93,0.08,92.56,7.0000000000000007E-2,88.88,0.14000000000000001,92.37,0.08,93.36,0.08,81.400000000000006,0.12,84.5,0.09,94.01,0.21,94.5,0.11,75.709999999999994,0.02,76.92,0.03,86.45,0.1,85.71,0.09,76.41,0.03,77.33,0.04,82.94,0.06,84.51,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-TOER-DM",75.001000000000005,1.4999999999999999E-2,62.003999999999998,3.3000000000000002E-2,65.899000000000001,6.2E-2,61.819000000000003,5.6000000000000001E-2,95.001000000000005,1.4999999999999999E-2,75,0.02,1103.9000000000001,12.5,1071.3,12.2,0.40799999999999997,4.0000000000000001E-3,-2.8000000000000001E-2,1E-3,1E-3,1.2E-2,0.74750000000000005,1.6899999999999998E-2,29.582000000000001,1E-3,3332,9,357.3,5.8,0.58850574712643666,660.06804597701125,13.029,2.4E-2,0.87576299773407429,4966.6359875548405,51.349517858267703,741.677562616655,3156.0889380033682,1810.5470495514724,1.2047700209244326E-2,34.312794200577258,65.02323700226593,14.099936545245674,13.335787073175082,1.3920538693801237E-2,38.15710605694683,8.7830267917590708E-3,27.611510117885846,1.0819383465606751E-2,27.611691885652771,87.753235514054879,70.684414886410082,27.397301770426914,{"$f":"(XZ39-YL39)*XT39","v":34346.733575247781},{"$f":"0.24*(YJ39-YA39)*XT39","v":27093.990865372551},{"$f":"XK39-XM39","v":2974.7},{"$f":"YO39*3.413/YM39","v":0.29559291505136254},{"$f":"YM39-(XM39-XU39)*3.413","v":33302.524579698045},{"$f":"YN39-(XM39-XU39)*3.413","v":26049.781869822818},{"$f":"YQ39/XK39","v":9.9947552760198217},{"$f":"(YA39-YW39)/(YJ39-YW39)","v":0.22739702300805895},{"$f":"-XZ39+YL39","v":-6.9154924301503442},{"$f":"-YJ39+YA39","v":-22.729998511788949},{"$f":"(-(-0.0182984848494437-(YU39/YV39))+SQRT((-0.0182984848494437-(YU39/YV39))^2-4*0.00577826340327261*(6.76723916086377-XZ39+(YU39/YV39)*YJ39)))/(2*0.00577826340327261)","v":58.333211014167347},{"$f":"XT39*(XZ39-YL39)","v":34346.733575247781},{"$f":"XT39*(YG39-YI39)","v":-0.90277433258785023},{"$f":"XT39*(YI39-YL39)","v":1064.7976616567712},{"$f":"XW39*(YE39-YG39)","v":33282.838687923613},{"$f":"SUM(YY39:ZA39)","v":34346.733575247796},{"$f":"ZB39/YX39","v":1.0000000000000004}]
[5,"C-55-CE","30N0052","C-55-CE","closed","Off","N/A","3 turns","unsealed","unsealed",null,null,"horizontal",0,0,"CUST 2","6/17/2015","0:48:14","10 Ton","0:10:00","75/62 55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,1.4,2.2000000000000002,0,5674,17,5319,69,2708,61,8385,69,null,942,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.727272726999999,".","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed:installed economizer. No compressor;",74.959999999999994,7.4999999999999997E-2,61.997999999999998,2.1999999999999999E-2,54.999000000000002,4.0000000000000001E-3,51.006,1.7000000000000001E-2,74.45,0.09,70.13,0.05,72.67,0.16,1.0999999999999999E-2,3.0000000000000001E-3,0.79149999999999998,2.8999999999999998E-3,5674,17,2708,61,17.725000000000001,0.246,null,null,null,null,null,null,230.1,1.4,230.1,1.4,230.1,1.4,0,0,0,0,0,0,-0.1,0.2,-0.1,0.2,-0.1,0.2,229.8,1.4,229.8,1.4,229.8,1.4,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0.5,0.3,473,null,null,null,null,null,null,null,null,null,null,230.1,1.4,0,0,98.28,0.04,55.46,0.02,58,0.02,2.5499999999999998,0.03,98.31,0.05,57.49,0.03,58.02,0.03,-0.53,0.02,98.17,0.06,58.23,0.05,57.94,0.04,-0.28000000000000003,0.09,99.12,0.05,56.22,0.09,58.47,0.03,null,null,98.97,0.04,56.18,0.09,58.38,0.02,-2.2000000000000002,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.23,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69.959999999999994,0.05,70.069999999999993,0.05,70.150000000000006,0.05,70.19,0.03,69.989999999999995,0.05,70.05,0.04,null,null,null,null,null,null,56.63,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.6,0.09,62.63,0.1,57.45,0.03,54.65,0.04,56.01,0.09,73.709999999999994,0.09,74.03,0.08,74.61,0.06,74.7,0.06,74.89,0.06,74.88,0.06,74.930000000000007,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.71,0.05,null,null,null,null,null,null,null,null,null,null,null,null,74.489999999999995,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.78,0.05,59.83,0.22,67.540000000000006,0.39,72.61,0.04,62.88,0.18,68.849999999999994,0.11,72.819999999999993,0.12,74.819999999999993,0.04,74.41,0.03,74.37,7.0000000000000007E-2,65.87,0.23,75.06,0.04,74.510000000000005,0.06,68.099999999999994,0.3,59.52,0.15,74.599999999999994,0.05,64.66,0.41,54.88,0.09,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.959999999999994,7.4999999999999997E-2,61.997999999999998,2.1999999999999999E-2,70.343999999999994,7.3999999999999996E-2,59.582000000000001,1.6E-2,54.999000000000002,4.0000000000000001E-3,51.006,1.7000000000000001E-2,1145.3,2.2000000000000002,1096.7,2,0.56000000000000005,2E-3,-0.184,1E-3,1.0999999999999999E-2,3.0000000000000001E-3,0.79149999999999998,2.8999999999999998E-3,29.242999999999999,1E-3,473,5,472.5,5.2,0.17564250288061725,192.62713290917296,13.03,0.184,1.1122440362829993,5117.2506769201291,72.150770393700796,192.62345980280287,887.01829356370672,4230.2323833564224,8.4760557132421577E-3,26.424462925596039,69.231755963716992,13.029503080184339,13.428695277706945,6.9847663014663336E-3,20.781161937701349,8.7887574443450394E-3,27.607781183014563,8.3243601977757951E-3,25.974698714266157,71.509381841026311,60.257221681204655,25.703649273884519]
[5,"C-EB10-55-CE","30N0053","C-EB10-55-CE","closed","Off","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,10,"CUST 2","6/18/2015","11:17:04","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.2,1.1000000000000001,2.1,0,5385,22,5147,47,2454,70,7842,80,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.649681528999999,"10% evaporator coil block, economizer closed (2V), no compressor, factory charge (5.5 lbs)--unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley--3 turns open from fully closed, adjust code tester speed to match total st","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer.;with outlet hose, with code tester, 6\" evap coil blockage",74.991,1.2999999999999999E-2,61.991999999999997,3.7999999999999999E-2,54.991999999999997,8.0000000000000002E-3,50.999000000000002,1.9E-2,74.569999999999993,0.06,70.33,0.06,72.34,0.01,1.9E-2,3.0000000000000001E-3,1.0687,3.3E-3,5385,22,2454,70,16.643999999999998,0.245,null,null,null,null,null,null,230.2,1.1000000000000001,230.2,1.1000000000000001,230.2,1.1000000000000001,0,0,0,0,0,0,0,0.2,0,0.2,0,0.2,229.8,1.1000000000000001,229.8,1.1000000000000001,229.8,1.1000000000000001,2.1,0,2.1,0,2.1,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0.5,0.3,null,null,null,null,null,null,null,null,null,null,null,230.2,1.1000000000000001,0,0,99.76,0.04,55.99,0.03,58.8,0.02,2.81,0.02,100.23,0.02,58.77,0.03,59.06,0.01,-0.28999999999999998,0.03,100.06,0.04,59.4,0.04,58.97,0.02,-0.43,0.06,100.84,0.02,57.91,0.06,59.39,0.01,null,null,100.17,0.03,57.97,0.04,59.03,0.02,-1.05,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.48,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.209999999999994,0.05,70.28,0.06,70.37,0.05,70.53,0.05,70.290000000000006,0.05,70.260000000000005,0.06,null,null,null,null,59.55,0.05,58.41,0.06,null,null,null,null,null,null,null,null,null,null,59.4,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,67.42,0.14000000000000001,69.25,0.15,58.85,0.05,54.44,0.05,56,0.13,74.28,7.0000000000000007E-2,74.39,0.05,74.760000000000005,0.04,74.83,0.04,74.959999999999994,0.04,74.98,0.04,74.989999999999995,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.510000000000005,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.54,0.06,63.45,0.91,59.53,0.2,71.37,0.05,69.63,0.72,75.23,0.03,74.400000000000006,0.06,70.69,0.21,74.62,0.04,66.98,0.2,73.56,0.22,null,null,74.349999999999994,0.11,74.42,0.09,69.14,0.82,65.23,0.14000000000000001,61.84,0.45,54.97,0.1,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.991,1.2999999999999999E-2,61.991999999999997,3.7999999999999999E-2,70.548000000000002,1.4E-2,59.706000000000003,2.4E-2,54.991999999999997,8.0000000000000002E-3,50.999000000000002,1.9E-2,1130.5,1.7,1082,1.7,0.55500000000000005,1E-3,-0.19500000000000001,1E-3,1.9E-2,3.0000000000000001E-3,1.0687,3.3E-3,29.210999999999999,1E-3,471,5,470.6,5,0.16565828291414558,179.24226211310551,13.029,0.19500000000000001,1.1264215148805625,5049.090753827255,70.54810393700788,179.24439263186082,825.42082256354468,4223.6699312637102,8.4840672214526285E-3,26.487124175343332,69.42157848511944,13.029309733803942,13.43410196154313,6.9826918099913761E-3,20.777208541879528,8.7774771107841671E-3,27.60299812753258,8.354152000719383E-3,26.056954982377224,71.730522066005321,60.351759320642508,25.782435647136715]
[5,"C-EB20-55-CE","30N0054","C-EB20-55-CE","closed","Off","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,20,"CUST 2","6/18/2015","12:58:46","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,1,2.1,0,5090,14,4844,55,2518,73,7611,72,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.29764454,"20% evaporator coil block, economizer closed (2V), no compressor, factory charge (5.5 lbs)--unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley--3 turns open from fully closed, adjust code tester speed to match total st","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer.;with outlet duct, with code tester, 9\" evap coil blockage",74.971000000000004,2.3E-2,61.988,2.5999999999999999E-2,54.994999999999997,5.0000000000000001E-3,51.000999999999998,0.02,74.53,0.04,70.48,0.05,72.69,0.05,1.2E-2,2E-3,1.0405,3.0999999999999999E-3,5090,14,2518,73,16.309000000000001,0.23,null,null,null,null,null,null,230.1,1,230.1,1,230.1,1,0,0,0,0,0,0,0,0.2,0,0.2,0,0.2,229.8,1,229.8,1,229.8,1,2.1,0,2.1,0,2.1,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0.5,0.3,null,null,null,null,null,null,null,null,null,null,null,230.2,1,0,0,97.73,0.02,55.67,0.01,57.68,0.01,2.02,0.02,97.77,0.05,56.95,0.03,57.71,0.02,-0.76,0.04,98.02,0.04,58.89,0.05,57.84,0.02,-1.04,0.05,98.85,0.03,55.33,0.02,58.3,0.02,null,null,97.86,0.02,56.37,0.03,57.76,0.01,-1.4,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.98,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.25,0.03,70.41,0.04,70.48,0.03,70.599999999999994,0.02,70.42,0.04,70.38,0.04,null,null,null,null,58.26,0.05,56.24,0.05,null,null,null,null,null,null,null,null,null,null,58.89,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61,0.09,62.03,0.09,56.94,0.04,54.6,0.03,56.13,0.12,74.290000000000006,0.05,74.41,0.03,74.81,0.03,74.86,0.02,74.98,0.02,74.989999999999995,0.02,74.989999999999995,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.489999999999995,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.67,0.05,69.59,0.43,60.49,0.15,72.86,7.0000000000000007E-2,70.540000000000006,0.28999999999999998,75.180000000000007,0.02,73.430000000000007,1.39,71.650000000000006,0.14000000000000001,74.61,0.03,67.98,0.13,74.38,0.08,66.06,0.14000000000000001,74.5,0.05,74.540000000000006,0.03,69.900000000000006,0.37,68.959999999999994,0.26,65.5,0.3,54.99,0.1,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.971000000000004,2.3E-2,61.988,2.5999999999999999E-2,70.718000000000004,0.02,59.741,1.2999999999999999E-2,54.994999999999997,5.0000000000000001E-3,51.000999999999998,0.02,1115.9000000000001,1.7,1066.9000000000001,1.6,0.54100000000000004,1E-3,-0.19,1E-3,1.2E-2,2E-3,1.0405,3.0999999999999999E-3,29.202000000000002,1E-3,467,5,466.1,4.9000000000000004,0.15583700440528631,166.26249999999996,13.029,0.19,1.1364887743727987,4982.3397308984604,67.808803685039379,166.2649785666581,765.64596578535873,4216.693765113102,8.5034912662581789E-3,26.552043008350424,69.58151122562721,13.029388463853188,13.438264674080395,6.9830494597846399E-3,20.778326042269644,8.7795654134891765E-3,27.600405386296941,8.3360642837507961E-3,26.078626553603716,71.909749628548823,60.448494260844022,25.801662861248712]
[5,"C-EB35-55-CE","30N0055","C-EB35-55-CE","closed","Off","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,35,"CUST 2","6/18/2015","14:08:38","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,1,2.1,0,4900,13,4667,54,2456,59,7358,67,null,945,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.960954447000001,"35% evaporator coil block, economizer closed (2V), no compressor, factory charge--(5.5 lbs) unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow.--4.75\" ID pulley 3 turns open from fully closed, adjust code tester speed to match--total s","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer.;with outlet duct, with code tester, 14.5\" evap coil blockage",74.957999999999998,2.1000000000000001E-2,61.993000000000002,0.02,54.973999999999997,1.0999999999999999E-2,51.005000000000003,1.7999999999999999E-2,74.45,0.05,70.44,0.08,72.459999999999994,0.02,1.7999999999999999E-2,2E-3,0.98440000000000005,2.3E-3,4900,13,2456,59,15.967000000000001,0.224,null,null,null,null,null,null,230.1,1,230.1,1,230.1,1,0,0,0,0,0,0,0,0.2,0,0.2,0,0.2,229.8,1,229.8,1,229.8,1,2.1,0,2.1,0,2.1,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0.5,0.3,null,null,null,null,null,null,null,null,null,null,null,230.1,1,0,0,96.06,0.03,55.48,0.02,56.76,0.02,1.28,0.04,96.37,0.04,56.17,0.03,56.93,0.03,-0.76,0.04,96.74,0.05,57.54,0.09,57.13,0.03,-0.41,0.11,96.43,0.03,55.1,0.02,56.96,0.02,null,null,96.79,0.01,55.62,0.03,57.16,0.01,-1.54,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.86,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.290000000000006,0.05,70.5,0.04,70.569999999999993,0.03,70.650000000000006,0.03,70.510000000000005,0.04,70.459999999999994,0.04,null,null,null,null,57.09,0.09,55.7,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,57.54,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.79,0.08,59.52,0.08,56.11,0.06,54.6,0.04,56.08,0.14000000000000001,73.849999999999994,7.0000000000000007E-2,74.069999999999993,0.06,74.599999999999994,0.04,74.680000000000007,0.03,74.88,0.03,74.87,0.03,74.94,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.45,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.66,0.05,60.84,0.16,60.5,0.15,74.61,0.04,63.06,0.18,null,null,70.709999999999994,0.17,74.84,0.04,73.62,0.08,65.14,0.26,62.66,0.15,76.05,0.09,72.94,0.17,67.48,0.27,64.06,0.43,74.59,0.03,61.56,0.22,54.98,0.08,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.957999999999998,2.1000000000000001E-2,61.993000000000002,0.02,70.748999999999995,0.02,59.76,1.4E-2,54.973999999999997,1.0999999999999999E-2,51.005000000000003,1.7999999999999999E-2,1085.3,1.3,1037.5,1.2,0.51100000000000001,1E-3,-0.18099999999999999,1E-3,1.7999999999999999E-2,2E-3,0.98440000000000005,2.3E-3,29.184999999999999,1E-3,461,5,460.3,4.9000000000000004,0.15207165732586084,157.77434447558062,13.029,0.18099999999999999,1.1677971380229428,4845.4183395823848,62.283657480314965,157.77381001970622,726.57093683290577,4118.8474027494794,8.5166494412023848E-3,26.581045737889564,69.581202861977047,13.02891172945365,13.439087285415354,6.9901102936494874E-3,20.780884821099797,8.7859332650724372E-3,27.60420293188524,8.3407150974465077E-3,26.091261898469327,71.969728745531683,60.491238532859434,25.806665908474201]
[5,"C-EB5-55-CE","30N0056","C-EB5-55-CE","closed","Off","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,5,"CUST 2","6/18/2015","16:10:53","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,1.4,2.1,0,5359,16,5122,59,2652,54,8013,53,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.976694914999999,"5% evaporator coil block, economizer closed (2V), no compressor, factory charge--(5.5 lbs) unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow.--4.75\" ID pulley 3 turns open from fully closed, adjust code tester speed to match--total st","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer.;with outlet hose, with code tester, 19\" evap coil blockage",74.974000000000004,0.02,61.994,2.1000000000000001E-2,54.996000000000002,1.2E-2,51,2.5999999999999999E-2,74.45,0.05,70.25,0.05,72.430000000000007,0.02,0.01,3.0000000000000001E-3,1.079,2.8E-3,5359,16,2652,54,16.991,0.221,null,null,null,null,null,null,230.1,1.4,230.1,1.4,230.1,1.4,0,0,0,0,0,0,0,0.2,0,0.2,0,0.2,229.8,1.4,229.8,1.4,229.8,1.4,2.1,0,2.1,0,2.1,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0.5,0.3,null,null,null,null,null,null,null,null,null,null,null,230.1,1.4,0,0,95.88,0.06,55.61,0.02,56.65,0.03,1.05,0.04,95.8,7.0000000000000007E-2,55.52,0.01,56.61,0.04,-1.0900000000000001,0.04,95.89,7.0000000000000007E-2,59.9,0.05,56.67,0.04,-3.24,7.0000000000000007E-2,95.69,0.02,55.94,0.01,56.55,0.01,null,null,95.93,0.03,55.29,0.01,56.68,0.02,-1.39,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-0.62,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.2,0.05,70.290000000000006,0.04,70.37,0.03,70.55,0.02,70.37,0.04,70.27,0.04,null,null,null,null,59.66,0.05,55.66,0.04,null,null,null,null,null,null,null,null,null,null,59.9,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.06,0.05,57.42,0.05,55.5,0.03,54.66,0.09,55.99,0.11,74.44,0.05,74.489999999999995,0.04,74.86,0.05,74.900000000000006,0.04,75,0.03,75,0.03,74.989999999999995,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.56,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.69,0.09,65.16,0.33,66.03,0.46,74.84,0.03,60.03,0.22,74.86,0.04,72.95,0.11,73.75,0.1,74.45,0.04,70.260000000000005,0.28999999999999998,61.32,0.28999999999999998,70.739999999999995,0.28000000000000003,73.650000000000006,0.18,63.97,0.17,63.45,0.31,72.23,0.24,67.61,0.4,54.96,0.16,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.974000000000004,0.02,61.994,2.1000000000000001E-2,70.575999999999993,1.4E-2,59.67,1.9E-2,54.996000000000002,1.2E-2,51,2.5999999999999999E-2,1136.7,1.5,1086.5,1.4,0.56200000000000006,1E-3,-0.192,2E-3,0.01,3.0000000000000001E-3,1.079,2.8E-3,29.175999999999998,1E-3,472,5,471.2,5.2,0.16408048853739163,178.27345079587602,13.029,0.192,1.1186736624799201,5076.6017231029346,71.735007559055134,178.27624084040988,820.95630115130837,4255.6454219516263,8.4916419258344988E-3,26.500677925683444,69.457326337520072,13.02940782039644,13.434577640712256,6.9822831007333511E-3,20.777737322663206,8.782812245564018E-3,27.604690051536142,8.3248979373868031E-3,26.031823582159475,71.752164355401405,60.371648823418781,25.759207000399265]
[5,"C-EB50-55-CE","30N0057","C-EB50-55-CE","closed","Off","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,50,"CUST 2","6/18/2015","15:04:47","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,55,51,5.5,null,5.5,null,230.1,1,2,0,4711,14,4483,33,2359,58,7072,64,null,945,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.750556792999999,"50% evaporator coil block, economizer closed (2V), no compressor, factory charge--(5.5 lbs) unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow.--4.75\" ID pulley 3 turns open from fully closed, adjust code tester speed to match--total s","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer.;with code tester, with ouitlet hose, 19\" evap coil blockage",74.988,1.4999999999999999E-2,61.991999999999997,2.7E-2,54.994999999999997,8.0000000000000002E-3,51.000999999999998,2.1999999999999999E-2,74.599999999999994,0.04,70.58,0.03,72.56,0.01,8.9999999999999993E-3,2E-3,0.90300000000000002,1.9E-3,4711,14,2359,58,15.734999999999999,0.23,null,null,null,null,null,null,230.1,1,230.1,1,230.1,1,0,0,0,0,0,0,0,0.2,0,0.2,0,0.2,229.8,1,229.8,1,229.8,1,2,0,2,0,2,0,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0.5,0.3,null,null,null,null,null,null,null,null,null,null,null,230.2,1,0,0,96.21,0.04,55.46,0.01,56.84,0.02,1.39,0.03,96,0.03,55.69,0.01,56.73,0.02,-1.04,0.02,96.24,0.04,57.29,0.04,56.86,0.02,-0.42,0.05,95.95,0.03,55.24,0.02,56.7,0.02,null,null,96.28,0.02,55.36,0.02,56.88,0.01,-1.52,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-1.46,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.3,0.02,70.5,0.02,70.56,0.02,70.64,0.02,70.48,0.02,70.45,0.02,null,null,null,null,57.01,0.04,55.63,0.03,null,null,null,null,null,null,null,null,null,null,57.29,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.86,0.04,58.41,0.03,55.77,0.03,54.76,0.05,56.07,0.11,73.56,0.08,73.89,7.0000000000000007E-2,74.63,0.05,74.709999999999994,0.04,74.94,0.02,74.92,0.02,75.010000000000005,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.48,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.79,0.06,60.63,0.13,59.87,0.15,74.760000000000005,0.02,65.27,0.25,null,null,71.510000000000005,0.15,74.83,0.03,73.67,0.08,66.14,0.21,65.17,0.25,null,null,73.09,0.14000000000000001,70.819999999999993,0.24,67.25,0.3,73.989999999999995,0.09,61.2,0.22,54.96,0.1,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.988,1.4999999999999999E-2,61.991999999999997,2.7E-2,70.762,7.0000000000000001E-3,59.747999999999998,1.2999999999999999E-2,54.994999999999997,8.0000000000000002E-3,51.000999999999998,2.1999999999999999E-2,1039.3,1.1000000000000001,993.2,1.1000000000000001,0.46400000000000002,1E-3,-0.16400000000000001,1E-3,8.9999999999999993E-3,2E-3,0.90300000000000002,1.9E-3,29.178000000000001,0,449,5,448.9,5,0.15085279847946775,149.82699944980737,13.029,0.16400000000000001,1.2095287774477297,4639.9628556119351,54.140192251968507,149.82923300340681,689.95977862999905,3950.0030769819359,8.5112501605992957E-3,26.588210762652299,69.552471222552271,13.029388463853188,13.439331723222599,6.9830494597846399E-3,20.778326042269644,8.7781859063916553E-3,27.603042067189879,8.3300888412233386E-3,26.082821724020658,72.023327264601875,60.502585131643947,25.788061303348766]
[5,"C-R100-EB0-CB0-95CE","30N0058","C-R100-EB0-CB0-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,0,"CUST 2","6/22/2015","10:11:08","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230,1,16,0,18687,25,18192,41,451,83,19138,92,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.4016370309999999,"Baseline 100% factory charge, 0% evaporator and condenser blockage, economizer closed (2V),--factory charge (5.5 lbs) 95F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns op","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Cond/Evap Coil are blocked 0\"., with outlet hose, with code tester",74.998000000000005,1.4E-2,62.003999999999998,2.9000000000000001E-2,95.025999999999996,1.0999999999999999E-2,75.001000000000005,2.1000000000000001E-2,74.44,0.04,59.28,0.02,64.94,0.04,7.0000000000000001E-3,2E-3,1.0568,2.0999999999999999E-3,18687,25,451,83,5.4020000000000001,0.03,null,null,null,null,null,null,230,1,230,1,230,1,13.8,0,13.8,0,13.8,0,3066.9,4.8,3066.9,4.8,3066.9,4.8,229.9,1,229.9,1,229.9,1,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,228.3,1,228.3,1,228.3,1,13,0,13,0,13,0,2846.3,4.0999999999999996,null,null,null,null,null,null,null,null,null,228.8,1,0.7,0,170.9,0.9,13,0.2,3506,null,null,null,null,null,null,null,null,null,null,230.3,1,0,0,257.3,0.21,102.69,0.04,119.17,0.06,16.48,0.04,273.87,0.2,179.46,0.03,123.81,0.05,55.65,0.05,256.67,0.2,102.39,0.03,118.99,0.06,16.600000000000001,0.05,78.3,0.03,66.31,0.08,46.26,0.02,null,null,77.19,0.02,63.07,0.16,45.55,0.02,17.52,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.059999999999999,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.47,0.04,58.79,0.03,58.84,0.03,58.78,0.02,58.63,0.03,58.72,0.03,null,null,null,null,54.96,0.21,58.09,0.16,null,null,null,null,null,null,null,null,null,null,102.39,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,148.82,0.05,87.21,0.09,181.75,7.0000000000000007E-2,95.23,0.09,94.25,7.0000000000000007E-2,75.16,0.03,75.08,0.03,74.92,0.04,74.959999999999994,0.04,74.900000000000006,0.03,74.95,0.03,75.02,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.58,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.08,0.1,85.13,0.25,85.23,0.27,74.81,0.03,90.65,0.32,75.67,0.04,76.95,0.09,76.260000000000005,7.0000000000000007E-2,75.11,0.04,79.099999999999994,0.28999999999999998,87.12,0.28999999999999998,77.290000000000006,0.13,75.28,0.05,81.89,0.41,90.21,0.26,80.28,0.14000000000000001,83.52,0.28999999999999998,95.21,0.1,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE",74.998000000000005,1.4E-2,62.003999999999998,2.9000000000000001E-2,59.432000000000002,0.01,56.170999999999999,8.0000000000000002E-3,95.025999999999996,1.0999999999999999E-2,75.001000000000005,2.1000000000000001E-2,1113.8,1.1000000000000001,1085.8,1.1000000000000001,0.56599999999999995,1E-3,-0.20100000000000001,1E-3,7.0000000000000001E-3,2E-3,1.0568,2.0999999999999999E-3,29.356000000000002,0,3543,8,475.8,5.3,0.17564250288061725,192.62713290917296,13.03,0.184,1.1295901860795818,5079.5948025761927,72.199031307086599,209.4363620597629,891.18507526018175,4188.4097273160114,9.6840611299264471E-3,29.461800097575892,58.30240981392042,14.100529814098461,13.156167489207441,1.3915429353158535E-2,38.157623993533882,8.7837355997183262E-3,27.611554066814552,8.8287794212409659E-3,23.863987102178722,78.538816958036321,64.568749862575544,23.588457488769976,{"$f":"(XZ46-YL46)*XT46","v":29834.200589439832},{"$f":"0.24*(YJ46-YA46)*XT46","v":24670.25965249605},{"$f":"XK46-XM46","v":3067.2},{"$f":"YO46*3.413/YM46","v":0.35088433385761292},{"$f":"YM46-(XM46-XU46)*3.413","v":28456.710483290917},{"$f":"YN46-(XM46-XU46)*3.413","v":23292.769546347135},{"$f":"YQ46/XK46","v":8.0318121601159795},{"$f":"(YA46-YW46)/(YJ46-YW46)","v":0.20548082255861011},{"$f":"-XZ46+YL46","v":-5.8733426088059169},{"$f":"-YJ46+YA46","v":-20.236407144115901},{"$f":"(-(-0.0182984848494437-(YU46/YV46))+SQRT((-0.0182984848494437-(YU46/YV46))^2-4*0.00577826340327261*(6.76723916086377-XZ46+(YU46/YV46)*YJ46)))/(2*0.00577826340327261)","v":53.068812307822952},{"$f":"XT46*(XZ46-YL46)","v":29834.200589439832},{"$f":"XT46*(YG46-YI46)","v":19036.121675870399},{"$f":"XT46*(YI46-YL46)","v":1399.5787922268969},{"$f":"XW46*(YE46-YG46)","v":9398.5001213425057},{"$f":"SUM(YY46:ZA46)","v":29834.200589439803},{"$f":"ZB46/YX46","v":0.999999999999999}]
[5,"C-R100-EB20-CB30-95CE","30N0059","C-R100-EB20-CB30-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",30,20,"CUST 2","6/22/2015","11:14:56","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230,1.3,17.2,0,17323,29,16852,63,-378,86,16945,94,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.4312238490000002,"Baseline 100% factory charge, 20% evaporator blockage, 30% condenser blockage,--economizer closed (2V), factory charge (5.5 lbs) 95F OD, 75F DB, 62F WB ID conditions,--unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Evap coil block 9\", Cond coil block 33\", with outlet hose, with code tester",75.025000000000006,1.7999999999999999E-2,61.997999999999998,3.4000000000000002E-2,94.995999999999995,8.9999999999999993E-3,75.007000000000005,2.5000000000000001E-2,74.5,0.05,60.16,0.03,65.510000000000005,0.02,0.01,2E-3,1.0176000000000001,2.3999999999999998E-3,17323,29,-378,86,4.431,2.7E-2,null,null,null,null,null,null,230,1.3,230,1.3,230,1.3,15.1,0,15.1,0,15.1,0,3354,4.9000000000000004,3354,4.9000000000000004,3354,4.9000000000000004,229.9,1.3,229.9,1.3,229.9,1.3,2.1,0,2.1,0,2.1,0,null,228.1,1.3,228.1,1.3,228.1,1.3,14.2,0,14.2,0,14.2,0,3121.9,4,null,null,null,null,null,null,null,null,null,228.7,1.3,0.8,0,176,1.1000000000000001,13,0.2,3781.2,null,null,null,null,null,null,null,null,null,null,230.3,1.3,0,0,285.3,0.19,109.87,0.06,126.89,0.05,17.02,0.04,302.11,0.19,170.33,0.04,131.28,0.05,39.06,7.0000000000000007E-2,284.66000000000003,0.19,109.28,0.04,126.72,0.05,17.440000000000001,0.04,78.16,0.02,58.89,0.04,46.17,0.02,null,null,77.17,0.02,53.16,0.03,45.54,0.01,7.62,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.72,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.39,0.03,59.68,0.03,59.74,0.03,59.71,0.03,59.5,0.02,59.59,0.02,null,null,null,null,51.38,0.06,49.06,0.04,null,null,null,null,null,null,null,null,null,null,109.28,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,140.16999999999999,0.05,65.17,0.2,172.65,0.09,95.24,0.09,94.42,0.08,75.430000000000007,0.05,75.290000000000006,0.05,75.09,0.05,75.11,0.05,75.010000000000005,0.05,75.05,0.05,75.06,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.59,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.16,0.08,87.92,0.37,89.72,0.25,74.849999999999994,0.04,89.63,0.16,76.48,7.0000000000000007E-2,77.84,0.13,75.44,0.05,75.27,0.06,82.89,0.31,88.54,0.14000000000000001,75.83,0.06,75.59,0.06,81.709999999999994,0.33,85.9,0.24,78.92,0.24,88.37,0.28000000000000003,95,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,"C-EB20-55-CE",75.025000000000006,1.7999999999999999E-2,61.997999999999998,3.4000000000000002E-2,60.293999999999997,7.0000000000000001E-3,56.756999999999998,1.0999999999999999E-2,94.995999999999995,8.9999999999999993E-3,75.007000000000005,2.5000000000000001E-2,1093.2,1.3,1064.7,1.3,0.53500000000000003,1E-3,-0.192,1E-3,0.01,2E-3,1.0176000000000001,2.3999999999999998E-3,29.366,1E-3,3824,8,470.3,5.5,0.15583700440528631,166.26249999999996,13.029,0.19,1.1522581081815866,4976.9582128635966,66.918490866141738,173.8681901734256,739.87145734645503,4237.0867555171417,9.5396604998874198E-3,29.176246123570788,59.141741891818413,14.099870060970016,13.179134160795028,1.3927871436253956E-2,38.163964475146969,8.7734000459551067E-3,27.606829055029184,8.9718847712626521E-3,24.22991190656661,78.017560136996792,64.182478216427597,23.948779921026858,26016.88084921789,22546.598073566653,3353.7,0.43995197450212753,24640.139758544032,21169.856982892794,6.4435511920878747,0.22432612989908846,-5.2274662025439298,-18.87581824517838,53.682824918028125,26016.88084921789,16806.775536200726,1399.1821443307156,7810.923168686425,26016.880849217869,0.99999999999999911]
[5,"C-R120-EB0-CB0-95CE","30N0060","C-R120-EB0-CB0-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,0,"CUST 2","6/22/2015","18:43:02","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,229.9,1.1000000000000001,16.2,0,18671,42,18313,65,574,46,19246,50,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.347596555,"Baseline 120% factory charge, 0% evaporator and condenser blockage, economizer closed (2V),--120% factory charge (6.6 lbs), 95F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 tu","R22 6.6 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 0 in. with outlet hose, with code tester, added 35.2 oz of R2",75.022000000000006,2.1999999999999999E-2,61.997,1.9E-2,95.007000000000005,0.01,74.998000000000005,2.5999999999999999E-2,74.599999999999994,0.05,58.92,0.05,64.25,0.04,-5.8000000000000003E-2,2E-3,1.0015000000000001,3.0999999999999999E-3,18671,42,574,46,5.3479999999999999,1.7999999999999999E-2,null,null,null,null,null,null,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,14.1,0,14.1,0,14.1,0,3131.6,4.5999999999999996,3131.6,4.5999999999999996,3131.6,4.5999999999999996,229.8,1.1000000000000001,229.8,1.1000000000000001,229.8,1.1000000000000001,2.1,0,2.1,0,2.1,0,null,228.1,1.1000000000000001,228.1,1.1000000000000001,228.1,1.1000000000000001,13.3,0,13.3,0,13.3,0,2910.8,3.8,null,null,null,null,null,null,null,null,null,228.6,1.1000000000000001,0.7,0,169.2,1,0.1,0.2,3547,null,null,null,null,null,null,null,null,null,null,230.1,1.1000000000000001,0,0,265.94,0.2,100.6,0.05,121.6,0.06,21.01,0.05,283.32,0.17,150.99,0.05,126.35,0.05,24.63,0.06,265.24,0.26,100.13,0.06,121.41,7.0000000000000007E-2,21.28,0.06,79.86,0.03,50.03,0.03,47.22,0.02,null,null,79.819999999999993,0.03,51.85,0.04,47.2,0.02,4.6500000000000004,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.81,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58,0.03,58.4,0.03,58.51,0.03,58.51,0.02,58.26,0.03,58.33,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,129.97999999999999,0.09,59.78,0.08,152.62,7.0000000000000007E-2,95.56,0.09,94.64,7.0000000000000007E-2,75.650000000000006,0.05,75.510000000000005,0.04,75.63,0.04,75.55,0.04,75.349999999999994,0.04,75.349999999999994,0.04,75.3,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.64,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.24,0.08,85.84,0.21,84.84,0.39,75.09,0.04,90.94,0.3,75.84,0.04,77.180000000000007,0.09,75.75,0.06,75.23,0.05,80.16,0.28999999999999998,88.12,0.27,76.489999999999995,0.11,75.47,7.0000000000000007E-2,82.94,0.35,90.3,0.27,78.7,0.25,84.05,0.31,95.06,0.11,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE",75.022000000000006,2.1999999999999999E-2,61.997,1.9E-2,59.04,1.0999999999999999E-2,55.965000000000003,1.2E-2,95.007000000000005,0.01,74.998000000000005,2.5999999999999999E-2,1084.7,1.6,1056.2,1.6,0.58099999999999996,1E-3,-0.188,1E-3,-5.8000000000000003E-2,2E-3,1.0015000000000001,3.0999999999999999E-3,29.29,1E-3,3599,8,467,5.3,0.17564250288061725,192.62713290917296,13.03,0.184,1.1340358044776342,4950.7031558779709,72.09205373228346,202.54698728273718,861.89824080470964,4088.8049150732613,9.668982514533235E-3,29.442676389069099,57.905964195522365,14.100062700693965,13.146011374713131,1.3917349278363958E-2,38.155064632027106,8.7734494881126553E-3,27.606151473896279,8.8004502557845303E-3,23.737570612284461,78.528176099160447,64.543467829948469,23.460970887805427,29613.648302638681,24502.667892606074,3132,0.36096585907814421,28265.827482026965,23154.847071994358,7.8538003562175511,0.19120192569291539,-5.9817055012636722,-20.622211903638082,53.030820753321386,29613.648302638681,19152.195480350747,1369.3631288933316,9092.0896933946133,29613.648302638692,1.0000000000000004]
[5,"C-R120-EB0-CB30-95CE","30N0061","C-R120-EB0-CB30-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",30,0,"CUST 2","6/22/2015","19:50:21","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,229.9,1,17.5,0,17996,25,17630,55,-981,77,17014,84,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.395246706,"Baseline 120% factory charge, 0% evaporator blockage, 30% condenser blockage,--economizer closed (2V), 120% factory charge (6.6 lbs), 95F OD,--75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow.--4.75\" ID","R22 6.6 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Evap coil block 0\", Cond coil block 33\", with outlet hose, with code tester, added 35.2",75.013000000000005,0.01,61.997999999999998,2.5999999999999999E-2,95.001000000000005,7.0000000000000001E-3,75.003,2.3E-2,74.569999999999993,0.03,59.91,0.03,64.69,0.03,-1E-3,2E-3,1.0672999999999999,2.5999999999999999E-3,17996,25,-981,77,4.3949999999999996,2.1999999999999999E-2,null,null,null,null,null,null,229.9,1,229.9,1,229.9,1,15.3,0,15.3,0,15.3,0,3397.4,4.3,3397.4,4.3,3397.4,4.3,229.9,1,229.9,1,229.9,1,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,228,1,228,1,228,1,14.4,0,14.4,0,14.4,0,3164.9,3.7,null,null,null,null,null,null,null,null,null,228.6,1,0.8,0,174.5,0.9,0,0.2,3339.4,null,null,null,null,null,null,null,null,null,null,230.2,1,0,0,294.47000000000003,0.16,108.29,0.03,129.30000000000001,0.04,21.01,0.04,311.77,0.12,152.49,0.06,133.71,0.03,18.78,0.05,293.63,0.14000000000000001,107.63,0.03,129.08000000000001,0.04,21.45,0.04,81.97,0.02,51.77,0.02,48.53,0.01,null,null,81.93,0.02,54.39,0.05,48.51,0.01,5.88,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.24,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.02,0.02,59.41,0.03,59.53,0.03,59.55,0.02,59.3,0.02,59.38,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133.87,0.03,64.13,0.19,153.76,0.12,95.54,7.0000000000000007E-2,94.86,0.05,75.63,0.04,75.489999999999995,0.03,75.62,0.04,75.540000000000006,0.03,75.33,0.02,75.34,0.02,75.28,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.599999999999994,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.39,0.05,85.62,0.26,84.62,0.42,75.06,0.04,90.69,0.3,75.78,0.03,77.09,7.0000000000000007E-2,75.72,0.06,75.180000000000007,0.03,79.989999999999995,0.28999999999999998,87.8,0.28999999999999998,76.489999999999995,0.12,75.41,0.06,82.9,0.37,90.32,0.25,78.709999999999994,0.25,83.88,0.34,94.9,0.08,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE",75.013000000000005,0.01,61.997999999999998,2.5999999999999999E-2,60.051000000000002,5.0000000000000001E-3,56.868000000000002,8.0000000000000002E-3,95.001000000000005,7.0000000000000001E-3,75.003,2.3E-2,1120.2,1.4,1089.9000000000001,1.3,0.56000000000000005,1E-3,-0.19900000000000001,1E-3,-1E-3,2E-3,1.0672999999999999,2.5999999999999999E-3,29.298999999999999,0,3871,8,473.9,5.3,0.17564250288061725,192.62713290917296,13.03,0.184,1.1207406403643148,5101.8895136052506,71.703405354330727,208.38756178236014,886.75820572779423,4215.1313078774565,9.6708223788219225E-3,29.441219589323961,58.930259359635684,14.099958281953242,13.173942677661914,1.3923168090216126E-2,38.16000675565126,8.7762351933354035E-3,27.607004828496468,9.0956076526619647E-3,24.305192668280945,78.513959427428645,64.541272424979269,24.031688859781063,27598.828102580268,23979.329763231202,3397.1,0.42010125418752925,26226.131125054599,22606.632785705533,6.7750274154106425,0.1970256305932363,-5.4095307295428974,-19.583700067792961,54.125011518342369,27598.828102580268,16845.480836097875,1395.3862125166465,9357.9610539657388,27598.828102580257,0.99999999999999956]
[5,"C-R120-EB20-CB0-95CE","30N0062","C-R120-EB20-CB0-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,20,"CUST 2","6/22/2015","21:38:53","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,229.9,1.1000000000000001,16.100000000000001,0,17953,39,17612,63,427,52,18379,80,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.1611906769999996,"Baseline 120% factory charge, 20% evaporator blockage, 0% condenser blockage,--economizer closed (2V), 120% factory charge (6.6 lbs), 95F OD, 75F DB, 62F WB ID conditions,--unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\"--ID","R22 6.6 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Evap coil block 9\", Cond coil block 0\", with outlet hose, with code tester, added 35.2",75.016000000000005,0.02,61.993000000000002,2.7E-2,95.004999999999995,8.0000000000000002E-3,75.001000000000005,2.1000000000000001E-2,74.61,0.06,59.58,0.06,64.42,0.02,-1E-3,2E-3,1.0083,3.0000000000000001E-3,17953,39,427,52,5.1619999999999999,2.4E-2,null,null,null,null,null,null,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,14,0,14,0,14,0,3093.4,5.4,3093.4,5.4,3093.4,5.4,229.8,1.1000000000000001,229.8,1.1000000000000001,229.8,1.1000000000000001,2.1,0,2.1,0,2.1,0,null,228.2,1.1000000000000001,228.2,1.1000000000000001,228.2,1.1000000000000001,13.1,0,13.1,0,13.1,0,2873.5,4.5,null,null,null,null,null,null,null,null,null,228.7,1.1000000000000001,0.7,0,169.5,1,0,0.2,3510.1,null,null,null,null,null,null,null,null,null,null,230.2,1.1000000000000001,0,0,262.97000000000003,0.22,100.59,0.04,120.77,0.06,20.18,0.04,280.14,0.19,147.52000000000001,0.06,125.51,0.05,22.02,7.0000000000000007E-2,262.2,0.2,100.16,7.0000000000000007E-2,120.56,0.06,20.39,7.0000000000000007E-2,78.2,0.03,48.76,0.03,46.18,0.02,null,null,77.94,0.04,50.81,0.05,46.01,0.02,4.79,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.58,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.68,0.03,59.1,0.03,59.19,0.03,59.16,0.03,58.92,0.03,59.04,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,127.73,0.1,55.53,0.1,148.86000000000001,0.09,95.56,0.09,94.69,0.05,75.739999999999995,0.05,75.55,0.04,75.650000000000006,0.04,75.569999999999993,0.04,75.36,0.03,75.37,0.03,75.290000000000006,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.64,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.26,0.08,89.11,0.23,89.91,0.14000000000000001,75.150000000000006,0.04,89.81,0.18,76.02,0.06,77.099999999999994,0.1,75.61,0.05,75.319999999999993,0.05,82.72,0.36,88.3,0.2,76.010000000000005,0.08,75.650000000000006,7.0000000000000007E-2,83.24,0.24,87.71,0.27,78.39,0.15,88.27,0.13,95.03,0.09,null,null,null,null,null,null,null,null,null,null,null,null,"C-EB20-55-CE",75.016000000000005,0.02,61.993000000000002,2.7E-2,59.704000000000001,8.0000000000000002E-3,56.265000000000001,1.4E-2,95.004999999999995,8.0000000000000002E-3,75.001000000000005,2.1000000000000001E-2,1088,1.7,1060.2,1.6,0.52500000000000002,1E-3,-0.189,1E-3,-1E-3,2E-3,1.0083,3.0000000000000001E-3,29.318000000000001,1E-3,3561,9,467.1,5.4,0.15583700440528631,166.26249999999996,13.029,0.19,1.1515551091197451,4959.3590990106377,65.390130708661417,172.50552163456462,734.06409436434058,4225.2950046462975,9.5342494602525061E-3,29.165609291022299,58.552444890880253,14.100037554672523,13.16299116412501,1.3920457404014482E-2,38.158001102376133,8.7722298241346159E-3,27.603353414471183,8.8198376220532948E-3,23.920609052910404,77.998282323609317,64.168030326377078,23.639726327812241,27404.837953663668,23145.333794372767,3093.9,0.38531447322746659,26033.802169772331,21774.298010481431,7.310812179099222,0.21875917667755226,-5.5258829632100586,-19.445837432729064,53.107318036783987,27404.837953663668,18264.051758836573,1392.9982984704779,7747.7878963566282,27404.837953663678,1.0000000000000004]
[5,"C-R120-EB20-CB30-95CE","30N0063","C-R120-EB20-CB30-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",30,20,"CUST 2","6/22/2015","20:47:48","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,229.9,1.1000000000000001,17.2,0,17104,24,16745,36,-484,52,16620,58,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.3519245880000001,"Baseline 120% factory charge, 20% evaporator blockage, 30% condenser blockage,--economizer closed (2V), 120% factory charge (6.6 lbs), 95F OD, 75F DB, 62F WB ID conditions,--unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\"--ID","R22 6.6 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Evap coil block 9\", Cond coil block 33\", with outlet hose, with code tester, added 35.2",75.009,1.2E-2,61.997,1.7000000000000001E-2,94.994,4.0000000000000001E-3,74.995000000000005,2.9000000000000001E-2,74.569999999999993,0.06,60.13,0.04,65.02,0.03,-1.2999999999999999E-2,2E-3,0.9919,2.5999999999999999E-3,17104,24,-484,52,4.3520000000000003,1.7999999999999999E-2,null,null,null,null,null,null,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,15.1,0,15.1,0,15.1,0,3353.4,4.5,3353.4,4.5,3353.4,4.5,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,2.1,0,2.1,0,2.1,0,null,228,1.1000000000000001,228,1.1000000000000001,228,1.1000000000000001,14.2,0,14.2,0,14.2,0,3121.9,3.9,null,null,null,null,null,null,null,null,null,228.6,1.1000000000000001,0.8,0,174.6,1,0.1,0.2,3761.9,null,null,null,null,null,null,null,null,null,null,230.2,1.1000000000000001,0,0,290.29000000000002,0.15,108.33,0.03,128.21,0.04,19.88,0.03,307.36,0.14000000000000001,150.28,0.05,132.6,0.04,17.68,0.04,289.47000000000003,0.16,107.7,0.04,127.99,0.04,20.3,0.05,80.11,0.02,50.41,0.03,47.38,0.01,null,null,79.790000000000006,0.03,53.28,0.04,47.18,0.02,6.1,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.03,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.27,0.02,59.71,0.03,59.78,0.03,59.75,0.03,59.53,0.02,59.63,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,132.19999999999999,0.03,61.41,0.56999999999999995,151.33000000000001,0.13,95.51,0.05,94.85,0.06,75.69,0.03,75.52,0.03,75.59,0.02,75.510000000000005,0.03,75.319999999999993,0.03,75.319999999999993,0.03,75.25,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.63,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.35,0.06,89.15,0.17,89.94,0.14000000000000001,75.17,0.03,89.76,0.18,75.98,0.06,77.040000000000006,0.1,75.58,7.0000000000000007E-2,75.31,0.05,82.65,0.35,88.21,0.2,75.95,0.1,75.61,0.08,83.22,0.24,87.68,0.23,78.31,0.16,88.24,0.16,94.89,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,"C-EB20-55-CE",75.009,1.2E-2,61.997,1.7000000000000001E-2,60.265999999999998,5.0000000000000001E-3,56.795999999999999,0.01,94.994,4.0000000000000001E-3,74.995000000000005,2.9000000000000001E-2,1079.9000000000001,1.4,1050.4000000000001,1.4,0.52700000000000002,1E-3,-0.186,1E-3,-1.2999999999999999E-2,2E-3,0.9919,2.5999999999999999E-3,29.306999999999999,0,3819,8,465.4,5.3,0.15583700440528631,166.26249999999996,13.029,0.19,1.1576919206675256,4916.5855188241285,65.032497133858271,171.12912517708256,728.22266603823948,4188.3628527858891,9.5380290336175202E-3,29.168376531406448,59.108308079332474,14.099736233815314,13.178658187053445,1.3917832802679284E-2,38.152397714153146,8.7765209003599146E-3,27.606341892241371,9.0017528832926526E-3,24.255569649006947,77.992657499542773,64.171575637299938,23.973096550123078,25543.038322214707,22283.164534036983,3353.6,0.44810005198346309,24176.584034932566,20916.710246754843,6.3306059269265686,0.2189159336236943,-5.1952799812833703,-18.884349420210299,53.81555514509234,25543.038322214707,16474.358287964209,1388.8031474298089,7679.8768868206898,25543.038322214707,1]
[5,"C-R80-EB0-CB0-95CE","30N0064","C-R80-EB0-CB0-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,0,"CUST 2","6/22/2015","17:25:26","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230,1,15.4,0,16724,47,16318,83,-861,78,15862,60,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.6694141890000003,"Baseline 80% factory charge, 0% evaporator and condenser blockage, economizer closed (2V),--80% factory charge (4.4 lbs), 95F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turn","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Evap coil block 0\", Cond coil block 0\", with outlet hose, with code tester, removed 17.",74.911000000000001,3.2000000000000001E-2,61.975999999999999,2.3E-2,95.004999999999995,8.0000000000000002E-3,74.997,2.9000000000000001E-2,74.44,0.06,60.96,0.03,66.319999999999993,0.03,1.0999999999999999E-2,2E-3,1.0845,3.0999999999999999E-3,16724,47,-861,78,4.67,2.1000000000000001E-2,null,null,null,null,null,null,230,1,230,1,230,1,13.2,0,13.2,0,13.2,0,2920.8,4.4000000000000004,2920.8,4.4000000000000004,2920.8,4.4000000000000004,229.9,1,229.9,1,229.9,1,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,228.4,1,228.4,1,228.4,1,12.4,0,12.4,0,12.4,0,2704.7,3.5,null,null,null,null,null,null,null,null,null,228.8,1,0.7,0,169.4,0.9,13,0.2,3362.7,null,null,null,null,null,null,null,null,null,null,230.2,1,0,0,242.24,0.13,105.55,0.04,114.76,0.04,9.2100000000000009,0.03,258.14,0.13,190.46,0.03,119.4,0.04,71.06,0.04,241.66,0.14000000000000001,105.81,0.04,114.58,0.04,8.77,0.05,71.72,0.02,72.3,0.05,41.94,0.01,null,null,72.42,0.02,72.58,0.02,42.4,0.01,30.17,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30.35,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.16,0.02,60.51,0.02,60.62,0.02,60.63,0.03,60.36,0.02,60.49,0.02,null,null,null,null,69.88,0.04,68.95,0.04,null,null,null,null,null,null,null,null,null,null,105.81,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,156.75,0.06,97.83,7.0000000000000007E-2,193.83,0.04,95.51,0.06,94.57,0.05,75.510000000000005,0.05,75.38,0.05,75.42,0.05,75.36,0.04,75.209999999999994,0.04,75.22,0.05,75.16,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.510000000000005,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.22,0.06,85.24,0.27,84.09,0.4,74.94,0.05,91.02,0.3,75.650000000000006,0.05,76.959999999999994,0.1,75.680000000000007,7.0000000000000007E-2,75.040000000000006,0.04,79.900000000000006,0.31,88.02,0.27,76.56,0.14000000000000001,75.290000000000006,7.0000000000000007E-2,82.74,0.35,89.88,0.24,78.94,0.25,83.49,0.36,95.05,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE",74.911000000000001,3.2000000000000001E-2,61.975999999999999,2.3E-2,61.094000000000001,1.0999999999999999E-2,57.241999999999997,1.2E-2,95.004999999999995,8.0000000000000002E-3,74.997,2.9000000000000001E-2,1131.2,1.6,1096.9000000000001,1.6,0.57299999999999995,1E-3,-0.20200000000000001,1E-3,1.0999999999999999E-2,2E-3,1.0845,3.0999999999999999E-3,29.289000000000001,1E-3,3397,8,475.6,5.3,0.17564250288061725,192.62713290917296,13.03,0.184,1.110849756345855,5141.7393554615892,73.83916223622046,209.95282098317492,893.41571624153914,4248.3236392200497,9.6774022456949885E-3,29.427769093573257,59.983150243654144,14.100008573819167,13.200202364965451,1.3916951761366302E-2,38.154133739736984,8.7858317137050265E-3,27.592628463381413,9.0728427954548264E-3,24.53495374441658,78.429385610702624,64.521934832192116,24.263874919940914,26551.39790000422,22762.97624324655,2921.4,0.37552592287423087,25180.18816071644,21391.76650395877,7.4124781161955964,0.24866260919738675,-5.1638941736323432,-18.44623536704848,53.878184522010152,26551.39790000422,15721.766438701436,1393.8166602387944,9435.814801064007,26551.397900004238,1.0000000000000007]
[5,"C-R80-EB0-CB30-95CE","30N0065","C-R80-EB0-CB30-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,30,"CUST 2","6/22/2015","15:04:33","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,229.9,1.1000000000000001,16.600000000000001,0,16831,27,16366,75,-1230,98,15600,92,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2310821809999997,"Baseline 80% factory charge, 0% evaporator and 30% condenser blockage, economizer closed (2V),--80% factory charge (4.4 lbs), 95F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3-","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Evap coil block 0\", Cond coil block 33\", with outlet hose, with code tester, removed 17",75.009,0.02,61.991999999999997,3.3000000000000002E-2,94.998999999999995,8.9999999999999993E-3,75.001999999999995,3.3000000000000002E-2,74.53,7.0000000000000007E-2,61.04,0.04,66.17,0.03,0.02,3.0000000000000001E-3,1.0898000000000001,3.8999999999999998E-3,16831,27,-1230,98,4.2320000000000002,2.7E-2,null,null,null,null,null,null,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,14.4,0,14.4,0,14.4,0,3210.4,4.0999999999999996,3210.4,4.0999999999999996,3210.4,4.0999999999999996,229.8,1.1000000000000001,229.8,1.1000000000000001,229.8,1.1000000000000001,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,228.1,1.1000000000000001,228.1,1.1000000000000001,228.1,1.1000000000000001,13.6,0,13.6,0,13.6,0,2983,3.2,null,null,null,null,null,null,null,null,null,228.6,1.1000000000000001,0.8,0,174.5,1,13,0.2,3646.5,null,null,null,null,null,null,null,null,null,null,230.2,1.1000000000000001,0,0,270.61,0.13,113.55,0.03,122.91,0.04,9.36,0.03,286.88,0.11,196.37,0.03,127.31,0.03,69.06,0.04,270.05,0.12,113.44,0.05,122.75,0.03,9.31,0.06,75.41,0.02,74.94,0.05,44.39,0.02,null,null,76.05,0.02,74.319999999999993,0.03,44.81,0.02,29.51,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30.55,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.2,0.04,60.54,0.04,60.63,0.04,60.62,0.03,60.39,0.04,60.51,0.03,null,null,null,null,68.790000000000006,0.04,69.13,0.04,null,null,null,null,null,null,null,null,null,null,113.44,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,158.75,0.05,99.12,0.04,200.52,0.04,95.47,0.08,94.75,0.05,75.489999999999995,0.04,75.34,0.04,75.39,0.04,75.37,0.04,75.22,0.05,75.23,0.05,75.16,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.55,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.34,0.06,84.78,0.3,83.83,0.31,74.91,0.04,90.86,0.27,75.72,0.05,77.08,0.1,75.900000000000006,7.0000000000000007E-2,75.09,0.04,80.05,0.27,87.84,0.26,76.760000000000005,0.11,75.319999999999993,0.06,82.52,0.4,90.03,0.28000000000000003,79.489999999999995,0.24,83.54,0.31,94.93,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE",75.009,0.02,61.991999999999997,3.3000000000000002E-2,61.139000000000003,1.2E-2,57.350999999999999,0.02,94.998999999999995,8.9999999999999993E-3,75.001999999999995,3.3000000000000002E-2,1133.0999999999999,2,1100.3,2,0.56899999999999995,1E-3,-0.20300000000000001,1E-3,0.02,3.0000000000000001E-3,1.0898000000000001,3.8999999999999998E-3,29.324000000000002,1E-3,3687,8,476,5.2,0.17564250288061725,192.62713290917296,13.03,0.184,1.1110189102410519,5149.7625035378378,73.550983023622038,210.47108525452521,895.62772748010207,4254.1347760577355,9.6688144665537067E-3,29.438654483266944,60.027981089758953,14.099904154153235,13.201773859142877,1.392277047341731E-2,38.159075749154418,8.7732243755509424E-3,27.602734491970001,9.1278221858500114E-3,24.605760607942447,78.512466486613846,64.537878744810072,24.334613384206932,26284.599468455304,22845.770350539853,3211,0.41694160160790339,24911.040973514926,21472.211855599475,6.7564526643653178,0.24202142540202354,-5.1040410990600122,-18.484485396854893,54.125912543900014,26284.599468455304,15433.703732047254,1396.3438057315379,9454.5519306765236,26284.599468455315,1.0000000000000004]
[5,"C-R80-EB20-CB0-95CE","30N0066","C-R80-EB20-CB0-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,20,"CUST 2","6/22/2015","16:27:21","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,229.9,1.2,15.2,0,16105,32,15655,48,-441,74,15664,83,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.6329488320000003,"Baseline 80% factory charge, 20% evaporator blockage, 0% condenser blockage, economizer closed (2V),--80% factory charge (4.4 lbs), 95F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pul","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Evap coil block 9\", Cond coil block 0\", with outlet hose, with code tester, removed 17.",74.992000000000004,1.0999999999999999E-2,62.002000000000002,3.4000000000000002E-2,95.004999999999995,5.0000000000000001E-3,75.001000000000005,1.7000000000000001E-2,74.5,0.06,61.32,0.06,66.31,0.02,1.4E-2,3.0000000000000001E-3,1.0421,3.3E-3,16105,32,-441,74,4.633,2.8000000000000001E-2,null,null,null,null,null,null,229.9,1.2,229.9,1.2,229.9,1.2,13.1,0,13.1,0,13.1,0,2910.4,5.5,2910.4,5.5,2910.4,5.5,229.8,1.2,229.8,1.2,229.8,1.2,2.1,0,2.1,0,2.1,0,null,228.3,1.2,228.3,1.2,228.3,1.2,12.3,0,12.3,0,12.3,0,2694.3,4.4000000000000004,null,null,null,null,null,null,null,null,null,228.8,1.2,0.7,0,169.5,1.1000000000000001,0.1,0.2,null,null,null,null,null,null,null,null,null,null,null,230.2,1.2,0,0,241.13,0.16,105.59,0.04,114.43,0.05,8.84,0.03,256.91000000000003,0.16,188.92,0.04,119.05,0.05,69.87,0.05,240.54,0.17,105.95,0.05,114.25,0.05,8.3000000000000007,7.0000000000000007E-2,70.61,0.02,69.98,0.06,41.2,0.01,null,null,70.849999999999994,0.02,70.23,0.05,41.36,0.01,28.87,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28.79,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.59,0.04,60.87,0.04,60.94,0.04,60.93,0.03,60.66,0.03,60.82,0.04,null,null,null,null,67.17,0.05,66.22,0.04,null,null,null,null,null,null,null,null,null,null,105.95,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,155.51,0.09,96.3,0.05,192.23,0.05,95.55,0.08,94.62,0.06,75.64,0.05,75.459999999999994,0.04,75.489999999999995,0.03,75.44,0.03,75.239999999999995,0.05,75.25,0.04,75.17,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.540000000000006,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.27,0.08,86.33,1.25,88.36,0.45,74.92,0.03,90.86,0.54,75.91,0.06,77.83,0.13,75.599999999999994,7.0000000000000007E-2,75.180000000000007,0.05,83.2,0.38,89.38,0.43,76.72,0.08,75.37,0.08,82.58,0.91,86.09,0.42,79.78,0.16,86.91,0.53,95.07,0.09,null,null,null,null,null,null,null,null,null,null,null,null,"C-EB20-55-CE",74.992000000000004,1.0999999999999999E-2,62.002000000000002,3.4000000000000002E-2,61.432000000000002,1.7000000000000001E-2,57.235999999999997,2.1000000000000001E-2,95.004999999999995,5.0000000000000001E-3,75.001000000000005,1.7000000000000001E-2,1108.5,1.8,1075.4000000000001,1.7,0.54300000000000004,1E-3,-0.19500000000000001,1E-3,1.4E-2,3.0000000000000001E-3,1.0421,3.3E-3,29.300999999999998,1E-3,3381,9,470.6,5.5,0.15583700440528631,166.26249999999996,13.029,0.19,1.1349477086172275,5035.5409287016601,68.601713574803156,175.22231115805207,745.62487005569528,4289.9160586459648,9.5444266947202032E-3,29.172037639410526,60.297052291382776,14.100037554672523,13.208114270485856,1.3920457404014482E-2,38.158001102376133,8.7838343464384169E-3,27.610198725127962,8.9892364124351254E-3,24.526448520045857,77.978948096697039,64.176139733419248,24.249531242886505,24787.48243149243,21369.098405927562,2910.4,0.40073433142931458,23415.462279923235,19997.078254358366,6.9256025672650798,0.27489417062515453,-4.922506396524021,-17.681895805314262,53.593685850827605,24787.48243149243,15528.350371583074,1394.4282830005407,7864.7037769088211,24787.482431492434,1.0000000000000002]
[5,"C-R80-EB20-CB30-95CE","30N0067","C-R80-EB20-CB30-95CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",30,20,"CUST 2","6/22/2015","13:44:41","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230,0.9,16.399999999999999,0,15937,39,15533,55,-702,59,15234,79,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.1634326320000001,"Baseline 80% factory charge, 20% evaporator blockage, 30% condenser blockage,--economizer closed (2V), 80% factory charge (4.4 lbs), 95F OD, 75F DB, 62F WB ID conditions,--unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pu","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Evap coil block 9\", Cond coil block 33\", with outlet hose, with code tester, removed 17",75.012,0.02,61.988999999999997,2.8000000000000001E-2,94.998000000000005,0.01,75.004999999999995,2.3E-2,74.64,0.05,61.53,0.05,66.61,0.04,1.0999999999999999E-2,2E-3,1.0371999999999999,3.2000000000000002E-3,15937,39,-702,59,4.1639999999999997,2.3E-2,null,null,null,null,null,null,230,0.9,230,0.9,230,0.9,14.3,0,14.3,0,14.3,0,3187.5,4.7,3187.5,4.7,3187.5,4.7,229.9,0.9,229.9,0.9,229.9,0.9,2.1,0,2.1,0,2.1,0,null,228.2,1,228.2,1,228.2,1,13.5,0,13.5,0,13.5,0,2960.3,4.0999999999999996,null,null,null,null,null,null,null,null,null,228.7,1,0.8,0,174.8,0.9,13,0.2,3619.2,null,null,null,null,null,null,null,null,null,null,230.2,0.9,0,0,268.19,0.18,113.31,0.05,122.24,0.05,8.93,0.03,284.23,0.18,194.8,0.06,126.61,0.05,68.2,0.05,267.62,0.19,113.4,0.05,122.08,0.05,8.68,0.04,73.73,0.03,73.28,0.05,43.29,0.02,null,null,74.62,0.08,71.61,0.03,43.88,0.05,27.73,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,29.99,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.63,0.03,60.9,0.03,61,0.03,61.05,0.03,60.74,0.03,60.85,0.03,null,null,null,null,65.680000000000007,7.0000000000000007E-2,66.36,0.05,null,null,null,null,null,null,null,null,null,null,113.4,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,157.33000000000001,0.06,97.33,0.04,198.86,0.06,95.52,7.0000000000000007E-2,94.74,0.06,75.709999999999994,0.04,75.510000000000005,0.04,75.489999999999995,0.04,75.459999999999994,0.04,75.3,0.03,75.319999999999993,0.03,75.22,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.55,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.35,7.0000000000000007E-2,87.38,0.53,89.51,0.28000000000000003,74.94,0.03,89.69,0.21,76.489999999999995,0.05,77.87,0.12,75.489999999999995,0.05,75.3,0.05,82.97,0.35,88.63,0.17,75.92,0.06,75.599999999999994,0.06,81.91,0.39,86.07,0.32,79.2,0.26,88.1,0.35,94.98,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,"C-EB20-55-CE",75.012,0.02,61.988999999999997,2.8000000000000001E-2,61.56,0.01,57.343000000000004,1.9E-2,94.998000000000005,0.01,75.004999999999995,2.3E-2,1105.4000000000001,1.7,1073.3,1.7,0.54500000000000004,2E-3,-0.19500000000000001,1E-3,1.0999999999999999E-2,2E-3,1.0371999999999999,3.2000000000000002E-3,29.341000000000001,1E-3,3659,8,471.1,5.2,0.15583700440528631,166.26249999999996,13.029,0.19,1.1395143642947556,5020.1238796580365,68.719934015748024,175.22147168188263,745.62844230231406,4274.4954373557221,9.5362142531712664E-3,29.169198972949921,60.420485635705248,14.099902450677115,13.21162616499374,1.3925639436137347E-2,38.161994547190176,8.770537857034506E-3,27.600526306378562,9.0233430546266778E-3,24.594798768267516,78.004165996502252,64.172894149294535,24.316750011149807,24359.8949079546,21185.340881162661,3187.9,0.4466481789478941,22986.571742750348,19812.017715958409,6.2822005309511741,0.27516314395550845,-4.8524489618001141,-17.583680360797004,53.745354907958912,24359.8949079546,15089.124589817022,1395.8392053158486,7874.931112821725,24359.894907954593,0.99999999999999967]
[5,"C-CB0-115-CE","30N0076","C-CB0-115-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,0,"CUST 2","6/20/2015","1:44:08","10 Ton","0:10:00","75/62 115/80","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,115,80,5.5,null,5.5,null,229.9,1.2,19.2,0,14018,45,13706,76,-3334,91,10681,69,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.4938127479999999,"Baseline no condenser coil blockage, economizer closed (2.8V),--factory charge (5.5 lbs) 115F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed,--adjus","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer.",74.918000000000006,0.03,61.976999999999997,3.2000000000000001E-2,114.99,1.7999999999999999E-2,79.995999999999995,2.4E-2,74.39,0.06,62.9,0.02,67.27,0.02,3.0000000000000001E-3,2E-3,1.0684,3.3999999999999998E-3,14018,45,-3334,91,2.4940000000000002,1.7000000000000001E-2,null,null,null,null,null,null,229.9,1.2,229.9,1.2,229.9,1.2,17,0.1,17,0.1,17,0.1,3809.9,4.5999999999999996,3809.9,4.5999999999999996,3809.9,4.5999999999999996,229.9,1.2,229.9,1.2,229.9,1.2,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,227.9,1.2,227.9,1.2,227.9,1.2,16.3,0.1,16.3,0.1,16.3,0.1,3583.1,4.2,null,null,null,null,null,null,null,null,null,228.6,1.2,0.7,0,167.4,1,0.1,0.2,4223.3999999999996,null,null,null,null,null,null,null,null,null,null,230.3,1.2,0,0,331.78,0.31,124.53,7.0000000000000007E-2,138.59,7.0000000000000007E-2,14.06,0.04,347.67,0.3,190.72,0.05,142.33000000000001,7.0000000000000007E-2,48.39,0.08,331.1,0.32,123.95,0.05,138.43,0.08,14.48,0.06,84.64,0.03,53.34,0.03,50.15,0.02,null,null,84.12,0.03,55.79,0.03,49.83,0.02,5.96,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.2,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.29,0.03,62.6,0.04,62.64,0.03,62.59,0.03,62.45,0.03,62.51,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,159.80000000000001,7.0000000000000007E-2,68.989999999999995,0.13,193.35,0.06,114.9,0.11,113.72,0.17,75.73,7.0000000000000007E-2,75.599999999999994,7.0000000000000007E-2,75.180000000000007,0.06,75.23,0.06,75.06,0.05,75.11,0.05,75.12,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.78,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.11,7.0000000000000007E-2,94.72,0.57999999999999996,94.32,0.46,74.94,0.05,105.5,0.51,76.16,7.0000000000000007E-2,78.94,0.17,77.099999999999994,0.11,75.55,0.05,83.59,0.62,98.9,0.57999999999999996,78.790000000000006,0.23,75.760000000000005,7.0000000000000007E-2,89.84,0.54,102.77,0.56000000000000005,85.08,0.32,91.36,0.62,113.67,0.28999999999999998,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.918000000000006,0.03,61.976999999999997,3.2000000000000001E-2,63.162999999999997,6.0000000000000001E-3,58.801000000000002,1.6E-2,114.99,1.7999999999999999E-2,79.995999999999995,2.4E-2,1125.0999999999999,1.8,1085.8,1.7,0.56899999999999995,1E-3,-0.20100000000000001,1E-3,3.0000000000000001E-3,2E-3,1.0684,3.3999999999999998E-3,29.228000000000002,1E-3,4283,8,472.9,5.4,0.16622533100174824,191.8074094429173,13.029,0.182,1.1175903138963836,5092.3774076946856,72.581711685039352,213.42670977789805,876.69156089836349,4215.685846796322,9.6423041621478515E-3,30.229394583328972,62.045409686103611,14.606736459914961,13.256283773861117,1.3765547468862408E-2,42.905653599192362,8.7848368977703692E-3,27.59324717888834,9.5353300018467379E-3,25.543517473673937,81.868401068619917,65.62986181678059,25.270564271291065,25252.235449613429,24227.076832620594,3810.1,0.51495921325250704,23885.949131594469,22860.790514601635,5.5769201801528059,0.24185021388602621,-4.9588303120379074,-19.822991382516307,55.721864136752622,25252.235449613429,10437.997242714517,1389.9807211724549,13424.257485726455,25252.235449613429,1]
[5,"C-CB10-115-CE","30N0077","C-CB10-115-CE","closed","on","N/A",null,"unsealed","unsealed",null,null,"horizontal",10,0,"CUST 2","6/20/2015","0:21:45","10 Ton","0:10:00","75/62 115/80","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,115,80,5.5,null,5.5,null,229.9,1,19.8,0,13681,39,13435,51,-3962,52,9716,55,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2056753690000002,".","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 12`.;",74.975999999999999,2.7E-2,61.978000000000002,1.4999999999999999E-2,114.98399999999999,1.7999999999999999E-2,80.004999999999995,2.5000000000000001E-2,74.47,0.03,63.23,0.03,67.23,0.02,0,2E-3,1.0770999999999999,3.0000000000000001E-3,13681,39,-3962,52,2.206,1.4E-2,null,null,null,null,null,null,229.9,1,229.9,1,229.9,1,17.600000000000001,0.1,17.600000000000001,0.1,17.600000000000001,0.1,3930.7,4.5,3930.7,4.5,3930.7,4.5,229.9,1,229.9,1,229.9,1,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,227.7,1,227.7,1,227.7,1,16.8,0.1,16.8,0.1,16.8,0.1,3700.6,4.3,null,null,null,null,null,null,null,null,null,228.5,1,0.7,0,167.6,0.9,0.1,0.2,4342,null,null,null,null,null,null,null,null,null,null,230.2,1,0,0,343.32,0.32,126.65,0.06,141.32,7.0000000000000007E-2,14.67,0.03,359.25,0.31,190.47,0.06,144.97999999999999,7.0000000000000007E-2,45.5,0.1,342.57,0.31,126.36,0.06,141.15,7.0000000000000007E-2,14.78,7.0000000000000007E-2,85.56,0.04,54.15,0.05,50.7,0.02,null,null,84.87,0.04,56.52,0.04,50.29,0.02,6.23,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.45,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.71,0.04,63.01,0.04,63.04,0.03,63,0.03,62.86,0.04,62.92,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,157.08000000000001,0.05,69.040000000000006,7.0000000000000007E-2,193.57,0.08,115.2,0.13,113.78,0.1,75.849999999999994,0.05,75.709999999999994,0.05,75.25,0.04,75.290000000000006,0.04,75.13,0.04,75.2,0.03,75.25,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.89,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.33,0.08,96.26,1.65,95.34,0.92,75.069999999999993,0.04,106.12,0.68,76.27,0.05,79.150000000000006,0.16,77.260000000000005,0.12,75.67,0.05,83.97,0.56999999999999995,99.59,0.75,79.069999999999993,0.25,75.91,0.09,90.4,0.6,102.82,0.94,85.54,0.38,92.69,1.42,114.92,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.975999999999999,2.7E-2,61.978000000000002,1.4999999999999999E-2,63.533999999999999,7.0000000000000001E-3,59.104999999999997,1.0999999999999999E-2,114.98399999999999,1.7999999999999999E-2,80.004999999999995,2.5000000000000001E-2,1129.5,1.6,1090.3,1.6,0.56999999999999995,1E-3,-0.20599999999999999,1E-3,0,2E-3,1.0770999999999999,3.0000000000000001E-3,29.236999999999998,0,4405,7,473.8,5.0999999999999996,0.16622533100174824,191.8074094429173,13.029,0.182,1.1154046794368178,5108.3604749039996,73.010608818897623,216.06448381606239,887.53067841681968,4220.8297964871799,9.64118617614604E-3,30.255248136825845,62.418595320563185,14.606671458488329,13.266487424475187,1.3775761659341983E-2,42.915535647877014,8.771792535440491E-3,27.59311909931127,9.6366720978124289E-3,25.744510904106697,81.979258686245487,65.665111068633522,25.472041318658331,24434.34465321825,23981.500704036986,3931.2,0.54911174375339022,23066.450461117147,22613.606511935883,5.2364246222740398,0.244093054753308,-4.783206818167514,-19.560663365682302,56.10218017984463,24434.34465321825,9443.357037966658,1391.8728609179125,13599.114754333659,24434.344653218228,0.99999999999999911]
[5,"C-CB20-115-CE","30N0078","C-CB20-115-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",20,0,"CUST 2","6/19/2015","23:33:22","10 Ton","0:10:00","75/62 115/80","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,115,80,5.5,null,5.5,null,229.9,1.1000000000000001,20.2,0,13363,35,13131,59,-4351,65,9009,47,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.996675532,"20% condenser coil block, economizer closed (2.8V), factory charge (5.5 lbs)--115F OD, 75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%:--Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed,--adjust code test","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 24`.;",74.927999999999997,3.3000000000000002E-2,61.966000000000001,8.0000000000000002E-3,114.99299999999999,6.0000000000000001E-3,79.998000000000005,3.6999999999999998E-2,74.42,0.04,63.45,0.02,67.430000000000007,0.02,0,2E-3,1.0827,2.5000000000000001E-3,null,null,null,null,null,null,null,null,null,null,null,null,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,18,0.1,18,0.1,18,0.1,4037.2,2.9,4037.2,2.9,4037.2,2.9,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,227.6,1.1000000000000001,227.6,1.1000000000000001,227.6,1.1000000000000001,17.3,0.1,17.3,0.1,17.3,0.1,3803.5,2.6,null,null,null,null,null,null,null,null,null,228.5,1.1000000000000001,0.7,0,168.3,1,0.1,0.2,4446.1000000000004,null,null,null,null,null,null,null,null,null,null,230.2,1.1000000000000001,0,0,353.16,0.17,129.30000000000001,0.03,143.59,0.04,14.3,0.03,369.15,0.15,191.25,0.05,147.19,0.03,44.06,7.0000000000000007E-2,352.42,0.15,128.78,0.03,143.41999999999999,0.03,14.65,0.04,86.4,0.03,54.91,0.04,51.21,0.02,null,null,85.79,0.03,57.84,0.03,50.84,0.02,7.01,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.7,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.95,0.03,63.27,0.04,63.29,0.03,63.23,0.03,63.13,0.03,63.2,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,159.11000000000001,0.02,67.459999999999994,0.13,194.23,7.0000000000000007E-2,115.24,0.11,113.85,0.09,75.87,7.0000000000000007E-2,75.72,0.06,75.28,0.03,75.319999999999993,0.04,75.14,0.03,75.19,0.04,75.22,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.87,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.36,0.06,95.77,0.65,95.05,0.52,75.040000000000006,0.04,106.4,0.55000000000000004,76.260000000000005,0.05,79.180000000000007,0.2,77.2,0.1,75.650000000000006,0.06,84.23,0.6,99.95,0.65,78.86,0.2,75.89,0.1,90.7,0.77,103.51,0.56000000000000005,85.22,0.26,92.13,0.6,114.67,0.28999999999999998,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.927999999999997,3.3000000000000002E-2,61.966000000000001,8.0000000000000002E-3,63.768000000000001,8.9999999999999993E-3,59.308999999999997,0.01,114.99299999999999,6.0000000000000001E-3,79.998000000000005,3.6999999999999998E-2,1132.5999999999999,1.3,1093,1.3,0.56999999999999995,1E-3,-0.20300000000000001,1E-3,0,2E-3,1.0827,2.5000000000000001E-3,29.242000000000001,0,4512,6,474.3,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,1.1137832013790077,5119.8717125144567,73.191411023622052,214.4865435335976,881.03979507307213,4238.8319174413846,9.6341844396961515E-3,30.221917725888005,62.654216798620993,14.606823305805959,13.272988819992454,1.3766783753666465E-2,42.907766753938418,8.7752250556927223E-3,27.585168252049964,9.7088758533772513E-3,25.880324604798925,81.874268641538009,65.620399993630556,25.608215405691549,23621.563999136153,23617.007938466922,4037.7,0.58339363559940238,22252.580384959776,22248.024324290545,4.9318662200708721,0.24616687715537749,-4.613702320196456,-19.220051842917016,56.377840771150325,23621.563999136153,8728.5807638205679,1393.1641912248199,13499.819044090766,23621.563999136153,1]
[5,"C-CB30-115-CE","30N0079","C-CB30-115-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",30,0,"CUST 2","6/19/2015","22:56:28","10 Ton","0:10:00","75/62 115/80","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,115,80,5.5,null,5.5,null,229.9,1.2,21,0,13005,26,12690,37,-4673,48,8328,57,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.7791070280000001,"30% condenser coil block, economizer closed (2.8V), factory charge (5.5 lbs) 115F OD,--75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%:--Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed,--adjust code test","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 33\"",75.004999999999995,1.2999999999999999E-2,62.003,2.1000000000000001E-2,115.024,1.0999999999999999E-2,79.989000000000004,2.5999999999999999E-2,74.42,0.02,63.75,0.01,67.59,0.02,-3.0000000000000001E-3,3.0000000000000001E-3,1.0723,3.0000000000000001E-3,13005,26,-4673,48,1.7789999999999999,1.2999999999999999E-2,null,null,null,null,null,null,229.9,1.2,229.9,1.2,229.9,1.2,18.8,0.1,18.8,0.1,18.8,0.1,4207.8,3.8,4207.8,3.8,4207.8,3.8,229.9,1.2,229.9,1.2,229.9,1.2,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,227.5,1.2,227.5,1.2,227.5,1.2,18,0.1,18,0.1,18,0.1,3965.4,3.6,null,null,null,null,null,null,null,null,null,228.4,1.2,0.8,0,172.2,1.1000000000000001,0.1,0.2,4610.3999999999996,null,null,null,null,null,null,null,null,null,null,230.2,1.2,0,0,368.4,0.18,132.38999999999999,0.04,147.02000000000001,0.04,14.63,0.03,384.32,0.18,192.87,0.05,150.5,0.04,42.37,0.06,367.63,0.19,131.81,0.02,146.85,0.04,15.04,0.04,87.42,0.03,55.4,0.02,51.81,0.02,null,null,86.87,0.04,59.02,0.03,51.48,0.03,7.54,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.58,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.24,0.04,63.57,0.04,63.6,0.04,63.51,0.03,63.44,0.03,63.49,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162.65,0.04,74.790000000000006,0.21,195.99,7.0000000000000007E-2,115.33,0.11,113.9,0.09,75.88,0.05,75.75,0.05,75.290000000000006,0.04,75.34,0.04,75.150000000000006,0.03,75.209999999999994,0.03,75.23,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.86,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.47,7.0000000000000007E-2,95.9,0.46,95.09,0.56999999999999995,75.03,0.03,106.54,0.51,76.260000000000005,0.06,79.150000000000006,0.17,77.13,0.12,75.650000000000006,0.05,84.33,0.62,100.1,0.6,78.7,0.2,75.91,0.1,90.77,0.72,103.46,0.49,85.1,0.31,92.26,0.63,114.7,0.31,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.004999999999995,1.2999999999999999E-2,62.003,2.1000000000000001E-2,64.075999999999993,8.9999999999999993E-3,59.54,1.2E-2,115.024,1.0999999999999999E-2,79.989000000000004,2.5999999999999999E-2,1127.4000000000001,1.6,1087.2,1.5,0.57099999999999995,1E-3,-0.20399999999999999,2E-3,-3.0000000000000001E-3,3.0000000000000001E-3,1.0723,3.0000000000000001E-3,29.234000000000002,1E-3,4681,7,472.8,5.3,0.16622533100174824,191.8074094429173,13.029,0.182,1.1161672910046689,5093.1504125188476,72.930745700787398,215.01896593599329,883.18754602975253,4209.9628664890952,9.6431137875425711E-3,30.261545994300221,62.959832708995322,14.607472687035589,13.281367036349955,1.375060971871315E-2,42.897409570289305,8.7814222793694708E-3,27.610729895071469,9.7810633072310128E-3,26.034216916110619,81.996380319813895,65.673512649895173,25.761489483766457,22919.464672983162,23269.440076074072,4208.2,0.62665454036237689,21554.710908059948,21904.686311150857,4.6047235437000529,0.24927423163523757,-4.5000565105337635,-19.036547610818573,56.638855091548251,22919.464672983162,8029.4177291357673,1389.0418345488747,13501.005109298536,22919.46467298318,1.0000000000000009]
[5,"C-CB40-115-CE","30N0080","C-CB40-115-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",40,0,"CUST 2","6/19/2015","21:38:33","10 Ton","0:10:00","75/62 115/80","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,115,80,5.5,null,5.5,null,229.8,1.1000000000000001,21.6,0,12809,19,12512,43,-4846,51,7958,50,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.651722707,"40% condenser coil block, economizer closed (2.8V), factory charge (5.5 lbs) 115F OD,--75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%:--Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed,--adjust code test","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 37`.;",75.004000000000005,1.0999999999999999E-2,61.987000000000002,1.6E-2,115.011,1.0999999999999999E-2,80.010000000000005,2.1999999999999999E-2,74.42,0.03,63.88,0.02,67.650000000000006,0.01,-7.0000000000000001E-3,3.0000000000000001E-3,1.0693999999999999,3.0999999999999999E-3,12809,19,-4846,51,1.6519999999999999,1.0999999999999999E-2,null,null,null,null,null,null,229.8,1.1000000000000001,229.8,1.1000000000000001,229.8,1.1000000000000001,19.399999999999999,0.1,19.399999999999999,0.1,19.399999999999999,0.1,4345.3,3.6,4345.3,3.6,4345.3,3.6,229.8,1.1000000000000001,229.8,1.1000000000000001,229.8,1.1000000000000001,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,227.4,1.1000000000000001,227.4,1.1000000000000001,227.4,1.1000000000000001,18.600000000000001,0.1,18.600000000000001,0.1,18.600000000000001,0.1,4095.3,3.7,null,null,null,null,null,null,null,null,null,228.3,1.1000000000000001,0.8,0,175.8,1,0.1,0.2,4743.8,null,null,null,null,null,null,null,null,null,null,230.2,1.1000000000000001,0,0,379.85,0.19,134.88,0.04,149.53,0.04,14.66,0.03,395.78,0.19,194.02,0.04,152.94,0.04,41.09,0.06,379.09,0.2,134.38,0.03,149.37,0.04,14.99,0.04,88.2,0.03,55.84,0.03,52.27,0.02,null,null,87.85,0.04,59.01,0.04,52.06,0.03,6.95,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.58,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.37,0.03,63.73,0.03,63.74,0.03,63.66,0.03,63.6,0.03,63.66,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162.76,0.15,77.05,0.53,197.13,0.1,115.28,0.08,113.74,0.09,75.84,0.06,75.69,0.04,75.27,0.04,75.3,0.04,75.14,0.03,75.2,0.03,75.22,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.88,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.33,0.06,96.09,0.43,95.15,0.46,75.069999999999993,0.03,106.38,0.5,76.260000000000005,0.05,79.11,0.2,77.099999999999994,0.09,75.64,0.04,84.2,0.62,99.76,0.65,78.599999999999994,0.16,75.88,0.1,90.63,0.61,103.77,0.51,85.02,0.27,92.36,0.6,114.64,0.24,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.004000000000005,1.0999999999999999E-2,61.987000000000002,1.6E-2,64.213999999999999,6.0000000000000001E-3,59.628999999999998,0.01,115.011,1.0999999999999999E-2,80.010000000000005,2.1999999999999999E-2,1126.4000000000001,1.6,1085.2,1.6,0.57199999999999995,1E-3,-0.20399999999999999,1E-3,-7.0000000000000001E-3,3.0000000000000001E-3,1.0693999999999999,3.0999999999999999E-3,29.21,0,4818,6,472.7,5.0999999999999996,0.16622533100174824,191.8074094429173,13.029,0.182,1.1172072499278527,5087.2218189224677,72.924072818897628,215.01802174804391,883.19142428624082,4204.0303946362274,9.6396954952314672E-3,30.259118949272615,63.096792750072147,14.607344399102109,13.285050741961763,1.3774203349888627E-2,42.920447850486305,8.7711095103308323E-3,27.599200714645519,9.804468552272393E-3,26.093436493726344,82.001801192062274,65.670514247103696,25.820443344977019,22580.527381291427,23081.753143921349,4345.3,0.65678310561902431,21216.092141822326,21717.317904452248,4.4035060485309936,0.25191176887808353,-4.4386756042955966,-18.905008441990127,56.730706613234226,22580.527381291427,7660.1565988128204,1388.7767027339146,13531.594079744711,22580.527381291446,1.0000000000000009]
[5,"C-CB5-115-CE","30N0081","C-CB5-115-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",5,0,"CUST 2","6/20/2015","1:08:12","10 Ton","0:10:00","75/62 115/80","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,115,80,5.5,null,5.5,null,229.9,1.2,19.5,0,13791,56,13545,74,-3664,114,10124,93,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.3257523550000001,"5% condenser coil block, economizer closed (2.8V), factory charge (5.5 lbs) 115F OD,--75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%:--Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed,--adjust code teste","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 7.`.;",74.924999999999997,3.9E-2,61.972000000000001,1.9E-2,115.011,5.2999999999999999E-2,80.013999999999996,4.3999999999999997E-2,74.45,0.05,63.07,0.02,67.22,0.02,-2E-3,3.0000000000000001E-3,1.0663,3.5000000000000001E-3,13791,56,-3664,114,2.3250000000000002,2.5000000000000001E-2,null,null,null,null,null,null,229.9,1.2,229.9,1.2,229.9,1.2,17.3,0.1,17.3,0.1,17.3,0.1,3880.3,7.7,3880.3,7.7,3880.3,7.7,229.9,1.2,229.9,1.2,229.9,1.2,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,227.8,1.2,227.8,1.2,227.8,1.2,16.600000000000001,0.1,16.600000000000001,0.1,16.600000000000001,0.1,3650.9,7.3,null,null,null,null,null,null,null,null,null,228.6,1.2,0.7,0,168.2,1,0.1,0.2,4291.8999999999996,null,null,null,null,null,null,null,null,null,null,230.2,1.2,0,0,338.51,0.62,125.72,0.11,140.19,0.15,14.48,7.0000000000000007E-2,354.44,0.62,190.02,7.0000000000000007E-2,143.88999999999999,0.14000000000000001,46.14,0.1,337.8,0.63,125.08,0.1,140.03,0.15,14.94,0.1,85.13,0.05,54.01,0.03,50.44,0.03,null,null,84.42,0.05,55.93,0.04,50.01,0.03,5.92,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.56,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.48,0.04,62.8,0.03,62.81,0.03,62.77,0.03,62.64,0.04,62.71,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,158.57,0.05,68.83,0.06,193.21,0.11,115.15,0.22,113.85,0.14000000000000001,75.8,7.0000000000000007E-2,75.67,0.05,75.22,0.05,75.25,0.06,75.09,0.06,75.150000000000006,0.06,75.19,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.84,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.11,0.13,95.26,0.52,94.84,0.41,75.010000000000005,0.05,106.2,0.53,76.180000000000007,0.05,78.989999999999995,0.16,77.16,0.12,75.59,0.05,83.94,0.55000000000000004,99.63,0.6,78.89,0.2,75.8,0.11,89.99,0.74,103.32,0.54,85.29,0.27,92,0.49,114.64,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.924999999999997,3.9E-2,61.972000000000001,1.9E-2,63.341000000000001,0.01,58.960999999999999,1.4E-2,115.011,5.2999999999999999E-2,80.013999999999996,4.3999999999999997E-2,1123.8,1.8,1084.9000000000001,1.8,0.57099999999999995,2E-3,-0.20399999999999999,1E-3,-2E-3,3.0000000000000001E-3,1.0663,3.5000000000000001E-3,29.234999999999999,0,4353,10,472.8,5.3,0.16622533100174824,191.8074094429173,13.029,0.182,1.118477952478258,5084.5895812378758,72.776458803149609,215.0182679670107,883.19041293738212,4201.3991683004933,9.6480758457967546E-3,30.253263492535559,62.222522047521743,14.607377853110059,13.261247328360419,1.377810810910046E-2,42.924790196086263,8.7798877127593031E-3,27.58953875381167,9.5926172617205388E-3,25.649383965354232,81.940183800571106,65.661857948727544,25.376185522633723,24797.939832647651,24061.49220382256,3880.2,0.53404124251341256,23432.659486542801,22696.21185771771,5.3831057860194811,0.24188000842379262,-4.877077969901837,-19.717661753049363,55.93155459656559,24797.939832647651,9864.8908233794627,1389.101955467117,13543.947053801083,24797.939832647662,1.0000000000000004]
[5,"C-CB50-115-CE","30N0082","C-CB50-115-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",50,0,"CUST 2","6/19/2015","20:30:46","10 Ton","0:10:00","75/62 115/80","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,115,80,5.5,null,5.5,null,229.9,0.9,22.4,0,12397,37,12097,24,-5106,70,7286,62,null,943,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.4577831130000001,"50% condenser coil block, economizer closed (2.8V), factory charge (5.5 lbs)--115F OD, 75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%:--Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed,--adjust code test","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 43.75\".",75.016000000000005,1.6E-2,62.015999999999998,1.9E-2,115.011,1.7000000000000001E-2,79.994,2.8000000000000001E-2,74.459999999999994,0.04,64.27,0.03,67.95,0.02,-8.0000000000000002E-3,3.0000000000000001E-3,1.0728,4.3E-3,12397,37,-5106,70,1.458,1.2999999999999999E-2,null,null,null,null,null,null,229.9,0.9,229.9,0.9,229.9,0.9,20.2,0.1,20.2,0.1,20.2,0.1,4524.8,6,4524.8,6,4524.8,6,229.9,0.9,229.9,0.9,229.9,0.9,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,227.3,0.9,227.3,0.9,227.3,0.9,19.399999999999999,0.1,19.399999999999999,0.1,19.399999999999999,0.1,4273.7,5.7,null,null,null,null,null,null,null,null,null,228.3,0.9,0.8,0,171.5,1,0.1,0.2,4918.8,null,null,null,null,null,null,null,null,null,null,230.2,0.9,0,0,393.45,0.25,138.1,0.05,152.44,0.05,14.34,0.04,409.24,0.25,196.98,0.05,155.72999999999999,0.05,41.24,0.06,392.67,0.25,137.53,0.04,152.28,0.05,14.75,0.06,89.39,0.03,56.49,0.03,52.96,0.02,null,null,89.24,0.03,58.83,0.02,52.87,0.01,5.96,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.53,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.58,0.05,63.98,0.04,63.99,0.03,63.91,0.03,63.84,0.04,63.93,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,165.77,0.04,74.47,0.15,199.39,0.1,115.18,0.1,113.61,0.1,75.84,7.0000000000000007E-2,75.72,0.05,75.260000000000005,0.06,75.290000000000006,0.05,75.099999999999994,0.05,75.17,0.04,75.239999999999995,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.81,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.64,0.06,95.9,0.39,94.93,0.45,75.069999999999993,0.03,106.21,0.56999999999999995,76.28,0.05,79.150000000000006,0.18,77.040000000000006,0.1,75.680000000000007,0.05,84.35,0.6,99.92,0.54,78.53,0.19,75.91,0.11,90.86,0.52,103.51,0.51,84.85,0.28999999999999998,92.19,0.57999999999999996,114.47,0.2,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.016000000000005,1.6E-2,62.015999999999998,1.9E-2,64.575000000000003,7.0000000000000001E-3,59.863,7.0000000000000001E-3,115.011,1.7000000000000001E-2,79.994,2.8000000000000001E-2,1128.9000000000001,2.2999999999999998,1086.3,2.2000000000000002,0.57499999999999996,1E-3,-0.20300000000000001,1E-3,-8.0000000000000002E-3,3.0000000000000001E-3,1.0728,4.3E-3,29.196999999999999,0,4998,8,473.6,5,0.16622533100174824,191.8074094429173,13.029,0.182,1.1167793455450228,5094.8133128083973,73.380848031496058,214.48938712602379,881.02811469055052,4213.7851981178464,9.6470476538200508E-3,30.262809182366887,63.458220654454983,14.607210613343049,13.294697144194908,1.3758588147154506E-2,42.903082731869148,8.7873971023552291E-3,27.619951074776342,9.8669171262547092E-3,26.249696411958233,81.983879006500871,65.674880489526942,25.976776857880072,21836.534545922546,22652.344992130427,4524.3999999999996,0.70715328787751186,20470.586580254043,21286.397026461924,4.0957556182981278,0.25959568346674522,-4.2860323244868148,-18.525658352045888,56.962876375415021,21836.534545922546,6981.1916980634833,1390.4741774431461,13464.868670415945,21836.534545922572,1.0000000000000011]
[5,"C-CB30-82-CE","30N0089","C-CB30-82-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",30,0,"CUST 2","6/20/2015","6:20:53","10 Ton","0:10:00","75/62 82/68","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,82,68,5.5,null,5.5,null,230,1.3,15.4,0,22488,56,21970,74,4803,102,27296,93,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8.0235155789999997,"30% condenser coil block, economizer closed (2.8V), factory charge (5.5 lbs)--82F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed,--adjust code teste","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 33 in.",74.932000000000002,3.4000000000000002E-2,61.972000000000001,2.5000000000000001E-2,81.947000000000003,1.7000000000000001E-2,68.016999999999996,2.1000000000000001E-2,74.47,0.05,56.42,0.04,62.77,0.06,0.01,3.0000000000000001E-3,1.0748,3.3E-3,22488,56,4803,102,8.0220000000000002,3.4000000000000002E-2,null,null,null,null,null,null,230,1.3,230,1.3,230,1.3,13.2,0,13.2,0,13.2,0,2926.6,5.6,2926.6,5.6,2926.6,5.6,229.8,1.3,229.8,1.3,229.8,1.3,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,228.3,1.3,228.3,1.3,228.3,1.3,12.4,0,12.4,0,12.4,0,2705.4,4.0999999999999996,null,null,null,null,null,null,null,null,null,228.7,1.3,0.8,0,176.2,1.1000000000000001,0.1,0.2,3357.2,null,null,null,null,null,null,null,null,null,null,230.2,1.3,0,0,242.41,0.18,95.74,0.05,114.8,0.05,19.059999999999999,0.03,259.8,0.17,167.48,0.04,119.87,0.05,47.61,0.05,241.79,0.18,95.14,0.03,114.62,0.05,19.48,0.05,75.95,0.02,53.37,0.51,44.71,0.02,null,null,76.86,0.02,54.3,0.32,45.3,0.02,9,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8.66,0.51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.33,0.03,55.67,0.04,55.76,0.03,55.77,0.02,55.55,0.03,55.62,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,135.72999999999999,0.03,80.27,0.1,169.88,0.04,82.01,0.1,82.13,0.04,75.16,0.04,75.09,0.04,75.23,0.04,75.22,0.04,75.13,0.05,75.14,0.05,75.09,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.5,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,81.88,0.09,78.45,0.12,78.37,0.12,74.87,0.04,80.709999999999994,0.14000000000000001,75.459999999999994,0.05,75.86,0.05,75.41,0.05,74.89,0.05,76.790000000000006,0.12,79.47,0.11,75.77,0.05,75.11,0.05,77.34,0.16,80.39,0.12,76.760000000000005,0.06,78,0.12,81.7,0.1,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.932000000000002,3.4000000000000002E-2,61.972000000000001,2.5000000000000001E-2,56.460999999999999,0.01,53.552,1.0999999999999999E-2,81.947000000000003,1.7000000000000001E-2,68.016999999999996,2.1000000000000001E-2,1123.0999999999999,1.7,1096.2,1.7,0.56699999999999995,1E-3,-0.20300000000000001,2E-3,0.01,3.0000000000000001E-3,1.0748,3.3E-3,29.234999999999999,0,3402,9,475.6,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,1.1104803255397022,5153.9453559410604,73.0193493543307,208.08137540008556,908.15999268281803,4245.7853632582428,9.2346961191203409E-3,28.391830275302144,55.350519674460294,13.747448274090154,13.074643859450848,1.1368726327124046E-2,32.143143692328614,8.7782338412914166E-3,27.589436260089062,8.0281126506667796E-3,22.269721741513422,76.172888453979681,63.096286802496778,21.999248176233387,32947.01882196738,25756.164209015053,2926.4,0.30314740322850231,31573.011061313711,24382.156448361384,9.2807204765766347,0.19734632539435626,-6.3925820990687576,-20.822368779519387,50.230979211802797,32947.01882196738,27417.517937945155,1394.0059756798587,4135.4949083423653,32947.01882196738,1]
[5,"C-CB70-82-CE","30N0094","C-CB70-82-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",70,0,"CUST 2","6/20/2015","3:43:38","10 Ton","0:10:00","75/62 82/68","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,82,68,5.5,null,5.5,null,230,0.6,16.7,0,21826,34,21412,69,3843,84,25672,103,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.9215421949999998,"70% condenser coil block, economizer closed (2.8V), factory charge (5.5 lbs) 82F OD,--75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%:--Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed,--adjust code teste","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 46`",75.024000000000001,0.04,61.991999999999997,3.3000000000000002E-2,81.972999999999999,1.2E-2,68.013000000000005,2.7E-2,74.48,0.05,56.86,0.02,62.6,0.03,1E-3,3.0000000000000001E-3,1.0724,4.3E-3,21826,34,3843,84,6.9210000000000003,2.9000000000000001E-2,null,null,null,null,null,null,230,0.6,230,0.6,230,0.6,14.5,0,14.5,0,14.5,0,3233.4,3.5,3233.4,3.5,3233.4,3.5,229.9,0.6,229.9,0.6,229.9,0.6,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,228.2,0.6,228.2,0.6,228.2,0.6,13.7,0,13.7,0,13.7,0,3011.4,3.1,null,null,null,null,null,null,null,null,null,228.8,0.6,0.8,0,171.4,0.7,0,0.2,3658.6,null,null,null,null,null,null,null,null,null,null,230.3,0.6,0,0,273.70999999999998,0.22,104.21,0.05,123.75,0.06,19.53,0.04,291.27,0.22,165.77,0.05,128.44999999999999,0.06,37.31,0.05,273.10000000000002,0.22,103.85,0.04,123.58,0.06,19.73,0.06,77.72,0.04,48.18,0.03,45.84,0.03,null,null,78.040000000000006,0.04,49.55,0.04,46.05,0.03,3.5,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.34,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.15,0.03,56.47,0.03,56.5,0.03,56.43,0.03,56.36,0.03,56.39,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133.83000000000001,0.05,61.68,0.09,168.05,7.0000000000000007E-2,81.59,0.17,81.93,0.13,75.13,0.05,75.11,0.04,75,0.05,75.069999999999993,0.05,75.06,0.05,75.11,0.05,75.16,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.87,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,81,0.11,79.2,0.11,79,0.12,75.010000000000005,0.04,81.7,0.13,75.81,0.04,76.23,0.05,75.78,0.04,75.239999999999995,0.05,77.260000000000005,0.12,80.209999999999994,0.11,76.14,0.05,75.47,0.05,78.040000000000006,0.15,81.319999999999993,0.15,77.11,0.06,78.52,0.11,83.01,0.16,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",75.024000000000001,0.04,61.991999999999997,3.3000000000000002E-2,57.057000000000002,1.4E-2,54.106000000000002,1.9E-2,81.972999999999999,1.2E-2,68.013000000000005,2.7E-2,1121.9000000000001,2.2000000000000002,1094.7,2.2000000000000002,0.56499999999999995,1E-3,-0.20200000000000001,1E-3,1E-3,3.0000000000000001E-3,1.0724,4.3E-3,29.224,0,3709,6,475.8,4.9000000000000004,0.16622533100174824,191.8074094429173,13.029,0.182,1.1146052436768978,5141.977806115824,72.662220944881895,207.57264588053684,905.90109813844015,4236.0767079773841,9.2259543154951367E-3,28.401816711676524,55.942394756323104,13.748033619150034,13.091071672837115,1.1359532662756034E-2,32.139425842292212,8.7696804798235162E-3,27.602514798786068,8.1988285360078041E-3,22.600340525246153,76.253009056318078,63.111417240421652,22.328777791732161,31227.431342031527,25064.814710196682,3233.2,0.35337237568903784,29851.522102116407,23688.905470281563,8.0484017530645477,0.19715582320109862,-6.0730389199443628,-20.310614299994974,50.954682323754092,31227.431342031527,25721.069096865784,1396.369548697093,4109.9926964686329,31227.431342031508,0.99999999999999944]
[5,"C-CB60-95-CE","30N0103","C-CB60-95-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",60,0,"CUST 2","6/19/2015","12:09:14","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,229.9,1.1000000000000001,18.600000000000001,0,17193,61,16848,92,-910,50,16282,54,null,643,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.9519417479999999,"60% condenser coil block(~60 psig DP above C-CB0-95-CE), economizer closed (2.8V),--factory charge (5.5 lbs) 95F OD, 75F DB, 62F WB ID conditions, unsealed cabinet, Inlet--Meriam set @ 53.5%: Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from f","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer. Condenser Coil is blocked 43\", with outlet duct, with code tester",74.873000000000005,4.3999999999999997E-2,61.968000000000004,1.2999999999999999E-2,95.001999999999995,8.9999999999999993E-3,75.007999999999996,2.1999999999999999E-2,74.55,0.09,60.28,0.05,66,0.09,-2.1000000000000001E-2,2E-3,1.0311999999999999,3.2000000000000002E-3,17193,61,-910,50,3.952,1.4999999999999999E-2,null,null,null,null,null,null,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,16.399999999999999,0.1,16.399999999999999,0.1,16.399999999999999,0.1,3648.1,5,3648.1,5,3648.1,5,229.9,1.1000000000000001,229.9,1.1000000000000001,229.9,1.1000000000000001,2.2000000000000002,0,2.2000000000000002,0,2.2000000000000002,0,null,227.9,1.1000000000000001,227.9,1.1000000000000001,227.9,1.1000000000000001,15.5,0.1,15.5,0.1,15.5,0.1,3411.5,4.5,null,null,null,null,null,null,null,null,null,228.5,1.1000000000000001,0.8,0,171.9,1,0,0.2,4068.3,null,null,null,null,null,null,null,null,null,null,230.2,1.1000000000000001,0,0,315.08,0.17,116.98,0.06,134.53,0.04,17.559999999999999,0.04,332.06,0.17,175.68,0.05,138.66,0.04,37.020000000000003,0.05,314.39,0.18,116.55,7.0000000000000007E-2,134.36000000000001,0.04,17.809999999999999,0.06,81.88,0.02,51.56,0.04,48.47,0.01,null,null,82.95,0.02,53.96,0.04,49.13,0.01,4.83,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.09,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.22,0.03,59.57,0.03,59.65,0.03,59.65,0.03,59.42,0.03,59.52,0.03,null,null,null,null,53.13,0.05,51.07,0.04,null,null,null,null,null,null,null,null,null,null,116.55,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,145.27000000000001,0.05,64.91,0.05,177.95,7.0000000000000007E-2,95.17,0.08,94.81,0.12,75.5,0.05,75.38,0.05,75.349999999999994,0.06,75.349999999999994,0.05,75.2,0.05,75.23,0.05,75.16,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.56,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.35,7.0000000000000007E-2,85,0.27,85.02,0.24,74.92,0.05,90.62,0.34,75.709999999999994,0.05,76.989999999999995,0.09,76.09,0.08,75.14,0.06,79.33,0.27,87.22,0.28999999999999998,77.03,0.11,75.37,7.0000000000000007E-2,82.21,0.38,89.85,0.27,80.23,0.15,83.44,0.32,94.86,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,"C-55-CE-DM",74.873000000000005,4.3999999999999997E-2,61.968000000000004,1.2999999999999999E-2,60.307000000000002,1.4999999999999999E-2,56.972999999999999,1.2E-2,95.001999999999995,8.9999999999999993E-3,75.007999999999996,2.1999999999999999E-2,1102.8,1.7,1069.4000000000001,1.7,0.57599999999999996,1E-3,-0.19500000000000001,1E-3,-2.1000000000000001E-2,2E-3,1.0311999999999999,3.2000000000000002E-3,29.274000000000001,0,4120,8,471.9,5.2,0.16622533100174824,191.8074094429173,13.029,0.182,1.13144889841159,5020.1629276283602,72.364866519685037,206.53862538676054,878.88664848095095,4141.2762791474088,9.6890147502722221E-3,29.43921665487964,59.175551101588411,14.1000179541062,13.180448713296895,1.3927311398363293E-2,38.164823755898936,8.7895378534843336E-3,27.587415648607426,9.0977703086713036E-3,24.370018997398493,78.424155671507464,64.536844582900258,24.093900875765684,26834.356110774792,23191.471456916512,3648.1,0.46399344365116207,25470.742700206476,21827.858046348196,6.1822191019918629,0.20913165831187877,-5.3453157791139567,-19.248604569919053,54.085585576727091,26834.356110774792,16151.855391874718,1386.1579578674061,9296.3427610326744,26834.356110774796,1.0000000000000002]
[5,"C-EB35-115-CE","30N0109","C-EB35-115-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,35,"CUST 2","6/17/2015","23:09:27","10 Ton","0:10:00","75/62 115/80","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,115,80,5.5,null,5.5,null,229.9,1.9,19,0,11925,42,11769,66,-2205,44,9717,41,null,946,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.3036984349999998,"35% evaporator coil block, economizer closed damper, factory charge (5.5 lbs) 115F OD,--75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%: Outlet @ 52% Horiz airflow.--4.75\" ID pulley 3 turns open from fully closed, adjust code test","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer.;",74.959999999999994,3.2000000000000001E-2,61.969000000000001,1.9E-2,115.004,1.2999999999999999E-2,79.997,1.9E-2,74.599999999999994,0.06,63.66,0.06,67.81,0.03,-1.7999999999999999E-2,2E-3,0.87329999999999997,3.0999999999999999E-3,11925,42,-2205,44,2.3039999999999998,1.0999999999999999E-2,null,null,null,null,null,null,229.9,1.9,229.9,1.9,229.9,1.9,16.899999999999999,0.1,16.899999999999999,0.1,16.899999999999999,0.1,3763.4,5.9,3763.4,5.9,3763.4,5.9,229.8,1.9,229.8,1.9,229.8,1.9,2.1,0,2.1,0,2.1,0,null,227.8,1.9,227.8,1.9,227.8,1.9,16,0.1,16,0.1,16,0.1,3529.8,5.3,null,null,null,null,null,null,null,null,null,228.5,1.9,0.7,0,167.4,1.6,0.1,0.2,4151.5,null,null,null,null,null,null,null,null,null,null,230.2,1.9,0,0,326.35000000000002,0.27,124.79,0.05,137.27000000000001,7.0000000000000007E-2,12.48,0.03,341.84,0.26,181.02,7.0000000000000007E-2,140.94999999999999,0.06,40.06,0.06,325.64999999999998,0.28000000000000003,124.01,7.0000000000000007E-2,137.1,7.0000000000000007E-2,13.09,7.0000000000000007E-2,79.78,0.03,50.72,0.03,47.1,0.02,null,null,80.87,0.03,52.48,0.05,47.79,0.02,4.6900000000000004,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.62,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.98,0.04,63.36,0.03,63.37,0.03,63.34,0.03,63.17,0.04,63.26,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,154.66999999999999,7.0000000000000007E-2,64.540000000000006,0.08,182.11,7.0000000000000007E-2,115.42,0.09,114.09,0.1,78.099999999999994,0.14000000000000001,77.25,0.16,76.27,0.09,76.16,0.08,75.599999999999994,0.06,75.69,0.06,75.38,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.900000000000006,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.09,0.08,101.8,0.23,102.15,0.41,77.16,0.14000000000000001,92.04,0.35,78.44,0.25,91.35,0.35,76.66,0.06,75.78,0.05,78.47,0.16,89.01,0.4,null,null,76.42,0.1,81.3,0.41,90.07,0.4,76.400000000000006,0.09,103.55,0.44,114.81,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,"C-EB35-55-CE",74.959999999999994,3.2000000000000001E-2,61.969000000000001,1.9E-2,63.881,1.4999999999999999E-2,58.774999999999999,0.02,115.004,1.2999999999999999E-2,79.997,1.9E-2,1019.7,1.8,978,1.7,0.46899999999999997,1E-3,-0.16700000000000001,1E-3,-1.7999999999999999E-2,2E-3,0.87329999999999997,3.0999999999999999E-3,29.07,1E-3,4218,10,454.2,5.9,0.15207165732586084,157.77434447558062,13.029,0.18099999999999999,1.2346520660520122,4609.5004025662984,53.886105826771654,160.46539021362941,659.12753539209075,3950.3728671742074,9.4836845920174308E-3,29.77746390698762,62.646347933947986,14.607072070036441,13.273021945271436,1.3763184777227737E-2,42.906471706780039,8.7696415118751238E-3,27.586862957611697,9.3490442052999931E-3,25.515944375861466,80.730574201976296,65.024364748512028,25.214502869374787,21032.970739770688,20006.219583018366,3763.8,0.61074821806841206,19666.699418957462,18639.948262205136,4.662565059022632,0.29378278997773311,-4.5629610376128333,-18.08422626802831,55.123401208474597,21032.970739770688,9545.9000362597162,1389.4947455005379,10097.575958010439,21032.970739770695,1.0000000000000004]
[5,"C-EB20-95-CE","30N0120","C-EB20-95-CE","closed","on","N/A","3 turns","unsealed","unsealed",null,4.75,"horizontal",0,20,"CUST 2","6/17/2015","11:03:55","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU5","RTU5","3","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/1","TU3","AHRI 210/240 2008",75,62,95,75,5.5,null,5.5,null,230.1,1.8,15.8,0,17647,15,17131,63,904,70,18552,72,null,944,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.2869763470000004,"20% evaporator coil block, economizer closed damper, factory charge (5.5 lbs) 95F OD,--75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 53.5%:--Outlet @ 52% Horiz airflow. 4.75\" ID pulley 3 turns open from fully closed, adjust--code test","R22 5.5 LBS. unsealed cab:Inlet Meriam set @ 53.5%: Outlet Meriam set @ 52% manually: Horiz airflow. ID Pulley is 3 turns open from fully closed: installed economizer.;, with outlet duct, with code tester, 9\" coil blockage",74.998999999999995,1.2E-2,61.994,2.5999999999999999E-2,94.992000000000004,6.0000000000000001E-3,74.998999999999995,1.4999999999999999E-2,74.37,0.08,59.59,7.0000000000000007E-2,65.13,0.03,7.0000000000000001E-3,1E-3,0.71609999999999996,8.9999999999999998E-4,17647,15,904,70,5.2869999999999999,2.7E-2,null,null,null,null,null,null,230.1,1.8,230.1,1.8,230.1,1.8,13.7,0,13.7,0,13.7,0,3040.6,7.2,3040.6,7.2,3040.6,7.2,230,1.8,230,1.8,230,1.8,2.1,0,2.1,0,2.1,0,null,228.4,1.8,228.4,1.8,228.4,1.8,12.9,0,12.9,0,12.9,0,2821.2,6.3,null,null,null,null,null,null,null,null,null,228.9,1.8,0.7,0,169.4,1.5,13,0.2,3471.5,null,null,null,null,null,null,null,null,null,null,230.3,1.8,0,0,253.85,0.12,102.38,0.03,118.14,0.04,15.76,0.03,270.18,0.1,173.25,0.05,122.76,0.03,50.49,0.06,253.19,0.14000000000000001,101.89,7.0000000000000007E-2,117.95,0.04,16.059999999999999,7.0000000000000007E-2,75.209999999999994,0.02,48.33,7.0000000000000007E-2,44.18,0.02,null,null,75.95,0.01,50.15,0.11,44.66,0.01,5.48,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.1399999999999997,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.87,0.03,59.15,0.02,59.22,0.02,59.19,0.03,59.01,0.02,59.09,0.02,null,null,null,null,49.71,0.1,47.53,0.09,null,null,null,null,null,null,null,null,null,null,101.89,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,144.97,0.08,81.239999999999995,0.1,174.1,0.11,95.23,0.06,94.53,7.0000000000000007E-2,76.09,7.0000000000000007E-2,75.75,7.0000000000000007E-2,75.34,0.08,75.31,7.0000000000000007E-2,75.08,0.06,75.14,0.06,75.03,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.599999999999994,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.81,7.0000000000000007E-2,89.12,0.13,82.84,0.68,75.430000000000007,0.04,87.88,0.1,82.36,0.12,78.510000000000005,0.21,75.430000000000007,0.05,75.180000000000007,0.05,77.930000000000007,0.14000000000000001,86.36,0.16,75.62,0.05,75.8,7.0000000000000007E-2,80.45,0.2,88.36,0.2,75.2,0.06,86.95,0.36,94.96,0.05,null,null,null,null,null,null,null,null,null,null,null,null,"C-EB20-55-CE",74.998999999999995,1.2E-2,61.994,2.5999999999999999E-2,59.771999999999998,1.0999999999999999E-2,56.167000000000002,1.0999999999999999E-2,94.992000000000004,6.0000000000000001E-3,74.998999999999995,1.4999999999999999E-2,1084.3,0.7,1047,0.7,0.52400000000000002,1E-3,-0.185,1E-3,7.0000000000000001E-3,1E-3,0.71609999999999996,8.9999999999999998E-4,29.088000000000001,1E-3,3509,11,467.9,5.6,0.15583700440528631,166.26249999999996,13.029,0.19,{"$f":"(XM98-XU98)*3.412/XT98/0.24","v":1.1605823815595242},4942.0633525108306,64.452990236220472,170.66837231426885,726.26290104635677,4215.8004514644736,9.5329781210419101E-3,29.154993875320745,58.611417618440477,14.099718330790125,13.164137195235888,1.3921817173516522E-2,38.156300819185354,8.776905574636517E-3,27.604323873378664,8.7460145306600696E-3,23.85690986758415,77.960521209194624,64.15323478349319,23.573863287164187,27582.300945305742,22949.878982352428,3041.1,0.3763019742472376,26205.336300981962,21572.914338028648,7.4680354234773336,0.23221735184374129,-5.581130588156558,-19.349103590754147,52.759243689809701,27582.300945305742,18519.957424722877,1398.8341321470105,7663.5093884358421,27582.300945305731,0.99999999999999956]
[5,"C-22A","30N0014","C-22A","None","on","N/A","5.5 turns","sealed","unsealed",760,null,"horizontal",0,0,"CUST 1","2/24/2014","23:49:29","10 Ton","0:30:00","80/67 - 95/70","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 lbs","208/230/1","TU1","AHRI 210/240 2008",80,67,95,70,5.5,null,5.5,null,230.3,0.9,14.9,0,26354,69,25489,154,9625,105,35987,123,10.974992375999999,756,null,13.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A test factory chg, low speed fan 760 rpm, sealed cab, no econo","R22 5.5 lbs manuf. Sealed cab: Meriam set @ 100%: Horiz airflow. ID Pulley is 5.5 turns open from fully closed for 1200 scfm @ 0.15 esp.",79.894000000000005,3.5000000000000003E-2,67.152000000000001,2.9000000000000001E-2,94.847999999999999,1.4999999999999999E-2,70.007000000000005,2.1999999999999999E-2,79.489999999999995,0.14000000000000001,61.95,0.06,67.709999999999994,0.02,7.2999999999999995E-2,2E-3,1.0677000000000001,3.5999999999999999E-3,26354,69,9625,105,10.975,4.3999999999999997E-2,null,null,null,null,null,null,229.7,0.9,229.7,0.9,229.7,0.9,13.5,0,13.5,0,13.5,0,2986.2,5.5,2986.2,5.5,2986.2,5.5,230,0.9,230,0.9,230,0.9,1.4,0,1.4,0,1.4,0,null,227.8,0.9,227.8,0.9,227.8,0.9,12.8,0,12.8,0,12.8,0,2789.8,5.0999999999999996,null,null,null,null,null,null,null,null,null,228.2,0.9,0.8,0,173.7,0.9,23,null,3278.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,265.77999999999997,0.18,184.73,0.05,121.57,0.05,63.15,7.0000000000000007E-2,null,null,103.15,0.05,null,null,null,null,null,null,70.31,7.0000000000000007E-2,null,null,null,null,80.180000000000007,7.0000000000000007E-2,71.63,0.08,47.46,0.04,24.18,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.41,0.06,62.29,0.08,61.97,0.09,62.34,7.0000000000000007E-2,61.69,7.0000000000000007E-2,62.09,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.03,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.44,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.61,0.09,94.61,0.09,79.400000000000006,0.13,79.459999999999994,0.12,79.459999999999994,0.1,79.37,0.13,79.37,0.13,79.41,0.13,79.39,0.12,80.010000000000005,0.11,79.959999999999994,0.11,79.790000000000006,0.11,79.61,0.09,80.16,7.0000000000000007E-2,79.84,0.12,79.680000000000007,0.13,79.760000000000005,0.11,80.099999999999994,0.1,79.98,0.11,79.62,0.14000000000000001,79.64,0.13,79.760000000000005,0.11,79.87,0.11,80.02,0.1,79.86,0.11,79.98,0.09,79.849999999999994,0.1,79.94,0.1,79.94,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",79.894000000000005,3.5000000000000003E-2,67.152000000000001,2.9000000000000001E-2,61.749000000000002,0.02,58.704000000000001,2.9000000000000001E-2,94.847999999999999,1.4999999999999999E-2,70.007000000000005,2.1999999999999999E-2,1322.4,2.2000000000000002,1282.5,2.2000000000000002,0.154,1E-3,-0.10299999999999999,1E-3,7.2999999999999995E-2,2E-3,1.0677000000000001,3.5999999999999999E-3,29.399000000000001,1E-3,3279,7,291.8,3.7,null,0,null,null,0.63635787334196336,6000.6403520132353,23.202949606299214,0,0,6000.6403520132353,1.1213593147458508E-2,31.469961401503308,61.112642126658038,14.062101462873807,13.222588814772045,9.8297142332913878E-3,33.606800760128216,1.1213593147458508E-2,31.469961401503312,9.8105219225176673E-3,25.497694483469179,79.893999999999991,67.152009445186451,25.342196700594165,36770.51213191772,27048.04174089053,2987.2,0.27726874087103653,35853.790398924022,26131.320007896829,10.934367306777682,0.23423940516746219,-6.1277647009091432,-18.781357873341953,55.367590571150757,36770.51213191772,35837.425861349344,933.08627056839714,0,36770.512131917741,1.0000000000000007]
[5,"C-22C-D#7","30N0038","C-22C-D#7","None","on","N/A",null,"sealed","unsealed",760,null,"horizontal",0,0,"CUST 1","2/25/2014","7:44:31","10 Ton","","80/57  82","ENG 1","TECH 1","RTU5","RTU5","3","R22","PSC Air Handler","5.5 lbs","208/230/1","","",80,57,82,null,5.5,null,5.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11.715,null,null,null,7,6.45,81.853999999999999,30.016999999999999,58.959000000000003,0.32,452.7,1282,13.436,33139.089999999997,0.2419,3066.3820000000001,4.3299999999999996E-3,20.441240310000001,142.41999999999999,1.51,131.846,250.7,10.707000000000001,4.8600000000000003,12.96,3.35,30.8,0.185,286.39,0.106,253.5,282.74,12.27312,282.74,0.99,null,"C/D test factory chg, low speed fan 760 rpm, sealed cab, no econo","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",79.69,null,55.35,null,58.262,null,47.661999999999999,null,null,null,null,null,1266.0999999999999,null,1234.5,null,0.21199999999999999,null,null,null,-3.1E-2,null,0.98470000000000002,null,29.448,null,2656,null,289.10000000000002,null,null,0,null,null,0.63302513108828673,5802.1855102476839,30.7462431496063,0,0,5802.1855102476839,3.6070987845449164E-3,23.080359478152484,57.628974868911712,11.593798628049566,13.092652736771452,7.8407761683729174E-4,0.83190635146436653,3.6070987845449164E-3,23.080359478152484,4.5046347221530253E-3,18.878824808717201,79.69,55.350000841099259,18.725632690394452,25266.932669017096,30720.518485634511,2366.9,0.31971548766209024,24385.171296886703,29838.757113504118,9.1811638919001144,0.44614004558039194,-4.3547267877580325,-22.061025131088286,39.858586020619384,25266.932669017096,24378.083579800692,888.84908921640636,0,25266.9326690171,1.0000000000000002]
[4,"L-55-3ER-DM","30T0012","L-55-3ER-DM","3 Finger","off","N/A","3 turns","unsealed","unsealed",null,null,null,0,0,"CUST 4","3/22/2014","15:21:14","10 Ton","0:20:00","75/62  55/51","ENG 1","TECH 4","RTU4","RTU4","3","R22","PSC Air Handler","7 LBS","380/460/3","TU5","AHRI 210/240 2008",75,62,55,51,7,null,7,null,458.3,0.8,1.6,0,9768,32,9422,73,3988,73,13760,84,28.547717842000001,785,null,13.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 3F-open, no compressor, 55/51 ambient, 60% inlet 54% outlet Meriam,--adjust code tester speed to match total static of run L-55-3E-DM-SPWCT-SSR","R22 7 LBS: OFB: Econo 3 Finger Opened: Unsealed around damper perimeter: Unsealed cab:Inlet Meriam set @ 60%: Outlet @ 54% Horiz airflow. ID Pulley is 3 turns open from fully closed",75,2.1999999999999999E-2,61.999000000000002,2.4E-2,55.003,1.0999999999999999E-2,51.009,0.02,74.75,0.05,67.86,0.05,70.989999999999995,0.05,1.0999999999999999E-2,4.0000000000000001E-3,1.1884999999999999,6.6E-3,9768,32,3988,73,28.562000000000001,0.35799999999999998,null,null,null,null,null,null,458.3,2.2000000000000002,463.1,2.2000000000000002,461.7,2.2000000000000002,1.6,0,1.3,0,1.6,0,615.79999999999995,7.6,555.5,8.8000000000000007,-10,0,460,null,465,null,456,null,1.3,null,1.5,null,1.3,null,0.36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,null,null,485,487,487,0.9,0.8,1.1000000000000001,510,0.61,13.8,18.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,67.78,0.05,69.97,0.04,68.25,0.04,69.52,0.04,67.849999999999994,0.04,69.09,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72.3,0.03,null,null,55.04,0.08,54.83,0.06,54.86,0.1,54.66,7.0000000000000007E-2,54.83,0.11,54.84,0.11,null,null,null,null,null,null,null,null,73.5,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.62,0.05,55.58,0.09,74.349999999999994,0.05,74.56,0.03,74.22,0.04,73.66,0.08,74.09,0.06,73.569999999999993,0.1,74.12,0.06,58.62,0.04,66.61,0.11,63.93,0.1,72.08,0.09,58.36,7.0000000000000007E-2,64.95,0.06,61.3,0.06,61.67,0.18,57.53,0.03,58.23,0.08,59.57,7.0000000000000007E-2,60.27,0.12,58.65,0.05,57.79,0.08,57.37,0.09,62.46,0.2,57.54,0.1,57.82,7.0000000000000007E-2,57.37,0.08,60.87,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75,2.1999999999999999E-2,61.999000000000002,2.4E-2,67.850999999999999,8.0000000000000002E-3,58.381999999999998,1.7999999999999999E-2,55.003,1.0999999999999999E-2,51.009,0.02,1257.2,3.5,1212.0999999999999,3.4,0.66500000000000004,1E-3,-0.13,1E-3,1.0999999999999999E-2,4.0000000000000001E-3,1.1884999999999999,6.6E-3,29.337,1E-3,482,6,390,null,0.32049807471120673,388.47571635745362,13.03,0.13,0.74380560678806895,5644.2952908240404,94.694596692913393,388.46989413983198,1788.8635702026222,3855.4317206214182,8.2112152734900648E-3,25.444825978559525,67.107194393211927,13.029609432847822,13.36429015729035,6.9854205045364924E-3,20.782844428614112,8.7799660037902651E-3,27.607916797947688,8.1682467019802436E-3,25.19682507669841,68.676447431728533,58.768349695433422,25.015614170132885]
[4,"L-75629575-OE3","30T0018","L-75629575-OE3","open","on","N/A","3 turns","sealed","unsealed",null,null,null,0,0,"CUST 4","3/21/2014","22:30:26","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU4","RTU4","3","R22","PSC Air Handler","7 LBS","380/460/3","TU5","AHRI 210/240 2008",75,62,95,75,7,null,7,null,458.9,1.4,6.2,0,11177,58,10804,71,-12699,230,-1535,247,-0.49104286600000002,786,null,12.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Factory charge, 3 turns, Econo fully open unsealed cab, 60% inlet 54% outlet Meriam,--adust code tester speed to match total static of run L-OE3-SPWCT-SS","R22 7 LBS: OFB: Econo Closed: sealed around damper perimeter: Unsealed cab:Inlet Meriam set @ 60%: Outlet @ 54% Horiz airflow. ID Pulley is 3 turns open from fully closed",74.997,2.3E-2,61.899000000000001,6.8000000000000005E-2,94.998000000000005,8.9999999999999993E-3,75.004000000000005,0.02,74.69,0.04,66,0.05,70.05,0.08,1E-3,4.0000000000000001E-3,1.0808,6.6E-3,11177,58,-12699,230,0,0,null,null,null,null,null,null,458.9,2.6,461.4,2.6,461.2,2.6,6.2,0,5,0,5.5,0,2785.5,25.9,1494.1,29.1,340,19.399999999999999,460,null,460,null,460,null,1.3,null,1.4,null,1.4,null,0.36,460,null,460,null,460,null,4,null,4,null,3.5,null,2360,null,0.67,null,null,null,null,null,null,null,null,458.5,2.6,0.8,0,367,1.5,21,null,3128,480,480,480,0.5,0.6,0.6,280,0.62,12.12,17.7,null,null,null,null,216.06,0.22,99.99,0.05,null,null,null,null,224.11,0.15,167.74,0.06,109.19,0.05,58.55,7.0000000000000007E-2,null,null,96.96,0.06,106.62,7.0000000000000007E-2,6.63,7.0000000000000007E-2,null,null,66.86,0.32,null,null,null,null,81.760000000000005,0.16,70.83,0.14000000000000001,48.39,0.1,22.44,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65.489999999999995,0.05,65.94,0.06,66.36,7.0000000000000007E-2,65.92,0.06,66.290000000000006,0.06,65.25,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.82,0.04,null,null,93.8,0.19,94.15,0.14000000000000001,94,0.2,94.47,0.15,94.3,0.2,94.32,0.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.74,7.0000000000000007E-2,94.01,0.1,75.209999999999994,0.05,75.09,0.04,75.05,0.04,75.48,7.0000000000000007E-2,75.41,0.06,75.58,0.06,75.290000000000006,0.04,93.02,0.05,94.05,0.08,94.91,0.17,94.45,0.13,94.23,0.13,95.53,0.19,95.29,0.2,93.67,0.14000000000000001,93.76,7.0000000000000007E-2,94.95,0.17,95.23,0.18,92.02,0.17,90.85,0.13,93.63,0.16,92.95,0.21,91.05,0.19,93.72,0.19,93.3,0.11,93.57,0.15,91.62,0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L-55-OER-DM",74.997,2.3E-2,61.899000000000001,6.8000000000000005E-2,66.015000000000001,2.1000000000000001E-2,62.262,3.1E-2,94.998000000000005,8.9999999999999993E-3,75.004000000000005,0.02,1200.9000000000001,3.7,1149.9000000000001,3.6,0.51100000000000001,2E-3,-1.6E-2,3.0000000000000001E-3,1E-3,4.0000000000000001E-3,1.0808,6.6E-3,29.225999999999999,1E-3,3126,9,380,null,0.57830843782784613,694.25927961232924,13.029,1.4E-2,0.81853887865637542,5401.0119889427579,69.031303842519691,772.09380384551446,3285.5299673021191,2115.4820216406388,1.1884115319828524E-2,33.999344802799428,65.196461121343631,14.099895204660301,13.340833189689787,1.3924762905989469E-2,38.161027577440002,8.7148098242257593E-3,27.535884782523564,1.1086197714326987E-2,27.930999546798347,87.208902328704212,70.31421663354017,27.730521145093352,33857.991731838505,28533.470128044504,2746,0.27680608094622777,32796.655571853022,27472.133968059024,10.491572479799432,0.20757199413605648,-6.2688236577060756,-22.012441207360581,59.430427761337619,33857.991731838505,-2134.0195788563969,1082.7862511327601,34909.225059562152,33857.991731838512,1.0000000000000002]
[4,"L-95-3+30-1","30T0036","L-95-3+30-1","1 Finger","on","N/A","3 turns","unsealed","unsealed",null,null,null,0,0,"CUST 4","3/23/2014","8:37:26","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 3","RTU4","RTU4","3","R22","PSC Air Handler","9.1 LBS","380/460/3","TU5","AHRI 210/240 2008",75,62,95,75,9.1,null,7,null,458.4,1.5,6.3,0,20278,84,19537,182,-1070,128,19208,130,6.0213166139999998,785,null,14.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1 Finger Open, +30% charge 95F Test, adjust code tester speed to match total static--of run L-1E3-SPWCT-SS (see row 33)","R22 9.1 LBS: OFB: Econo 1 Finger Open: Unsealed around damper perimeter: Unsealed cab:Inlet Meriam set @ 60%: Outlet @ 54% Horiz airflow. ID Pulley is 3 turns open from fully closed",75.001999999999995,4.2000000000000003E-2,61.994999999999997,3.6999999999999998E-2,95.001999999999995,1.0999999999999999E-2,75.009,0.02,74.48,0.13,60.1,0.06,65.53,0.02,7.5999999999999998E-2,5.0000000000000001E-3,1.1732,7.4000000000000003E-3,20278,84,-1070,128,6.0209999999999999,4.3999999999999997E-2,null,null,null,null,null,null,458.4,2.6,461.4,2.7,461.5,2.6,6.3,0,5.0999999999999996,0,5.6,0,2810.7,26.1,1502.4,29.8,379.3,19.8,460,null,460,null,460,null,1.2,null,1.5,null,1.3,null,0.4,460,null,460,null,460,null,4.0999999999999996,null,4.0999999999999996,null,3.5,null,2400,null,0.68,null,null,null,null,null,null,null,null,458.1,2.6,0.8,0,371.4,1.5,21,null,3202.4,480,480,480,0.9,0.9,1.1000000000000001,520,0.64,0.14149999999999999,18.399999999999999,null,null,null,null,220.75,0.24,95.78,0.04,null,null,null,null,226.1,0.19,169.97,0.1,109.88,0.06,60.09,0.13,null,null,91.89,0.06,108.19,0.08,12.41,7.0000000000000007E-2,null,null,null,null,null,null,null,null,75.430000000000007,0.27,65.2,0.28999999999999998,44.51,0.18,20.69,0.22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.61,7.0000000000000007E-2,60.14,0.08,60.18,0.09,60.15,7.0000000000000007E-2,60.05,7.0000000000000007E-2,59.48,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,91.77,0.04,null,null,94.56,0.22,95.24,0.68,94.32,0.22,94.44,0.18,93.08,0.36,93.11,0.36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.81,7.0000000000000007E-2,94.54,0.1,74.91,0.11,74.86,0.1,74.8,0.09,75.209999999999994,0.11,75.069999999999993,0.11,75.31,0.11,75,0.09,91.4,0.1,86.46,0.2,86.1,0.16,77.45,0.12,88.96,0.26,87.97,0.3,88.58,0.11,86.92,0.28000000000000003,90.91,0.09,89.77,0.15,87.75,0.18,89.04,0.24,88.5,0.3,89.08,0.16,89.34,0.19,83.63,0.26,89.31,0.24,89.05,0.15,89.82,0.17,83.65,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L-55-1ER-DM",75.001999999999995,4.2000000000000003E-2,61.994999999999997,3.6999999999999998E-2,60.078000000000003,2.5000000000000001E-2,56.829000000000001,3.2000000000000001E-2,95.001999999999995,1.0999999999999999E-2,75.009,0.02,1236.2,3.9,1216.0999999999999,3.9,0.66200000000000003,2E-3,-0.19900000000000001,2E-3,7.5999999999999998E-2,5.0000000000000001E-3,1.1732,7.4000000000000003E-3,29.657,3.0000000000000001E-3,3190,9,410,null,0.21418915535973576,251.45806839232978,13.03,0.18,0.79648899057238443,5630.0118488552098,94.578490897637778,275.03856748993331,1170.3747911348698,4459.6370577203397,9.8477222243932641E-3,29.80039318680064,59.281511009427618,14.100025200811363,13.174395008614754,1.3928188009863833E-2,38.165790816952537,8.7768560912097025E-3,27.605001414458986,9.0659345548127143E-3,24.279507030642002,79.190451966485753,65.023314315749673,24.085143585729032,32176.922973198169,26901.017636735058,2780,0.29487406262877169,31100.389362631806,25824.484026168695,9.749338358191789,0.21550284528887523,-5.7152496010716085,-19.908940957058135,53.812487448068602,32176.922973198169,18722.572784191078,1094.268497844336,12360.081691162737,32176.92297319815,0.99999999999999944]
[4,"L-95-3-10-1","30T0044","L-95-3+10-1","1 Finger","on","N/A",null,"unsealed","unsealed",null,null,null,null,null,"CUST 4","2014-03-22","4:27:17","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 1","RTU4","RTU4","3","R22","PSC Air Handler","4.2 LBS","380/460/3","TU5","AHRI 210/240 2008",75,62,95,75,7.7,null,7,null,458.7,1.3,6.2,0,19438,65,18759,141,-1437,127,17999,155,5.75415601,785,null,12.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1 Finger Open, -10% charge, 95F Test, adjust code tester speed to match total--static of run L-1E3-SPWCT-SS (see row 33)","R22 6.3 LBS: OFB: Econo open 1F: Unsealed around damper perimeter: Unsealed cab:Inlet Meriam set @ 60%: Outlet @ 54% Horiz airflow. ID Pulley is 3 turns open from fully closed",75.004000000000005,2.1999999999999999E-2,62.000999999999998,2.7E-2,94.995000000000005,1.7999999999999999E-2,75.004000000000005,2.5000000000000001E-2,74.569999999999993,0.09,60.42,0.05,65.8,0.02,3.4000000000000002E-2,5.0000000000000001E-3,1.1263000000000001,6.7999999999999996E-3,19438,65,-1437,127,5.7539999999999996,5.1999999999999998E-2,null,null,null,null,null,null,458.7,2.5,461.4,2.5,461.1,2.5,6.2,0,5,0,5.5,0,2789.7,25.2,1485.3,27.9,338.5,18.899999999999999,457,null,459,null,459,null,1.4,null,1.5,null,1.3,null,0.37,458,null,458,null,459,null,4.0999999999999996,null,4,null,3.4,null,2330,null,0.68,null,null,null,null,null,null,null,null,458.3,2.5,0.8,0,370.1,1.5,21,null,3121.1,491,490,491,0.8,0.8,1.1000000000000001,500,0.64,12.9,17.899999999999999,null,null,null,null,211.61,0.21,102.99,0.05,null,null,null,null,220.59,0.17,166.85,0.06,108.11,0.05,58.74,0.06,null,null,101.17,7.0000000000000007E-2,105.21,7.0000000000000007E-2,2.2200000000000002,0.05,null,null,null,null,null,null,null,null,76.27,0.08,65.34,0.1,44.99,0.05,20.350000000000001,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.82,0.06,60.51,0.05,60.57,0.06,60.45,0.05,60.4,0.05,59.71,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101.07,0.06,null,null,94.18,0.24,94.26,0.75,94.01,0.28999999999999998,94.31,0.22,93.49,0.32,93.52,0.32,null,null,null,null,null,null,null,null,98.06,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.14,0.08,94.8,0.1,75.14,0.08,75.02,7.0000000000000007E-2,74.849999999999994,7.0000000000000007E-2,75.52,0.09,75.37,0.09,75.55,0.08,75.150000000000006,0.06,91.45,0.15,86.14,0.33,85.95,0.25,77.36,0.13,88.55,0.47,86.99,0.43,88.08,0.17,86.7,0.4,90.57,0.13,89.56,0.14000000000000001,87.49,0.27,88.54,0.37,88.08,0.45,88.89,0.14000000000000001,89.39,0.19,84.93,0.31,89.34,0.23,89.08,0.14000000000000001,89.84,0.15,85.18,0.31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L-55-1ER-DM",75.004000000000005,2.1999999999999999E-2,62.000999999999998,2.7E-2,60.347000000000001,3.4000000000000002E-2,57.075000000000003,3.5000000000000003E-2,94.995000000000005,1.7999999999999999E-2,75.004000000000005,2.5000000000000001E-2,1215.2,3.7,1187.0999999999999,3.6,0.66200000000000003,1E-3,-0.17899999999999999,2E-3,3.4000000000000002E-2,5.0000000000000001E-3,1.1263000000000001,6.7999999999999996E-3,29.477,1E-3,3128,9,400,null,0.21418915535973576,251.45806839232978,13.03,0.18,0.7908071154108931,5531.2348471732394,92.323103811023614,260.84978891465113,1110.0128878553319,4421.221959317907,9.8128710627129381E-3,29.726841500885172,59.556192884589109,14.099824881419631,13.181866620120458,1.3925481216258178E-2,38.1610814535834,8.7803397138764751E-3,27.609301342778359,9.1494025809843865E-3,24.435945853338705,79.045789733277601,64.924885647154795,24.242939622417808,30332.749168657472,25872.368939237647,2728,0.30695087834704465,29282.647921964497,24822.267692544672,9.3614603331088553,0.21693713186269736,-5.4839018784673641,-19.489596848688493,54.156859812428415,30332.749168657472,17552.574465657104,1067.5627901912312,11712.611912809158,30332.749168657494,1.0000000000000007]
[4,"L-75629575-TE3","30T0022","L-75629575-TE3","closed","on","N/A","3 turns","sealed","unsealed",null,null,null,0,0,"CUST 4","3/21/2014","9:36:25","10 Ton","0:30:00","75/62 95/75","ENG 1","TECH 1","RTU4","RTU4","3","R22","PSC Air Handler","7 LBS","380/460/3","TU5","AHRI 210/240 2008",75,62,95,75,7,null,7,null,458.8,1.4,6.2,0,22551,109,21872,157,4282,79,26838,111,8.6157303370000005,787,null,10.199999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Factory charge, 3 turns, Econo Closed damper, tape around damper perimeter--frame gaps, 60% inlet 54% outlet Meriam, adust code tester speed to match--total static of run L-TE3-SPWCT-SS","R22 7 LBS: OFB: Econo Closed: sealed around damper perimeter: Unsealed cab:Inlet Meriam set @ 60%: Outlet @ 54% Horiz airflow. ID Pulley is 3 turns open from fully closed",74.945999999999998,3.4000000000000002E-2,61.997999999999998,0.02,95,8.0000000000000002E-3,74.997,2.9000000000000001E-2,74.540000000000006,0.11,57.2,0.05,64.48,0.17,1.7999999999999999E-2,7.0000000000000001E-3,1.0002,9.1000000000000004E-3,22551,109,4282,79,8.6170000000000009,4.1000000000000002E-2,null,null,null,null,null,null,458.8,2.5,461.7,2.5,461.3,2.5,6.2,0,5,0,5.5,0,2788.9,25.2,1489.9,28.6,325.8,19.399999999999999,460,null,460,null,460,null,1.3,null,1.4,null,1.3,null,0.35,460,null,460,null,460,null,4.0999999999999996,null,4,null,3.4,null,2350,null,0.68,null,null,null,null,null,null,null,null,458.4,2.5,0.8,0,367.6,1.4,21,null,3108.6,480,480,480,0.8,0.8,1,430,0.61,10.199999999999999,16.899999999999999,null,null,null,null,213.9,0.2,99.73,7.0000000000000007E-2,null,null,null,null,220.72,0.17,167.17,0.1,108.12,0.05,59.05,0.11,null,null,96.97,0.08,105.92,0.06,6.19,7.0000000000000007E-2,null,null,57.21,0.4,null,null,null,null,72.47,0.16,61.41,0.22,42.44,0.11,18.97,0.18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.46,0.06,58.04,7.0000000000000007E-2,56.98,0.06,58.08,0.06,56.73,0.05,57.25,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.85,0.06,null,null,95.88,0.09,95.8,0.09,95.81,0.1,95.67,0.1,95.61,0.11,95.64,0.1,null,null,null,null,null,null,null,null,93.1,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.64,7.0000000000000007E-2,94.64,0.1,74.86,0.1,74.86,0.08,74.790000000000006,7.0000000000000007E-2,74.97,0.11,74.98,0.11,74.98,0.1,74.900000000000006,7.0000000000000007E-2,86.48,0.06,88.62,0.08,82.61,0.09,77.03,0.06,80.88,0.09,83.83,0.13,84.08,0.09,76.81,0.08,82.23,0.05,81.03,7.0000000000000007E-2,81.05,0.1,76.16,7.0000000000000007E-2,77.010000000000005,0.08,79.790000000000006,0.08,81.41,7.0000000000000007E-2,75.2,7.0000000000000007E-2,80.69,0.09,78.67,7.0000000000000007E-2,80.239999999999995,0.06,76.8,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L-55-TCE-DM",74.945999999999998,3.4000000000000002E-2,61.997999999999998,0.02,57.069000000000003,2.4E-2,54.05,2.7E-2,95,8.0000000000000002E-3,74.997,2.9000000000000001E-2,1147,5.3,1116.9000000000001,5.0999999999999996,0.68899999999999995,2E-3,-0.25600000000000001,2E-3,1.7999999999999999E-2,7.0000000000000001E-3,1.0002,9.1000000000000004E-3,29.265000000000001,1E-3,3115,9,370,null,6.2074829931972782E-2,68.431292517006796,13.029,0.245,0.75611334234514271,5257.0037461377142,90.406283244094482,72.768600861870596,309.65600637950917,4947.3477397582046,9.0940096542824461E-3,28.229196723063815,56.312886657654857,14.099891369008994,13.091107277707687,1.3918148917546582E-2,38.154223522859034,8.7920653040852309E-3,27.607986263702735,8.1643701995079247E-3,22.565830786332487,76.137618952120292,62.874958733287819,22.381622688147228,30740.718607374125,25012.486065163706,2745,0.30476467123812218,29786.465252086218,24058.2327098758,9.5622681387114667,0.21687444907591896,-5.8475740349165868,-19.824732294465434,50.822735187859976,30740.718607374125,26506.630233144184,968.3826622288102,3265.7057120011204,30740.718607374114,0.99999999999999967]
[4,"L-22C-L22D Cyclic #4","30T0027","L-22C/L22D Cyclic #4","none","on","N/A",null,"unsealed","unsealed",null,null,null,0,0,"CUST 4","3/20/2014","17:56:18","10 Ton","","80/57 82","ENG 1","TECH 1","RTU4","RTU4","3","R22","PSC Air Handler","7 LBS","380/460/3","","",80,57,82,null,7,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11.984999999999999,null,null,null,4,6.0330000000000004,81.888999999999996,30.016999999999999,62.539000000000001,0.36,434.3,1200.0999999999999,13.461,32699.942999999999,0.24199999999999999,2960.5239999999999,4.47E-3,22.540692856,149.989,11.99,135.988,266.7,10.622999999999999,12,14.03,0,0,0.18099999999999999,278.69,0.13900000000000001,272.5,272.45999999999998,13.054914999999999,272.45999999999998,0.98,null,"","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",79.66,null,53.996000000000002,null,56.518999999999998,null,46.204000000000001,null,null,null,null,null,1219.5,null,1184.5999999999999,null,0.39500000000000002,null,null,null,-0.23799999999999999,null,0.72319999999999995,null,29.358000000000001,null,2709,null,-0.1,null,null,0,null,null,{"$f":"(BO160-XU160)*3.412/XT160/0.24","v":0.96153262525546224},5608.5392101543684,54.971036535433072,0,0,5608.5392101543684,2.8541993133961632E-3,22.24765576119681,55.557467374744533,11.593798628049566,13.046177847437404,7.8407761683729174E-4,0.83190635146436653,2.8541993133961636E-3,22.24765576119681,4.1967375372828795E-3,18.122613288595279,79.66,53.996001489972173,17.890053785306556,24439.781544026646,32443.199830264839,{"$f":"XK160-BO160","v":2274.6999999999998},0.31766041304479242,{"$f":"YM160-(BO160-XU160)*3.413","v":23145.13179172208},{"$f":"YN160-(BO160-XU160)*3.413","v":31148.550077960273},8.5437917282104401,0.40407476326011937,-4.3576019758902547,-24.102532625255463,39.214435457184472,24439.781544026646,23135.462451137817,1304.3190928888262,0,24439.781544026642,0.99999999999999989]
[3,"3-21A AHRI Verification H","75N0007","3-21A AHRI Verification H","none","on","on","6 turns","sealed","sealed",null,10,"horizontal",0,0,"CUST 10","9/19/2013","19:19:57","10 Ton","0:30:00","80/67 95","ENG 1","TECH 4","RTU3","RTU3","7.5","R22","PSC Air Handler","ck1: 8.0 lbs / ck2: 8.5 lbs","230/208/3","TU2","AHRI 340-360",80,67,95,null,8,8.5,7.6,8.1,232.1,0.2,27.3,0,59613,75,60499,363,26631,80,86269,122,10.470809564,null,null,null,null,110.73,0.12,0.45,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,".","New R22 CK 1 : 8.0 lbs / Ck 2 : 8 lbs 8 oz: Sealed the unit and ductwork: 10` blower pulley with A55 belt @ 0.25 SP: motor pulley 6 turns opened from closed: No econo Meriam set to 100%: Horizontal airflow disch config. set on floor",79.698999999999998,1.4E-2,67.248999999999995,1.7000000000000001E-2,94.543000000000006,1.9E-2,70.768000000000001,6.0000000000000001E-3,79.7,0.14000000000000001,59.16,0.03,64.069999999999993,0.03,-0.66300000000000003,2E-3,0.94789999999999996,2.0999999999999999E-3,59613,75,26631,80,10.471,2.8000000000000001E-2,86658,96,10.516999999999999,2.5999999999999999E-2,0.45,0.18,232.1,0.4,231.4,0.4,231.6,0.4,27.3,0.1,24.9,0.1,28.2,0.1,6306,22.8,3777.2,26.6,1933.2,19.899999999999999,230,null,229,null,228,null,5.5,null,5.4,null,5.4,null,0.35,228,null,229,null,229,null,11.1,null,10.6,null,10.1,null,3450,null,0.81,229,229,229,10.7,9.8000000000000007,10.4,3370,0.87,null,null,null,null,null,null,null,null,8280,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,275.94,0.16,184.78,0.09,124.35,0.04,-60.42,0.1,256.12,0.16,101.18,0.05,118.81,0.05,17.63,0.04,null,null,null,null,null,null,null,null,78.290000000000006,0.05,56.96,0.67,46.21,0.03,10.75,0.67,666.18,0.37,39.85,0.02,86658,96,47221,88,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,264.98,0.25,203.51,0.06,121.32,7.0000000000000007E-2,82.19,7.0000000000000007E-2,null,null,null,null,null,null,252.93,0.24,102.33,0.04,117.89,7.0000000000000007E-2,15.56,0.06,null,null,null,null,null,null,69.59,0.06,76.27,0.05,40.47,0.04,35.799999999999997,7.0000000000000007E-2,101.63,0.06,570,0.51,40.21,0.01,114.67,0.01,86658,96,42440,36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.73,0.05,58.95,0.04,59.36,0.05,59.46,0.04,59.5,0.04,59.6,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101.18,0.05,null,null,null,null,null,null,null,null,null,null,null,null,102.13,0.04,101.5,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101.4,0.05,101.63,0.06,null,null,null,null,62.6,0.46,76.19,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,93.95,0.06,94.83,0.12,80.03,0.08,80.180000000000007,0.08,79.84,0.08,79.92,0.1,79.989999999999995,0.1,80.03,0.09,null,null,80.33,0.1,80.349999999999994,0.09,80.48,0.08,80.569999999999993,0.09,null,null,80.290000000000006,0.12,80.290000000000006,0.11,80.38,0.11,80.72,0.08,80.760000000000005,7.0000000000000007E-2,80.599999999999994,0.1,80.66,0.09,80.900000000000006,7.0000000000000007E-2,80.91,0.09,80.89,0.08,80.53,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,88.71,0.13,88.5,0.13,84.35,0.13,83.83,0.16,84.34,0.08,83.65,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",79.698999999999998,1.4E-2,67.248999999999995,1.7000000000000001E-2,59.469000000000001,2.1999999999999999E-2,57.076999999999998,1.9E-2,94.543000000000006,1.9E-2,70.768000000000001,6.0000000000000001E-3,2619.1999999999998,3,2539.5,2.8,0.25,2E-3,-0.29099999999999998,2E-3,-0.66300000000000003,2E-3,0.94789999999999996,2.0999999999999999E-3,29.224,1E-3,8239,19,850,null,null,0,null,null,0.9232276913162607,11940.512843506911,74.585314960629916,0,0,11940.512843506911,1.1331635129302265E-2,31.551610146937293,58.545772308683738,14.059946289541063,13.161243747202795,1.0500187453997393E-2,34.271786223464929,1.1331635129302265E-2,31.551610146937296,9.3585817262358002E-3,24.449121412061,79.698999999999984,67.249007838174876,24.223710560945406,87498.879122465092,60619.292863149043,7389,0.28821691492417278,84852.388802425718,57972.802543109676,10.298869863141851,0.17435898022683036,-7.3278995859918865,-21.153227691316246,54.078630875016678,87498.879122465092,84807.357959653556,2691.5211628115758,0,87498.879122465136,1.0000000000000004]
[3,"Run 1-1A Out of the Box Baseline","75N0034","Run 1-1A Out of the Box Baseline","none","on","off",null,"unsealed","unsealed",null,7,null,0,0,"CUST 9","3/1/2013","16:45:04","10 Ton","0:30:00","80/67 95","ENG 2","TECH 2","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. ck1: 7.6 lbs/ck2: 8.1 lbs","208/230/3","TU2","Ashrae 340/360",80,67,95,null,7.6,8.1,7.6,8.1,229.9,0,19.7,0,20485,39,20759,198,13757,66,34255,83,6.0270000000000001,null,null,null,null,114.04,0.01,7.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,".","Manuf. charge R-22: 3000 scfm at .8 ESP (per client): unsealed tape on unit`s base and doors: After two Brun In`s; The blower wheel is a 7` with A49 Belt. manuf mtr pully. New 2 compr/filters. The unit operated with Compressor 1 on and Compressor 2 off.",79.849000000000004,8.0000000000000002E-3,67.150999999999996,1.0999999999999999E-2,94.864999999999995,7.0000000000000001E-3,69.108000000000004,4.2000000000000003E-2,79.540000000000006,0.09,73.459999999999994,7.0000000000000007E-2,74.69,0.01,-0.46800000000000003,5.0000000000000001E-3,1.3361000000000001,2.8E-3,20485,39,13757,66,6.0270000000000001,3.1E-2,36951,31,6.5010000000000003,0.03,7.3,0.23,229.9,0.7,230.1,0.7,230.2,0.7,19.7,0.1,17.100000000000001,0.1,17,0.1,4474.2,24,2049.8000000000002,25.7,1209.7,20,229.7,null,230,null,229.4,null,6.5,null,6.7,null,6.6,null,0.56999999999999995,228.3,null,229.1,null,228.1,null,10.6,null,10.4,null,10.7,null,3280,null,2283,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,257.3,0.16,204.22,0.05,119.19,0.05,85.03,0.06,247.24,0.12,100.11,0.03,116.27,0.04,16.16,0.04,null,null,null,null,null,null,null,null,71.39,0.04,73.319999999999993,0.03,41.79,0.03,31.52,0.05,575.45000000000005,0.4,39.51,0.01,36951,31,42890,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.069999999999993,0.05,72.86,7.0000000000000007E-2,72.650000000000006,7.0000000000000007E-2,73.53,7.0000000000000007E-2,81.38,0.06,73.53,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,99.77,0.05,99.82,2.54,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98.74,7.0000000000000007E-2,106.13,0.09,null,null,null,null,null,null,null,null,null,null,null,null,74.459999999999994,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.01,0.08,95.29,0.1,81.63,0.09,81.23,0.06,81.209999999999994,0.06,81.099999999999994,0.05,81.05,0.06,81.87,7.0000000000000007E-2,null,null,82.46,0.06,81.819999999999993,0.05,81.95,0.05,81.92,0.06,81.239999999999995,0.06,81.819999999999993,0.05,81.03,0.06,81.25,0.06,80.8,0.06,81.11,0.06,80.91,0.06,80.94,0.05,80.63,0.06,80.8,0.05,80.47,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",79.849000000000004,8.0000000000000002E-3,67.150999999999996,1.0999999999999999E-2,73.846000000000004,0.01,63.914999999999999,1.4E-2,94.864999999999995,7.0000000000000001E-3,69.108000000000004,4.2000000000000003E-2,3128.3,3.3,3000.1,3.1,0.877,3.0000000000000001E-3,-0.38700000000000001,2E-3,-0.46800000000000003,5.0000000000000001E-3,1.3361000000000001,2.8E-3,29.521999999999998,1E-3,5684,26,1720,null,null,0,null,null,1.4462669165552353,13869.003285359302,309.1010116850394,0,0,13869.003285359302,1.1223565850542778E-2,31.469871953688283,72.399733083444772,14.056719927141582,13.533632961075281,9.1325586465023784E-3,32.841908642083219,1.1223565850542778E-2,31.469871953688283,1.0344470389940224E-2,29.03769368935107,79.849000000000004,67.151009180980395,28.683947005187168,38638.002263526418,24795.337761413488,3964,0.35015091897676237,33822.604016407458,19979.939514294529,5.9504933174538106,0.7500394136858981,-2.7859249485011155,-7.4492669165552314,50.047233943992921,38638.002263526418,33731.888338672303,4906.1139248541112,0,38638.002263526418,1]
[3,"Run 1-2B Out of the Box Baseline","75N0045","Run 1-2B Out the Box Baseline","none","on","on",null,"unsealed","unsealed",null,7,null,0,0,"CUST 9","3/1/2013","9:41:25","10 Ton","0:30:00","80/67 82","ENG 2","TECH 2","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. ck1: 7.6 lbs/ck2: 8.1 lbs","208/230/3","TU2","Ashrae 340/360",80,67,82,null,7.6,8.1,7.6,8.1,229.8,0,27.5,0,52707,58,52227,144,24104,75,76834,108,9.7929999999999993,null,null,null,null,114.35,0.01,1.71,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no doors external tape","Manuf. charge R-22: 3000 scfm at .8 ESP (per client): unsealed tape on unit`s base and doors: After two Brun In`s; The blower wheel is a 7` with A49 Belt. manuf mtr pully. New 2 compr/filters",79.849999999999994,6.0000000000000001E-3,67.150999999999996,0.01,81.995000000000005,1.6E-2,64.540000000000006,0.01,79.38,0.05,64.05,0.04,67.22,0.02,-0.438,3.0000000000000001E-3,1.3187,2.5999999999999999E-3,52707,58,24104,75,9.7929999999999993,4.1000000000000002E-2,78172,95,9.9629999999999992,3.9E-2,1.71,0.19,229.8,0.7,229.9,0.7,230.2,0.7,27.5,0.1,24.6,0.1,24.8,0.1,6227.9,34.1,3308.2,43.1,1617.4,28.1,229,null,228,null,228,null,6.5,null,6.7,null,6.5,null,0.57999999999999996,229,null,230,null,230,null,9.3000000000000007,null,9.3000000000000007,null,8.6999999999999993,null,2750,null,0.76,228,229,229,9.4,9.5,8.4,2710,0.77,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,212.82,0.19,187.67,0.05,105.63,0.06,82.04,0.06,203.29,0.16,86.96,0.04,102.47,0.05,15.51,0.05,65.34,0.05,73.31,0.03,null,null,null,null,null,null,null,null,null,null,null,null,538.67999999999995,0.89,35.44,0.01,78172,95,42511,71,null,null,null,null,null,null,null,null,null,null,null,null,null,null,37.65,0.03,35.659999999999997,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,210.28,0.26,191.08,0.06,104.8,0.09,86.28,7.0000000000000007E-2,null,null,null,null,null,null,203.7,0.2,85.93,0.06,102.61,7.0000000000000007E-2,16.68,7.0000000000000007E-2,null,null,null,null,null,null,60.36,0.06,77.099999999999994,0.04,34.020000000000003,0.05,43.07,0.06,86.39,0.06,493.35,0.94,35.119999999999997,0.02,115.15,0.01,78172,95,39483,76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.62,0.04,64.23,0.04,63.94,0.05,63.6,0.04,64,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,86.63,0.06,85.5,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85.52,0.06,86.39,0.06,null,null,null,null,null,null,null,null,null,null,null,null,74.03,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80.64,0.08,81.819999999999993,0.12,80.58,0.54,80.36,0.05,80.25,0.05,80.23,0.04,80,0.04,80.38,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",79.849999999999994,6.0000000000000001E-3,67.150999999999996,0.01,64.376000000000005,8.0000000000000002E-3,59.502000000000002,0.01,81.995000000000005,1.6E-2,64.540000000000006,0.01,3081,3,3009.3,2.9,0.89700000000000002,3.0000000000000001E-3,-0.39100000000000001,2E-3,-0.438,3.0000000000000001E-3,1.3187,2.5999999999999999E-3,29.609000000000002,1E-3,7845,29,1740,null,null,0,null,null,1.4540864739571835,13911.563915181798,317.11956009448824,0,0,13911.563915181798,1.1223327841515265E-2,31.469855971144071,62.921913526042822,13.728151608444779,13.288225617700743,8.8466137097981141E-3,29.387125018559694,1.1223327841515265E-2,31.469855971144071,9.6859631316233465E-3,26.003900224429625,79.849999999999994,67.151009186905512,25.648666073458141,80981.855324068398,56519.077666603116,6105,0.25729671068436583,76125.564382670884,51662.786725205602,9.7037048288936756,0.3497630956679123,-5.8211898976859295,-16.928086473957173,53.816278503762533,80981.855324068398,76039.992727973266,4941.862596095134,0,80981.855324068398,1]
[3,"C8-55-3FE3","75N0142","C8-55-3FE3","3 finger","off","off","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 3","6/25/2015","8:03:29","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/3","TU2","AHRI 340-360",75,62,55,51,5.5,null,7.6,8.1,229.7,1.6,6.5,0,14709,57,14141,47,7746,83,22462,93,14.069000000000001,898,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 3-Finger open, unsealed cabinet, Inlet static location inside Cabinet,--no compressor 55F OD ambient, factory charge (CK1 7.6 lbs, CK2 8.1 lbs) 75F DB,--62F WB ID conditions, duct removed from supply sampling box (without code tester),--record total","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch.",75.03,0.02,62.014000000000003,1.4E-2,54.976999999999997,1.7999999999999999E-2,50.997,1.7000000000000001E-2,74.42,0.06,69.540000000000006,0.06,71.02,0.02,0.11899999999999999,6.0000000000000001E-3,0.93899999999999995,3.0000000000000001E-3,14709,57,7746,83,14.069000000000001,0.107,null,null,null,null,null,null,229.7,1.2,230.1,1.2,230.3,1.2,6.5,0.1,6.3,0,6.6,0.1,1391.2,14.5,1140.8,20.8,205.6,10.7,230,null,230,null,230,null,6.5,null,6.2,null,6.3,null,0.63,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,0,null,0,null,15,null,1595,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,93.17,0.04,55.44,0.02,55.18,0.02,-0.26,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,93.57,0.04,55.58,0.01,55.41,0.02,0.17,0.03,null,null,null,null,null,null,null,null,93.57,0.04,55.06,0.05,55.41,0.02,0.35,0.05,93.03,0.04,55.1,0.02,-0.09,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,93.89,0.04,55.64,0.02,55.59,0.02,0.05,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,93.64,0.03,55.03,0.02,55.45,0.02,-0.41,0.03,null,null,null,null,null,null,null,null,null,null,null,null,95.52,0.04,55.07,0.02,56.51,0.02,1.43,0.03,94.33,0.03,55.84,0.02,-0.78,0.02,null,null,null,null,null,null,null,null,null,null,null,null,70.819999999999993,0.04,68.91,0.04,68.67,0.04,69.77,0.04,68.790000000000006,0.05,null,null,55.09,0.03,null,null,55.59,0.02,56.11,0.02,56.08,0.04,null,null,55.48,0.03,55.57,0.04,55.75,0.03,null,null,55.58,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.78,0.04,null,null,null,null,null,null,null,null,55.06,0.02,55.01,0.02,null,null,null,null,null,null,null,null,55.58,0.03,55.56,0.03,55.68,0.05,55.28,0.02,null,null,null,null,null,null,null,null,null,null,56.09,0.04,55.2,0.13,54.61,0.18,75,0.05,74.97,0.04,75.010000000000005,7.0000000000000007E-2,75.08,7.0000000000000007E-2,75.08,0.06,75.08,0.05,null,null,61.78,0.09,62.23,0.09,74.92,0.04,72.42,0.17,74.989999999999995,0.05,60.19,0.12,64.75,0.16,60.91,0.13,74.3,0.09,61.7,0.1,62.39,0.1,63.65,0.08,74.62,0.05,60.91,0.1,63.06,0.19,62.55,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.8,0.12,null,null,null,null,null,null,null,null,70.150000000000006,0.03,70.66,0.03,"Economizer test",75.03,0.02,62.014000000000003,1.4E-2,69.95,1.9E-2,59.247,1.2999999999999999E-2,54.976999999999997,1.7999999999999999E-2,50.997,1.7000000000000001E-2,2614.1999999999998,4.2,2522.5,4.0999999999999996,1.115,2E-3,-0.27400000000000002,2E-3,0.11899999999999999,6.0000000000000001E-3,0.93899999999999995,3.0000000000000001E-3,29.359000000000002,0,1597,11,1580,null,0.17752954670124158,447.81828155388189,13.029,0.27400000000000002,1.5196768347148433,11689.860514025695,330.42366535433069,447.81740749610844,2062.2572213371459,9627.6032926885491,8.4656452046668624E-3,26.411264583737712,68.430323165285159,13.028949139693108,13.417782001060344,6.9851543518201767E-3,20.776234904156414,8.7827701276189038E-3,27.618302337151466,8.2077641211532413E-3,25.751352829065542,71.50190618357513,60.238086352335387,25.381092310578104]
[3,"3-42115CF","75N0012","3-42115CF","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 10","10/8/2013","13:51:45","10 Ton","0:30:00","75/62 115/80","ENG 1","TECH 4","RTU3","RTU3","7.5","R22","PSC Air Handler","ck1: 7.6 lbs / ck2: 8.1 lbs","230/208/3","TU2","AHRI 340-360",75,62,115,80,7.6,8.1,7.6,8.1,230.3,0.2,33.299999999999997,0,46821,76,45937,176,-767,80,46053,103,4.2661417320000004,null,null,null,null,109.45,0.01,40.97,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100% airflow, both stages, closed damper","New R22 CK 1 : 7.6 lbs /Ck 2 : 8.1 lbs: No tape: Sealed ductwork: 7` blower pulley with A49 belt : motor pulley 4.5 turns opened from closed: With econo Meriam set @ 100%: Horiz airflow disch config. set on floor:",75.003,1.2E-2,62,1.0999999999999999E-2,115.02500000000001,1.6E-2,80.012,0.03,74.53,0.06,60.74,0.04,63.99,0.01,-0.26900000000000002,6.0000000000000001E-3,1.7218,4.4999999999999997E-3,46821,76,-767,80,4.266,1.6E-2,78024,58,7.2279999999999998,2.1000000000000001E-2,40.97,0.13,230.3,0.8,230,0.8,229.6,0.8,33.299999999999997,0.1,30,0.1,33.5,0.1,7660.9,33.1,3723.1,39.4,3134,29.3,230,null,230,null,230,null,6.7,null,6.5,null,6.4,null,0.56999999999999995,230,null,230,null,230,null,13.3,null,12.4,null,12.1,null,4290,null,0.86,230,230,230,12.8,11.6,12.3,4200,0.87,null,null,null,null,null,null,null,null,10800,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,343.75,0.21,190.24,0.06,141.44,0.05,48.8,0.06,324.85000000000002,0.22,123.76,7.0000000000000007E-2,136.94,0.05,13.18,0.04,null,null,null,null,null,null,null,null,79.680000000000007,0.04,50.43,0.04,47.13,0.02,3.3,0.03,693.21,0.42,47.17,0.02,78024,58,43166,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,333,0.31,235.2,0.05,138.9,7.0000000000000007E-2,96.3,0.05,null,null,null,null,null,null,321.39999999999998,0.3,123.84,0.06,136.1,7.0000000000000007E-2,12.26,0.06,null,null,null,null,null,null,74.94,0.03,82.37,0.03,44.1,0.02,38.270000000000003,0.04,123.66,0.08,578.03,0.53,47.2,0.02,115.48,0.01,78024,58,39466,39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.12,0.06,60.4,0.05,61.2,0.05,61.03,0.08,60.95,0.08,61.04,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,123.76,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,125.6,0.06,124.31,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,123.94,7.0000000000000007E-2,123.66,0.08,125.6,0.06,124.31,7.0000000000000007E-2,52.39,0.03,82.37,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.53,0.11,114.9,0.1,74.599999999999994,0.05,74.64,0.04,74.510000000000005,0.05,74.5,0.05,74.62,0.05,74.64,0.05,null,null,76.42,0.08,75.41,0.08,75.34,0.08,75.78,0.08,95.26,0.54,87.23,0.17,75.52,0.08,75.48,0.08,92.1,0.51,81.56,0.14000000000000001,79.569999999999993,0.15,78.430000000000007,0.16,84.18,0.14000000000000001,81.010000000000005,0.12,83.1,0.12,77.900000000000006,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.51,0.11,115.24,0.11,115.19,0.1,115.34,0.1,115.15,0.1,114.99,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C8-55-CE3",75.003,1.2E-2,62,1.0999999999999999E-2,60.948999999999998,7.0000000000000001E-3,56.997,8.0000000000000002E-3,115.02500000000001,1.6E-2,80.012,0.03,3071.5,4,3000,3.9,0.92400000000000004,3.0000000000000001E-3,-0.312,2E-3,-0.26900000000000002,6.0000000000000001E-3,1.7218,4.4999999999999997E-3,29.385000000000002,1E-3,10795,31,1700,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.3990145733272126,13965.972167615162,325.65543307086614,20.04270793820562,82.323941016893841,13883.648226598269,8.8093477802093038E-3,27.69886302211323,59.549985426672784,14.607688376405076,13.195644226424767,1.3772817081489641E-2,42.922351841910974,8.7799165855169062E-3,27.608594414380043,8.9601788865467345E-3,24.37698438929861,75.241045552534956,62.129767761057707,24.035655164846276,51160.258978779457,52593.81815956012,9095,0.60674507165562741,46469.620971850323,47903.180152630986,4.3047356157341659,0.25077745242352706,-3.6632078572669542,-15.691060125862172,54.297922342190581,51160.258978779457,45132.575666873439,4766.9944486949662,1260.6888632110763,51160.258978779486,1.0000000000000007]
[3,"3-21151","75N0020","3-21151","1 finger","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 10","9/25/2013","0:41:27","10 Ton","0:30:00","76/62  115/80","ENG 1","TECH 4","RTU3","RTU3","7.5","R22","PSC Air Handler","ck1: 7.6 lbs / ck2: 8.1 lbs","230/208/3","TU2","AHRI 340-360",76,62,115,80,7.6,8.1,7.6,8.1,230.3,0.2,32.700000000000003,0,36202,49,36612,137,-4537,134,31660,145,2.9825718320000001,null,null,null,null,109.48,0.01,59.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"83.3% Airflow Both Stages 1 Finger (0.74\")","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1 lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: With econo Meriam set to 75%: Horiz airflow disch config. set on floor: VFD 25.02%",75.003,0.01,62.000999999999998,2.4E-2,114.995,2.1999999999999999E-2,80.022000000000006,2.1999999999999999E-2,74.790000000000006,0.05,61.6,0.02,65.23,0.01,9.1999999999999998E-2,2E-3,0.92259999999999998,1.9E-3,36202,49,-4537,134,2.9830000000000001,1.7000000000000001E-2,77825,75,7.3319999999999999,2.1999999999999999E-2,59.32,0.19,230.3,0.8,229.7,0.8,229.7,0.8,32.700000000000003,0.1,29.9,0.1,33.1,0.1,7528,37.200000000000003,3783.3,41.7,3087.2,31.9,230,null,228,null,229,null,6.4,null,6.2,null,6.2,null,0.53,229,null,229,null,229,null,13.3,null,12.5,null,12.1,null,4310,null,0.86,230,228,228,12.7,11.6,12.2,4180,0.87,null,null,null,null,null,null,null,null,10620,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,346.54,0.37,197.09,0.06,142.07,0.09,55.02,0.09,327.49,0.35,124.07,0.09,137.56,0.09,13.5,0.04,null,null,null,null,null,null,null,null,81.33,0.05,51.15,0.03,48.12,0.03,3.03,0.02,697.84,0.67,47.28,0.03,77825,75,43405,41,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330.66,0.39,235.48,0.06,138.32,0.09,97.16,0.06,null,null,null,null,null,null,318.51,0.38,124.79,0.06,135.37,0.1,10.58,7.0000000000000007E-2,null,null,null,null,null,null,75.72,0.08,84.51,0.03,44.56,0.05,39.950000000000003,0.05,124.6,0.1,581.39,0.6,47.52,0.02,115.82,0.01,77825,75,39710,42,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.12,0.03,61.73,0.02,62.19,0.03,61.72,0.03,61.71,0.02,61.82,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,124.07,0.09,null,null,null,null,null,null,null,null,null,null,null,null,124.9,0.08,124.68,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,124.19,0.09,124.6,0.1,null,null,null,null,53.88,7.0000000000000007E-2,84.49,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,114.93,0.12,115.63,0.11,75.239999999999995,0.04,75.55,0.04,75.28,0.05,74.83,0.04,74.989999999999995,0.04,75.08,0.04,null,null,77.98,0.12,75.98,0.05,75.650000000000006,0.05,75.72,0.05,91.46,0.12,80.86,0.18,76.08,7.0000000000000007E-2,75.91,0.06,94.49,0.18,91.2,0.11,90.05,0.16,90.58,0.16,90.88,0.11,89.67,0.13,89.5,0.12,90.01,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.03,0.2,114.56,0.19,114.85,0.18,114.93,0.13,115.18,0.14000000000000001,115.24,0.21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C8-55-1FE3",75.003,0.01,62.000999999999998,2.4E-2,61.959000000000003,1.0999999999999999E-2,57.942999999999998,1.6E-2,114.995,2.1999999999999999E-2,80.022000000000006,2.1999999999999999E-2,2584.5,2.7,2504.5,2.6,1.153,2E-3,-0.436,3.0000000000000001E-3,9.1999999999999998E-2,2E-3,0.92259999999999998,1.9E-3,29.215,1E-3,10615,32,1520,null,9.1282153938544691E-2,224.4628165348814,13.029,0.35299999999999998,1.4314864071486413,11726.536882593346,339.24655448818902,264.13522631872331,1084.9617855052763,10641.575097088069,9.2440329756505249E-3,29.027165066137837,60.527513592851363,14.607070765854479,13.223853005586248,1.3789734474426189E-2,42.933781506419855,8.780575980845761E-3,27.609315991566721,9.2926348165483109E-3,24.9852840284635,78.733730179283739,63.999412223047429,24.635821078238468,51495.25723825649,51239.008870387668,9095,0.60279794033030021,47465.345728724678,47209.097360855856,4.4715351605016185,0.22750073074591609,-4.3913439878993685,-18.206216586432376,55.165789973965381,51495.25723825649,30770.80759643374,4097.9901749137198,16626.459466909091,51495.257238256556,1.0000000000000013]
[3,"3-52951CF","75N0030","3-52951CF","1 finger","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 10","10/8/2013","4:17:37","10 Ton","0:30:00","75/62  95/75","ENG 1","TECH 4","RTU3","RTU3","7.5","R22","PSC Air Handler","ck1: 7.6 lbs / ck2: 8.1 lbs","230/208/3","TU2","AHRI 340-360",75,62,95,75,7.6,8.1,7.6,8.1,230.5,0.1,28.8,0,45941,72,45093,204,5047,105,50993,125,5.8317703569999999,null,null,null,null,109.7,0.03,35.159999999999997,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"83.3% Airflow, Both Stages, 1 Finger opened (0.74\")","New R22 CK 1 : 7.6 lbs /Ck 2 : 8.1 lbs: No tape: Sealed ductwork: 7` blower pulley with A49 belt : motor pulley 4.5 turns opened from closed: With econo Meriam set @ 75%: Horiz airflow disch config. set on floor:",75.006,2.3E-2,62.003999999999998,2.3E-2,95,0.02,75.046000000000006,2.3E-2,74.37,0.09,58.21,0.05,62.61,0.02,0.28299999999999997,4.0000000000000001E-3,1.1907000000000001,2.8999999999999998E-3,45941,72,5047,105,5.8310000000000004,2.5999999999999999E-2,78647,65,8.9939999999999998,3.3000000000000002E-2,35.159999999999997,0.15,230.5,0.8,230.3,0.8,229.5,0.8,28.8,0.1,25.4,0.1,28.8,0.1,6600.6,36.1,3529.5,43,2143.8000000000002,30,230,null,231,null,230,null,6.3,null,6.3,null,6.2,null,0.52,231,null,230,null,230,null,11.2,null,10.4,null,10,null,3400,null,0.81,229,228,229,10.6,9.6,10,3220,0.81,null,null,null,null,null,null,null,null,8750,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,269.77999999999997,0.19,180.63,7.0000000000000007E-2,122.69,0.05,57.94,0.06,250.7,0.19,101.98,0.06,117.27,0.06,15.29,0.05,null,null,null,null,null,null,null,null,74.760000000000005,0.04,50.13,0.19,44,0.03,6.13,0.19,642.9,0.44,40.1,0.02,78647,65,44744,43,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,253.92,0.21,207.31,0.05,118.21,0.06,89.11,0.04,null,null,null,null,null,null,243.07,0.21,102.43,0.05,115.03,0.06,12.59,0.05,null,null,null,null,null,null,63.39,0.04,77.5,0.04,36.19,0.03,41.31,0.05,101.67,0.08,521.6,0.46,40.24,0.02,115.19,0.01,78647,65,39089,34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.13,0.05,58.23,0.04,58.58,0.04,58.46,0.06,58.42,0.06,58.56,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101.98,0.06,null,null,null,null,null,null,null,null,null,null,null,null,103.79,0.06,102.29,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102.19,0.08,101.67,0.08,103.79,0.06,102.29,7.0000000000000007E-2,52.45,0.34,77.52,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.86,0.1,94.55,0.08,74.48,0.06,74.61,0.06,74.34,0.08,74.37,0.06,74.52,0.06,74.540000000000006,0.06,null,null,75.86,0.15,74.930000000000007,0.15,74.959999999999994,0.13,74.959999999999994,0.1,87.51,0.26,77.58,0.21,78.94,0.23,75.78,0.16,81.680000000000007,0.47,81.33,0.11,83.8,0.14000000000000001,84.48,0.14000000000000001,81.260000000000005,0.09,81.09,0.09,82.81,0.09,82.44,0.31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.93,0.11,94.6,0.11,94.61,0.11,94.73,0.11,94.57,0.1,94.56,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C8-55-1FE3",75.006,2.3E-2,62.003999999999998,2.3E-2,58.537999999999997,1.9E-2,55.265999999999998,1.7000000000000001E-2,95,0.02,75.046000000000006,2.3E-2,2544.3000000000002,3.1,2499.9,3.1,1.2130000000000001,2E-3,-0.33300000000000002,2E-3,0.28299999999999997,4.0000000000000001E-3,1.1907000000000001,2.8999999999999998E-3,29.419,1E-3,8744,32,1520,null,9.1282153938544691E-2,224.4628165348814,13.029,0.35299999999999998,1.4231114831499472,11625.736906968397,356.24480475590559,226.79683184233829,965.0760257115727,10660.660881256825,9.2117872379571634E-3,28.490549828564557,57.114888516850051,14.10024655882105,13.131038593217925,1.3961116292083544E-2,38.201624271100727,8.7818454492251657E-3,27.611436869923374,8.512110653426155E-3,23.301706581728183,76.68008110831569,63.239917315640106,22.954781350779168,64357.387900621863,54590.347584611212,7224,0.38310305629669228,60385.491419253769,50618.451103243118,6.9059345172980064,0.19998536150868024,-5.5357684777853891,-19.565192591465639,52.224037868454495,64357.387900621863,50103.790470550375,4033.2614614025006,10220.335968669009,64357.387900621885,1.0000000000000004]
[3,"3-3000-95 Rerun","75N0054","3-3000-95","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 10","10/11/2013","5:35:26","10 Ton","0:30:00","75/62 - 95/75","ENG 1","TECH 4","RTU3","RTU3","7.5","R22","PSC Air Handler","ck1: 7.6 lbs / ck2: 8.1 lbs","230/208/3","TU2","AHRI 340-360",75,62,95,75,7.6,8.1,7.6,8.1,230.6,0.9,28.1,0,34656,62,34119,114,142,107,34798,123,4.1264081580000003,null,null,null,null,116.11,0.02,20.260000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lg rstrct CK1, 3000 cfm, clsd dmpr, 75/62 ID, 95/75 OD","New R22 CK 1 : 7.6 lbs /Ck 2 : 8.1 lbs: Unsealed cabinet/Economizer: Sealed ductwork: 7` blower pulley with A49 belt : motor pulley 4.5 turns opened from closed: No econo Meriam set @ 75%: Horiz airflow disch config. set on floor.",75.004000000000005,5.0000000000000001E-3,61.997999999999998,2.1999999999999999E-2,94.998999999999995,1.4E-2,75,2.5000000000000001E-2,74.459999999999994,0.04,64.23,0.03,67.06,0.02,-0.49299999999999999,6.0000000000000001E-3,1.3248,3.5000000000000001E-3,34656,62,142,107,4.1269999999999998,2.1000000000000001E-2,43640,124,5.1749999999999998,2.3E-2,20.260000000000002,0.35,230.6,0.8,230.5,0.8,229.4,0.8,28.1,0.1,24.7,0.1,28,0.1,6455.8,38.6,3475.7,44.9,1976.7,33.799999999999997,230,null,230,null,230,null,6.8,null,6.5,null,6.4,null,0.56000000000000005,230,null,230,null,230,null,10.199999999999999,null,9.4,null,8.9,null,2950,null,0.78,230,230,230,10.6,9.4,9.9,3210,0.81,null,null,null,null,null,null,null,null,8490,null,null,null,null,null,null,null,null,null,null,null,null,null,null,221.83,0.14000000000000001,98.46,0.04,null,null,10.01,0.03,226.65,0.14000000000000001,253.31,0.05,109.99,0.04,143.32,0.05,139.49,0.1,98.21,0.03,78.069999999999993,0.04,-20.14,0.04,null,null,null,null,null,null,null,null,32.22,0.04,74.099999999999994,0.1,8.99,0.04,65.11,0.08,122.03,1.54,38.92,0.01,43640,124,9421,118,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,108.47,0.04,81.06,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,252.13,0.16,206.49,0.03,117.66,0.05,88.82,0.04,241.82,0.19,null,null,13.66,0.05,241.23,0.17,100.86,0.03,114.45,0.05,13.59,0.06,null,null,null,null,null,null,63.29,0.04,77.77,0.03,36.04,0.03,41.73,0.05,101.12,0.06,521.98,0.36,39.75,0.01,115.24,0.01,43640,124,39407,28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100.96,0.04,114.62,0.06,null,null,null,null,null,null,null,null,64.7,0.04,64.31,0.04,64.239999999999995,0.03,64.67,0.05,64.569999999999993,0.05,64.59,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98.21,0.03,null,null,null,null,null,null,null,null,null,null,null,null,81.73,0.05,100.92,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98.6,0.04,101.12,0.06,81.73,0.05,100.92,0.04,75.63,7.0000000000000007E-2,77.33,0.03,null,null,null,null,null,null,null,null,null,null,null,null,98.91,0.05,101.53,0.05,101.41,0.05,null,null,null,null,null,null,94.73,0.08,94.44,7.0000000000000007E-2,74.510000000000005,0.04,74.680000000000007,0.04,74.25,0.06,74.31,0.05,74.5,0.05,74.56,0.05,null,null,75.47,0.09,74.66,0.06,74.86,0.05,75.02,0.05,87.73,0.19,77.28,0.15,74.709999999999994,0.09,74.77,7.0000000000000007E-2,82.7,0.18,77.84,7.0000000000000007E-2,78.3,0.09,76.83,0.09,80.13,0.06,79.83,0.06,79.61,7.0000000000000007E-2,76.41,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.76,7.0000000000000007E-2,94.24,0.09,94.35,0.09,94.56,0.08,94.49,0.08,94.53,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C8-55-CE3",75.004000000000005,5.0000000000000001E-3,61.997999999999998,2.1999999999999999E-2,64.602999999999994,1.0999999999999999E-2,58.287999999999997,1.9E-2,94.998999999999995,1.4E-2,75,2.5000000000000001E-2,3107.2,4.2,3000,4,0.95499999999999996,3.0000000000000001E-3,-0.54500000000000004,3.0000000000000001E-3,-0.49299999999999999,6.0000000000000001E-3,1.3248,3.5000000000000001E-3,29.233000000000001,1E-3,8433,30,1720,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.401773550954017,14030.515352995952,336.58110236220472,26.025223115353274,110.74649690304445,13919.768856092907,8.8189538906861403E-3,27.690410588167254,63.201226449045976,14.099889663221212,13.287608851815337,1.3921017560975253E-2,38.157141971984878,8.778361573076392E-3,27.607136659787649,8.877823210764536E-3,25.17873952834212,75.163291495311938,62.116506749436574,24.836788430304654,40037.789497540631,40280.144948440997,6713,0.57224610268275078,35316.180799902839,35558.536250803205,4.1878549507770471,0.43380856619150232,-2.8536221578625991,-11.962065046265963,54.036046659050641,40037.789497540631,34071.663235917818,4797.750130988491,1168.3761306343529,40037.78949754066,1.0000000000000007]
[3,"3-282OD","75N0066","3-282OD","open","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 10","9/24/2013","17:24:20","10 Ton","0:30:00","75/62 82/68","ENG 1","TECH 2","RTU3","RTU3","7.5","R22","PSC Air Handler","ck1: 7.6 lbs / ck2: 8.1 lbs","230/208/3","TU2","AHRI 340-360",75,62,82,68,7.6,8.1,7.6,8.1,230.3,0.2,25.8,0,42929,102,44001,176,939,130,43868,192,5.7134670490000001,null,null,null,null,113.69,0.01,45.23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"83.3% airflow both stages economizer fully open (5.047\")","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1 lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: With econo Meriam set to 75%: Horiz airflow disch config. set on floor: VFD 25.02%",74.998999999999995,0.01,62.009,1.2E-2,81.98,0.03,67.991,1.2E-2,75.040000000000006,0.06,59.15,0.04,63.31,0.02,8.4000000000000005E-2,4.0000000000000001E-3,0.90820000000000001,2.3E-3,42929,102,939,130,5.7140000000000004,3.4000000000000002E-2,80102,68,10.432,0.04,45.23,0.25,230.3,0.8,229.6,0.8,229.7,0.8,25.8,0.1,23.7,0.1,26.6,0.1,5904.8,39.4,3593.3,46.8,1773.2,31.4,230,null,230,null,230,null,6.4,null,6.4,null,6.1,null,0.54,230,null,230,null,230,null,9.8000000000000007,null,9.3000000000000007,null,8.9,null,2870,null,0.77,230,230,230,9.3000000000000007,8.4,8.9,2680,0.77,null,null,null,null,null,null,null,null,7680,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,226.7,0.26,178.84,0.06,110,0.08,68.849999999999994,0.05,207.83,0.25,87.36,7.0000000000000007E-2,103.92,0.08,16.559999999999999,0.04,null,null,null,null,null,null,null,null,71.48,7.0000000000000007E-2,71.28,0.06,41.75,0.05,29.53,0.06,602.29,0.57999999999999996,35.56,0.02,80102,68,47058,41,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,207.1,0.24,189.43,0.08,103.67,0.08,85.76,0.06,null,null,null,null,null,null,196.26,0.25,88.87,0.06,100,0.09,11.13,7.0000000000000007E-2,null,null,null,null,null,null,56.97,0.06,74.77,0.05,31.29,0.05,43.48,0.06,88.12,0.08,485.13,0.49,36.020000000000003,0.02,115.04,0.01,80102,68,38335,38,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.35,0.04,59.2,0.05,59.37,0.05,59.44,0.05,59.4,0.04,59.46,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,87.36,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,88.4,7.0000000000000007E-2,87.91,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,87.61,7.0000000000000007E-2,88.12,0.08,null,null,null,null,72.3,0.06,74.569999999999993,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80.83,0.09,81.94,0.1,75.14,0.04,75.3,0.04,75.069999999999993,0.05,75.099999999999994,0.05,75.19,0.04,75.22,0.04,null,null,75.849999999999994,0.11,76.290000000000006,0.08,76.97,0.08,77.08,0.08,77.349999999999994,0.1,78.61,0.13,79.16,0.14000000000000001,79.56,0.16,78.06,0.09,78.34,0.08,79.27,0.1,80.77,0.11,78.67,0.09,78.680000000000007,0.08,78.78,0.09,79.66,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,79.069999999999993,0.1,78.73,0.1,79.89,0.11,79.87,0.11,80.78,0.12,80.95,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C8-55-OE3",74.998999999999995,0.01,62.009,1.2E-2,59.500999999999998,2.5999999999999999E-2,56.25,2.5999999999999999E-2,81.98,0.03,67.991,1.2E-2,2560.4,3.2,2489.6,3.1,0.78400000000000003,2E-3,-8.5000000000000006E-2,7.0000000000000001E-3,8.4000000000000005E-2,4.0000000000000001E-3,0.90820000000000001,2.3E-3,29.187000000000001,1E-3,7678,30,1520,null,0.40678135627125417,1006.8652130426083,13.03,0.11,1.5716569223616306,11675.195281628998,229.30352982677164,909.14471268138925,3967.7356586909923,7707.4596229380059,9.6549435745053886E-3,29.146493935475309,57.929343077638364,13.748063745476349,13.15815250145995,1.1341347897838562E-2,32.121185202701888,8.7867967536325135E-3,27.6151477861623,8.8590092055097387E-3,23.913690005637076,77.378717122306767,64.130296720348838,23.530310388794746,65570.039644967328,54498.05761846801,6158,0.32053136026452178,61164.8925922661,50092.910565766782,7.966253268073209,0.19375528141057066,-5.6161835466805634,-19.449374044668403,53.255304470753302,65570.039644967328,43215.242414337044,4476.031893630302,17878.765336999957,65570.039644967299,0.99999999999999956]
[3,"3-2CH Retest","75N0076","3-2CH Retest","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 10","10/1/2013","2:57:26","10 Ton","0:30:00","75/62  65/57","ENG 1","TECH 2","RTU3","RTU3","7.5","R22","PSC Air Handler","ck1: 7.6 lbs / ck2: 8.1 lbs","230/208/3","TU2","AHRI 340-360",75,62,65,57,7.6,8.1,7.6,8.1,230.6,0.3,24.4,0,59145,94,58106,288,21159,98,80323,122,12.076830552000001,null,null,null,null,113.07,0.01,-4.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer Closed 2 Stage 65/57","New R22 CK 1 : 7.6 lbs /Ck 2 : 8.1 lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: With econo Meriam set to 75%: Horiz airflow disch config. set on floor:VFD at 25.02%",74.998999999999995,1.7999999999999999E-2,61.994,2.3E-2,64.986000000000004,1.2E-2,57.033000000000001,1.4999999999999999E-2,74.36,0.12,54.14,0.04,59.43,0.03,0.14699999999999999,3.0000000000000001E-3,0.94359999999999999,2E-3,59145,94,21159,98,12.077999999999999,5.5E-2,77209,63,11.61,0.05,-4.03,0.17,230.6,0.5,230.4,0.5,229.4,0.5,24.4,0.1,21.2,0.1,24.5,0.1,5529.7,29.1,3414.2,30.5,1121,24.5,230,null,231,null,228,null,6.5,null,6.2,null,6.2,null,0.52,231,null,229,null,229,null,8.9,null,8.1999999999999993,null,7.5,null,2310,null,0.7,229,228,229,8.5,7.3,7.9,2200,0.69,null,null,null,null,null,null,null,null,6710,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,174.92,0.13,158.12,0.05,92.33,0.05,65.78,0.05,156.49,0.12,69.84,0.04,85.18,0.05,15.34,0.03,null,null,null,null,null,null,null,null,61.21,0.05,64.650000000000006,0.05,34.5,0.04,30.15,0.06,537.87,0.41,30.29,0.01,77209,63,44526,33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,164.62,0.16,166.3,0.04,88.41,0.06,77.900000000000006,0.06,null,null,null,null,null,null,153.74,0.15,71.040000000000006,0.03,84.07,0.06,13.03,0.06,null,null,null,null,null,null,51.24,0.04,67.75,0.04,26.72,0.04,41.02,0.05,69.78,0.05,455.71,0.47,30.64,0.01,114.12,0.01,77209,63,38042,40,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.42,0.03,54.1,0.04,53.46,0.04,54.9,0.03,54.83,0.03,54.87,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69.84,0.04,null,null,null,null,null,null,null,null,null,null,null,null,71.489999999999995,0.04,70.150000000000006,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.08,0.04,69.78,0.05,71.489999999999995,0.04,70.150000000000006,0.04,65.08,0.04,67.44,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64.63,0.09,64.84,0.06,74.58,7.0000000000000007E-2,74.48,7.0000000000000007E-2,74.13,7.0000000000000007E-2,73.7,7.0000000000000007E-2,69.88,0.06,71.349999999999994,7.0000000000000007E-2,null,null,73.989999999999995,0.08,74.25,0.09,74.260000000000005,0.08,73.55,0.08,66.44,7.0000000000000007E-2,71.45,0.09,74.39,0.08,74.41,0.08,71.11,0.19,71.61,0.09,73.78,0.08,73.52,0.09,71.02,7.0000000000000007E-2,71.989999999999995,0.09,73.37,0.11,71.66,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.53,0.08,63.27,7.0000000000000007E-2,63.58,0.08,64.319999999999993,0.08,63.79,7.0000000000000007E-2,63.78,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C8-55-CE3",74.998999999999995,1.7999999999999999E-2,61.994,2.3E-2,54.406999999999996,2.1000000000000001E-2,51.276000000000003,0.02,64.986000000000004,1.2E-2,57.033000000000001,1.4999999999999999E-2,2599.1,2.8,2553.5,2.7,1.22,2E-3,-0.44800000000000001,2E-3,0.14699999999999999,3.0000000000000001E-3,0.94359999999999999,2E-3,29.190999999999999,1E-3,6651,29,1590,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.4524874852531391,11980.442702935274,365.98290078740155,22.908657318943789,103.42042900122941,11877.022273934044,8.7704411338301921E-3,27.576196954890456,52.95451251474686,13.290598892413101,13.016714312384497,8.0280509872535082E-3,24.346041746603174,8.776905574636517E-3,27.604323873378664,7.2678720681949825E-3,20.944460127687616,74.912680216669756,61.953254052247139,20.591176048235642,83683.642750982995,63136.456803439483,5061,0.20641062497004051,79506.072391370399,58958.886443826887,11.954002765203789,0.2098310442369356,-6.9850209066548139,-21.958167701922896,47.123474450267629,83683.642750982995,79788.116014607498,4232.4996717336107,-336.97293535815942,83683.642750982937,0.99999999999999933]
[3,"4-1CH Retest","75N0078","4-1CH Retest","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 10","10/1/2013","7:17:37","10 Ton","0:30:00","75/62  60/54","ENG 1","TECH 5","RTU3","RTU3","7.5","R22","PSC Air Handler","ck1: 7.6 lbs / ck2: 8.1 lbs","230/208/3","TU2","AHRI 340-360",75,62,60,54,7.6,8.1,7.6,8.1,230.8,0.3,15.7,0,33940,78,33017,169,13541,127,47494,101,10.981271676,null,null,null,null,113.2,0.01,-21.95,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo Closed 1st Stage 60/54 Ambient","New R22 CK 1 : 7.6 lbs /Ck 2 : 8.1 lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: With econo Meriam set to 75%: Horiz airflow disch config. set on floor:VFD at 25.02%",75.007999999999996,0.01,62.005000000000003,4.5999999999999999E-2,59.994,1.7999999999999999E-2,54.005000000000003,0.02,74.41,0.06,62.75,0.04,65.98,0.03,0.14099999999999999,2E-3,0.93120000000000003,2.0999999999999999E-3,33940,78,13541,127,10.981999999999999,7.4999999999999997E-2,38947,30,9.0050000000000008,5.8000000000000003E-2,-21.95,0.26,230.8,0.8,230.8,0.8,229.2,0.8,15.7,0.1,13.5,0.1,16.3,0.1,3574.6,27.2,2239.6,28.8,750.6,22.2,229.8,null,228.9,null,230.2,null,6.6,null,6.2,null,6.2,null,0.53,230.3,null,228.9,null,230.3,null,8.6999999999999993,null,7.9,null,7.4,null,2170,null,0.68,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,4350,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,161.74,0.11,153.53,0.03,87.29,0.04,66.25,0.05,143.18,0.11,63.79,0.04,79.67,0.05,15.88,0.02,null,null,null,null,null,null,null,null,59.1,0.05,64.790000000000006,0.05,32.94,0.04,31.85,0.06,523.05999999999995,0.37,28.5,0.01,38947,30,44305,30,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102.49,0.06,71.08,0.05,60.28,0.03,10.8,7.0000000000000007E-2,null,null,null,null,null,null,101.9,7.0000000000000007E-2,73.13,0.03,59.97,0.04,13.16,0.05,null,null,null,null,null,null,101.74,7.0000000000000007E-2,75.930000000000007,0.13,59.88,0.04,16.05,0.13,61.08,0.05,35.36,22.88,31.26,0.01,112.89,0.02,38947,30,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.51,0.04,62.42,0.04,63.79,0.04,62.81,0.04,62.7,0.04,62.7,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.79,0.04,null,null,null,null,null,null,null,null,null,null,null,null,65.510000000000005,0.04,65.930000000000007,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64.209999999999994,0.04,61.08,0.05,65.510000000000005,0.04,65.930000000000007,0.04,64.98,0.04,74.58,0.36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.7,7.0000000000000007E-2,59.68,0.06,74.5,0.04,74.430000000000007,0.04,74.13,0.03,73.47,0.05,67.900000000000006,7.0000000000000007E-2,70.02,0.09,null,null,73.790000000000006,0.06,74.16,0.06,74.180000000000007,0.05,73.52,0.05,63.04,0.09,70.11,0.11,74.319999999999993,0.05,74.349999999999994,0.04,69.75,0.21,70.489999999999995,0.13,73.63,7.0000000000000007E-2,73.58,0.06,69.94,7.0000000000000007E-2,71.069999999999993,7.0000000000000007E-2,72.95,0.1,71.89,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.87,7.0000000000000007E-2,58.66,7.0000000000000007E-2,58.9,7.0000000000000007E-2,59.6,7.0000000000000007E-2,59.01,7.0000000000000007E-2,59.02,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C8-55-CE3",75.007999999999996,0.01,62.005000000000003,4.5999999999999999E-2,63.017000000000003,2.9000000000000001E-2,55.856000000000002,4.2999999999999997E-2,59.994,1.7999999999999999E-2,54.005000000000003,0.02,2595.8000000000002,2.9,2520.8000000000002,2.8,1.204,2E-3,-0.44600000000000001,2E-3,0.14099999999999999,2E-3,0.93120000000000003,2.0999999999999999E-3,29.245000000000001,1E-3,4325,28,1570,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.4663797321530423,11764.417126685947,356.55783105511813,22.744543676384684,103.70163113338032,11660.715495552566,8.7702871533112212E-3,27.567075536738248,61.550620267846959,13.159606128353454,13.238904938750199,7.4495985023535433E-3,22.501021469369398,8.7820323646042933E-3,27.612129210365435,7.7977919083776753E-3,23.61571590778318,74.87597196240786,61.939853025927491,23.258707843406011,50685.43467949819,37623.598966705402,2755,0.1855131569741347,46543.956556889309,33482.12084409652,10.761608452459956,0.53191138689633799,-4.3083676933322366,-13.325351694560901,46.408388429009889,50685.43467949819,47015.473102214222,4199.9917869237652,-530.03020963973574,50685.434679498256,1.0000000000000013]
[3,"5-2115 recalc","75N0088","5-2115","closed","on","on",null,"unsealed","unsealed",null,null,null,0,0,"CUST 11","6/20/2013","2:36:05","10 Ton","0:30:00","115/80 75/62","ENG 2","TECH 4","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. ck1: 8.59 lbs ck2: 10.35 lbs","208/230/3","TU2","Ashrae 340/360",115,80,75,62,8.59,10.35,7.6,8.1,230.4,1.3,32.9,0,38728,46,39736,146,-3579,0,35146,46,3.2476436889999998,896.7,null,null,null,109.94,0.01,56.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"83.3% air flow both stages closed","2511.4 SCFM, VFD Setpoint 25.022%, (Manual Mode) Damper close 28% (set to 72% on Meriam M334 damper controller) with Both Stages Cooling, with Econo fully closed, The unit has NO Tape around the Unit. -0.488 Inlet static.",74.998999999999995,0.01,62.002000000000002,3.2000000000000001E-2,115,4.2999999999999997E-2,80.010000000000005,2.5999999999999999E-2,74.739999999999995,0.05,60.55,0.02,63.77,0.02,-3.4000000000000002E-2,3.0000000000000001E-3,0.92359999999999998,1.9E-3,39066,46,0,0,3.609,1.0999999999999999E-2,80047,69,7.3970000000000002,2.1000000000000001E-2,51.2,0.08,230.4,0.9,230.2,0.9,229.6,0.9,32.9,0.1,30.8,0.1,33,0.1,7573.3,34.5,3810.3,42.9,3248.4,31.4,229,null,228,null,227,null,6.3,null,6.4,null,6,null,0.55000000000000004,227,null,228,null,228,null,13,null,12.3,null,12.8,null,4290,null,0.86,227,228,229,13.2,12.5,12.3,4330,0.87,null,null,null,null,null,null,null,null,10730,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,346.4,0.41,184.83,0.09,142.04,0.1,42.79,0.08,327.7,0.41,126.24,0.14000000000000001,137.62,0.1,11.38,0.09,null,null,null,null,null,null,null,null,78.099999999999994,0.08,52.55,0.05,46.1,0.05,6.46,0.03,689.05,0.64,48.01,0.05,80047,69,42674,41,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350.35,0.41,226.82,0.08,142.94999999999999,0.09,83.86,7.0000000000000007E-2,null,null,null,null,null,null,336.84,0.41,125.59,0.09,139.80000000000001,0.1,14.21,0.05,null,null,null,null,null,null,84.24,0.06,78.930000000000007,0.09,49.92,0.04,29.01,0.11,124.58,0.11,649.27,0.69,47.79,0.03,114.39,0.02,80047,69,43243,48,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.16,0.03,60.96,0.03,60.97,0.03,59.99,0.03,60.45,0.04,60.75,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,125.43,0.11,125.32,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,125.26,0.08,125.2,0.1,125.02,0.12,124.58,0.11,null,null,null,null,53.07,0.1,80.63,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,114.63,0.22,null,null,77.02,0.06,75.400000000000006,0.05,75.25,0.04,76.42,0.06,75.209999999999994,0.04,75.28,0.04,null,null,89.56,0.1,90.11,0.2,88.72,0.19,96.54,0.17,80.180000000000007,0.1,80.23,0.06,79.45,0.04,88.3,0.12,76.680000000000007,0.05,76.44,0.04,76.91,0.04,82.81,0.1,76.67,0.06,75.900000000000006,0.04,76.91,0.06,77.599999999999994,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,114.76,0.11,114.42,0.1,114.29,0.11,114.44,0.13,114.48,0.1,113.94,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,126.12,0.11,125.94,0.1,125.68,0.1,125.75,0.11,null,null,null,null,"C8-55-CE3",74.998999999999995,0.01,62.002000000000002,3.2000000000000001E-2,61.040999999999997,0.01,57.463000000000001,1.2E-2,115,4.2999999999999997E-2,80.010000000000005,2.5999999999999999E-2,2580.5,2.7,2511.4,2.6,1.1419999999999999,2E-3,-0.48799999999999999,3.0000000000000001E-3,-3.4000000000000002E-2,3.0000000000000001E-3,0.92359999999999998,1.9E-3,29.263000000000002,2E-3,10822,30,1500,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.4096793530635259,11729.544517123775,336.93575193700786,25.065713779377869,102.95980291321044,11626.584714210565,8.8260225552715781E-3,27.744489498478824,59.631320646936473,14.6070872729857,13.20000105494004,1.3776826549548683E-2,42.920657732691105,8.782180462684433E-3,27.610096181027448,9.2186275437012265E-3,24.68064894815641,75.353285734806605,62.195057764497072,24.336555986264262,39973.507842918691,44258.757454761238,9322,0.79592679544225187,36003.969564279701,40289.219176122249,3.3269238185436798,0.21870257403866908,-3.4079335122145622,-15.721965087870132,55.230391987236182,39973.507842918691,34361.081728525896,4036.0537145429248,1576.3723998498674,39973.507842918691,1]
[3,"8-3B","75N0101","8-3B","1 finger","on","on",null,"unsealed","unsealed",null,null,null,0,0,"CUST 11","6/26/2013","10:54:22","10 Ton","0:30:06","95/75  75/62","ENG 2","TECH 5","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. ck1: 5.55 lbs ck2: 7.11 lbs","208/230/3","TU2","Ashrae 340/360",95,75,75,62,5.55,7.11,7.6,8.1,230.3,1.4,24.3,0,36109,51,36816,133,2805,103,38916,105,5.4788117700000001,null,null,null,null,115.27,0.01,9.7200000000000006,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1 Finger, -40% charge, both stages B-Test","2552.5 SCFM, VFD Setpoint 25.022%, (Manual Mode) Damper closed 28% (set to 72% on Meriam M334 damper controller) with 2 Stages ON,  Economizer 1 Finger Open, The unit has NO Tape around the Unit. -0.363 Inlet static.",74.998000000000005,2.4E-2,62,1.4E-2,82.001000000000005,2.8000000000000001E-2,68.004000000000005,1.7999999999999999E-2,74.790000000000006,0.05,61.9,0.02,65.2,0.02,7.4999999999999997E-2,2E-3,0.95420000000000005,1.9E-3,36109,51,2805,103,5.4790000000000001,2.7E-2,43111,319,6.07,0.05,9.7200000000000006,0.72,230.3,1.1000000000000001,229.9,1.1000000000000001,229.7,1.1000000000000001,24.3,0.1,22.8,0.1,25.1,0.1,5513.7,44.8,3592.9,58.3,1588.7,33.9,227.5,null,230.9,null,227.9,null,6.2,null,6.5,null,6.2,null,0.56000000000000005,227.5,null,228.5,null,230.9,null,8.9,null,8.5,null,8.4,null,2540,null,0.75,230.5,228.7,227.8,8.8000000000000007,8.1999999999999993,7.9,2380,0.73,null,null,null,null,null,null,null,null,7070,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,198.29,0.15,193.46,0.03,100.71,0.05,92.74,0.06,183.67,0.21,91.38,0.08,95.57,0.08,4.18,0.08,null,null,null,null,null,null,null,null,49.48,7.0000000000000007E-2,74,0.03,25.29,0.06,48.7,0.06,392.88,2.2200000000000002,36.79,0.02,43111,319,30831,174,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,184.59,0.2,208.63,0.06,95.9,7.0000000000000007E-2,112.73,0.1,null,null,null,null,null,null,175.62,0.28000000000000003,91.65,0.05,92.61,0.11,0.96,0.08,null,null,null,null,null,null,37.56,0.12,76.650000000000006,0.02,14.49,0.12,62.16,0.12,91.33,0.06,221.26,3.06,36.880000000000003,0.02,116.28,0.01,43111,319,17570,243,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.58,0.03,62.33,0.03,62.36,0.03,61.76,0.03,62.12,0.03,62.19,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.4,0.04,91.3,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,91.17,0.04,91.31,0.05,92.98,0.05,91.33,0.06,null,null,null,null,74.180000000000007,0.03,78.739999999999995,0.03,94.4,0.03,91.37,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,81.2,0.13,81.91,0.11,75.180000000000007,0.05,74.819999999999993,0.44,74.59,0.05,74.540000000000006,0.05,74.55,0.05,74.58,0.05,null,null,76.61,0.05,75.989999999999995,0.04,76.459999999999994,0.04,78.260000000000005,0.04,75.319999999999993,0.05,75.540000000000006,0.04,75.91,0.04,77.63,0.04,75.19,0.05,74.86,0.05,74.86,0.05,75.72,0.05,74.83,0.05,74.75,0.05,74.87,0.05,75.62,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,79.44,0.06,79.27,0.06,79.36,0.06,79.290000000000006,0.06,79.37,0.06,79.27,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.42,0.05,94.07,0.05,91.15,7.0000000000000007E-2,91.65,7.0000000000000007E-2,null,null,null,null,"C8-55-1FE3",74.998000000000005,2.4E-2,62,1.4E-2,62.354999999999997,1.9E-2,57.088000000000001,1.0999999999999999E-2,82.001000000000005,2.8000000000000001E-2,68.004000000000005,1.7999999999999999E-2,2625,2.6,2552.5,2.5,1.113,2E-3,-0.36299999999999999,2E-3,7.4999999999999997E-2,2E-3,0.95420000000000005,1.9E-3,29.285,0,7103,29,1540,null,9.1282153938544691E-2,224.4628165348814,13.029,0.35299999999999998,1.4404009195938583,11905.575812483617,333.75364488188978,233.82159750213714,1020.413695326365,10885.162117157253,9.0009421688065153E-3,27.996319377654132,60.914599080406141,13.748635396000987,13.229095549906376,1.1346108928618715E-2,32.131555744809972,8.7810979208495076E-3,27.608667657170663,8.6821266358271584E-3,24.417306419444003,75.600780795622754,62.546289438265205,24.066057648764996,46792.028976192538,41963.387953541293,5563,0.40576396055961178,42675.110166174425,37846.46914352318,6.0080402880718609,0.35723943051111945,-3.9302617288891355,-14.686181715216613,52.752176801611455,46792.028976192538,37994.993160776306,4181.8188683605886,4615.2169470556237,46792.028976192523,0.99999999999999967]
[3,"8-4F","75N0105","8-4F","1 finger","on","on",null,"unsealed","unsealed",null,null,null,0,0,"CUST 11","6/25/2013","4:26:05","10 Ton","0:30:00","115/80  75/62","ENG 2","TECH 4","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. ck1: 10.11 lbs ck2: 11.97 lbs","208/230/3","TU2","Ashrae 340/360",115,80,75,62,10.11,11.97,7.6,8.1,230.3,1.4,33.9,0,35506,54,36204,133,-10654,142,24841,126,2.2024115609999999,null,null,null,null,109.88,0.02,70.78,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1 Finger Open, +20% Charge, Both Stages 115F Ambient","2540.5 SCFM, VFD Setpoint 25.022%, (Manual Mode) Damper closed 28% (set to 72% on Meriam M334 damper controller) with 2 Stages ON,  Economizer One Finger Opened (0.74\"), The unit has NO Tape around the Unit. -0.346 Inlet static.",75.015000000000001,0.02,61.914999999999999,1.6E-2,115.012,0.02,80.013999999999996,3.2000000000000001E-2,74.8,0.04,61.94,0.02,65.28,0.01,6.0999999999999999E-2,2E-3,0.94830000000000003,1.9E-3,35506,54,-10654,142,2.2029999999999998,1.2999999999999999E-2,85016,84,7.5380000000000003,2.1000000000000001E-2,70.78,0.14000000000000001,230.3,1.3,230,1.3,229.7,1.3,33.9,0.1,32,0.1,34.200000000000003,0.1,7802.7,46.3,3910.2,60.9,3475.9,38.5,229,null,229,null,226,null,6.3,null,6.5,null,6.1,null,0.55000000000000004,227,null,228,null,231,null,13.3,null,12.7,null,12.8,null,4400,null,0.87,226,229,231,13.9,13.3,13.2,4660,0.88,null,null,null,null,null,null,null,null,11260,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,352.47,0.34,172.86,0.22,143.44,0.08,29.42,0.21,332.76,0.35,125.17,0.1,138.83000000000001,0.08,13.66,0.08,null,null,null,null,null,null,null,null,78.790000000000006,0.05,52.49,0.1,46.54,0.03,5.95,0.09,721.51,0.79,47.65,0.03,85016,84,44903,54,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,376.72,0.45,217.99,0.14000000000000001,148.86000000000001,0.1,69.13,0.16,null,null,null,null,null,null,361.68,0.44,124.53,0.08,145.53,0.1,21,0.05,null,null,null,null,null,null,90.03,7.0000000000000007E-2,62.52,0.28999999999999998,53.35,0.04,9.17,0.28999999999999998,123.73,0.1,713.67,0.76,47.43,0.03,111.05,0.05,85016,84,45403,59,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.71,0.03,62.23,0.02,62.24,0.03,61.54,0.03,61.86,0.03,62.04,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,123.84,0.08,124.44,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,124.44,0.06,124.24,0.08,123.34,0.08,123.73,0.1,null,null,null,null,54.5,0.04,67.709999999999994,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,113.87,0.16,116.75,0.12,76.239999999999995,0.04,75.41,0.04,75.3,0.04,75.819999999999993,0.04,75.14,0.04,75.290000000000006,0.04,null,null,95.19,0.4,84.66,0.11,88.05,0.11,101.63,0.15,81.33,0.19,81.459999999999994,0.11,83.31,0.08,100.94,0.23,78.36,0.05,76.73,0.04,77.27,0.05,83.51,0.14000000000000001,76.55,0.04,76.319999999999993,0.04,77.180000000000007,0.06,82.99,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.27,0.14000000000000001,114.48,0.17,115.24,0.15,115.24,0.15,115.02,0.16,115.02,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,124.59,0.08,124.59,0.1,124.89,0.08,124.93,0.09,null,null,null,null,"C8-55-1FE3",75.015000000000001,0.02,61.914999999999999,1.6E-2,62.401000000000003,1.2999999999999999E-2,58.804000000000002,1.4999999999999999E-2,115.012,0.02,80.013999999999996,3.2000000000000001E-2,2618.4,2.7,2540.5,2.6,1.101,2E-3,-0.34599999999999997,3.0000000000000001E-3,6.0999999999999999E-2,2E-3,0.94830000000000003,1.9E-3,29.274000000000001,1E-3,11279,30,1590,null,9.1282153938544691E-2,224.4628165348814,13.029,0.35299999999999998,1.5111155642733678,11867.29861747615,328.6030729133858,235.30222939088759,966.50550928753421,10900.793108188616,9.132924817679737E-3,28.799539412731043,60.889884435726636,14.60740122822531,13.238396122319177,1.3777869635031078E-2,42.924771114822072,8.7210864576860708E-3,27.547142993081675,9.7178956985046316E-3,25.556171781923595,78.299992720089236,63.687495898466892,25.186983967129741,42871.274245140266,49586.628953550317,9689,0.7713453257981604,38566.12653299365,45281.481241403701,3.4192859768590878,0.19298506217607067,-3.612555445601302,-17.4101082843626,56.726528006650369,42871.274245140266,23627.449901611093,4381.2620440921428,14862.56229943701,42871.274245140245,0.99999999999999944]
[3,"C8-CB50-115-CE","75N0116","C8-CB50-115-CE","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",50,0,"CUST 3","6/30/2015","22:00:05","10 Ton","0:15:00","75/62 115/80","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,115,80,7.6,8.1,7.6,8.1,229.9,1.7,36.200000000000003,0,39850,65,39576,122,-3160,137,36687,130,3.024,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50% condenser coil block, economizer closed (2.0V), factory charge (CK1 7.6 lbs, CK2 8.1 lbs)--115F OD, 75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @--75%: Outlet @ 75% Horiz airflow. 7\" ID pulley 4.5 turns open from fully closed,--ad","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch: Condenser coil blockage 44.5\"",75.010000000000005,5.0000000000000001E-3,62.011000000000003,2.9000000000000001E-2,114.99,0.02,79.998999999999995,3.5000000000000003E-2,74.569999999999993,0.05,60.24,0.03,63.58,0.02,7.0999999999999994E-2,3.0000000000000001E-3,0.87590000000000001,2.0999999999999999E-3,39850,65,-3160,137,3.024,1.0999999999999999E-2,null,null,null,null,null,null,229.9,1.1000000000000001,229.8,1.1000000000000001,230.1,1.1000000000000001,36.200000000000003,0.1,33,0.1,37.200000000000003,0.1,8318.2000000000007,36.6,3988.4,50.3,3812.4,30.9,230,null,230,null,230,null,6.2,null,6.3,null,6.2,null,0.63,230,null,230,null,230,null,13.9,null,13.8,null,13.1,null,4770,null,0.89,230,230,230,15.2,14.9,13.4,5080,0.77,228.3,null,2.4,null,529.79999999999995,null,115,null,12064.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,373.32,0.28999999999999998,238.34,0.05,148.11000000000001,0.06,90.22,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,75.42,0.05,81.78,0.04,44.37,0.03,37.4,0.05,null,null,null,null,null,null,null,null,361.44,0.32,137.52000000000001,0.08,145.47,7.0000000000000007E-2,7.96,0.05,358.23,0.3,144.75,7.0000000000000007E-2,8.01,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,411.62,0.22,228.41,0.09,156.22999999999999,0.05,72.180000000000007,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,88.78,0.03,56.57,0.04,52.62,0.02,3.95,0.04,null,null,null,null,null,null,null,null,null,null,null,null,400.31,0.21,137.29,0.05,153.88999999999999,0.04,16.600000000000001,0.04,396.15,0.24,153.02000000000001,0.05,14.98,0.04,null,null,null,null,null,null,null,null,null,null,null,null,60.96,0.03,60.57,0.03,60.18,0.03,59.44,0.03,60.64,0.03,null,null,137.35,0.08,null,null,75.930000000000007,0.09,79.319999999999993,0.04,222.08,7.0000000000000007E-2,null,null,138.26,0.06,60.79,0.06,63.02,0.08,null,null,137.56,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.81,0.03,null,null,null,null,null,null,null,null,138.04,0.05,136.74,7.0000000000000007E-2,null,null,null,null,null,null,null,null,78.94,0.03,138.15,0.19,58.92,0.06,138.44999999999999,0.05,null,null,null,null,null,null,null,null,null,null,237.48,0.06,114.8,0.12,114.86,0.08,74.84,0.05,74.95,0.05,74.73,0.06,74.81,0.06,74.84,0.05,74.930000000000007,0.05,null,null,80.75,0.11,80.75,0.16,75.02,0.05,94.52,0.28000000000000003,76.37,0.04,78.97,0.2,75.8,0.05,76.34,0.11,77.989999999999995,0.2,82.43,0.13,82.32,0.09,87.51,0.16,75.37,0.05,79.52,0.17,75.58,0.06,92.81,0.25,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,114.36,0.12,null,null,null,null,null,null,null,null,60.87,0.03,60.61,0.03,"C8-55-CE3",75.010000000000005,5.0000000000000001E-3,62.011000000000003,2.9000000000000001E-2,60.578000000000003,1.2E-2,57.252000000000002,1.9E-2,114.99,0.02,79.998999999999995,3.5000000000000003E-2,2511.8000000000002,3,2446.1999999999998,2.9,1.1499999999999999,1E-3,-0.42099999999999999,2E-3,7.0999999999999994E-2,3.0000000000000001E-3,0.87590000000000001,2.0999999999999999E-3,29.263000000000002,1E-3,12131,17,1570,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.5420395741353528,11427.552042951032,330.48739842519677,23.28125409459976,95.632097622662371,11331.919945328371,8.8272169937875875E-3,27.744406031759667,59.035960425864651,14.606761541377731,13.188126331304934,1.3768475036913917E-2,42.908909217521327,8.7855168340760081E-3,27.61643007922412,9.2010338901925264E-3,24.548493780058308,75.347584143195135,62.194826895893037,24.172104651144377,40822.659940087047,44736.462944358835,10561,0.88295797120767283,36592.203430912246,40506.006435184034,3.0164210230741282,0.19356851376549794,-3.5723013806152899,-16.311623717330484,55.12066592910741,40822.659940087047,35059.001723175905,4301.2063590649586,1462.4518578461661,40822.659940087025,0.99999999999999944]
[3,"C8-CB80-82-CE","75N0127","C8-CB80-82-CE","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",80,0,"CUST 3","7/1/2015","14:11:53","10 Ton","0:15:00","75/62 82/68","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,82,68,7.6,8.1,7.6,8.1,229.8,1.7,30,0,50290,75,49732,159,9782,144,60082,169,6.22,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"80% condenser coil block, economizer closed (2.0V), factory charge (CK1 7.6 lbs, CK2 8.1 lbs)--82F OD, 75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 75%:--Outlet @ 75% Horiz airflow. 7\" ID pulley 4.5 turns open from fully closed, adju","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch: Condenser coil blockage. 51.5\"",74.995999999999995,0.01,61.999000000000002,2.1999999999999999E-2,82.018000000000001,3.5999999999999997E-2,67.988,1.4E-2,74.62,0.06,56.78,0.04,61.03,0.02,0.128,4.0000000000000001E-3,0.87419999999999998,2.7000000000000001E-3,50290,75,9782,144,6.22,2.5000000000000001E-2,null,null,null,null,null,null,229.8,1.4,229.6,1.4,230.3,1.4,30,0.1,27.5,0.1,31.6,0.1,6896.6,53.9,3803.8,73,2762.9,41.5,230,null,230,null,230,null,6.4,null,6.3,null,6.3,null,0.62,230,null,230,null,230,null,10.6,null,10.6,null,9.9,null,3430,null,0.83,230,230,230,12.3,12.2,10.8,3990,0.75,228.2,null,2.4,null,540.20000000000005,null,115,null,9645.2000000000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,269.85000000000002,0.7,200.23,0.08,122.69,0.19,77.540000000000006,0.18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.58,0.17,75.58,0.04,36.25,0.13,39.32,0.11,null,null,null,null,null,null,null,null,258.10000000000002,0.66,110.01,0.2,119.38,0.19,9.3699999999999992,0.11,255.43,0.69,118.62,0.2,8.74,0.17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,329.02,1.1100000000000001,194.12,0.2,137.93,0.27,56.18,0.35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,77.489999999999995,0.12,49.16,0.25,45.7,0.08,3.46,0.28999999999999998,null,null,null,null,null,null,null,null,null,null,null,null,317.36,1.06,115.01,0.23,135.09,0.26,20.079999999999998,0.12,313.8,1.07,134.21,0.27,19.100000000000001,0.18,null,null,null,null,null,null,null,null,null,null,null,null,57.79,0.03,57,0.03,55.94,0.03,55.82,0.03,56.18,0.03,null,null,109.69,0.19,null,null,73.08,0.04,74.41,0.04,189.09,0.18,null,null,115.54,0.23,53.19,0.05,57.9,0.15,null,null,113.75,0.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.57,0.03,null,null,null,null,null,null,null,null,115.11,0.22,109.87,0.17,null,null,null,null,null,null,null,null,74.569999999999993,0.04,110.83,0.18,50.53,0.04,115.61,0.24,null,null,null,null,null,null,null,null,null,null,197.83,0.08,90.05,0.87,80.56,0.11,74.959999999999994,7.0000000000000007E-2,74.989999999999995,0.06,74.959999999999994,7.0000000000000007E-2,75.03,7.0000000000000007E-2,75,7.0000000000000007E-2,75.03,0.06,null,null,74.97,0.06,75.430000000000007,0.05,74.89,0.06,77.91,0.06,75.540000000000006,0.06,75.400000000000006,0.06,75.23,0.06,75.14,0.06,75.790000000000006,0.06,75.180000000000007,0.06,75.540000000000006,0.05,76.819999999999993,0.05,74.959999999999994,0.06,75.3,0.06,75.150000000000006,7.0000000000000007E-2,77.099999999999994,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,79.42,0.14000000000000001,null,null,null,null,null,null,null,null,57.42,0.03,57.3,0.03,"C8-55-CE3",74.995999999999995,0.01,61.999000000000002,2.1999999999999999E-2,56.953000000000003,8.9999999999999993E-3,53.926000000000002,1.0999999999999999E-2,82.018000000000001,3.5999999999999997E-2,67.988,1.4E-2,2503,3.9,2452.9,3.8,1.149,2E-3,-0.41799999999999998,3.0000000000000001E-3,0.128,4.0000000000000001E-3,0.87419999999999998,2.7000000000000001E-3,29.247,1E-3,9659,32,1570,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.5349289353121875,11474.775891013369,331.10441678740159,22.506659908755438,98.218475757928857,11376.55741525544,8.8027304635986889E-3,27.646579846349617,55.418071064687815,13.748936583515581,13.087837307360013,1.1330050898283794E-2,32.118099045950601,8.7809110720388339E-3,27.607975391234032,8.1218424791340525E-3,22.4913729732143,75.056381409326718,62.053704853381859,22.117454924482377,63445.469351843378,54082.850419896218,8089,0.43514150469749607,59217.118726338776,49854.499794391617,6.1307711695143157,0.18244944953024517,-5.5291249218672398,-19.638310344638903,51.03546877786318,63445.469351843378,58711.866070193515,4290.6258108038337,442.97747084604083,63445.469351843385,1.0000000000000002]
[3,"C8-CB70-95-CE","75N0137","C8-CB70-95-CE","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",70,0,"CUST 3","6/27/2015","17:53:06","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,95,75,7.6,8.1,7.6,8.1,229.9,1.4,32.200000000000003,0,44832,67,44307,170,1041,131,45875,132,4.3150000000000004,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"70% condenser coil block(~70 psig DP CK1 above C8-CB0-95-CE), economizer closed (2.8V),--factory charge (CK1 7.6 lbs, CK2 8.1 lbs) 95F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 75%: Outlet @ 75% Horiz airflow. 7\" ID pulley 4.","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch.: Cond coil block 50`",74.998000000000005,8.0000000000000002E-3,61.994999999999997,2.8000000000000001E-2,95.012,2.1000000000000001E-2,75,0.02,74.58,7.0000000000000007E-2,58.5,0.04,62.27,0.02,9.9000000000000005E-2,4.0000000000000001E-3,0.86399999999999999,2.7000000000000001E-3,44832,67,1041,131,4.3150000000000004,1.2E-2,null,null,null,null,null,null,229.9,1.2,229.5,1.2,230.3,1.2,32.200000000000003,0.1,29.8,0.1,33.799999999999997,0.1,7396.1,44.3,3910,60.3,3234.9,34,230,null,230,null,230,null,6.3,null,6.3,null,6.1,null,0.63,230,null,230,null,230,null,12.3,null,12.3,null,11.6,null,4130,null,0.86,230,230,230,12.9,12.8,11.5,4230,0.75,228,null,2.4,null,540.79999999999995,null,115,null,10605.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,326.19,0.3,212.5,0.05,137.25,7.0000000000000007E-2,75.25,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,73.78,0.05,76.17,0.05,43.3,0.03,32.869999999999997,0.05,null,null,null,null,null,null,null,null,313.41000000000003,0.3,120.88,0.08,134.12,7.0000000000000007E-2,13.24,0.03,310.25,0.31,133.32,0.08,12.52,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,348.2,0.37,215.72,7.0000000000000007E-2,142.44999999999999,0.09,73.27,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82.33,0.06,66.81,0.17,48.74,0.03,18.07,0.18,null,null,null,null,null,null,null,null,null,null,null,null,337.12,0.38,121.21,0.08,139.87,0.09,18.649999999999999,0.03,333.41,0.37,138.99,0.09,17.309999999999999,0.05,null,null,null,null,null,null,null,null,null,null,null,null,59.13,0.03,57.89,0.03,58.18,0.03,57.85,0.04,58.3,0.03,null,null,120.52,0.08,null,null,73.83,0.05,75.66,0.04,209.39,7.0000000000000007E-2,null,null,121.85,0.09,69.489999999999995,0.18,74.709999999999994,0.13,null,null,121.04,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.91,0.03,null,null,null,null,null,null,null,null,121.67,0.08,120.81,7.0000000000000007E-2,null,null,null,null,null,null,null,null,75.62,0.05,122,0.09,68.69,0.26,122.13,0.09,null,null,null,null,null,null,null,null,null,null,211.68,0.09,95.83,0.1,95.8,0.08,75.05,0.06,75.05,0.06,75.319999999999993,0.06,75.260000000000005,0.06,75.14,0.06,75.14,0.06,null,null,81.03,0.09,80.7,0.1,75.5,0.08,86.86,0.12,75.52,0.06,82.24,0.08,77.19,0.1,79.41,0.14000000000000001,85.74,0.2,82.26,0.08,81.22,0.09,83.73,7.0000000000000007E-2,74.900000000000006,0.06,82.58,0.08,77.77,0.1,82.37,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.07,0.13,null,null,null,null,null,null,null,null,58.58,0.02,58.76,0.02,"C8-55-CE3",74.998000000000005,8.0000000000000002E-3,61.994999999999997,2.8000000000000001E-2,58.72,0.01,55.918999999999997,1.6E-2,95.012,2.1000000000000001E-2,75,0.02,2491.6,3.9,2433.3000000000002,3.8,1.149,2E-3,-0.38100000000000001,2E-3,9.9000000000000005E-2,4.0000000000000001E-3,0.86399999999999999,2.7000000000000001E-3,29.254000000000001,1E-3,10631,19,1590,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.5761888289618602,11378.656942946393,328.45871310236225,21.7602254764751,92.595427547141099,11286.061515399251,8.8196294700060643E-3,27.690927160631656,57.143811171038138,14.100194395925298,13.138281675033035,1.391790493912955E-2,38.156908525346452,8.7778011496329675E-3,27.605060003355938,8.849176007400511E-3,23.712488628980566,75.162378217613721,62.117202309083126,23.328010410298155,49644.132972679399,49206.502326350965,9041,0.62156253221264757,45338.492560497762,44900.861914169327,4.2647439150124882,0.15535318343459542,-4.3629167503335005,-18.018567046575583,53.829713850458873,49644.132972679399,44292.234294950707,4374.8457524222713,977.05292530638053,49644.132972679356,0.99999999999999911]
[3,"C8-R105-95-CE","75N0173","C8-R105-95-CE","closed","on","on","4.5 turns","unsealed","sealed",865,7,"horizontal",0,0,"CUST 3","6/30/2015","0:37:36","10 Ton","0:15:00","75/62  95/75","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,95,75,7.6,8.1,7.6,8.1,230.1,1.7,28.1,0,45361,101,45088,163,5822,123,51188,121,5.85,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"105% charge CK1 and CK2, 90% airflow, 360 cfm/ton, closed damper, 4.5 turns,--7\" AK49 pulley (865 rpm), adjust code tester speed to match total static of--run C8-R105-95-CE-SPWCT-SS","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch.",75.025000000000006,4.2000000000000003E-2,62.006,0.02,94.978999999999999,3.3000000000000002E-2,75.001999999999995,1.2999999999999999E-2,74.680000000000007,7.0000000000000007E-2,58.54,0.03,62.59,0.03,0.151,5.0000000000000001E-3,0.88380000000000003,2.7000000000000001E-3,45361,101,5822,123,5.85,1.7999999999999999E-2,null,null,null,null,null,null,230.1,1.3,229.8,1.3,230,1.4,28.1,0.1,25.6,0.1,29.2,0.1,6463.2,50.8,3669.3,71.2,2286.1999999999998,39.200000000000003,230,null,230,null,230,null,6.4,null,6.3,null,6.3,null,0.62,230,null,230,null,230,null,10.3,null,10.1,null,9.5,null,3190,null,0.82,230,230,230,10.8,10.5,9.4,3320,0.72,228.6,null,2.4,null,525.9,null,115,null,8710.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250.04,0.36,199.61,0.09,117.05,0.11,82.56,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.25,0.06,78.81,0.06,33.06,0.05,45.75,0.09,null,null,null,null,null,null,null,null,239.14,0.36,100.75,0.12,113.82,0.11,13.07,0.04,236.93,0.35,113.15,0.11,11.78,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,272.85000000000002,0.42,197.54,0.09,123.51,0.12,74.03,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.55,7.0000000000000007E-2,74.67,0.04,43.81,0.05,30.87,0.08,null,null,null,null,null,null,null,null,null,null,null,null,261.77,0.44,102.67,0.12,120.42,0.13,17.760000000000002,0.04,258.67,0.43,119.54,0.12,16.170000000000002,0.06,null,null,null,null,null,null,null,null,null,null,null,null,59.38,0.04,58.82,0.05,57.98,0.05,57.66,0.05,58.39,0.05,null,null,100.79,0.12,null,null,74.36,0.05,78.03,0.03,192.17,0.09,null,null,103.35,0.1,77.83,0.05,79.44,0.05,null,null,104.79,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.22,0.04,null,null,null,null,null,null,null,null,103.38,0.12,101.38,0.09,null,null,null,null,null,null,null,null,75.930000000000007,0.04,101.8,0.1,73.87,0.05,103.53,0.1,null,null,null,null,null,null,null,null,null,null,198.96,0.09,95.18,0.21,95.76,0.16,74.97,7.0000000000000007E-2,75.03,7.0000000000000007E-2,74.88,0.08,74.97,0.08,74.98,7.0000000000000007E-2,75.040000000000006,7.0000000000000007E-2,null,null,77.66,0.09,77.05,0.1,75.13,0.08,88.64,0.15,75.83,7.0000000000000007E-2,76.239999999999995,0.12,75.47,0.08,75.739999999999995,0.1,78.87,0.14000000000000001,77.430000000000007,0.16,78.34,0.1,80.37,0.1,75.2,0.09,76.66,0.12,75.430000000000007,7.0000000000000007E-2,83.1,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.12,0.16,null,null,null,null,null,null,null,null,59.18,0.04,58.95,0.04,"C8-55-CE3",75.025000000000006,4.2000000000000003E-2,62.006,0.02,58.783999999999999,1.7000000000000001E-2,55.249000000000002,7.0000000000000001E-3,94.978999999999999,3.3000000000000002E-2,75.001999999999995,1.2999999999999999E-2,2520.1999999999998,3.9,2461.9,3.8,1.159,2E-3,-0.42699999999999999,3.0000000000000001E-3,0.151,5.0000000000000001E-3,0.88380000000000003,2.7000000000000001E-3,29.257000000000001,1E-3,8750,20,1560,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.5127259705609097,11510.61710709969,335.21152859842522,23.035792119440913,98.028573103525375,11412.588533996164,8.8225250483417502E-3,27.702422456774695,57.271274029439091,14.099435332051662,13.136741374772445,1.3927559215106034E-2,38.159434914358549,8.7786752930016781E-3,27.612601816427489,8.444166279741934E-3,23.287813973347419,75.196514621166259,62.133782969604141,22.919088213336593,55059.128971494363,49519.339440962991,7190,0.44569302962828855,50878.925918600791,45339.136388069419,5.8147343906972333,0.21957225426290852,-4.7833342434381017,-17.925240591727167,52.228032670544046,55059.128971494363,49780.976931134224,4244.261041008941,1033.8909993512159,55059.128971494378,1.0000000000000002]
[3,"C8-R110-110C2-95-CE","75N0174","C8-R110-110C2-95-CE","closed","on","on","4.5 turns","unsealed","sealed",865,7,"horizontal",0,0,"CUST 3","6/30/2015","1:55:21","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,95,75,7.6,8.1,7.6,8.1,230.1,1.7,28.4,0,46352,103,46315,213,6185,160,52542,140,5.9340000000000002,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"110% charge CK1 and CK2, 90% airflow, 360 cfm/ton, closed damper,--4.5 turns, 7\" AK59 pulley (865 rpm), duct removed from supply sampling box--(without code tester), record total static, 5 minute snapshot","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch.",74.989999999999995,4.8000000000000001E-2,61.997999999999998,0.03,95.007000000000005,1.7000000000000001E-2,75.007000000000005,2.4E-2,74.69,7.0000000000000007E-2,58.15,0.04,62.3,0.03,8.7999999999999995E-2,4.0000000000000001E-3,0.88580000000000003,2.7000000000000001E-3,46352,103,6185,160,5.9340000000000002,0.02,null,null,null,null,null,null,230.1,1.3,229.9,1.3,230,1.3,28.4,0.1,25.8,0.1,29.5,0.1,6524,49.5,3676.1,65.400000000000006,2331.3000000000002,37.1,230,null,230,null,230,null,6.3,null,6.1,null,6.3,null,0.64,230,null,230,null,230,null,10.4,null,10.199999999999999,null,9.5,null,3220,null,0.8,230,230,230,11,10.7,9.5,3370,0.72,228.6,null,2.4,null,526.20000000000005,null,115,null,8791.2000000000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,253.31,0.25,199.14,0.05,118.01,7.0000000000000007E-2,81.13,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.48,0.05,78.42,0.05,34,0.04,44.42,0.05,null,null,null,null,null,null,null,null,242.29,0.24,100.58,0.06,114.77,7.0000000000000007E-2,14.2,0.04,239.91,0.24,114.06,7.0000000000000007E-2,12.82,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,278.31,0.23,196.09,0.06,125.01,0.06,71.08,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,76.45,0.04,73,0.04,45.06,0.03,27.95,0.04,null,null,null,null,null,null,null,null,null,null,null,null,266.89,0.26,102.49,0.05,121.87,7.0000000000000007E-2,19.37,0.04,263.68,0.26,120.97,7.0000000000000007E-2,17.78,0.05,null,null,null,null,null,null,null,null,null,null,null,null,59.03,0.04,58.52,0.05,57.74,0.05,57.34,0.05,58.11,0.05,null,null,100.64,7.0000000000000007E-2,null,null,74.09,0.04,77.83,0.05,190.86,0.05,null,null,103.3,7.0000000000000007E-2,76.5,0.04,78.36,0.14000000000000001,null,null,104.83,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.87,0.04,null,null,null,null,null,null,null,null,103.18,0.06,101.24,7.0000000000000007E-2,null,null,null,null,null,null,null,null,75.67,0.04,101.67,7.0000000000000007E-2,72.25,0.04,103.47,0.06,null,null,null,null,null,null,null,null,null,null,198.57,0.06,95.28,0.14000000000000001,95.76,0.13,75.06,0.09,75.11,0.09,74.97,0.09,75.06,0.09,75.069999999999993,0.09,75.13,0.08,null,null,77.739999999999995,0.08,77.12,0.11,75.23,0.1,88.58,0.15,75.87,0.08,76.260000000000005,0.11,75.52,0.1,75.8,0.1,78.89,0.14000000000000001,77.45,0.12,78.39,0.08,80.42,0.1,75.23,0.09,76.72,0.1,75.489999999999995,0.09,83.24,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.25,0.1,null,null,null,null,null,null,null,null,58.89,0.04,58.64,0.04,"C8-55-CE3",74.989999999999995,4.8000000000000001E-2,61.997999999999998,0.03,58.43,0.02,55.055,1.6E-2,95.007000000000005,1.7000000000000001E-2,75.007000000000005,2.4E-2,2520.9,3.9,2467.1999999999998,3.7,1.1559999999999999,2E-3,-0.43099999999999999,3.0000000000000001E-3,8.7999999999999995E-2,4.0000000000000001E-3,0.88580000000000003,2.7000000000000001E-3,29.297000000000001,5.0000000000000001E-3,8855,19,1560,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.5114304010005286,11521.874914815788,335.06363262992119,23.144005003530822,98.484234241832112,11423.390680573955,8.8256344079648899E-3,27.697573700918444,56.918569598999468,14.100127912879797,13.127550951408525,1.3925237623132813E-2,38.163766920726189,8.781669307617139E-3,27.607341732713707,8.4158977844923828E-3,23.170800512297681,75.162685302651482,62.126395533439549,22.802409516626696,56401.469418895773,50449.540576537176,7295,0.44143947412225859,52220.76159706169,46268.832754703093,5.8973192091543414,0.20773085594206489,-4.8951641842917475,-18.244115703652014,52.135011133483154,56401.469418895773,51117.272996057618,4244.5549718655384,1039.641450972598,56401.469418895751,0.99999999999999967]
[3,"C8-R80-E20C30-95CE","75N0186","C8-R80-E20C30-95CE","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",30,20,"CUST 3","6/29/2015","19:36:49","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,95,75,7.6,8.1,7.6,8.1,229.9,1.7,27.9,0,34637,56,34436,96,2023,95,36663,93,4.2149999999999999,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline 80% factory charge, 20% evaporator blockage, 30% condenser blockage,--economizer closed (2.0V), 80% factory charge (CK1 6.08 lbs, CK2 6.48 lbs), 95F OD, 75F DB, 62F WB ID conditions,--unsealed cabinet, Inlet Meriam set @ 75%: Outlet @ 75% Horiz a","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch.: Removed: CK1:6.1 oz CK2",74.997,1.0999999999999999E-2,61.997999999999998,0.02,94.988,1.0999999999999999E-2,74.998000000000005,2.4E-2,74.73,0.09,61.85,0.09,65.17,0.02,7.0999999999999994E-2,2E-3,0.81879999999999997,1.6999999999999999E-3,34637,56,2023,95,4.2149999999999999,1.4999999999999999E-2,null,null,null,null,null,null,229.9,1.4,229.8,1.4,230.1,1.4,27.9,0.1,25.4,0.1,29.3,0.1,6395.9,51.8,3698.8,71.099999999999994,2301.4,38.700000000000003,230,null,230,null,230,null,6.2,null,6.1,null,6.1,null,0.61,230,null,230,null,230,null,10.1,null,10.1,null,9.3000000000000007,null,3150,null,0.81,230,230,230,10.8,10.7,9.5,3350,0.72,228.5,null,2.4,null,535.5,null,115,null,8640.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243.82,0.19,225.28,0.06,115.21,0.06,110.07,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43.91,0.06,78.8,0.04,20.399999999999999,0.05,58.4,7.0000000000000007E-2,null,null,null,null,null,null,null,null,235.8,0.19,110.42,0.11,112.8,0.06,2.38,0.09,233.46,0.21,112.08,0.06,1.75,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,274.49,0.14000000000000001,207.71,0.04,123.95,0.04,83.76,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,66.959999999999994,0.04,72.39,0.03,38.630000000000003,0.03,33.76,0.04,null,null,null,null,null,null,null,null,null,null,null,null,264.14999999999998,0.15,111.5,7.0000000000000007E-2,121.08,0.04,9.58,0.06,261.55,0.16,120.35,0.04,9.2100000000000009,0.06,null,null,null,null,null,null,null,null,null,null,null,null,62.63,0.03,62.08,0.05,61.42,0.05,61.19,0.04,61.83,0.03,null,null,110.55,0.09,null,null,73.81,0.05,77.650000000000006,7.0000000000000007E-2,201.78,0.1,null,null,111.42,0.04,75.63,0.11,79.069999999999993,0.06,null,null,110.92,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.43,0.04,null,null,null,null,null,null,null,null,111.14,0.06,110.33,0.05,null,null,null,null,null,null,null,null,75.66,0.06,110.41,0.08,72.25,0.13,111.56,0.04,null,null,null,null,null,null,null,null,null,null,224.66,0.11,95.3,0.11,95.2,0.09,75.2,0.05,75.150000000000006,0.05,75.31,7.0000000000000007E-2,75.33,0.06,75.3,0.06,75.3,0.05,null,null,78.56,0.05,78.8,7.0000000000000007E-2,75.25,0.05,85.97,0.1,75.849999999999994,0.05,77.900000000000006,7.0000000000000007E-2,75.989999999999995,0.06,76.650000000000006,0.09,78.930000000000007,0.15,78.78,0.06,78.87,0.06,79.38,0.09,75.09,0.05,78.28,0.06,75.63,0.05,81.34,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.43,7.0000000000000007E-2,null,null,null,null,"closed","20% blockage",null,null,62.34,0.04,62.26,0.04,"C8-EB20-55-CE",74.997,1.0999999999999999E-2,61.997999999999998,0.02,62.045999999999999,7.0000000000000001E-3,57.061,1.4999999999999999E-2,94.988,1.0999999999999999E-2,74.998000000000005,2.4E-2,2435.1999999999998,2.5,2358.3000000000002,2.5,1.06,1E-3,-0.38800000000000001,2E-3,7.0999999999999994E-2,2E-3,0.81879999999999997,1.6999999999999999E-3,29.167999999999999,1E-3,8698,19,1490,null,1.0570083158000437E-2,24.875633704038229,13.03,0.36699999999999999,1.5390332888662757,11050.91399789591,293.67705637795279,26.606542304059236,113.2224018448119,10937.691596051098,8.8326967204670342E-3,27.715310687573524,60.506966711133721,14.099617321593716,13.221711799387785,1.3921898503108977E-2,38.155405814784537,8.7800154353673832E-3,27.607239195941968,8.7390105115672193E-3,24.403876119685929,75.203715630192917,62.151735499047057,24.028536495486481,40742.224526416088,38979.002004766284,7208,0.60381837972665142,36659.174319834041,34895.951798184236,4.2146670866675144,0.32785495846231238,-3.6867741920870429,-14.696748919059196,53.338272889684148,40742.224526416088,35400.089859740765,4147.8459070306708,1194.2887596446242,40742.224526416059,0.99999999999999933]
[3,"C8-EB35-55-CE","75N0197","C8-EB35-55-CE","closed","off","off","4.5 turns","unsealed","sealed",null,7,"horizontal",0,35,"CUST 3","6/27/2015","1:03:14","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,55,51,7.6,8.1,7.6,8.1,230,1.8,6.3,0,4646,21,4402,122,3427,58,8075,60,5.5759999999999996,901,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"35% evaporator coil block, economizer closed (2V), no compressor, factory charge (CK1 7.6 lbs,--CK2 8.1 lbs) 95F OD, 75F DB, 62F WB ID conditions, Inlet Meriam @ 75%: Outlet @ 75% Horiz airflow.--7` blower pulley A49 belt, 4.5 turns open from closed, 870-","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch.: 16 1/4` evap coil block",74.991,1.2E-2,61.984000000000002,2.4E-2,54.969000000000001,2.3E-2,50.991,2.9000000000000001E-2,74.459999999999994,0.02,72.78,0.05,73.77,0.01,5.2999999999999999E-2,3.0000000000000001E-3,0.755,2.2000000000000001E-3,4646,21,3427,58,5.5759999999999996,5.7000000000000002E-2,null,null,null,null,null,null,230,1.3,230.4,1.3,230.1,1.3,6.3,0.1,6,0.1,6.3,0.1,1337.7,16.100000000000001,1126.8,22.4,110.5,11.8,230,null,230,null,230,null,6.2,null,5.9,null,6.1,null,0.57999999999999996,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,0,null,0,null,15,null,1430,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.27,0.04,58.54,0.05,56.88,0.02,-1.66,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.04,0.04,63.14,0.1,56.75,0.02,6.38,0.09,null,null,null,null,null,null,null,null,97.67,0.04,56.14,0.15,57.66,0.02,1.51,0.14000000000000001,97.22,0.03,57.41,0.02,-0.49,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.58,0.04,56.65,0.03,57.05,0.02,-0.41,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.45,0.04,60.77,7.0000000000000007E-2,56.99,0.02,3.78,0.06,null,null,null,null,null,null,null,null,null,null,null,null,97.74,0.04,56.2,0.03,57.69,0.02,1.5,0.03,97.54,0.04,57.59,0.02,-1.45,0.02,null,null,null,null,null,null,null,null,null,null,null,null,74.64,0.03,73.87,0.03,72.12,0.03,72.14,0.03,72.44,0.04,null,null,56.21,0.14000000000000001,null,null,57.11,0.03,62.8,0.09,57.34,0.03,null,null,56.54,0.02,56.99,0.04,59.55,0.05,null,null,56.52,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74.36,0.02,null,null,null,null,null,null,null,null,56.14,0.02,56.92,0.02,null,null,null,null,null,null,null,null,57.19,0.03,57.23,0.03,56.95,0.04,56.36,0.02,null,null,null,null,null,null,null,null,null,null,59.16,0.05,55.33,0.11,55.32,0.09,75.180000000000007,0.02,75.05,0.03,75.23,0.04,75.27,0.03,75.28,0.03,75.260000000000005,0.03,null,null,69.25,7.0000000000000007E-2,68.650000000000006,7.0000000000000007E-2,74.11,0.09,62.32,0.15,75.23,0.03,71.25,0.08,72.739999999999995,0.11,68.37,0.16,68.66,0.21,70.61,0.06,70.12,7.0000000000000007E-2,68.28,0.08,74.680000000000007,0.03,69.91,7.0000000000000007E-2,73.92,7.0000000000000007E-2,66.31,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54.69,0.1,null,null,null,null,null,null,null,null,74.010000000000005,0.02,74.05,0.02,"Economizer test",74.991,1.2E-2,61.984000000000002,2.4E-2,73.209000000000003,1.0999999999999999E-2,60.920999999999999,2.1000000000000001E-2,54.969000000000001,2.3E-2,50.991,2.9000000000000001E-2,2354.1999999999998,3.4,2247.1999999999998,3.3,0.96699999999999997,2E-3,-0.33300000000000002,2E-3,5.2999999999999999E-2,3.0000000000000001E-3,0.755,2.2000000000000001E-3,29.216999999999999,1E-3,1449,11,1430,null,9.0900009989010287E-3,20.427050244730388,13.029,0.33300000000000002,1.5964466098302681,10461.022988749028,255.28970557480312,20.426843637985723,94.069799003291592,10366.953189745736,8.7561217192052808E-3,27.535859672230401,71.612553390169737,13.0287364410788,13.502694731855426,6.9838467300413357E-3,20.772870792055073,8.7722033536988282E-3,27.597227076228027,8.5000232362362604E-3,26.864976174935791,74.811534892102387,61.895206968225388,26.475803982600667]
[3,"C8-EB0-82-CE","75N0201","C8-EB0-82-CE","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,0,"CUST 3","7/1/2015","17:05:18","10 Ton","0:15:00","75/62 82/68","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,82,68,7.6,8.1,7.6,8.1,229.8,1.6,25.4,0,49317,80,49116,294,11596,145,60923,177,7.9930000000000003,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline no evaporator coil blockage, economizer closed damper, factory charge--(CK1 7.6 lbs, CK2 8.1 lbs) 82F OD, 75F DB, 62F WB ID conditions, unsealed cabinet,--Inlet Meriam set @ 75%: Outlet @ 75% Horiz airflow. 7\" ID pulley 4.5 turns open from fully-","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch: Condenser coil blockage.",74.989000000000004,1.2E-2,62.000999999999998,3.1E-2,81.981999999999999,1.2E-2,68.004000000000005,1.7999999999999999E-2,74.64,0.08,57.28,0.11,61.41,0.02,0.183,4.0000000000000001E-3,0.90159999999999996,2.3999999999999998E-3,49317,80,11596,145,7.9930000000000003,3.1E-2,null,null,null,null,null,null,229.8,1.1000000000000001,229.6,1.1000000000000001,230.1,1.1000000000000001,25.4,0.1,23.3,0.1,27,0.1,5806.3,44.1,3639.9,61.5,1815.4,33.4,230,null,230,null,230,null,6.2,null,6.2,null,6.2,null,0.63,230,null,230,null,230,null,9.1999999999999993,null,9,null,8.4,null,2680,null,0.76,230,230,230,9.3000000000000007,9.4,8.1999999999999993,2730,0.68,228.3,null,2.4,null,530.6,null,115,null,7625.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,206.53,0.16,179.35,0.04,103.49,0.05,75.86,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.26,0.05,76.06,0.04,30.75,0.04,45.31,0.06,null,null,null,null,null,null,null,null,194.88,0.14000000000000001,88.04,0.06,99.53,0.05,11.49,0.06,192.59,0.15,98.72,0.05,10.050000000000001,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,221.53,0.22,182.77,0.04,108.37,7.0000000000000007E-2,74.400000000000006,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.85,0.05,71.959999999999994,0.04,36.44,0.04,35.53,0.06,null,null,null,null,null,null,null,null,null,null,null,null,211.53,0.23,88.96,0.05,105.14,0.08,16.18,0.05,208.97,0.19,104.3,0.06,14.7,0.05,null,null,null,null,null,null,null,null,null,null,null,null,58.22,0.04,57.61,0.04,56.87,0.04,56.57,0.05,57.18,0.04,null,null,88.01,0.06,null,null,72.7,0.05,75.430000000000007,0.04,177.84,0.05,null,null,89.59,0.06,72.63,0.06,75.930000000000007,0.05,null,null,91.05,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.04,0.03,null,null,null,null,null,null,null,null,89.6,0.05,88.68,0.05,null,null,null,null,null,null,null,null,73.790000000000006,0.06,89.11,0.06,71.02,7.0000000000000007E-2,89.72,0.06,null,null,null,null,null,null,null,null,null,null,178.87,0.04,82.47,0.15,83.15,0.11,75.05,7.0000000000000007E-2,75.040000000000006,7.0000000000000007E-2,75.12,0.08,75.17,0.08,75.14,7.0000000000000007E-2,75.14,0.06,null,null,75.69,0.05,75.81,0.05,74.94,0.06,78.52,7.0000000000000007E-2,75.55,0.06,75.83,0.06,75.2,7.0000000000000007E-2,75.09,7.0000000000000007E-2,75.849999999999994,7.0000000000000007E-2,76.400000000000006,0.05,76.180000000000007,0.06,76.63,0.06,74.94,7.0000000000000007E-2,75.87,0.05,75.209999999999994,0.06,77.73,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,81.2,0.08,null,null,null,null,null,null,null,null,57.86,0.03,57.79,0.04,"C8-55-CE3",74.989000000000004,1.2E-2,62.000999999999998,3.1E-2,57.561999999999998,1.6E-2,53.938000000000002,2.1999999999999999E-2,81.981999999999999,1.2E-2,68.004000000000005,1.7999999999999999E-2,2544.6999999999998,3.5,2488.9,3.4,1.1579999999999999,2E-3,-0.42699999999999999,2E-3,0.183,4.0000000000000001E-3,0.90159999999999996,2.3999999999999998E-3,29.202999999999999,1E-3,7622,18,1570,null,8.7942837155845673E-3,21.378903712586084,13.029,0.39800000000000002,1.5022936857232787,11653.159618680907,338.59544333858264,22.747048357768577,99.272916479602017,11553.886702201306,8.8057497884108434E-3,27.648046773478004,56.059706314276717,13.748189837321341,13.1021976010042,1.1350631693170687E-2,32.131863310890566,8.7838837397561063E-3,27.609521075926924,7.9849282768877546E-3,22.490963929792457,75.048849133247273,62.055582478523128,22.125087351163764,64359.927715725542,53108.042949934126,6052,0.32093690488954807,60157.143963840128,48905.259198048712,7.8925667756284605,0.23459973225991257,-5.5229594223142406,-18.989142818970556,50.239421152463187,64359.927715725542,59647.363441244765,4263.6181714970207,448.94610298372231,64359.927715725513,0.99999999999999956]
[3,"C8-EB35-95-CE","75N0210","C8-EB35-95-CE","closed","on","on","4.5 turns","unsealed","sealed",null,7,"horizontal",0,35,"CUST 3","6/26/2015","19:45:00","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. CK1 7.6 lbs/CK2 8.1 lb","208/230/3","TU2","AHRI 340-360",75,62,95,75,7.6,8.1,7.6,8.1,229.9,1.8,27.6,0,42740,67,41948,117,7237,152,49984,159,5.7949999999999999,901,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"35% evaporator coil block, economizer closed damper, factory charge (CK1 7.6 lbs, CK2 8.1 lbs)--95F OD, 75F DB, 62F WB ID conditions, unsealed cabinet, Inlet Meriam set @ 75%: Outlet @ 75% Horiz airflow.--7\" ID pulley 4.5 turns open from fully closed, adj","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch.: 16 1/4` evap coil block",75.022999999999996,1.2E-2,62.009,3.4000000000000002E-2,94.994,1.0999999999999999E-2,75.004999999999995,2.1999999999999999E-2,74.45,7.0000000000000007E-2,58.22,7.0000000000000007E-2,62.35,0.02,0.106,3.0000000000000001E-3,0.75360000000000005,1.9E-3,42740,67,7237,152,5.7949999999999999,2.1999999999999999E-2,null,null,null,null,null,null,229.9,1.4,229.5,1.4,230.1,1.4,27.6,0.1,25.5,0.1,29.1,0.1,6340.1,54.8,3730,74.8,2285.1,41.1,230,null,230,null,230,null,6.1,null,6.1,null,6.2,null,0.61,230,null,230,null,230,null,10.3,null,10.3,null,9.1999999999999993,null,3250,null,0.82,230,230,230,10.5,10.3,9.1999999999999993,3220,0.71,228.3,null,2.4,null,528.6,null,115,null,8583.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,255.03,0.17,191.55,0.04,118.5,0.05,73.06,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.95,0.04,73.59,0.03,35.06,0.03,38.54,0.04,null,null,null,null,null,null,null,null,243.54,0.16,100.89,0.06,115.13,0.05,14.25,0.04,241.06,0.16,114.39,0.05,12.4,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,264.31,0.23,195.69,0.05,121.14,0.06,74.55,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68.94,0.05,69.98,0.04,40.020000000000003,0.03,29.96,0.04,null,null,null,null,null,null,null,null,null,null,null,null,254.09,0.23,102.46,0.06,118.22,7.0000000000000007E-2,15.76,0.03,251.37,0.22,117.44,0.06,14.5,0.03,null,null,null,null,null,null,null,null,null,null,null,null,59.11,0.05,58.58,0.06,57.75,0.05,57.42,0.06,58.48,0.04,null,null,100.88,0.06,null,null,68.3,0.05,73.02,0.05,190.1,0.06,null,null,103.14,0.05,71.42,0.06,77.09,0.04,null,null,104.78,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.96,0.04,null,null,null,null,null,null,null,null,102.94,0.06,101.99,0.05,null,null,null,null,null,null,null,null,70.06,0.04,102.08,0.05,68.62,0.08,103.1,0.05,null,null,null,null,null,null,null,null,null,null,192.38,0.04,95.64,0.1,95.44,0.1,74.94,0.08,74.94,7.0000000000000007E-2,75.06,0.09,75.069999999999993,0.09,75.02,0.08,75.03,7.0000000000000007E-2,null,null,80.09,0.11,79.400000000000006,0.09,77.69,0.14000000000000001,82.47,7.0000000000000007E-2,75.540000000000006,0.06,78.91,0.11,78.83,0.09,80.63,0.09,86.91,0.1,79.3,0.15,78.900000000000006,0.13,78.099999999999994,0.08,74.94,7.0000000000000007E-2,80.040000000000006,0.1,75.680000000000007,7.0000000000000007E-2,78.599999999999994,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.12,0.09,null,null,null,null,null,null,null,null,58.87,0.04,58.77,0.04,"C8-EB35-55-CE",75.022999999999996,1.2E-2,62.009,3.4000000000000002E-2,58.491,1.4E-2,54.837000000000003,2.1999999999999999E-2,94.994,1.0999999999999999E-2,75.004999999999995,2.1999999999999999E-2,2326.9,3,2271.1,2.9,0.95699999999999996,2E-3,-0.33200000000000002,2E-3,0.106,3.0000000000000001E-3,0.75360000000000005,1.9E-3,29.213999999999999,5.0000000000000001E-3,8626,19,1470,null,9.0900009989010287E-3,20.427050244730388,13.029,0.33300000000000002,{"$f":"(XM337-XU337)*3.412/XT337/0.24","v":1.6237661723684513},10634.821117611333,255.33673294488182,21.217961164308399,90.290421535696709,10544.530696075635,8.8248117148509407E-3,27.704343273930281,56.867233827631551,14.099808686297772,13.128006428692846,1.3926597186021447E-2,38.162066383220235,8.7811262845502724E-3,27.614796166044979,8.2762857885692286E-3,23.033914396706237,75.194129881185148,62.136388820679485,22.638243709051839,53877.062636490838,46776.782680943892,7156,0.45331773494752581,49731.416906031722,42631.136950484775,5.7652929406482407,0.22605274066198772,-5.0660995648784422,-18.326896053553597,51.514356056248658,53877.062636490838,48716.85817784442,4207.8869846867929,952.31747395965328,53877.06263649086,1.0000000000000004]
[3,"C8-95-T2FE","75N0164","C8-95-T2FE","2 finger","on","on","4.5 turns","unsealed","sealed",870,7,"horizontal",0,0,"CUST 3","6/25/2015","22:23:04","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU3","RTU3","7.5","R22","PSC Air Handler","Manuf. 5.5 lbs","208/230/3","TU2","AHRI 340-360",75,62,95,75,5.5,null,7.6,8.1,230,1.7,28.2,0,40300,55,40114,137,346,165,40646,171,4.5919999999999996,900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 2-Finger open with perimeter tape and on damper with hood removed, Inlet static location inside Cabinet, unsealed cabinet,--95F OD ambient, factory charge (CK1 7.6 lbs, CK2 8.1 lbs) 75F DB, 62F WB ID conditions,--2700 cfm (370 cfm/ton) 7\" pulley, 87","New R22 CK 1 : 7.6 lbs / Ck 2 : 8.1lbs: No tape on unit: Sealed ductwork: 7` blower pulley with A49 belt at 2500 scfm : motor pulley 4.5 turns opened from closed: inlet M set to 75%: outlet M set @ 75% Horizontal air disch.",74.992000000000004,4.0000000000000001E-3,62.002000000000002,3.4000000000000002E-2,95,6.0000000000000001E-3,75.013999999999996,2.1999999999999999E-2,74.69,0.04,60.38,0.03,63.73,0.01,0.05,3.0000000000000001E-3,0.90010000000000001,2.0999999999999999E-3,40300,55,346,165,4.5919999999999996,2.1000000000000001E-2,null,null,null,null,null,null,230,1.3,229.8,1.3,230.2,1.3,28.2,0.1,25.8,0.1,29.7,0.1,6479.5,50.3,3724.7,67.400000000000006,2372.1999999999998,37.9,230,null,230,null,230,null,6.4,null,6.2,null,6.2,null,0.64,230,null,230,null,230,null,10.6,null,10.5,null,9.8000000000000007,null,3350,null,0.82,230,230,230,10.6,10.4,9.3000000000000007,3250,0.71,228.6,null,2.4,null,527.70000000000005,null,115,null,8822.7000000000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,261.81,0.11,197.01,0.03,120.44,0.03,76.58,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,66.010000000000005,0.04,81.5,0.03,38,0.03,43.5,0.04,null,null,null,null,null,null,null,null,249.82,0.11,101,0.03,116.99,0.03,15.99,0.02,247.21,0.11,116.23,0.03,14.39,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,267.56,0.15,201.25,0.04,122.05,0.04,79.2,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,71.489999999999995,0.04,77.540000000000006,0.03,41.77,0.02,35.76,0.03,null,null,null,null,null,null,null,null,null,null,null,null,257.10000000000002,0.15,102.71,0.04,119.1,0.04,16.39,0.03,254.38,0.14000000000000001,118.31,0.04,15.16,0.03,null,null,null,null,null,null,null,null,null,null,null,null,61.2,0.04,60.7,0.06,60.06,0.05,59.57,0.05,60.22,0.06,null,null,100.98,0.03,null,null,77.05,0.03,80.87,0.03,194.94,0.03,null,null,103.21,0.03,78.75,0.02,83.28,0.02,null,null,105.12,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.06,0.05,null,null,null,null,null,null,null,null,103.15,0.04,101.84,0.03,null,null,null,null,null,null,null,null,78.56,0.03,101.92,0.03,76.17,0.03,103.26,0.04,null,null,null,null,null,null,null,null,null,null,197.69,0.03,95.42,0.08,95.24,0.09,74.900000000000006,0.06,74.97,0.05,74.8,0.05,74.87,0.05,74.92,0.05,75.02,0.05,null,null,85.08,0.08,84.84,0.08,75.010000000000005,0.05,77.8,0.14000000000000001,75.709999999999994,0.05,86.77,0.09,82.28,0.1,84.46,0.1,76.430000000000007,7.0000000000000007E-2,85.67,0.08,85.22,7.0000000000000007E-2,82.9,7.0000000000000007E-2,75.22,0.06,85.82,0.08,85.04,0.14000000000000001,83.41,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.81,0.14000000000000001,null,null,null,null,null,null,null,null,61,0.05,60.96,0.05,"C8-55-T2FE3",74.992000000000004,4.0000000000000001E-3,62.002000000000002,3.4000000000000002E-2,60.622,1.2E-2,56.767000000000003,2.5000000000000001E-2,95,6.0000000000000001E-3,75.013999999999996,2.1999999999999999E-2,2547.3000000000002,3,2479.8000000000002,2.9,1.145,2E-3,-0.36599999999999999,2E-3,0.05,3.0000000000000001E-3,0.90010000000000001,2.0999999999999999E-3,29.25,1E-3,8852,18,1580,null,0.10041506225933922,247.4729209381415,13.029,0.34799999999999998,1.5288910214473743,11590.150475329558,333.5701993700788,264.01757850634334,1123.4778977884102,10466.672577541147,9.2829676655740989E-3,28.63386511714711,59.093108978552628,14.100014554415399,13.186886600422172,1.3933050265524313E-2,38.170662391921113,8.7838343464384169E-3,27.610198725127962,8.9002323180033018E-3,24.231986637711909,76.947855197513277,63.438254189564354,23.859011069100312,55341.276914598857,49665.406890378094,7272,0.4484778339737357,51087.212005048939,45411.341980828176,5.7712620882341774,0.23499357468302184,-4.774854048046798,-17.854746218960649,53.608513686018668,55341.276914598857,39153.986430729223,4322.8429638300149,11864.447520039656,55341.276914598893,1.0000000000000007]
[2,"T2-TRN-100A-55-NE-SC","75T0004","T2-TRN-100A-55-NE-SC","none","off","off","3 turns","sealed","unsealed",950,5.75,null,0,0,"CUST 5","10/23/2014","23:18:51","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460,0,3.6,0,-2192,21,-2510,142,496,60,-1696,57,-1.0101250740000001,945,1580,null,-1.305539011,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No economizer, no compressor, 55/51 ambient, 100% airflow (400 cfm/ton), 2 HP fan motor,--3 turns, 5.75\" AK59 pulley (950 rpm), Econo closed sealed cab,--adjust code tester speed to match total static of run T2-TRN-100A-55-NE-SPWCT-SS-SC","WO/ECO: No comp: 55/51 amb:2HP blwr mtr 5.75` AK59 mtr. pulley:3 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.995999999999995,8.9999999999999993E-3,62.002000000000002,2.1000000000000001E-2,55.021000000000001,0.01,51.006999999999998,1.6E-2,74.83,0.06,75.61,0.06,75.62,0,0.192,4.0000000000000001E-3,1.8891,2.8999999999999998E-3,-2192,21,496,60,0,0,null,null,null,null,null,null,460,2,462,2,460.1,2,3.6,0,3.1,0,3.5,0,1582.9,14.3,1083.2,17.8,96.4,10.1,460,null,460,null,460,null,3.2,null,3.2,null,3.1,null,0.55000000000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.6,null,0,null,0,null,85,null,1665,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.58,0.01,55.6,0.05,56.01,0.01,0.4,0.05,93.87,0.02,57.01,0.02,55.6,0.01,1.4,0.01,null,null,71.87,0.02,null,null,null,null,93.86,0.01,73.39,0.02,55.6,0,17.79,0.02,93.23,0.02,57.27,0.01,55.24,0.01,2.0299999999999998,0.01,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.96,0.02,58.1,0.02,56.21,0.01,1.88,0.02,95.66,0.01,56.61,0.01,0.66,0.04,null,null,74.180000000000007,0.02,null,null,null,null,94.65,0.01,56.04,0.01,17.149999999999999,0.03,94.48,0.01,59.1,0.02,55.95,0.01,3.15,0.02,58.48,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.16,0.05,58.45,0.05,58.48,0.04,59.63,0.05,75.64,0.05,75.53,0.04,75.41,0.05,75.760000000000005,0.03,75.78,0.02,null,null,55.4,0.03,72.14,0.03,73.459999999999994,0.03,57.45,0.03,58.65,0.03,56.07,0.03,74.77,0.03,74.39,0.02,60.98,0.02,71.87,0.02,74.180000000000007,0.02,55.94,0.03,56.47,0.03,59.38,0.02,57.21,0.03,57.96,0.02,58.45,0.05,59.63,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.6,0.05,55.94,0.04,57.16,0.05,58.48,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,73.19,0.04,null,null,null,null,null,null,null,null,null,null,null,null,57.05,0.03,55.6,0.04,55.35,0.02,75.28,0.03,75.14,0.02,74.900000000000006,0.02,75.61,0.03,75.63,0.03,75.61,0.03,75.430000000000007,0.03,75.13,0.03,75,0.03,74.760000000000005,0.03,75.02,0.03,74.849999999999994,0.03,74.819999999999993,0.03,74.900000000000006,0.03,74.760000000000005,0.03,74.739999999999995,0.03,74.790000000000006,0.03,74.78,0.03,74.930000000000007,0.03,74.78,0.03,74.459999999999994,0.03,74.56,0.02,75.010000000000005,0.03,74.47,0.03,74.239999999999995,0.05,74.38,0.03,null,null,75.03,0.02,75.790000000000006,0.02,75.59,0.03,75.42,0.03,75.22,null,75.06,0.02,75.44,0.03,76.77,0.05,75.03,0.03,74.88,0.03,74.95,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",74.995999999999995,8.9999999999999993E-3,62.002000000000002,2.1000000000000001E-2,75.674000000000007,5.0000000000000001E-3,62.216999999999999,1.9E-2,55.021000000000001,0.01,51.006999999999998,1.6E-2,3065.7,2.4,2939.8,2.2999999999999998,0.72499999999999998,3.0000000000000001E-3,-0.32500000000000001,2E-3,0.192,4.0000000000000001E-3,1.8891,2.8999999999999998E-3,29.451000000000001,1E-3,1679,10,1580,null,null,0,null,null,1.3942271398805808,13557.75507686273,250.39225669291341,0,0,13557.75507686273,8.7828892687881119E-3,27.610140128423488,74.279772860119422,13.030023961788491,13.56729037788196,6.9801274511825315E-3,20.781475020770898,8.7828892687881119E-3,27.610140128423488,8.7647832541451649E-3,27.755685228988558,74.995999999999995,62.002009067814676,27.415644991599702,2636.917428697795,2330.5037140566501,99,0.12813711810720627,-1901.0337992092909,-2207.4475138504358,-1.1322416910120852,0.96917750052350771,-0.19449513682378594,-0.71622713988057285,51.75884687986364,2636.917428697795,-1973.2648260985666,4610.1822547963611,0,2636.9174286977945,0.99999999999999978]
[2,"T2-TRN-88A-55-RD-DM","75T0093","T2-TRN-88A-55-RD-DM","none","off","off","4.5 turns","unsealed","unsealed",864,5.75,null,0,0,"CUST 5","10/24/2014","22:21:08","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,459.7,0,3.3,0,1126,16,801,102,477,78,1603,79,1.1641249090000001,858,1270,null,0.81771967999999995,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Relief damper and no economizer, no compressor, 55/51 ambient, 87.5% airflow (350 cfm/ton),--2 HP fan motor, 4.5 turns, 5.75\" AK59 pulley (864 rpm), 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-TRN-88A-55-RD-DM-SPWCT","WO/ECO: No comp: 55/51 amb:2HP blwr mtr 5.75` AK59 mtr. pulley: 4.5 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",75.004000000000005,8.9999999999999993E-3,62.006999999999998,2.9000000000000001E-2,55,1.0999999999999999E-2,50.994,1.4999999999999999E-2,74.97,0.04,74.7,0.05,74.790000000000006,0.01,0.151,3.0000000000000001E-3,1.5679000000000001,2.7000000000000001E-3,1126,16,477,78,1.165,5.8000000000000003E-2,null,null,null,null,null,null,459.7,2,461.5,2.1,460.3,2.1,3.3,0,2.9,0,3.2,0,1400.8,14.8,1096.5,19.2,-9.6,1.6,460,null,460,null,460,null,2.9,null,3,null,2.8,null,0.48,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,null,0,null,0,null,85,null,1355,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.89,0.01,56.43,7.0000000000000007E-2,56.73,0,0.28999999999999998,0.08,94.94,0.02,57.34,0.02,56.21,0.01,-1.1299999999999999,0.02,null,null,68.84,0.03,null,null,null,null,95.17,0.01,71.28,0.02,56.33,0,14.95,0.02,94.71,0.04,58.63,0.02,56.08,0.02,2.56,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.03,0.01,59.03,0.04,56.81,0,2.21,0.04,96.65,0.04,57.15,0.02,0.89,0.03,null,null,72.489999999999995,0.01,null,null,null,null,95.72,0.01,56.64,0.01,14.2,0.05,95.49,0.01,60.05,0.02,56.51,0.01,3.54,0.02,57.76,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.13,0.03,58.8,0.03,57.76,0.03,59.68,0.06,74.69,0.06,74.5,0.04,74.36,0.04,74.97,0.01,74.95,0.02,null,null,56.09,0.02,69.150000000000006,0.02,71.67,0.02,58.93,0.03,59.74,0.04,56.58,0.03,73.069999999999993,0.01,72.12,0.01,62.1,0.02,68.84,0.03,72.489999999999995,0.01,56.1,0.03,57.23,0.02,59.81,0.03,57.46,0.02,58.47,0.04,58.8,0.03,59.68,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.43,7.0000000000000007E-2,56.26,0.04,57.13,0.03,57.76,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.84,0.06,null,null,null,null,null,null,null,null,null,null,null,null,57.45,0.02,56.06,0.05,55.73,0.03,75.38,0.02,73,0.04,74.739999999999995,0.02,73.89,0.04,75.8,0.02,75.78,0.03,75.459999999999994,0.03,73.97,0.04,73.88,0.05,74.180000000000007,0.03,74.34,0.03,74.27,0.03,74.5,0.03,74.650000000000006,0.03,74.150000000000006,0.05,74.599999999999994,0.02,74.61,0.03,74.56,0.02,74.88,0.02,74.45,0.06,72.73,0.09,73.010000000000005,0.04,74.63,0.03,73.010000000000005,7.0000000000000007E-2,69.400000000000006,0.1,68.989999999999995,0.09,null,null,73.44,0.05,75.75,0.02,75.569999999999993,0.02,75,0.03,72.930000000000007,null,75.05,0.02,74.37,0.03,74.61,0.04,74.34,0.03,74.48,0.03,74.900000000000006,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",75.004000000000005,8.9999999999999993E-3,62.006999999999998,2.9000000000000001E-2,74.629000000000005,5.0000000000000001E-3,61.847000000000001,2.5000000000000001E-2,55,1.0999999999999999E-2,50.994,1.4999999999999999E-2,2790.3,2.4,2677.7,2.2999999999999998,0.58299999999999996,3.0000000000000001E-3,-0.253,2E-3,0.151,3.0000000000000001E-3,1.5679000000000001,2.7000000000000001E-3,29.431000000000001,0,1377,10,1270,null,null,0,null,null,1.2494279629599805,12363.940144022363,183.3984139527559,0,0,12363.940144022363,8.7842963883453737E-3,27.61363113867673,73.37957203704002,13.029476983773396,13.540829060139227,6.9781552094125929E-3,20.774229227400618,8.7842963883453737E-3,27.61363113867673,8.7675488706365264E-3,27.503844503417383,75.004000000000005,62.007009086915808,27.199118029504827,5125.015270714016,4820.2392245552219,107,7.1256568168063555E-2,1416.4440575347717,1111.6680113759776,1.0286449219569873,0.92646993052589111,-0.41451310917190298,-1.6244279629599845,52.911977313526535,5125.015270714016,1357.3953869601821,3767.6198837538332,0,5125.0152707140151,0.99999999999999978]
[2,"T2-TRN-100A-55-RD","75T0098","T2-TRN-100A-55-RD","none","off","off","3 turns","unsealed","unsealed",950,5.75,null,0,0,"CUST 5","10/24/2014","21:31:33","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,459.5,0,3.6,0,373,12,73,119,535,75,909,79,0.53818827700000005,945,1590,null,0.22084073400000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Relief damper and no economizer, no compressor, 55/51 ambient, 100% airflow (400 cfm/ton),--2 HP fan motor, 3 turns, 5.75\" AK59 pulley (950 rpm), Econo closed unsealed cab,--adjust code tester speed to match total static of run T2-TRN-100A-55-RD-SPWCT-SS","WO/ECO: No comp: 55/51 amb:2HP blwr mtr 5.75` AK59 mtr. pulley: 3 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.981999999999999,4.0000000000000001E-3,62.003999999999998,0.03,55.014000000000003,0.01,51,1.4E-2,74.95,0.05,74.930000000000007,0.03,74.92,0.01,0.20100000000000001,4.0000000000000001E-3,1.9323999999999999,2.5000000000000001E-3,373,12,535,75,0.53800000000000003,4.7E-2,null,null,null,null,null,null,459.5,2,461,2,460.5,2,3.6,0,3.1,0,3.4,0,1557.6,14,1103.5,18.100000000000001,131.5,9.6,460,null,460,null,460,null,3.1,null,3.2,null,3.1,null,0.56000000000000005,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,null,0,null,0,null,85,null,1675,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.05,0.02,56.58,0.04,56.81,0.01,0.24,0.04,95.08,0.02,57.38,0.02,56.28,0.01,-1.1000000000000001,0.02,null,null,69.010000000000005,0.02,null,null,null,null,95.3,0.02,71.37,0.02,56.4,0.01,14.96,0.02,94.83,0.03,58.76,0.02,56.13,0.01,2.63,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.19,0.02,56.48,0.03,56.89,0.01,-0.42,0.03,96.8,0.03,57.23,0.02,0.8,0.09,null,null,72.63,0.02,null,null,null,null,95.89,0.02,56.73,0.01,14.2,0.04,95.64,0.02,60.22,0.03,56.59,0.01,3.63,0.03,57.84,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.91,0.04,58.91,0.03,57.84,0.04,59.85,0.04,74.89,0.03,74.760000000000005,0.02,74.650000000000006,0.03,75.19,0.01,75.180000000000007,0.01,null,null,56.2,0.02,69.349999999999994,0.02,71.739999999999995,0.02,59.05,0.01,56.92,0.02,56.72,0.05,73.2,0.03,72.22,0.02,62.39,0.01,69.010000000000005,0.02,72.63,0.02,56.1,0.06,57.28,0.02,59.98,0.02,57.54,0.02,58.68,0.06,58.91,0.03,59.85,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.58,0.04,56.43,0.09,56.91,0.04,57.84,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.930000000000007,0.04,null,null,null,null,null,null,null,null,null,null,null,null,57.49,0.02,56.1,0.06,55.7,0.04,75.36,0.02,73.02,0.04,74.739999999999995,0.02,73.900000000000006,0.04,75.77,0.02,75.760000000000005,0.03,75.44,0.03,74.03,0.04,73.900000000000006,0.04,74.150000000000006,0.03,74.400000000000006,0.04,74.290000000000006,0.03,74.489999999999995,0.02,74.62,0.03,74.17,0.05,74.59,0.02,74.61,0.03,74.56,0.02,74.87,0.02,74.45,7.0000000000000007E-2,72.8,0.08,73.040000000000006,0.06,74.62,0.02,73.06,7.0000000000000007E-2,69.430000000000007,0.09,68.959999999999994,0.08,null,null,73.45,0.05,75.77,0.02,75.58,0.03,75.010000000000005,0.03,72.98,null,75.040000000000006,0.02,74.400000000000006,0.03,74.739999999999995,0.03,74.39,0.03,74.52,0.03,74.900000000000006,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",74.981999999999999,4.0000000000000001E-3,62.003999999999998,0.03,74.873999999999995,3.0000000000000001E-3,61.942,3.3000000000000002E-2,55.014000000000003,0.01,51,1.4E-2,3100.3,2,2974.2,1.9,0.71,3.0000000000000001E-3,-0.308,2E-3,0.20100000000000001,4.0000000000000001E-3,1.9323999999999999,2.5000000000000001E-3,29.423999999999999,0,1689,10,1590,null,null,0,null,null,1.3893595066619964,13731.229448099368,248.08106645669289,0,0,13731.229448099368,8.7875159397275675E-3,27.611788463016484,73.484640493338006,13.029830614807651,13.547075351344304,6.9780529271947665E-3,20.777521583812739,8.7875159397275675E-3,27.611788463016484,8.7721727816732018E-3,27.568657924550884,74.981999999999999,62.004008977253747,27.229800303420163,5245.1670658742942,4934.54086854449,99,6.4418729805259131E-2,665.19774569098718,354.57154836118298,0.3938411756607384,0.9321063949020193,-0.38198815959632171,-1.4973595066619936,52.927500102681577,5245.1670658742942,592.23531989123842,4652.9317459830554,0,5245.1670658742942,1]
[2,"3T-22A-Retest-OB","75T0048","3T-22A-Retest-OB","none","on","on","6 turns","sealed","sealed",null,5.375,null,0,0,"CUST 8","2/20/2014","11:19:05","10 Ton","0:30:00","80/67 95/75","ENG 1","TECH 2","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1-6.4 LBS / CK2-6.2 LBS","380/460/3","TU4","AHRI 210/240 2008",80,67,95,75,6.4,6.2,6.4,6.2,459.3,0,14.4,0,65989,227,64473,456,23177,276,89187,371,11.008022710000001,749,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Out of box, AHRI Verification H (IEER 100%), sealed cab, no econo.","R22 CK1 : 6.4 lbs /Ck2 : 6.2 lbs: Sealed cab/ Sealed ductwork: 5.375` blower pulley with AX35 (notched) belt : motor pulley 6 turns opened. No econo Meriam set @ 100%: Horiz airflow. set on floor.",80.006,3.2000000000000001E-2,67.150999999999996,3.1E-2,94.796999999999997,3.5000000000000003E-2,74.753,7.1999999999999995E-2,79.69,0.14000000000000001,59.6,0.05,64.67,0.03,0.7,8.9999999999999993E-3,1.1827000000000001,6.8999999999999999E-3,65989,227,23177,276,11.007999999999999,5.1999999999999998E-2,null,null,null,null,null,null,459.3,2,461.1,2,460.8,2,14.4,0,12.3,0,12.7,0,6541.5,41.4,3227.9,49.4,1560.5,33.4,460,null,460,null,459,null,2.4,null,2.5,null,5.6,null,0.5,460,null,459,null,460,null,5.0999999999999996,null,5,null,4.4000000000000004,null,3210,null,0.73,460,460,459,4.9000000000000004,4.7,4.4000000000000004,3050,0.82,458.5,null,1.7,null,707.9,null,115,null,8102.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,252,0.28999999999999998,174.75,0.09,117.61,0.08,57.13,0.09,null,null,103.77,0.08,null,null,null,null,null,null,57.34,0.41,null,null,null,null,82.16,0.06,63.14,0.17,48.61,0.04,14.52,0.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,254.39,0.28999999999999998,172.21,0.28999999999999998,118.3,0.08,53.9,0.3,null,null,null,null,null,null,null,null,100.87,0.1,null,null,null,null,null,null,null,null,null,null,81.84,0.15,58.89,0.98,48.41,0.09,10.47,1.02,102.68,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.39,0.1,59.97,7.0000000000000007E-2,60.11,7.0000000000000007E-2,59.74,0.06,59.99,0.06,59.79,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107.19,0.08,102.37,0.1,94.56,0.19,94.68,0.17,94.58,0.17,94.56,0.15,94.71,0.22,94.72,0.18,null,null,null,null,null,null,null,null,107.62,0.08,102.68,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,51.23,0.83,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.84,0.12,94.67,0.14000000000000001,79.89,0.1,79.84,0.11,79.73,0.14000000000000001,79.959999999999994,0.11,79.900000000000006,0.11,79.930000000000007,0.12,79.8,0.11,80.52,0.09,80.48,0.09,80.36,0.09,80.25,0.09,80.239999999999995,0.12,79.849999999999994,0.13,79.8,0.13,79.84,0.13,80.08,0.12,80.16,0.11,79.63,0.14000000000000001,79.650000000000006,0.14000000000000001,79.83,0.14000000000000001,79.91,0.13,80.05,0.12,79.77,0.12,80.03,0.11,79.89,0.12,79.98,0.12,79.989999999999995,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Economizer",80.006,3.2000000000000001E-2,67.150999999999996,3.1E-2,59.433,2.5999999999999999E-2,57.625,3.9E-2,94.796999999999997,3.5000000000000003E-2,74.753,7.1999999999999995E-2,2927.9,8.6999999999999993,2837.7,8.4,0.25,6.0000000000000001E-3,-0.318,3.0000000000000001E-3,0.7,8.9999999999999993E-3,1.1827000000000001,6.8999999999999999E-3,29.164000000000001,2E-3,8102,21,1020,null,null,0,null,null,0.99775716225258548,13346.066695629035,83.343472440944865,0,0,13346.066695629035,1.1186200947589407E-2,31.467362863090059,58.435242837747417,14.093370315283572,13.162979326151197,1.3753514876008805E-2,37.922642909112589,1.1186200947589407E-2,31.467362863090059,9.6979191021836584E-3,24.809323300560898,80.006,67.151010152794655,24.565565362920317,92111.849756991127,69092.343303033762,{"$f":"XK375-XM375","v":7082},0.2624077799302415,{"$f":"YM375-(XM375-XU375)*3.413","v":88915.041028432068},{"$f":"YN375-(XM375-XU375)*3.413","v":65895.534574474703},10.974455816888678,0.11069344329626918,-6.9017975001697422,-21.570757162252583,55.750295373008477,92111.849756991127,88858.64006365095,3253.2096933401735,0,92111.849756991127,1]
[2,"T2-55-T1ER-DMM","75T0055","T2-55-T1ER-DMM","1 finger","off","off","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/2/2014","1:49:02","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.2,0.9,3.7,0,null,null,null,null,null,null,null,null,null,957,1670,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 1F-open, tape around damper perimeter frame gaps, no compressor, 55/51 ambient,--2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm), unsealed cab, 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-55-T1E-DMM-SPWCT-SSR","Installed FM:SG:FD:LSV on 2 circuits: unsealed cab: dampers on S/R: AX38 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",74.941999999999993,1.9E-2,62,5.8999999999999997E-2,54.968000000000004,3.6999999999999998E-2,51.021000000000001,4.2999999999999997E-2,74.98,0.03,71.94,0.03,72.33,0.03,0.27300000000000002,5.0000000000000001E-3,1.7195,3.0000000000000001E-3,null,null,null,null,null,null,null,null,null,null,null,null,460.2,2.6,460.1,2.6,459.5,2.5,3.7,0,3.3,0,3.5,0,1624.6,21.3,1103.3,23.7,147,16.7,460,null,460,null,460,null,3.1,null,3.2,null,3.2,null,0.56999999999999995,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,null,0,null,0,null,105,null,1775,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,51.99,7.0000000000000007E-2,52.53,0.11,59.77,0.05,53.41,0.06,71.58,0.03,71.760000000000005,0.03,71.900000000000006,0.04,71.989999999999995,0.03,72.319999999999993,0.22,72.11,0.03,52.38,0.1,73.08,0.02,72.31,0.03,55.04,7.0000000000000007E-2,57.06,0.04,51.88,0.08,73.180000000000007,0.03,72.83,0.03,56.83,0.06,null,null,null,null,56.87,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72.11,0.03,54.06,0.08,52.08,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.56,0.03,55.3,0.15,54.91,0.12,75.540000000000006,0.03,75.45,0.03,75.12,0.03,75.930000000000007,0.02,75.900000000000006,0.03,75.83,0.03,75.64,0.03,65.709999999999994,0.15,63.97,0.15,64.260000000000005,0.31,66.400000000000006,0.17,66.58,0.13,65.77,0.16,69.28,0.12,69.73,0.08,73.02,0.19,68.900000000000006,0.14000000000000001,74.25,7.0000000000000007E-2,74.540000000000006,0.03,74.12,0.15,73.09,7.0000000000000007E-2,74.540000000000006,0.04,74.81,0.03,74.67,0.02,74.55,0.03,73.790000000000006,0.04,null,null,75.25,0.03,75.89,0.03,75.66,0.03,75.47,0.03,75.3,null,75.13,0.03,null,null,64.52,0.13,67.290000000000006,0.13,74.55,0.04,74.760000000000005,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.941999999999993,1.9E-2,62,5.8999999999999997E-2,71.870999999999995,3.5000000000000003E-2,60.241,6.3E-2,54.968000000000004,3.6999999999999998E-2,51.021000000000001,4.2999999999999997E-2,3090.2,2.7,2978.4,2.7,0.65600000000000003,3.0000000000000001E-3,-0.22500000000000001,4.0000000000000001E-3,0.27300000000000002,5.0000000000000001E-3,1.7195,3.0000000000000001E-3,29.395,0,1772,11,1670,null,7.9152898768398858E-2,235.74899369179917,13.029,0.22500000000000001,1.4875099604161586,13767.02569740579,229.53661077165356,235.74751831523383,1085.6572372903424,12681.368460115447,8.6528316940003187E-3,27.071723070833642,70.383490039583833,13.02883692298475,13.46783278213379,7.0000242987072097E-3,20.790186917957545,8.7943292237180719E-3,27.609487997948513,8.3803765763625897E-3,26.408043431465078,73.371605858186356,61.216583416072453,26.045506184193755]
[2,"T2-TRN-75A-55-T3E-DM-2","75T0212","T2-TRN-75A-55-T3E-DM-2","30% open","off","off",null,"unsealed","unsealed",null,null,null,null,null,"CUST 5","10/29/2014","23:58:09","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.6,0,3.2,0,6506,14,6116,50,3501,63,10011,64,9.3039033460000002,748,990,null,6.0464684010000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 30%-open (4.4V), tape around damper perimeter inside/outside frame gaps, no compressor,--55/51 ambient, 75% airflow (300 cfm/ton), 2 HP fan motor, 3 turns, 7.25\" AK74 pulley (725 rpm),--unsealed cab, 100% inlet/outlet Meriam, adjust code tester spee","W/ECO: 4.4 V No comp: 55/51 amb:2HP blwr mtr 7.25` AK74 mtr. pulley: 3 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.992999999999995,2E-3,62,1.9E-2,54.999000000000002,1.2999999999999999E-2,51.000999999999998,1.7999999999999999E-2,75.069999999999993,0.01,72.760000000000005,0.01,73.22,0,0.123,2E-3,1.1992,2E-3,6506,14,3501,63,9.3059999999999992,8.8999999999999996E-2,null,null,null,null,null,null,460.6,1.9,461.3,1.9,459.4,1.9,3.2,0,2.7,0,3.1,0,1286,14.6,1097.5,17.899999999999999,-10,0,460,null,460,null,460,null,2.7,null,2.8,null,2.7,null,0.39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,null,0,null,0,null,85,null,1075,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.39,0.02,58.6,0.01,57.01,0.01,-1.58,0.02,96.42,0.03,59.76,0.02,57.05,0.02,-2.71,0.03,null,null,71.180000000000007,0.02,null,null,null,null,96,0.01,70.75,0.02,56.8,0.01,13.95,0.02,95.65,0.03,61.27,0.02,56.61,0.01,4.66,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.8,0.03,60.62,0.08,57.24,0.02,3.39,0.08,97.44,0.03,57.6,0.02,0.05,0.25,null,null,72.010000000000005,0.14000000000000001,null,null,null,null,96.51,0.04,57.09,0.02,13.75,0.03,96.54,0.03,61.62,0.02,57.1,0.02,4.51,0.04,60.75,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.87,0.02,60.73,0.02,60.75,0.08,61.98,0.02,73,0.01,72.33,0.02,72.14,0.02,73.27,0.01,73.209999999999994,0.02,null,null,57.9,0.03,71.59,0.02,71.739999999999995,0.02,61.37,0.02,61.35,7.0000000000000007E-2,57.72,0.16,72.58,0.12,72.05,0.02,63.65,0.04,71.180000000000007,0.02,72.010000000000005,0.14000000000000001,55.6,0.04,59.59,0.02,61.64,0.02,58.62,0.09,59.53,0.06,60.73,0.02,61.98,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.6,0.01,57.55,0.25,59.87,0.02,60.75,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.84,0.02,null,null,null,null,null,null,null,null,null,null,null,null,60.09,0.02,56.61,0.11,55.96,0.04,75.5,0.01,73.08,0.04,74.94,0.02,74.069999999999993,0.04,75.91,0.9,75.989999999999995,0.02,75.569999999999993,0.02,67.430000000000007,0.1,70.209999999999994,0.17,71.39,0.05,69.319999999999993,0.14000000000000001,67,0.12,70.5,0.08,71.180000000000007,0.03,70.98,0.05,68.739999999999995,0.1,70.05,0.08,68.260000000000005,0.11,74.34,0.03,74.41,0.03,74.63,0.02,74.53,0.03,74.75,0.02,74.709999999999994,0.01,71.849999999999994,0.15,70.23,0.09,null,null,73.45,0.06,75.92,0.02,75.75,0.02,75.06,0.02,73.510000000000005,null,75.16,0.02,64.44,0.09,null,null,66.75,0.12,67.349999999999994,0.16,74.48,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.992999999999995,2E-3,62,1.9E-2,72.534000000000006,5.0000000000000001E-3,60.674999999999997,1.7999999999999999E-2,54.999000000000002,1.2999999999999999E-2,51.000999999999998,1.7999999999999999E-2,2432.5,2,2345.8000000000002,1.9,0.40400000000000003,2E-3,-0.16400000000000001,1E-3,0.123,2E-3,1.1992,2E-3,29.475999999999999,1E-3,1076,8,990,null,6.5469640892267159E-2,153.5786836050803,13.029,0.16400000000000001,1.1542145576017429,10822.655484503068,111.33647042519686,153.58152682008247,707.23389566066692,10115.421588842401,8.6646425928409692E-3,27.162386969573163,71.379785442398259,13.029482418396816,13.485599741115793,6.9821094129436387E-3,20.778278098940707,8.7822792612631401E-3,27.60874090027631,8.5011367654739024E-3,26.701646033809027,73.69044406082503,61.350652874676541,26.420277951684582]
[2,"T2-TRN-100A-55-OE-DM","75T0020","T2-TRN-100A-55-OE-DM","open","off","off","3 turns","unsealed","unsealed",950,5.75,null,0,0,"CUST 5","10/28/2014","4:33:32","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.1,0,3.7,0,42708,116,42141,389,22562,216,65291,218,37.740462428000001,945,null,null,24.686705201999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo fully open, no compressor, 55/51 ambient, 2 HP fan motor, 100% airflow (400 cfm/ton),--3 turns, 5.75\" pulley, (950 rpm), unsealed cab, 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-TRN-100A-55-OE-DM-SPWCT-SSR","W/ECO:  2 V No comp: 55/51 amb:2HP blwr mtr 5.75` AK59 mtr. pulley: 3 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.968999999999994,1.2E-2,62.015000000000001,3.5999999999999997E-2,55.006,1.7000000000000001E-2,50.962000000000003,0.02,74.930000000000007,0.12,62.54,0.06,64.739999999999995,0.03,0.18,5.0000000000000001E-3,1.9576,3.3E-3,42708,116,22562,216,37.744,0.27200000000000002,null,null,null,null,null,null,460.1,2,461,2,459.9,2,3.7,0,3.2,0,3.5,0,1599.8,14.4,1098.8,17.7,130.19999999999999,10.3,460,null,460,null,460,null,3.2,null,3.3,null,3.1,null,0.56000000000000005,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.5,null,0,null,0,null,85,null,1725,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97.06,7.0000000000000007E-2,59.8,0.06,57.32,0.04,-2.4700000000000002,7.0000000000000007E-2,97.56,0.1,59.36,0.06,57.6,0.06,-1.76,0.04,null,null,62.61,0.04,null,null,null,null,97.42,0.09,59.96,0.04,57.53,0.05,2.4300000000000002,7.0000000000000007E-2,97.36,0.09,66.150000000000006,0.03,57.49,0.05,8.66,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98.15,0.09,56.99,0.06,57.92,0.04,-0.94,0.03,97.17,0.1,57.38,0.05,-4.54,7.0000000000000007E-2,null,null,60.21,0.03,null,null,null,null,94.64,0.23,55.97,0.13,3.34,0.17,94.94,0.23,62.63,0.04,56.14,0.13,6.49,0.1,60.73,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.9,0.05,61.45,0.05,60.73,0.12,61.01,0.08,62.89,7.0000000000000007E-2,62.34,0.06,62,7.0000000000000007E-2,62.79,0.06,62.55,0.06,null,null,58.29,0.05,62.28,0.06,60.63,0.05,65.59,0.04,57.58,0.05,61.98,0.1,60.79,0.02,60.55,0.05,63.22,0.05,62.61,0.04,60.21,0.03,55.26,0.2,61.25,0.09,62.35,0.03,60.86,0.16,60.97,0.23,61.45,0.05,61.01,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.8,0.06,61.93,0.09,60.9,0.05,60.73,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.31,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,59.37,0.06,58.98,0.36,56.91,0.11,75.27,0.05,74.77,0.05,74.87,0.06,75.650000000000006,0.06,75.67,0.06,75.66,0.06,75.44,7.0000000000000007E-2,54.54,0.1,58.07,0.12,59.05,0.18,54.5,0.12,59.03,0.24,62.29,0.15,58.87,0.21,60.55,0.23,61.81,0.13,62.42,0.13,60.63,0.2,59.21,0.17,62.72,0.13,61.36,0.12,59.89,0.13,63.69,0.19,65.040000000000006,0.21,64.47,0.14000000000000001,65.33,0.16,null,null,75.040000000000006,7.0000000000000007E-2,75.680000000000007,0.05,75.53,0.06,75.33,0.06,74.930000000000007,null,75,0.06,54.57,0.12,null,null,57.37,0.15,58.26,0.16,62.4,0.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.968999999999994,1.2E-2,62.015000000000001,3.5999999999999997E-2,62.411000000000001,3.6999999999999998E-2,54.856000000000002,3.9E-2,55.006,1.7000000000000001E-2,50.962000000000003,0.02,3100.3,2.6,3018.6,2.5,0.51300000000000001,3.0000000000000001E-3,-0.15,5.0000000000000001E-3,0.18,5.0000000000000001E-3,1.9576,3.3E-3,29.228999999999999,1E-3,1730,11,1640,null,0.55542754095075864,1676.61357511396,13.029,0.15,1.4731908096441226,14070.812831215693,181.92317839370079,1676.6448282680233,7720.848825892077,6349.9640053236162,7.7892557586590819E-3,23.853432634343317,60.937809190355878,13.029485742386374,13.220131788500833,6.9597498902351524E-3,20.755710266632747,8.7978424852802328E-3,27.61991793813819,7.3632314512683374E-3,22.995067277114373,64.031597931449639,56.249862144835561,22.636685217262723]
[2,"T2-CBASE-3000-95-CE","75T0029","T2-CBASE-3000-95-CE","closed","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/15/2014","13:21:55","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460.1,1.3,15.1,0,57427,68,57232,586,8295,124,65729,123,7.6553692056836713,949,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Factory charge, 2 HP fan motor, 3 turns, 5.75\" AK59 pulley (939 rpm), Econo closed unsealed cab,--adjust code tester speed to match total static of run T2-C-3000-95-CE-SPWCT-SS. Both stages.","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6: .;Added 20.5 oz in circuit #1",74.909000000000006,1.6E-2,62.195,1.9E-2,94.971999999999994,2.5000000000000001E-2,75.007000000000005,8.9999999999999993E-3,74.739999999999995,0.18,57.51,0.02,60.12,0.01,0.28299999999999997,3.0000000000000001E-3,1.2804,3.0999999999999999E-3,57427,68,8295,124,7.6559999999999997,2.5000000000000001E-2,null,null,null,null,null,null,460.1,2.6,460,2.6,459.9,2.6,15.1,0.1,13.3,0,13,0.1,6837.5,61.8,3320.1,72.599999999999994,1747.9,52.2,460,null,460,null,460,null,3.1,null,3.2,null,3.2,null,0.56999999999999995,460,null,460,null,460,null,4.7,null,4.9000000000000004,null,4.4000000000000004,null,3170,null,0.86,460,460,460,4.9000000000000004,4.7,4.4000000000000004,3000,0.81,459.2,null,1.6,null,697.7,null,85,null,8582.7000000000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,215.95,0.24,106.58,0.09,106.6,0.08,0.02,0.06,245.94,0.26,174.25,0.22,115.86,7.0000000000000007E-2,-58.39,0.21,208.9,0.05,98.87,0.13,104.28,0.03,5.41,0.12,76.180000000000007,0.05,51.57,0.41,44.88,0.03,6.69,0.41,75.599999999999994,0.05,58.11,0.13,44.5,0.03,13.61,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,248.1,0.27,170.3,0.3,116.49,0.08,53.81,0.34,230.57,0.39,111.21,0.12,11.14,0.19,221,0.39,99.79,0.17,108.21,0.12,8.42,0.19,78.44,0.18,46.32,0.11,3.3,1.0900000000000001,77.62,0.2,57.49,0.63,45.81,0.13,11.68,0.67,104.92,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105.36,0.1,104.92,0.1,100.92,0.15,101.26,0.14000000000000001,57.57,0.04,57.34,0.04,null,null,57.6,0.04,57.58,0.03,57.5,0.04,105.63,0.09,100.04,0.08,52.47,0.5,58.11,0.16,169.7,0.33,101.19,0.15,100.22,0.14000000000000001,49.45,0.19,59.02,0.97,98.87,7.0000000000000007E-2,99.79,0.14000000000000001,94.11,0.08,106.23,0.1,105.83,0.13,101.48,0.1,101.65,0.11,100.92,0.15,101.26,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,106.58,0.09,57.5,0.04,null,null,100.07,0.17,105.36,0.1,104.92,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,49.65,1,null,null,null,null,null,null,null,null,null,null,null,null,174.86,0.09,94.63,0.09,95.33,0.2,75.42,0.09,75.22,0.09,75.06,0.08,75.650000000000006,0.06,75.650000000000006,0.09,75.540000000000006,0.09,75.36,0.1,79.77,0.09,79.930000000000007,0.09,77.62,0.1,75.5,0.12,77.2,0.12,77.989999999999995,0.09,77.8,0.08,77.58,0.09,75.53,0.09,76.650000000000006,0.1,75.09,0.11,75.28,0.11,74.91,0.11,76.09,0.1,75.56,0.1,75.430000000000007,0.1,75.34,0.09,null,null,75.88,0.08,null,null,75.02,0.09,75.64,0.08,75.44,0.1,75.260000000000005,0.11,75.19,null,75.08,0.11,79.760000000000005,0.11,80.63,0.09,76.44,0.11,75.47,0.11,75.25,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-100A-55-CE-DM-2",74.909000000000006,1.6E-2,62.195,1.9E-2,57.621000000000002,8.9999999999999993E-3,54.875,1.4999999999999999E-2,94.971999999999994,2.5000000000000001E-2,75.007000000000005,8.9999999999999993E-3,3027.7,3.7,2976.9,3.6,0.64900000000000002,3.0000000000000001E-3,-0.28799999999999998,2E-3,0.28299999999999997,3.0000000000000001E-3,1.2804,3.0999999999999999E-3,29.3,0,8586,22,1630,null,0,0,13.029,0.27900000000000003,1.4392207837649749,13859.144159344358,226.97292009448819,0,0,13859.144159344358,8.9309937669419977E-3,27.750985631292469,56.181779216235029,14.099307472312812,13.107735796046008,1.3933618024463927E-2,38.164395509488834,8.9309937669419977E-3,27.750985631292469,8.5035590166049769E-3,23.068868823516414,74.909000000000006,62.195007642160107,22.718021941913353,69752.569319850809,62290.380611056469,6956,0.34035775644530447,64964.037896133297,57501.849187338958,7.566275086901153,0.16480852247439515,-5.0329636893791161,-18.727220783764977,52.48633251870875,69752.569319850809,64890.131809857558,4862.4375099932504,0,69752.569319850809,1]
[2,"T2-R-3000-115-CE","75T0167","T2-R-3000-115-CE","closed","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/16/2014","1:44:58","10 Ton","0:15:00","75/62 115/80","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,115,80,6.4,6.2,6.4,6.2,460.8,1,16.8,0,45413,60,45304,438,2445,242,47860,256,4.7574552680000002,949,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Restriction 115F OAT (leave restriction from run T2-R-3000-95-CE only move outdoor room conditions),--2 HP fan motor, 3 turns, 5.75\" AK59 pulley (939 rpm), Econo closed unsealed cab,--adjust code tester speed to match total static of run T2-C-3000-95-CE-S","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6: .;",74.882000000000005,6.0000000000000001E-3,62.119,4.9000000000000002E-2,114.952,1.7000000000000001E-2,80.007999999999996,2.3E-2,74.819999999999993,0.14000000000000001,61.04,0.04,63.09,0.02,0.27200000000000002,5.0000000000000001E-3,1.2730999999999999,3.3999999999999998E-3,45413,60,2445,242,4.758,2.7E-2,null,null,null,null,null,null,460.8,2.5,460.6,2.5,459.2,2.5,16.8,0.1,14.9,0,14.5,0.1,7714.8,66.900000000000006,3334.8,69,2345.1,58.6,460,null,460,null,460,null,3.2,null,3.2,null,3.1,null,0.56000000000000005,460,null,460,null,460,null,4.9000000000000004,null,5.7,null,5.3,null,3820,null,0.85,460,460,460,5.8,5.4,5.3,3790,0.85,459.9,null,1.6,null,683.3,null,85,null,10008.299999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,290.06,0.25,116.08,0.1,128.13999999999999,0.06,12.06,0.08,301.95999999999998,0.27,242.02,7.0000000000000007E-2,131.22,7.0000000000000007E-2,110.8,0.06,177.13,0.05,89.37,0.06,93.17,0.05,3.74,0.05,63.88,0.04,71.83,0.04,36.47,0.03,35.35,0.04,63.5,0.05,76.56,0.04,36.200000000000003,0.03,40.369999999999997,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,311.72000000000003,0.27,194.7,0.2,133.69,0.06,61.02,0.2,295.56,0.35,129.57,0.09,11.97,0.11,283.17,0.05,116.05,0.12,126.31,0.05,10.220000000000001,0.05,80.88,0.13,47.84,0.08,2.87,0.36,80.06,0.14000000000000001,59.3,0.42,47.33,0.09,11.97,0.43,95.16,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.23,7.0000000000000007E-2,95.16,7.0000000000000007E-2,117.5,0.13,117.77,0.13,61.18,0.05,60.91,0.04,null,null,61.3,0.05,61.24,0.04,61.13,0.04,116.18,7.0000000000000007E-2,90.67,0.08,72.33,0.06,76.790000000000006,0.05,191.61,0.22,118.14,0.13,116.43,0.12,51.21,7.0000000000000007E-2,60.93,0.83,89.37,0.06,116.05,0.12,114.41,0.04,116.69,7.0000000000000007E-2,96.27,0.06,117.87,0.1,118.78,0.08,117.5,0.13,117.77,0.13,null,null,null,null,null,null,null,null,null,null,null,null,116.08,0.1,61.13,0.04,null,null,117.6,0.13,96.23,7.0000000000000007E-2,95.16,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50.7,0.3,null,null,null,null,null,null,null,null,null,null,null,null,243.67,0.08,114.61,0.16,114.87,0.15,75.47,7.0000000000000007E-2,75.27,7.0000000000000007E-2,75.08,0.06,75.78,0.05,75.790000000000006,7.0000000000000007E-2,75.7,0.08,75.489999999999995,0.08,88.06,0.17,89.52,0.31,82.05,0.13,78.849999999999994,0.11,81.42,0.11,80.91,0.11,79.5,0.09,80.650000000000006,0.1,78.760000000000005,0.1,80.63,0.12,75.5,0.09,75.38,0.08,75.42,0.09,76.739999999999995,0.09,76.36,0.08,75.569999999999993,7.0000000000000007E-2,75.66,0.05,null,null,82.75,0.35,null,null,75.11,7.0000000000000007E-2,75.7,0.06,75.48,7.0000000000000007E-2,75.27,0.08,75.14,null,75.05,7.0000000000000007E-2,85.1,1.03,86.78,0.14000000000000001,80.8,0.11,75.650000000000006,0.09,75.33,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-100A-55-CE-DM-2",74.882000000000005,6.0000000000000001E-3,62.119,4.9000000000000002E-2,61.067999999999998,1.2999999999999999E-2,56.850999999999999,3.3000000000000002E-2,114.952,1.7000000000000001E-2,80.007999999999996,2.3E-2,3031,4.0999999999999996,2955.1,4,0.65300000000000002,3.0000000000000001E-3,-0.28799999999999998,2E-3,0.27200000000000002,5.0000000000000001E-3,1.2730999999999999,3.3999999999999998E-3,29.239000000000001,0,10060,21,1630,null,0,0,13.029,0.27900000000000003,1.4478093749083483,13779.615263263959,226.69944941732285,0,0,13779.615263263959,8.8870840297790837E-3,27.696350441680764,59.620190625091652,14.605948534828498,13.197755998662263,1.3786321216898149E-2,42.919402558385983,8.8870840297790837E-3,27.696350441680764,8.8447981895012941E-3,24.280470435372262,74.882000000000005,62.119007862956515,23.927310507102618,51935.920210364413,50472.446737802908,8430,0.55398248232556202,47146.455431225739,45682.981958664233,4.6865263848136918,0.27777192703552467,-3.7690399345781458,-15.261809374908353,53.750435129827693,51935.920210364413,47069.512272406821,4866.4079379575915,0,51935.920210364413,1]
[2,"T2-TRN-63A-55-3E-DM-2","75T0061","T2-TRN-63A-55-3E-DM-2","30% open","off","off","5.5 turns","unsealed","unsealed",620,7.25,null,0,0,"CUST 5","10/30/2014","3:21:59","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.4,0,3.1,0,6808,16,6491,41,3347,82,10158,79,12.745294855999999,634,710,null,8.5420326220000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 30%-open (4.4V), no compressor, 55/51 ambient, 62.5% airflow (250 cfm/ton),--2 HP fan motor, 5.5 turns, 7.25\" AK74 pulley (620 rpm), unsealed cab, 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-TRN-63A-55-3E-DM-2","W/ECO: 4.4 V No comp: 55/51 amb:2HP blwr mtr 7.25` AK74 mtr. pulley: 5.5 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.995000000000005,8.0000000000000002E-3,61.997999999999998,0.03,54.984999999999999,0.01,51.006999999999998,1.6E-2,75.099999999999994,0.02,72.17,0.01,72.95,0.02,7.8E-2,2E-3,0.84140000000000004,1.4E-3,6808,16,3347,82,12.750999999999999,0.16300000000000001,null,null,null,null,null,null,460.4,2,461.5,2,459.5,2,3.1,0,2.6,0,3,0,1151.7,15.3,1110.0999999999999,19.600000000000001,-10,0,460,null,460,null,460,null,2.6,null,2.6,null,2.5,null,0.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,null,0,null,0,null,85,null,795,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.18,0.01,58.67,0.03,56.9,0.01,-1.76,0.03,95.75,0.01,59.62,0.03,56.66,0,-2.97,0.02,null,null,71.66,0.02,null,null,null,null,95.85,0.01,70.650000000000006,0.01,56.72,0.01,13.93,0.01,95.57,0.03,61.1,0.03,56.56,0.01,4.54,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96.77,0.03,60.7,0.05,57.24,0.01,3.46,0.05,97.34,0.03,57.55,0.01,0.38,0.12,null,null,71.680000000000007,7.0000000000000007E-2,null,null,null,null,96.42,0.02,57.04,0.01,13.8,0.03,96.41,0.02,61.56,0.02,57.03,0.01,4.53,0.02,60.44,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.93,0.02,60.72,0.02,60.44,0.12,62.03,0.03,72.47,0.02,71.72,0.02,71.430000000000007,0.02,72.69,0.01,72.59,0.02,null,null,58.11,0.03,72.180000000000007,0.01,71.66,0.01,61.24,0.02,61.42,0.04,57.47,0.08,72.209999999999994,0.06,72.06,0.02,63.54,0.03,71.66,0.02,71.680000000000007,7.0000000000000007E-2,55.66,0.02,59.76,0.01,61.64,0.01,58.46,0.03,59.4,0.06,60.72,0.02,62.03,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.67,0.03,57.18,0.12,59.93,0.02,60.44,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.84,0.03,null,null,null,null,null,null,null,null,null,null,null,null,59.97,0.04,56.54,0.1,55.96,0.04,75.45,0.02,72.89,0.05,74.91,0.02,73.900000000000006,0.04,76.069999999999993,1.39,75.91,0.02,75.5,0.02,65.87,0.11,67.11,0.25,70.13,0.08,69.36,0.13,65.97,0.11,68.239999999999995,0.11,70.17,0.06,70.319999999999993,7.0000000000000007E-2,68.23,0.1,69.09,0.09,67.87,0.13,74.44,0.04,74.44,0.04,74.569999999999993,0.03,74.48,0.03,74.83,0.02,74.75,0.02,72.36,0.16,70.95,0.09,null,null,73.36,0.06,75.83,0.02,75.680000000000007,0.02,75.010000000000005,0.03,73.36,null,75.09,0.02,63.77,0.08,null,null,65.8,0.14000000000000001,66.39,0.18,74.58,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.995000000000005,8.0000000000000002E-3,61.997999999999998,0.03,71.921000000000006,8.0000000000000002E-3,60.378,2.8000000000000001E-2,54.984999999999999,0.01,51.006999999999998,1.6E-2,2034.6,1.6,1962.6,1.6,0.27500000000000002,2E-3,-0.115,1E-3,7.8E-2,2E-3,0.84140000000000004,1.4E-3,29.47,0,797,8,710,null,0.10314842578710634,202.43910044977488,13.029,0.115,1.0142786619365931,9063.0053664890911,63.405888188976377,202.44048617081032,932.24828339039755,8130.7570830986933,8.5961676836358528E-3,26.905191015212107,70.90672133806342,13.029178370889056,13.469704040050779,6.9885879275144742E-3,20.781906564287162,8.7804879692796791E-3,27.607268492099461,8.4558354863688741E-3,26.502701002980096,72.942736144914562,60.972570169754292,26.25546612548013]
[2,"T2-MF21-115C1-115C2-63A-95-CE","75T0035","T2-MF21-115C1-115C2-63A-95-CE","closed","on","on","3 turns","unsealed","unsealed",650,9.25,null,0,0,"CUST 5","10/8/2014","1:00:19","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 7.36 lbs/CK2- 7.13 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,7.36,7.13,6.4,6.2,461.2,1.4,14.7,0,52203,59,51484,238,19179,107,71401,141,9.1434242539999993,648,null,null,6.6849788710000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MF21, 115% charge CK1 and CK2, 62.5% airflow (250 cfm/ton), closed damper, 2 HP fan motor,--3 turns, 9.25\" AK94 pulley (650 rpm), adjust code tester speed to match total static of run--T2-MF20-115C1-100C2-63A-95-CE-SPWCT-SS","With econo: both stages: 95/75 amb: 2 HP blower motor: 9.25` mtr. pulley: 3 turns open: AX 38 belt: 100% inlet-outlet Meriam",74.984999999999999,1.0999999999999999E-2,62.000999999999998,0.02,95,1.2E-2,74.998000000000005,2.1999999999999999E-2,74.849999999999994,0.1,51.74,0.06,57.28,0.02,0.08,2E-3,1.5194000000000001,2.3E-3,52203,59,19179,107,9.1430000000000007,2.9000000000000001E-2,null,null,null,null,null,null,461.2,2.6,461.9,2.6,458.9,2.6,14.7,0.1,12.3,0,12.1,0.1,6632,55.8,3158.4,64.099999999999994,1177,41.5,460,null,460,null,460,null,2.7,null,2.7,null,2.6,null,0.32,460,null,460,null,460,null,5.0999999999999996,null,4.8,null,4.4000000000000004,null,3140,null,0.83,460,460,460,5.2,4.5999999999999996,4.4000000000000004,3110,0.82,460.3,null,1.6,null,702.5,null,85,null,7807.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,227.15,0.12,98.81,0.08,110.15,0.04,11.33,0.08,245.66,0.13,175.52,0.12,115.77,0.04,59.75,0.13,221.6,0.05,97.36,0.05,108.4,0.05,11.08,0.05,69.56,0.05,44.1,0.19,40.47,0.03,3.63,0.2,68.98,0.05,50.95,0.25,40.08,0.03,10.87,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,255.51,0.13,178.54,0.14000000000000001,118.64,0.04,59.89,0.15,242.15,0.22,114.74,7.0000000000000007E-2,17.14,0.08,232.5,0.05,91.52,0.04,111.8,0.05,20.28,0.05,71.069999999999993,0.13,41.49,0.09,2.79,0.35,70.73,0.11,52.61,0.2,41.27,7.0000000000000007E-2,11.34,0.21,97.33,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98.93,0.08,98.8,0.06,97.33,0.05,97.71,7.0000000000000007E-2,50.9,7.0000000000000007E-2,51.48,0.05,51.37,0.04,51.18,0.05,51.28,0.04,null,null,98.34,0.05,96.89,7.0000000000000007E-2,44.93,0.42,50.63,0.27,178.59,0.17,95.04,0.06,91.08,0.03,44.31,0.24,54.46,0.28000000000000003,97.36,0.05,97.6,7.0000000000000007E-2,93.08,0.2,98.61,0.1,99.28,0.06,98.05,0.05,98.37,0.05,98.8,0.06,97.71,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98.81,0.08,97.6,7.0000000000000007E-2,98.93,0.08,97.33,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,44.26,0.27,null,null,null,null,null,null,null,null,null,null,null,null,176.54,0.16,95.36,0.08,95.29,0.09,75.2,0.06,75.72,0.04,75.12,0.06,75.83,0.06,75.599999999999994,0.06,75.760000000000005,7.0000000000000007E-2,75.55,0.06,78.430000000000007,7.0000000000000007E-2,76.81,0.05,76.709999999999994,0.05,77.36,7.0000000000000007E-2,77.59,7.0000000000000007E-2,77.349999999999994,0.06,76.569999999999993,7.0000000000000007E-2,75.72,0.06,75.55,0.1,75.67,7.0000000000000007E-2,75.16,7.0000000000000007E-2,75.37,0.06,75.3,0.06,75.64,0.11,76.849999999999994,0.09,75.459999999999994,0.06,76.34,0.08,80.39,0.19,80.41,0.24,null,null,75.14,0.06,75.17,0.06,75.59,7.0000000000000007E-2,75.38,7.0000000000000007E-2,75.569999999999993,null,75.19,0.06,80.08,0.06,80.25,7.0000000000000007E-2,77.900000000000006,0.06,75.510000000000005,7.0000000000000007E-2,75.37,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-63A-55-CE-DM-2",74.984999999999999,1.0999999999999999E-2,62.000999999999998,0.02,51.542000000000002,5.0000000000000001E-3,49.417000000000002,0.01,95,1.2E-2,74.998000000000005,2.1999999999999999E-2,1989.8,1.5,1969.2,1.5,0.29199999999999998,2E-3,-0.13900000000000001,1E-3,0.08,2E-3,1.5194000000000001,2.3E-3,29.273,1E-3,7809,20,770,null,2.7204080612091459E-2,52.397779666949354,13.029,0.13200000000000001,1.0825476805035341,9224.9701323770551,67.551932976377955,55.93527424730334,238.0241551186682,8986.9459772583868,8.9173021799355007E-3,27.881679205151755,50.459452319496471,14.09989861392425,12.941830519427009,1.3919025299848052E-2,38.155190330286374,8.7848288210472473E-3,27.609579671912055,6.9648053006300609E-3,19.919125541661948,75.506131304171333,62.387094506305814,19.655966456523529,75881.954423608549,55453.167731726797,7039,0.31659842162058982,73484.499170856929,53055.712478975176,9.4102316776612795,0.14504871563588359,-8.2257127486282258,-25.046678984674863,46.210100708341855,75881.954423608549,70944.209655972998,2427.634700465585,2510.1100671699696,75881.954423608549,1]
[2,"T2-MF6-115C1-115C2-63A-95-CCE","75T0044","T2-MF6-115C1-115C2-63A-95-CCE","closed","on","on","3 turns","unsealed","unsealed",650,9.25,null,30,0,"CUST 5","10/10/2014","19:41:42","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 7.36 lbs/CK2: 7.13 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,7.36,7.13,6.4,6.2,461.2,1.4,15.5,0,51917,66,50493,250,18894,114,70829,150,8.2388042339999998,648,null,null,6.0389670820000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MF6, 115% charge CK1 and CK2, 62.5% airflow (250 cfm/ton), 30% condenser coil blockage,--2 HP fan motor, 3 turns, 9.25\" AK94 pulley (650 rpm), adjust code tester speed to match--total static of run T2-MF2-100C1-100C2-63A-95-CCE-SPWCT-SS","With econo: both stages: 95/75 amb: 2 HP blower motor: 9.25` mtr. pulley: 3  turns open: AX 38 belt: 100% inlet-outlet Meriam: condenser coil blocked 33.5` of 62` coil",75.004000000000005,1.4E-2,61.999000000000002,1.7999999999999999E-2,94.983999999999995,3.6999999999999998E-2,75.001000000000005,0.04,74.430000000000007,0.1,51.62,0.05,58.01,0.02,5.7000000000000002E-2,2E-3,0.81569999999999998,1.6999999999999999E-3,51917,66,18894,114,8.2390000000000008,2.4E-2,null,null,null,null,null,null,461.2,2.6,462,2.6,458.9,2.6,15.5,0.1,13.1,0,12.9,0.1,7054.6,55.3,3160.1,63.4,1542.5,41.8,460,null,460,null,460,null,2.7,null,2.7,null,2.6,null,0.32,460,null,460,null,460,null,5.5,null,5.2,null,4.8,null,3540,null,0.85,460,460,460,5.6,5.0999999999999996,4.9000000000000004,3500,0.84,460.2,null,1.6,null,695.4,null,85,null,8590.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,258.61,0.27,104.82,7.0000000000000007E-2,119.51,0.08,14.69,0.1,277.52,0.19,190.45,0.21,124.78,0.05,65.680000000000007,0.22,253.2,0.05,103.66,7.0000000000000007E-2,117.96,0.05,14.253333333,0.05,70.180000000000007,0.12,44.08,0.27,40.86,0.08,3.22,0.34,69.63,0.13,51.59,0.62,40.49,0.09,11.11,0.68,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,291.61,0.25,195.29,0.22,128.54,7.0000000000000007E-2,66.760000000000005,0.23,279.02,0.38,125.18,0.1,23.62,0.1,268.8,0.05,96.22,0.05,122.38,0.05,26.103333332999998,0.05,71.709999999999994,0.18,41.89,0.12,2.37,0.56999999999999995,71.400000000000006,0.13,53.79,0.49,41.69,0.09,12.1,0.48,101.99,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105.43,0.09,105.7,0.08,101.99,7.0000000000000007E-2,102.58,0.06,50.81,0.05,51.48,0.05,51.41,0.05,51.17,0.04,51.26,0.04,null,null,105.14,0.08,101.73,0.09,44.77,0.74,51.94,0.65,195.37,0.28000000000000003,101.95,0.06,95.36,0.05,44.9,0.43,55.35,0.57999999999999996,103.66,7.0000000000000007E-2,96.22,0.05,93.37,0.19,105.81,0.08,106.04,0.08,103.61,7.0000000000000007E-2,104.04,7.0000000000000007E-2,105.7,0.08,102.58,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.82,7.0000000000000007E-2,101.57,0.06,105.43,0.09,101.99,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,44.27,0.47,null,null,null,null,null,null,null,null,null,null,null,null,191.64,0.27,94.23,0.1,93.77,0.12,74.650000000000006,0.06,75.27,0.05,74.63,0.06,75.319999999999993,0.06,75.06,0.05,75.22,7.0000000000000007E-2,75.040000000000006,0.06,78.099999999999994,0.09,76.319999999999993,0.06,76.150000000000006,7.0000000000000007E-2,77.069999999999993,0.09,77.14,7.0000000000000007E-2,76.81,0.05,75.989999999999995,7.0000000000000007E-2,75.209999999999994,0.06,75.02,7.0000000000000007E-2,75.180000000000007,7.0000000000000007E-2,74.709999999999994,7.0000000000000007E-2,74.87,0.06,74.81,0.06,74.930000000000007,0.06,75.290000000000006,0.06,75,0.06,74.760000000000005,0.05,76.14,7.0000000000000007E-2,76.239999999999995,0.09,null,null,74.680000000000007,0.06,74.77,0.06,75.19,7.0000000000000007E-2,75.03,7.0000000000000007E-2,75.27,null,74.790000000000006,7.0000000000000007E-2,77.48,0.25,79.77,0.08,77.540000000000006,0.08,75.040000000000006,7.0000000000000007E-2,74.86,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-63A-55-CE-DM-2",75.004000000000005,1.4E-2,61.999000000000002,1.7999999999999999E-2,51.548000000000002,8.0000000000000002E-3,49.472999999999999,1.6E-2,94.983999999999995,3.6999999999999998E-2,75.001000000000005,0.04,1984.6,2.1,1954.3,2.1,0.29099999999999998,2E-3,-0.13900000000000001,1E-3,5.7000000000000002E-2,2E-3,0.81569999999999998,1.6999999999999999E-3,29.172999999999998,0,8597,19,770,null,2.7204080612091459E-2,52.397779666949354,13.029,0.13200000000000001,1.0865592744620138,9200.6031302697593,66.811207842519678,55.934573417516319,238.02713743189136,8962.5759928378684,8.9121641926670804E-3,27.88080879751449,50.46144072553799,14.099545292440784,12.942195018524696,1.392548554606441E-2,38.158378218058012,8.7790209387935362E-3,27.607858204862953,6.992328125089744E-3,19.950415736125521,75.525615255987901,62.38629325399711,19.686268185190006,75394.716008875315,55345.325434196406,7827,0.35431595759118362,72994.73266124184,52945.342086562923,8.4907214913623168,0.13946860743160716,-8.1945406123244844,-25.064174530449911,46.399223416124983,75394.716008875315,70453.089147726219,2430.3167839903931,2511.3100771587006,75394.716008875315,1]
[2,"T2-MFB3-100C1-100C2-90A-95-CE-3","75T0172","T2-MFB3-100C1-100C2-90A-95-CE-3","closed","on","on","4.5 turns","unsealed","unsealed",866,5.75,null,0,0,"CUST 5","11/4/2014","20:02:33","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460.2,0,14.9,0,57202,64,56963,564,9911,165,67122,150,8.1419213970000008,854,1310,null,6.9386220280000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo closed (2.0V), factory charge NC baseline, 90% airflow (350 cfm/ton),--4.5 turns, 5.75\" AK59 pulley (866 rpm), unsealed cab, adjust code tester speed--to match total static of run T2-MFB3-100C1-100C2-90A-95-CE-2-SPWCT-SS","W/ECO: 2.0 V With comps: 95/75 amb:2HP blwr mtr 5.75` AK59 mtr. pulley: 4.5 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.930999999999997,1.7999999999999999E-2,61.994999999999997,2.5000000000000001E-2,95.007999999999996,1.7000000000000001E-2,75.007999999999996,1.7999999999999999E-2,75.13,0.2,56.21,0.04,59.85,0.03,0.16,3.0000000000000001E-3,1.5277000000000001,2.5999999999999999E-3,57202,64,9911,165,8.1419999999999995,2.5000000000000001E-2,null,null,null,null,null,null,460.2,2.1,461.3,2.1,459.8,2.1,14.9,0,12.6,0,12.7,0.1,6756.6,43.2,3185,52.5,1487.8,34.1,460,null,460,null,460,null,2.9,null,3,null,2.9,null,0.5,460,null,460,null,460,null,5.0999999999999996,null,4.8,null,4.4000000000000004,null,3150,null,0.82,460,460,460,5,4.5999999999999996,4.2,2980,0.8,459.3,null,1.6,null,701.2,null,85,null,8226.2000000000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,221.12,0.24,106.31,0.12,108.29,0.08,1.99,0.11,248.3,0.28999999999999998,174.42,0.08,116.58,0.09,57.83,0.09,214.8,0.05,105.63,0.1,106.26,0.05,0.63,0.05,74.239999999999995,0.05,48.57,0.13,43.7,0.03,4.88,0.15,73.61,0.05,55.38,0.15,43.28,0.03,12.1,0.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,249.31,0.33,171.79,0.3,116.88,0.1,54.91,0.32,231.88,0.44,111.65,0.13,11.35,0.18,222.1,0.05,96.38,0.08,108.6,0.05,12.22,0.05,77.09,0.18,45.54,0.11,3.41,1.62,76.69,0.17,56.95,0.78,45.28,0.11,11.67,0.83,101.23,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106.6,0.11,106.3,0.09,101.23,0.13,101.45,0.12,55.45,0.05,56.1,0.05,56,0.05,55.82,0.04,55.87,0.04,null,null,106.16,0.12,102.2,0.12,49.54,0.34,55.22,0.18,172.1,0.35,101.3,0.13,95.25,7.0000000000000007E-2,50.33,1.4,57.83,0.76,105.63,0.1,96.38,0.08,92.57,0.16,106.75,0.1,107.05,0.11,101.92,0.09,102.27,0.1,106.3,0.09,101.45,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106.31,0.12,100.31,0.15,106.6,0.11,101.23,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48.94,1.5,null,null,null,null,null,null,null,null,null,null,null,null,175.36,0.11,94.65,0.28999999999999998,95.62,0.09,75.540000000000006,0.09,77.2,0.08,75.3,0.09,77.39,0.09,null,null,76,0.1,75.89,0.1,79.75,0.12,77.89,0.09,77.58,0.08,76.180000000000007,0.11,77.459999999999994,0.11,77.36,0.1,77.41,0.09,77.05,0.09,75.91,0.11,76.510000000000005,0.1,75.569999999999993,0.11,75.42,0.11,75.37,0.11,75.3,0.1,75.66,0.11,75.599999999999994,0.1,75.41,0.08,81.11,0.09,80.61,0.12,null,null,76.55,0.1,75.47,0.08,75.739999999999995,0.1,75.87,0.11,76.77,null,75.209999999999994,0.1,80.260000000000005,0.11,80.27,0.11,77.52,0.1,75.84,0.11,75.430000000000007,0.11,null,null,null,null,null,null,null,null,null,null,null,null,75.56,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-88A-55-CE-DM-2",74.930999999999997,1.7999999999999999E-2,61.994999999999997,2.5000000000000001E-2,55.933,1.4999999999999999E-2,53.573999999999998,2.1999999999999999E-2,95.007999999999996,1.7000000000000001E-2,75.007999999999996,1.7999999999999999E-2,2710.5,2.2999999999999998,2688.7,2.4,0.53200000000000003,2E-3,-0.247,2E-3,0.16,3.0000000000000001E-3,1.5277000000000001,2.5999999999999999E-3,29.533999999999999,3.0000000000000001E-3,8244,19,1310,null,0,0,13.029,0.23100000000000001,1.3039706214943789,12450.30305537867,168.0424797480315,0,0,12450.30305537867,8.7936313616371487E-3,27.606041397349138,54.629029378505621,14.100158600537428,13.062332641753811,1.3925874773698671E-2,38.164715997556094,8.7936313616371487E-3,27.606041397349134,8.1649979435433652E-3,22.289754434608948,74.931000000000012,61.995008738055425,21.972074254105632,{"$f":"(XZ443-YL443)*XT443","v":70144.598337427669},{"$f":"0.24*(YJ443-YA443)*XT443","v":60663.764846159909},{"$f":"XK443-XM443","v":6934},{"$f":"YO443*3.413/YM443","v":0.3373850953733733},{"$f":"YM443-(XM443-XU443)*3.413","v":66247.097320807705},{"$f":"YN443-(XM443-XU443)*3.413","v":56766.263829539937},{"$f":"YQ443/XK443","v":8.0357954052411085},{"$f":"(YA443-YW443)/(YJ443-YW443)","v":0.1392686230107533},{"$f":"-XZ443+YL443","v":-5.6339671432435061},{"$f":"-YJ443+YA443","v":-20.301970621494391},{"$f":"(-(-0.0182984848494437-(YU443/YV443))+SQRT((-0.0182984848494437-(YU443/YV443))^2-4*0.00577826340327261*(6.76723916086377-XZ443+(YU443/YV443)*YJ443)))/(2*0.00577826340327261)","v":51.344116607287319},{"$f":"XT443*(XZ443-YL443)","v":70144.598337427669},{"$f":"XT443*(YG443-YI443)","v":66189.383815473935},{"$f":"XT443*(YI443-YL443)","v":3955.2145219536887},{"$f":"XW443*(YE443-YG443)","v":0},{"$f":"SUM(YY443:ZA443)","v":70144.598337427626},{"$f":"ZB443/YX443","v":0.99999999999999933}]
[2,"T2-RC3-90C1-90C2-90A-95-CE","75T0189","T2-RC3-90C1-90C2-90A-95-CE","closed","on","on","4.5 turns","unsealed","unsealed",865,5.75,null,0,0,"CUST 5","11/7/2014","21:20:36","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 5.8 lbs/CK2: 5.6 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,5.8,5.6,6.4,6.2,460,0,14.7,0,55947,74,55998,382,8995,142,64951,167,7.9334310490000002,854,1320,null,6.8336386950000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RC3, 90% charge CK1 and CK2, 90% airflow, 360 cfm/ton, closed damper,--2 HP fan motor, 4.5 turns, 5.75\" AK59 pulley (865 rpm), adjust code tester--speed to match total static of run T2-RC3-90C1-90C2-90A-95-CE-SPWCT-SS","W/ECO: 2.0 V With comps: 95/75 amb:2HP blwr mtr 5.75` AK59 mtr. pulley: 4.5 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.962999999999994,1.0999999999999999E-2,61.993000000000002,2.5000000000000001E-2,95.010999999999996,1.4E-2,74.995000000000005,1.7999999999999999E-2,75.28,0.13,56.55,0.04,60.04,0.01,0.16300000000000001,3.0000000000000001E-3,1.5174000000000001,2E-3,55947,74,8995,142,7.9340000000000002,2.5999999999999999E-2,null,null,null,null,null,null,460,2,461.2,2,459.9,2,14.7,0.1,12.6,0,12.7,0,6689.8,43.6,3186.7,51.1,1497.2,33.9,460,null,460,null,460,null,2.9,null,3,null,2.9,null,0.5,460,null,460,null,460,null,5.0999999999999996,null,4.9000000000000004,null,4.4000000000000004,null,3140,null,0.82,460,460,460,5,4.5999999999999996,4.2,2920,0.8,459.2,null,1.6,null,699.1,null,85,null,8164.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,213.63,0.23,105.93,7.0000000000000007E-2,105.86,7.0000000000000007E-2,-7.0000000000000007E-2,0.06,246.03,0.24,178.46,0.08,115.89,7.0000000000000007E-2,62.57,0.08,203.5,0.05,102.61,7.0000000000000007E-2,102.5,0.05,-0.11,0.05,73.94,0.04,55.23,0.24,43.44,0.03,11.78,0.24,73.290000000000006,0.04,59.82,0.09,43.01,0.03,16.809999999999999,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,246.25,0.25,170.25,0.1,115.96,0.08,54.29,0.11,222.86,0.31,108.81,0.1,1.71,0.1,211.6,0.05,101.29,0.05,105.19,0.05,3.9,0.05,77.55,0.04,45.78,0.03,2.57,0.31,77.17,0.06,57.06,0.23,45.54,0.04,11.52,0.24,107.29,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.66,7.0000000000000007E-2,104.04,7.0000000000000007E-2,107.29,0.11,107.19,0.08,55.79,0.05,56.41,0.05,56.3,0.06,56.14,0.04,56.21,0.04,null,null,105.4,0.08,99.48,0.09,55.44,0.22,59.61,0.1,170.38,0.1,107.44,0.12,100.04,0.05,49.61,0.25,57.79,0.22,102.61,7.0000000000000007E-2,101.29,0.05,92.72,0.11,105.89,0.06,104.6,0.08,107.32,7.0000000000000007E-2,107.75,0.09,104.04,7.0000000000000007E-2,107.19,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105.93,7.0000000000000007E-2,107.1,0.13,104.66,7.0000000000000007E-2,107.29,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48.33,0.27,null,null,null,null,null,null,null,null,null,null,null,null,179.37,0.09,94.17,0.16,95.92,0.1,75.52,0.04,77.180000000000007,0.05,75.3,0.05,77.349999999999994,0.06,75.83,0.04,75.92,0.06,75.83,0.05,79.930000000000007,0.1,77.989999999999995,0.05,77.650000000000006,0.05,76.19,7.0000000000000007E-2,77.45,7.0000000000000007E-2,77.33,0.06,77.44,0.05,77.05,0.06,75.92,0.06,76.48,0.06,75.58,0.06,75.33,0.06,75.33,0.06,75.36,0.06,75.7,0.06,75.38,0.06,75.34,0.04,80.52,0.08,79.489999999999995,0.1,null,null,76.52,0.06,75.44,0.05,75.75,0.06,75.89,0.06,76.78,null,75.239999999999995,0.06,80.400000000000006,0.09,80.47,7.0000000000000007E-2,77.55,7.0000000000000007E-2,75.819999999999993,0.06,75.349999999999994,0.06,null,null,null,null,null,null,null,null,null,null,null,null,75.430000000000007,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-88A-55-CE-DM-2",74.962999999999994,1.0999999999999999E-2,61.993000000000002,2.5000000000000001E-2,56.253999999999998,1.4E-2,53.838999999999999,2.1999999999999999E-2,95.010999999999996,1.4E-2,74.995000000000005,1.7999999999999999E-2,2709.1,1.8,2671.5,1.8,0.53400000000000003,2E-3,-0.249,2E-3,0.16300000000000001,3.0000000000000001E-3,1.5174000000000001,2E-3,29.376999999999999,1E-3,8187,17,1320,null,0,0,13.029,0.23100000000000001,1.3174569164973511,12435.590805258071,167.59518519685042,0,0,12435.590805258071,8.784751907027594E-3,27.604129695955965,54.936543083502649,14.100134729781308,13.071031569426648,1.3913762492450486E-2,38.152092461237537,8.784751907027594E-3,27.604129695955965,8.2378663570528143E-3,22.447091547551079,74.962999999999994,61.993008927803906,22.126083140491595,68122.745375908373,59769.797638245909,6867,0.34404178620036246,64189.587742985226,55836.640005322763,7.8404284527892054,0.14216296461139685,-5.4780465554643705,-20.026456916497345,51.617707024364719,68122.745375908373,64130.816180668917,3991.9291952394574,0,68122.745375908373,1]
[2,"T2-RCB1-100C1-100C2-90A-95-CE-5","75T0196","T2-RCB1-100C1-100C2-90A-95-CE-5","closed","on","on","4.5 turns","unsealed","unsealed",865,5.75,null,0,0,"CUST 5","11/7/2014","19:05:50","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460.2,0,14.8,0,57018,63,57291,361,10020,140,67047,151,8.1111783210000006,854,1310,null,6.8978949920000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RCB1, 100% charge CK1 and CK2, 90% airflow, 360 cfm/ton, closed damper,--2 HP fan motor, 4.5 turns, 5.75\" AK59 pulley (865 rpm), adjust code tester speed to--match total static of run T2-RCB1-100C1-100C2-90A-95-CE-5-SPWCT-SS","W/ECO: 2.0 V With comps: 95/75 amb:2HP blwr mtr 5.75` AK59 mtr. pulley: 4.5 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.998999999999995,1.0999999999999999E-2,61.993000000000002,2.1999999999999999E-2,95.055999999999997,1.0999999999999999E-2,75.004000000000005,0.01,75.34,0.13,56.21,0.04,59.72,0.02,0.16500000000000001,3.0000000000000001E-3,1.5187999999999999,2.8999999999999998E-3,57018,63,10020,140,8.1110000000000007,2.3E-2,null,null,null,null,null,null,460.2,2.1,461.1,2.1,459.9,2.1,14.8,0.1,12.7,0,12.7,0,6731.8,45.1,3192.7,52.3,1534.5,33.799999999999997,460,null,460,null,460,null,2.9,null,3,null,2.9,null,0.49,460,null,460,null,460,null,5.0999999999999996,null,4.7,null,4.4000000000000004,null,3160,null,0.83,460,460,460,5,4.7,4.2,2960,0.8,459.4,null,1.6,null,699.3,null,85,null,8214.2999999999993,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220.88,0.24,107.18,0.12,108.19,0.08,1.02,0.11,248.5,0.25,174.58,0.14000000000000001,116.63,7.0000000000000007E-2,57.95,0.13,214,0.05,105.98,0.09,105.98,0.05,0,0.05,74.13,0.05,48.85,0.27,43.58,0.03,5.27,0.28000000000000003,73.48,0.05,55.1,0.22,43.15,0.04,11.94,0.23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250.15,0.24,171.87,0.25,117.11,7.0000000000000007E-2,54.76,0.26,231.96,0.33,111.66,0.1,10.28,0.13,221.8,0.05,96.5,0.06,108.48,0.05,11.98,0.05,77.03,0.08,45.46,0.05,2.35,0.44,76.75,0.09,56.18,0.65,45.29,0.06,10.9,0.69,101.64,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107.57,0.12,107.22,0.09,101.64,0.1,101.9,0.09,55.42,0.04,56.08,0.04,55.98,0.05,55.75,0.03,55.82,0.03,null,null,107.17,0.13,102.79,0.09,49.59,0.5,54.88,0.28000000000000003,172.01,0.27,101.82,0.09,95.36,7.0000000000000007E-2,49.06,0.32,56.95,0.55000000000000004,105.98,0.09,96.5,0.06,92.51,0.1,107.46,0.1,107.79,0.09,101.98,7.0000000000000007E-2,102.38,0.08,107.22,0.09,101.9,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107.18,0.12,101.37,0.11,107.57,0.12,101.64,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47.82,0.4,null,null,null,null,null,null,null,null,null,null,null,null,175.41,0.17,94.19,0.19,95.91,0.1,75.5,0.06,77.239999999999995,0.06,75.290000000000006,7.0000000000000007E-2,77.31,7.0000000000000007E-2,75.77,0.06,75.91,7.0000000000000007E-2,75.83,7.0000000000000007E-2,79.849999999999994,0.12,77.900000000000006,0.06,77.59,0.05,76.150000000000006,0.08,77.44,7.0000000000000007E-2,77.33,7.0000000000000007E-2,77.39,0.06,77,7.0000000000000007E-2,75.930000000000007,7.0000000000000007E-2,76.47,7.0000000000000007E-2,75.540000000000006,7.0000000000000007E-2,75.290000000000006,7.0000000000000007E-2,75.290000000000006,7.0000000000000007E-2,75.3,7.0000000000000007E-2,75.62,0.06,75.349999999999994,7.0000000000000007E-2,75.3,0.05,80.34,0.06,79.27,0.09,null,null,76.5,7.0000000000000007E-2,75.319999999999993,0.06,75.66,7.0000000000000007E-2,75.81,7.0000000000000007E-2,76.73,null,75.23,7.0000000000000007E-2,80.260000000000005,0.08,80.349999999999994,0.09,77.5,7.0000000000000007E-2,75.8,7.0000000000000007E-2,75.31,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,75.39,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-88A-55-CE-DM-2",74.998999999999995,1.0999999999999999E-2,61.993000000000002,2.1999999999999999E-2,55.963999999999999,8.0000000000000002E-3,53.561,1.6E-2,95.055999999999997,1.0999999999999999E-2,75.004000000000005,0.01,2708.3,2.6,2675.2,2.5,0.53300000000000003,3.0000000000000001E-3,-0.249,2E-3,0.16500000000000001,3.0000000000000001E-3,1.5187999999999999,2.8999999999999998E-3,29.404,0,8266,18,1310,null,0,0,13.029,0.23100000000000001,1.3057020930464398,12439.557736621511,167.5130194645669,0,0,12439.557736621511,8.7762462790981315E-3,27.603602406563734,54.658297906953557,14.101254776058258,13.063004605188899,1.3910875939936158E-2,38.159985999438142,8.7762462790981315E-3,27.603602406563734,8.1504100776034379E-3,22.281466612352098,74.998999999999995,61.993009133400903,21.963373058692056,70161.958620636826,60727.041141568603,6956,0.33837179672200712,66262.650556069391,56827.733077001169,8.0162896874025389,0.1420677108900382,-5.6402293478716778,-20.340702093046438,51.290016958752837,70161.958620636826,66205.015494235631,3956.9431264011996,0,70161.958620636826,1]
[2,"T2-MFB3-100C1-100C2-90A-95-CE-2","75T0206","T2-MFB3-100C1-100C2-90A-95-CE-2","closed","on","on","4.5 turns","unsealed","unsealed",866,5.75,null,0,0,"CUST 5","10/31/2014","15:53:25","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,459.8,0,14.8,0,57429,60,57166,531,9595,174,67034,186,8.1282890749999996,853,1310,null,6.9636231359999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo closed (2.0V), factory charge NC baseline, 90% airflow (350 cfm/ton), 4.5 turns,--5.75\" AK59 pulley (866 rpm), unsealed cab, adjust code tester speed to match total--match total static of run T2-MFB3-100C1-100C2-90A-95-CE-2-SPWCT-SS","W/ECO: 2.0 V With comps: 95/75 amb:2HP blwr mtr 5.75` AK59 mtr. pulley: 4.5 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",75,8.9999999999999993E-3,62.000999999999998,3.1E-2,94.995999999999995,1.2E-2,75,1.7000000000000001E-2,75.239999999999995,0.17,56.37,0.03,59.97,0.03,0.191,4.0000000000000001E-3,1.5435000000000001,2.5000000000000001E-3,57429,60,9595,174,8.1280000000000001,2.8000000000000001E-2,null,null,null,null,null,null,459.8,2.1,460.6,2.1,460.1,2.1,14.8,0,12.7,0,12.8,0,6690.2,43.4,3244.3,50.9,1556.7,33.700000000000003,460,null,460,null,459,null,2.9,null,3,null,2.9,null,0.5,460,null,459,null,460,null,5,null,4.9000000000000004,null,4.4000000000000004,null,3150,null,0.83,460,459,460,4.9000000000000004,4.7,4.3,2990,0.81,458.9,null,1.6,null,701.5,null,85,null,8236.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,219.55,0.17,107.05,0.1,107.8,0.05,0.75,0.09,247.37,0.17,173.78,0.09,116.32,0.05,57.46,0.09,214,0.05,105.51,0.06,106.01,0.06,0.5,0.06,74.47,0.05,48.38,0.23,43.87,0.03,4.51,0.23,73.83,0.05,55.31,0.16,43.45,0.03,11.85,0.15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,249.21,0.17,171.17,0.15,116.86,0.05,54.3,0.16,231.77,0.24,111.63,7.0000000000000007E-2,11.21,0.09,222,0.05,95.94,0.05,108.58,0.05,12.64,0.05,77.34,0.08,45.73,0.05,2.2799999999999998,0.23,76.930000000000007,7.0000000000000007E-2,56.12,0.42,45.47,0.04,10.65,0.44,100.89,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107.2,0.09,106.75,0.06,100.89,7.0000000000000007E-2,101.29,0.08,55.59,0.05,56.19,0.05,56,0.05,55.82,0.04,55.91,0.04,null,null,106.87,0.11,101.58,0.09,49.82,0.46,55.07,0.2,171.52,0.17,101.16,7.0000000000000007E-2,94.74,0.04,49.1,0.17,56.74,0.35,105.51,0.06,95.94,0.05,93.5,0.15,107.06,0.11,107.34,7.0000000000000007E-2,101.32,0.06,101.79,0.06,106.75,0.06,101.29,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107.05,0.1,100.43,0.11,107.2,0.09,100.89,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48.01,0.2,null,null,null,null,null,null,null,null,null,null,null,null,174.62,0.11,94.84,0.11,95.55,0.08,75.69,0.06,77.56,7.0000000000000007E-2,75.47,7.0000000000000007E-2,77.66,0.06,76,0.06,76.09,0.08,76.010000000000005,0.08,80.349999999999994,0.13,78.25,0.06,77.900000000000006,7.0000000000000007E-2,76.37,0.09,77.790000000000006,0.08,77.64,0.08,77.709999999999994,7.0000000000000007E-2,77.34,7.0000000000000007E-2,76.11,0.08,76.709999999999994,0.08,75.72,0.08,75.400000000000006,0.09,75.39,0.08,75.430000000000007,0.08,75.849999999999994,0.08,75.44,0.08,75.400000000000006,0.06,81.36,7.0000000000000007E-2,80.62,0.1,null,null,76.819999999999993,0.08,75.599999999999994,0.06,75.88,0.08,76.05,0.08,77.06,null,75.349999999999994,0.08,80.91,0.1,80.77,0.08,77.87,0.08,76.010000000000005,0.09,75.41,0.08,null,null,null,null,null,null,null,null,null,null,null,null,75.489999999999995,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-88A-55-CE-DM-2",75,8.9999999999999993E-3,62.000999999999998,3.1E-2,56.045000000000002,1.2E-2,53.634999999999998,2.1000000000000001E-2,94.995999999999995,1.2E-2,75,1.7000000000000001E-2,2720.6,2.2000000000000002,2706.6,2.2000000000000002,0.53300000000000003,2E-3,-0.249,2E-3,0.191,4.0000000000000001E-3,1.5435000000000001,2.5000000000000001E-3,29.623999999999999,0,8247,17,1310,null,0,0,13.029,0.23100000000000001,{"$f":"(XM469-XU469)*3.412/XT469/0.24","v":1.2977830844037488},12493.92469904933,169.47919351181105,0,0,12493.92469904933,8.7812847829730582E-3,27.609359938007415,54.747216915596255,14.099819340136801,13.065230016347122,1.3921735863287198E-2,38.157195844658276,8.7812847829730582E-3,27.609359938007415,8.1727102133391429E-3,22.325415093847358,75,62.001009096134673,22.009237909739998,69967.502926660527,60728.819232652895,6937,0.33838539335635581,66074.905414116336,56836.221720108704,8.0119928960975315,0.14291737279358122,-5.6001220282674176,-20.252783084403745,51.370092635740605,69967.502926660527,66017.208996865709,3950.2939297948146,0,69967.502926660527,1]
[2,"T2-MF35-115C1-115C2-90A-95-CE","75T0007","T2-MF35-115C1-115C2-90A-95-CE","closed","on","on","4.5 turns","unsealed","unsealed",848,5.75,null,0,0,"CUST 5","10/9/2014","1:55:01","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 7.36 lbs/CK2: 7.13 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,7.36,7.13,6.4,6.2,461.1,1.2,15.3,0,58963,71,58196,371,11529,182,70504,175,8.3102310230000001,865,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MF35, 115% charge CK1 and CK2, 87.5% airflow (360 cfm/ton), closed damper,--2 HP fan motor,  4.5 turns, 5.75\" AK59 pulley (848 rpm), adjust code tester speed--to match total static of run T2-MFB2-2700-95-C-SPWCT-SS","With econo: both stages: 95/75 amb: 2 HP blower motor: 5.75` mtr. pulley: 4.5 turns open: AX 35 belt: 100% inlet-outlet Meriam",74.989999999999995,1.2E-2,62.002000000000002,2.5000000000000001E-2,95.004999999999995,1.0999999999999999E-2,75.004999999999995,3.1E-2,74.72,0.12,55.61,0.05,59.78,0.01,0.2,4.0000000000000001E-3,1.0656000000000001,2.7000000000000001E-3,58963,71,11529,182,8.3109999999999999,3.1E-2,null,null,null,null,null,null,461.1,2.5,461.8,2.5,458.9,2.4,15.3,0.1,13,0,12.7,0.1,6961.3,52.4,3128.8,60.4,1522.3,40.700000000000003,460,null,460,null,460,null,3,null,3,null,2.9,null,0.81,460,null,460,null,460,null,5.2,null,4.8,null,4.5,null,3210,null,0.83,460,460,460,5.2,4.7,4.5,3140,0.82,460.2,null,1.6,null,701.5,null,85,null,8486.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,228.6,0.13,100.47,0.06,110.61,0.04,10.14,7.0000000000000007E-2,250.3,0.13,174.58,0.17,117.14,0.04,57.44,0.17,222.6,0.05,99.32,0.05,108.72,0.05,9.4533333329999998,0.05,74.510000000000005,0.05,47.69,0.27,43.8,0.03,3.89,0.28000000000000003,73.88,0.06,54.27,0.32,43.38,0.04,10.89,0.33,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,261.75,0.15,177.21,0.32,120.43,0.04,56.78,0.35,246.22,0.33,115.94,0.1,23.2,0.09,236.6,0.05,98.77,0.05,113.06,0.05,14.33,0.05,77.03,0.2,45.43,0.12,3.51,1.24,76.459999999999994,0.19,55.62,0.28000000000000003,45.06,0.12,10.56,0.28999999999999998,100.49,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100.62,7.0000000000000007E-2,100.49,0.06,98.3,0.05,98.6,0.06,55.07,0.06,55.66,0.05,55.52,0.04,55.23,0.04,55.29,0.04,null,null,99.98,7.0000000000000007E-2,97.9,0.06,48.67,0.52,53.75,0.34,177.21,0.39,96.19,0.06,92.43,0.03,49.19,1.26,57.5,0.64,99.32,0.05,98.77,0.05,93.45,0.11,100.99,0.08,101.07,0.06,99.45,0.04,99.67,0.04,98.3,0.05,98.6,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100.47,0.06,92.74,0.04,100.62,7.0000000000000007E-2,100.49,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48.94,1.1399999999999999,null,null,null,null,null,null,null,null,null,null,null,null,175.56,0.19,95.6,0.06,95.34,7.0000000000000007E-2,75.11,0.05,75.45,0.05,75.010000000000005,0.05,75.61,0.06,75.47,0.05,75.540000000000006,7.0000000000000007E-2,75.34,0.06,78.790000000000006,0.08,76.900000000000006,0.06,76.900000000000006,0.06,78.05,0.12,78.08,0.08,77.5,0.06,76.680000000000007,7.0000000000000007E-2,75.510000000000005,7.0000000000000007E-2,75.97,0.14000000000000001,75.53,0.08,75.010000000000005,7.0000000000000007E-2,75.23,7.0000000000000007E-2,75.13,0.06,75.28,0.1,76.709999999999994,0.09,75.33,7.0000000000000007E-2,75.73,0.06,80.16,0.14000000000000001,80.08,0.18,null,null,75,0.06,75.28,0.05,75.489999999999995,0.06,75.28,0.06,75.47,null,75.040000000000006,0.06,80.790000000000006,0.04,80.41,0.19,78.63,0.08,75.34,0.08,75.2,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-88A-55-CE-DM-2",74.989999999999995,1.2E-2,62.002000000000002,2.5000000000000001E-2,55.627000000000002,1.0999999999999999E-2,53.273000000000003,1.7000000000000001E-2,95.004999999999995,1.0999999999999999E-2,75.004999999999995,3.1E-2,2759,3.5,2716.6,3.5,0.55500000000000005,3.0000000000000001E-3,-0.249,2E-3,0.2,4.0000000000000001E-3,1.0656000000000001,2.7000000000000001E-3,29.308,1E-3,8484,24,1350,null,0,0,13.029,0.23100000000000001,1.3148740507879679,12681.328821474315,177.12659811023622,0,0,12681.328821474315,8.7843068864830367E-3,27.610228023555809,54.312125949212032,14.100066538096014,13.053837048975325,1.3923963381801727E-2,38.161868834734733,8.7843068864830367E-3,27.610228023555809,8.0693108947775469E-3,22.111317830730819,74.989999999999995,62.002009033479943,21.791037161930248,73795.072791192186,62933.500840097578,7134,0.32994536191996404,69792.055870542419,58930.483919447812,8.2263149305212657,0.13860149546125641,-5.819190861625561,-20.677874050787963,50.984996576108024,73795.072791192186,69733.488314970426,4061.5844762217484,0,73795.072791192171,0.99999999999999978]
[2,"T2-MFR12-115C1-115C2-90A-95-CC2F","75T0011","T2-MFR12-115C1-115C2-90A-95-CC2F","2 finger","on","on","4.5 turns","unsealed","unsealed",865,5.75,null,30,0,"CUST 5","10/15/2014","23:06:04","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 7.4 lbs/CK2: 7.1 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,7.4,7.1,6.4,6.2,460,0,15.7,0,48340,87,47810,466,-2016,143,46323,137,5.1055880079999998,864,null,null,5.3278959549999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MFR12, Restrict CK1 per MFR1, 115% charge C1, 115% charge C2, 6V open economizer damper,--90% airflow (360 cfm/ton), 4.5 turns, 5.75\" AK59 pulley (865 rpm), 30% condenser coil blockage,--2 HP fan motor, adjust code tester speed to match total static of ru","W/Econ: 2 stages:95/75 amb:2HP blwr mtr 5.75` mtr. pulley:4.5 turns open:AX 35 belt:100% inlet-outlet Meriam:adjusted CK1 liq ln sv.valve 8.5 turns.Rstrct CK1 to achieve 22 psig suction from T2-RBASE-100C1-100C2-100A-95-CE: cond coil blk 21. 6V Eco",74.97,2.1999999999999999E-2,61.997,2.3E-2,94.992000000000004,3.2000000000000001E-2,75.004000000000005,0.02,74.95,0.15,59.43,0.06,62.67,0.03,0.16400000000000001,4.0000000000000001E-3,1.6442000000000001,2.3999999999999998E-3,48340,87,-2016,143,5.1059999999999999,2.1999999999999999E-2,null,null,null,null,null,null,460,2,461.5,2,459.9,2,15.7,0,13.5,0,13.7,0,7169.6,41,3245,49.7,1903.5,31.8,460,null,460,null,460,null,2.9,null,3,null,2.9,null,0.5,460,null,460,null,460,null,5.4,null,5.3,null,4.8,null,3510,null,0.85,460,460,460,5.5,5.2,4.9000000000000004,3510,0.84,459,null,1.6,null,658.8,null,85,null,9073.7999999999993,null,null,null,null,null,null,null,null,null,null,null,null,null,null,260.08999999999997,0.36,100.26,0.13,119.96,0.1,19.7,0.12,272.8,0.37,219.18,0.08,123.51,0.1,95.67,0.1,155.9,0.05,85.58,0.08,84.97,0.05,-0.49666666700000001,0.05,64.36,0.09,71,0.03,36.85,7.0000000000000007E-2,34.15,0.08,63.88,0.09,74.22,0.03,36.5,0.06,37.72,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,294.92,0.4,188.85,0.3,129.41999999999999,0.11,59.43,0.32,278.68,0.56000000000000005,125.11,0.15,25.32,0.17,268.60000000000002,0.05,95.42,0.08,122.34,0.05,26.943333333000002,0.05,82.75,0.22,49.02,0.13,3.32,1.1599999999999999,82.38,0.15,60.34,0.82,48.79,0.09,11.55,0.86,100.37,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,87.64,0.11,88.72,0.09,100.37,0.14000000000000001,101.31,0.12,58.78,0.06,59.57,0.05,59.38,0.05,59.05,0.03,59.08,0.03,null,null,100.3,0.11,83.9,0.08,72.290000000000006,0.05,75.02,0.05,189.1,0.38,100.1,0.12,94.24,0.09,52.92,1.0900000000000001,61.82,0.76,85.58,0.08,95.42,0.08,92.73,0.18,100.36,0.11,88.01,0.09,101.5,0.11,102.08,0.13,88.72,0.09,101.31,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100.26,0.13,99.79,0.14000000000000001,87.64,0.11,100.37,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,52.35,1.04,null,null,null,null,null,null,null,null,null,null,null,null,220.96,0.12,95.96,0.31,93.86,0.19,75.28,7.0000000000000007E-2,75.510000000000005,0.06,75.12,7.0000000000000007E-2,75.84,0.08,75.64,0.08,75.72,0.09,75.52,0.08,85.51,0.16,86.32,0.14000000000000001,86.79,0.11,82.38,0.19,82.78,0.16,82.21,0.24,80.05,0.26,79.27,0.09,79.33,0.13,79.569999999999993,0.12,76.87,0.14000000000000001,75.16,0.09,76.27,0.1,76.59,0.08,76.5,0.08,75.180000000000007,0.09,75.25,0.08,76.260000000000005,0.14000000000000001,76.89,0.08,null,null,75.14,0.08,75.36,7.0000000000000007E-2,75.61,0.08,75.41,0.09,75.44,null,75.099999999999994,0.09,87.59,0.13,85.47,0.11,82.58,0.13,75.819999999999993,0.1,75.150000000000006,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-88A-55-2F-DM-2",74.97,2.1999999999999999E-2,61.997,2.3E-2,59.281999999999996,8.9999999999999993E-3,56.52,1.7999999999999999E-2,94.992000000000004,3.2000000000000001E-2,75.004000000000005,0.02,2831.3,2,2768.9,2,0.5,2E-3,-0.18099999999999999,4.0000000000000001E-3,0.16400000000000001,4.0000000000000001E-3,1.6442000000000001,2.3999999999999998E-3,29.321999999999999,1E-3,9073,25,1310,null,0,0,13.029,0.23100000000000001,1.2630613553895094,12914.301170163482,162.6456220472441,0,0,12914.301170163482,8.785735343185606E-3,27.606913160053235,58.018938644610486,14.099754558121701,13.154254168431285,1.3926199528388031E-2,38.161135329866383,8.785735343185606E-3,27.606913160053235,9.0705313187239619E-3,24.090261070676771,74.97,61.997008946272757,23.782039598297089,49395.569114314763,52538.666759380736,7763,0.53638655197358076,45479.648622362009,48622.746267427981,5.0126362418562778,0.16609634749434377,-3.8248735617561458,-16.951061355389513,54.642638074607142,49395.569114314763,45415.104192892322,3980.4649214224346,0,49395.569114314756,0.99999999999999989]
[2,"T2-TRN-88A-55-TCE-DM-2","75T0097","T2-TRN-88A-55-TCE-DM-2","closed","off","off","4.5 turns","unsealed","unsealed",866,5.75,null,0,0,"CUST 5","10/28/2014","22:08:18","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,459.9,0,3.3,0,1674,10,1402,95,1887,68,3563,67,2.6295202949999998,858,1270,null,1.2354243540000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo closed (2V), tape around damper perimeter inside/outside frame gaps, no compressor, 55/51 ambient,--87.5% airflow (350 cfm/ton), 2 HP fan motor, 4.5 turns, 5.75\" AK59 pulley (866 rpm), 100% inlet/outlet Meriam,--adjust code tester speed to match tot","W/ECO: 2 V No comp: 55/51 amb:2HP blwr mtr 5.75`` AK59 mtr. pulley: 4.5 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.991,4.0000000000000001E-3,62,1.4999999999999999E-2,55.005000000000003,1.0999999999999999E-2,51.006,1.2999999999999999E-2,74.849999999999994,0.06,74.39,7.0000000000000007E-2,74.61,0.01,0.158,3.0000000000000001E-3,1.5428999999999999,2E-3,1674,10,1887,68,2.629,5.3999999999999999E-2,null,null,null,null,null,null,459.9,2.1,460.2,2.1,460.2,2.1,3.3,0,2.9,0,3.2,0,1385.3,15,1117.8,19.3,-10,0.3,460,null,460,null,460,null,2.8,null,2.9,null,2.9,null,0.48,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.4,null,0,null,0,null,85,null,1355,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94.9,0.03,57.08,0.08,56.17,0.01,-0.9,0.08,95.6,0.01,57.72,0.01,56.56,0.01,-1.1499999999999999,0.01,null,null,70.989999999999995,0.03,null,null,null,null,95.22,0.01,71.709999999999994,0.02,56.35,0.01,15.35,0.02,95.04,0.01,59.52,0.02,56.25,0.01,3.26,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95.96,0.01,59.35,0.13,56.77,0.01,2.58,0.14000000000000001,95.92,0.02,56.75,0.01,0.14000000000000001,0.12,null,null,73.069999999999993,0.05,null,null,null,null,95.5,0.02,56.51,0.01,14.82,0.05,95.66,0.02,60.72,0.02,56.6,0.01,4.12,0.02,59.88,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.02,0.06,60.14,0.05,59.88,0.09,61.39,7.0000000000000007E-2,74.459999999999994,7.0000000000000007E-2,74.28,0.04,74.209999999999994,0.03,74.77,0.02,74.77,0.02,null,null,56.61,0.03,71.180000000000007,0.04,72.11,0.04,59.71,0.03,59.93,0.13,57.07,0.08,73.73,0.05,72.78,0.03,62.84,0.04,70.989999999999995,0.03,73.069999999999993,0.05,55.85,0.03,58.25,0.02,61.17,0.02,58.03,0.03,58.85,0.05,60.14,0.05,61.39,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.08,0.08,56.6,0.12,59.02,0.06,59.88,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,71.33,0.05,null,null,null,null,null,null,null,null,null,null,null,null,57.79,0.02,56.04,0.05,55.66,0.04,75.319999999999993,0.01,73.08,0.04,74.75,0.02,74.010000000000005,0.04,75.819999999999993,2.5,75.7,0.02,75.34,0.02,72.349999999999994,0.04,72.790000000000006,0.04,72.69,0.03,73.040000000000006,0.05,73.23,0.04,73.14,0.04,73.319999999999993,0.03,73.900000000000006,0.03,74.11,0.03,73.8,0.03,74.02,0.03,74.849999999999994,0.02,74.86,0.01,74.760000000000005,0.02,73.3,0.15,74.989999999999995,0.02,74.7,0.02,69.42,0.09,69.37,0.08,null,null,73.459999999999994,0.05,75.75,0.02,75.569999999999993,0.02,74.92,0.03,73.319999999999993,null,75.05,0.02,71.150000000000006,0.08,null,null,72.709999999999994,0.05,74.209999999999994,0.03,74.900000000000006,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.991,4.0000000000000001E-3,62,1.4999999999999999E-2,74.442999999999998,2E-3,61.609000000000002,1.4999999999999999E-2,55.005000000000003,1.0999999999999999E-2,51.006,1.2999999999999999E-2,2767.4,1.8,2656.9,1.7,0.56699999999999995,3.0000000000000001E-3,-0.248,2E-3,0.158,3.0000000000000001E-3,1.5428999999999999,2E-3,29.428999999999998,1E-3,1355,11,1270,null,0,0,13.03,0.248,1.2666830117157162,12267.556769950845,176.97966548031496,0,0,12267.556769950845,8.7827517988512856E-3,27.608770197606777,73.176316988284285,13.029644012000718,13.535213499620539,6.9833562235990052E-3,20.781090015269648,8.7827517988512856E-3,27.608770197606773,8.6554330869033601E-3,27.335819869152491,74.991000000000014,62.000009049879544,27.026948067958418]
[2,"T2-TRN-75A-55-1E-DM","75T0072","T2-TRN-75A-55-1E-DM","10% open","off","off","3 turns","unsealed","unsealed",725,7.25,null,0,0,"CUST 5","10/22/2014","4:14:38","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.4,0,3.2,0,3754,15,3333,77,2673,59,6429,64,5.9308118079999996,755,980,null,3.463099631,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 10%-open (2.8V), no compressor, 55/51 ambient, 75% airflow (300 cfm/ton), 2 HP fan motor,--3 turns, 7.25\" AK74 pulley (725 rpm), unsealed cab, 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-TRN-75A-55-1E-DM-SPWCT","W/ECO: Eco set at 2.8v: No Compr:55/51 amb:2HP blwr mtr 7.25` AK74 mtr. pulley:3 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",74.997,6.0000000000000001E-3,61.997,2.1999999999999999E-2,54.997,1.0999999999999999E-2,51.000999999999998,1.2E-2,74.569999999999993,0.04,73.31,0.05,74.11,0,0.112,3.0000000000000001E-3,1.1858,1.6000000000000001E-3,3754,15,2673,59,5.931,7.4999999999999997E-2,null,null,null,null,null,null,460.4,2,461.1,2,459.6,1.9,3.2,0,2.7,0,3.1,0,1272.2,14.6,1099,18.5,-10,0,460,null,460,null,460,null,2.8,null,2.7,null,2.7,null,0.38,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.5,null,0,null,0,null,85,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97.1,0.03,55.33,0.05,57.39,0.01,2.06,0.05,96.4,0.02,57.36,0.01,57.01,0.01,0.35,0.01,null,null,68.58,0.02,null,null,null,null,96.45,0.02,71.02,0.01,57.03,0.01,13.99,0.01,95.95,0.02,56.97,0.02,56.76,0,0.22,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97.2,0.01,56.99,0.01,57.46,0.01,0.47,0.01,97.8,0.03,57.79,0.01,1.28,0.02,null,null,72.459999999999994,0.02,null,null,null,null,97.32,0.01,57.52,0.01,13.12,0.02,96.8,0.01,58.87,0.02,57.24,0.01,1.63,0.02,57.26,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56.45,0.05,57.92,0.04,57.26,0.05,59.23,0.06,73.44,0.04,73.3,0.04,73.17,0.03,73.42,0.04,73.48,0.04,null,null,54.82,0.03,68.569999999999993,0.06,70.739999999999995,0.06,57.06,0.05,57.32,0.04,56.77,0.03,73.010000000000005,0.03,71.63,0.02,60.63,0.02,68.58,0.02,72.459999999999994,0.02,55.06,0.06,55.8,0.02,59.02,0.02,57.19,0.01,57.97,0.02,57.92,0.04,59.23,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55.33,0.05,56.51,0.03,56.45,0.05,57.26,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.64,0.02,null,null,null,null,null,null,null,null,null,null,null,null,57.08,0.05,56.29,0.15,56.08,0.16,74.790000000000006,0.05,74.459999999999994,0.03,74.55,0.02,74.95,0.06,75.23,6.76,75.03,0.05,74.92,0.04,71.62,0.09,72.989999999999995,0.05,72.56,0.05,72.400000000000006,0.12,72.89,0.1,72.91,0.1,73.33,0.06,74.16,0.06,74.260000000000005,0.08,73.98,7.0000000000000007E-2,74.44,0.04,74.540000000000006,0.04,74.680000000000007,0.02,74.55,0.03,72.430000000000007,0.09,74.8,0.02,73.67,0.05,68.44,0.16,68.989999999999995,0.11,null,null,74.72,0.03,75.459999999999994,0.02,75.33,0.02,75.2,0.02,74.62,null,74.86,0.02,68.2,0.1,69.97,7.0000000000000007E-2,72.59,0.11,74.209999999999994,7.0000000000000007E-2,74.77,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.997,6.0000000000000001E-3,61.997,2.1999999999999999E-2,73.575000000000003,4.0000000000000001E-3,61.152000000000001,0.02,54.997,1.0999999999999999E-2,51.000999999999998,1.2E-2,2423.6,1.7,2327.6,1.6,0.40100000000000002,2E-3,-0.182,2E-3,0.112,3.0000000000000001E-3,1.1858,1.6000000000000001E-3,29.408999999999999,0,1084,9,980,null,1.3599999999999857E-2,31.655359999999664,13.029,0.182,1.1497759959816964,10761.611739402562,109.65231962204726,31.655888971171979,145.77403194872892,10615.837707453833,8.7550174051102062E-3,27.514024408110931,72.425224004018304,13.029435441137775,13.512474109019738,6.9825794359606452E-3,20.778302070584594,8.7793560806120486E-3,27.606517664911465,8.5629230551391745E-3,27.022988937821811,74.726959304422991,61.863149820185996,26.742671321923602]
[2,"T2-HS-2250-95-CF","75T0149","T2-HS-2250-95-CF","closed","on","on","3 turns","unsealed","unsealed",859,7,null,0,0,"CUST 6","7/31/2014","11:01:22","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460.3,1.4,14.6,0,51883,129,52208,348,13738,434,65634,417,7.9875867100000004,888,null,null,null,109.13,0.04,19.920000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"75% airflow (300 cfm/ton), 3 HP fan motor, 3 turns, 7\" pulley (859 rpm),--both stages, closed damper adjust code tester speed to match total static of run--T2-2250-95-CF-SPWCT-SS","Installed FM:SG:FD:LSV on 2 circuits: unsealed cab: dampers on S/R: AX35 belt: 7` BP no name: ID Blw M: MQC 56T17D5563B: Mtr Pulley 3 T/O: With econo: Supply Meriam @85% Return Meriam @75%: Horiz Air Disch: Max Mtr Amp 4.7",74.944999999999993,3.5000000000000003E-2,62.008000000000003,8.3000000000000004E-2,94.849000000000004,2.1000000000000001E-2,75.001000000000005,1.7000000000000001E-2,74.8,0.12,54.36,0.1,58.46,0.03,0.106,3.0000000000000001E-3,0.97929999999999995,2E-3,51883,129,13738,434,7.9870000000000001,0.05,81959,231,9.9740000000000002,0.03,19.920000000000002,0.34,460.3,2.7,460,2.7,459.7,2.7,14.6,0.1,12.8,0,12.4,0.1,6608.9,64.8,3180.9,68.7,1608.2,54.3,460,null,461,null,459,null,2.6,null,2.7,null,2.6,null,0.52,460,null,460,null,461,null,5.0999999999999996,null,5,null,4.5,null,3160,null,0.82,459,459,460,4.9000000000000004,4.5999999999999996,4.5,3020,0.81,459.4,null,1.6,null,701.6,null,115,null,8236.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220.39,0.14000000000000001,107.1,7.0000000000000007E-2,null,null,null,null,245.9,0.17,177.03,0.22,115.85,0.05,61.19,0.21,211,null,100.51,0.33,108.02,0.04,7.51,0.34,72.13,0.14000000000000001,46.07,0.25,42.22,0.09,3.85,0.24,71.599999999999994,0.13,54.61,0.33,41.86,0.08,12.74,0.31,619.48,1.47,null,0.1,81959,231,43050,158,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,248.01,0.17,172.53,0.23,116.47,0.05,56.06,0.24,231.53,0.22,null,null,null,null,220,null,99.31,7.0000000000000007E-2,111.51,7.0000000000000007E-2,12.2,0.08,74.59,0.15,43.85,0.1,2.5099999999999998,0.43,74.209999999999994,0.17,54.5,0.47,43.6,0.11,10.9,0.5,105.55,0.05,610.54,1.99,39.26,0.02,109.03,7.0000000000000007E-2,81959,231,42593,118,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106.14,0.05,105.55,0.05,100.97,7.0000000000000007E-2,101.21,7.0000000000000007E-2,54.63,0.09,54.4,0.09,54.01,0.09,54.7,0.08,54.76,7.0000000000000007E-2,54.48,0.08,106.81,0.1,101.55,0.05,46.97,0.39,53.68,0.39,171.32,0.2,101.06,0.05,100.56,7.0000000000000007E-2,46.64,0.12,54.67,0.71,null,null,null,null,93.27,0.04,null,null,null,null,null,null,null,null,100.97,7.0000000000000007E-2,101.21,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,100.51,0.33,54.48,0.08,107.1,7.0000000000000007E-2,101.41,0.08,106.14,0.05,105.55,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,46.36,0.37,null,null,null,null,null,null,null,null,null,null,null,null,175.84,0.2,94.36,0.12,94.47,0.11,75.33,0.1,75.03,0.1,74.86,0.1,75.569999999999993,7.0000000000000007E-2,75.62,0.1,75.510000000000005,0.1,75.31,0.1,80.569999999999993,0.12,79.69,0.11,77.06,0.11,77.17,0.25,78.23,0.17,78.08,0.15,77.56,0.16,75.709999999999994,0.13,75.290000000000006,0.13,75.41,0.14000000000000001,74.87,0.11,74.88,0.13,74.86,0.13,75.3,0.15,74.849999999999994,0.12,75.11,0.12,75.099999999999994,0.1,75.64,0.1,76.13,0.1,null,null,74.92,0.08,75.59,0.11,75.349999999999994,0.1,75.08,0.11,74.94,null,74.73,0.13,80.78,0.17,81.41,0.17,77.989999999999995,0.19,75.23,0.13,74.89,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-75A-55-CE-DM-2",74.944999999999993,3.5000000000000003E-2,62.008000000000003,8.3000000000000004E-2,54.628999999999998,4.8000000000000001E-2,52.210999999999999,5.5E-2,94.849000000000004,2.1000000000000001E-2,75.001000000000005,1.7000000000000001E-2,2301.4,2.4,2272,2.4,0.67200000000000004,2E-3,-0.28299999999999997,2E-3,0.106,3.0000000000000001E-3,0.97929999999999995,2E-3,29.3,0,8217,16,1240,null,7.9571614453004501E-3,18.416850165147892,13.03,0.182,1.4224122503768726,10600.769844178181,179.3670651968504,{"$f":"XP505*SQRT(-XC505*YB505/(XR505*XQ505))","v":23.886607894318729},101.67123788277749,10499.098606295403,8.8483749893708743E-3,27.716359206165404,53.206587749623125,14.096380682524362,13.025846427166242,1.3957811494040868E-2,38.1608026964822,8.7988961956388338E-3,27.615217237842476,7.7201265760274834E-3,21.48926809802164,75.137673255576246,62.151843610907612,21.143013503969598,69682.524895195544,55796.733571584242,6977,0.34172844677793557,66062.584688712392,52176.79336510109,8.0397450028857715,0.14294660192214761,-6.5733457021958053,-21.931085505953121,49.548736142510904,69682.524895195544,64939.776908381988,3670.5652590350383,1072.1827277785185,69682.524895195544,1]
[2,"T2-TRN-110A-55-1F-DM-2","75T0107","T2-TRN-110A-55-1F-DM-2","1 finger","off","off","1 turn","unsealed","unsealed",1060,5.75,null,0,0,"CUST 5","10/27/2014","23:04:57","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lb","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460,0,4.2,0,11455,39,10902,91,7983,157,19446,155,8.6426666670000003,1057,2150,null,5.091111111,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 1F-open (5.1V), no compressor, 55/51 ambient, 110% airflow (450 cfm/ton),--2 HP fan motor, 1 turn, 5.75\" AK59 pulley (1060 rpm), unsealed cab, 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-TRN-110A-55-1F-DM-2-SP","W/ECO:  5.1 V No comp: 55/51 amb:2HP blwr mtr 5.75` AK59 mtr. pulley: 1 turns open: AX35 new belt browning tensioning tool 8 lbs:100% inlet-outlet Meriam:",75.004999999999995,8.0000000000000002E-3,61.997999999999998,2.8000000000000001E-2,55.002000000000002,1.6E-2,51.02,1.4999999999999999E-2,74.98,0.06,72.11,0.08,72.45,0.01,0.25,4.0000000000000001E-3,2.4537,3.0999999999999999E-3,11455,39,7983,157,8.6449999999999996,8.1000000000000003E-2,null,null,null,null,null,null,460,2,461,2,460.1,2,4.2,0,3.7,0,3.9,0,1868.1,13.8,1109.3,17.2,381.4,10.1,460,null,460,null,460,null,3.7,null,3.7,null,3.6,null,0.64,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.5,null,0,null,0,null,85,null,2235,null,null,null,null,null,null,null,null,null,null,null,null,null,null,97.83,0.02,60.49,0.09,57.74,0.01,-2.74,0.09,97.94,0.02,59.53,0.01,57.8,0.01,-1.73,0.02,null,null,72.150000000000006,0.02,null,null,null,null,97.44,0.02,71,0.02,57.52,0.01,13.48,0.02,97.26,0.02,65.11,0.02,57.42,0.01,7.69,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,98.38,0.03,62.09,0.09,58.04,0.02,4.0599999999999996,0.09,98.5,0.05,58.11,0.03,-0.92,0.39,null,null,71.78,0.09,null,null,null,null,97.75,0.03,57.69,0.02,13.47,0.06,97.86,0.03,63.57,0.02,57.75,0.02,5.82,0.03,63.08,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.7,7.0000000000000007E-2,61.98,0.05,63.08,0.05,63.17,0.08,72.53,7.0000000000000007E-2,71.73,0.05,71.48,0.04,72.760000000000005,0.04,72.680000000000007,0.03,null,null,60.3,0.04,72.41,0.04,71.77,0.04,64.66,0.04,62.64,0.1,59.16,0.32,72.34,0.09,72.319999999999993,0.02,65.48,0.04,72.150000000000006,0.02,71.78,0.09,55.26,0.03,62.72,0.02,62.84,0.02,60.16,0.22,61.32,0.15,61.98,0.05,63.17,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.49,0.09,59.04,0.39,61.7,7.0000000000000007E-2,63.08,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,71.16,0.05,null,null,null,null,null,null,null,null,null,null,null,null,59.6,0.03,57.52,0.19,55.99,0.05,75.42,0.02,73.27,0.03,74.87,0.02,74.25,0.04,75.83,0.66,75.78,0.02,75.400000000000006,0.03,63.59,0.17,68.33,0.1,68.430000000000007,0.3,61.32,7.0000000000000007E-2,66.069999999999993,0.11,69.34,7.0000000000000007E-2,69.930000000000007,0.04,69.540000000000006,0.05,67.41,7.0000000000000007E-2,68.900000000000006,0.08,65.81,0.08,68.569999999999993,7.0000000000000007E-2,72.11,7.0000000000000007E-2,73.03,7.0000000000000007E-2,73.540000000000006,0.05,69.56,0.09,72.7,0.06,73.23,0.06,69.48,7.0000000000000007E-2,null,null,73.5,0.04,75.790000000000006,0.02,75.61,0.02,75.03,0.02,73.760000000000005,null,75.099999999999994,0.02,62.03,0.08,null,null,62.16,0.06,64.08,0.13,70.58,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75.004999999999995,8.0000000000000002E-3,61.997999999999998,2.8000000000000001E-2,71.981999999999999,7.0000000000000001E-3,60.21,1.9E-2,55.002000000000002,1.6E-2,51.02,1.4999999999999999E-2,3502.3,2.2000000000000002,3349.7,2.1,0.79500000000000004,4.0000000000000001E-3,-0.26300000000000001,2E-3,0.25,4.0000000000000001E-3,2.4537,3.0999999999999999E-3,29.178999999999998,1E-3,2250,11,2150,null,6.7639854021896553E-2,226.57321901714687,13.03,0.26300000000000001,1.6742257114418841,15600.124082252942,312.85142976377955,226.5700143646213,1043.3296564006127,14556.794425852329,8.6586366984315859E-3,27.151142441467719,70.307774288558122,13.029631409861354,13.470277472924577,6.9915019507208959E-3,20.789202255805208,8.7781253078477797E-3,27.607122011816006,8.334472935468679E-3,26.384925606225629,73.671268843874088,61.334459613888811,25.976915953216913]
[2,"T2-MF7-100C1-100C2-110A-95-CCE","75T0045","T2-MF7-100C1-100C2-110A-95-CCE","closed","on","on","1 turn","unsealed","unsealed",1060,5.75,null,30,0,"CUST 5","10/10/2014","23:04:29","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1: 6.4 lbs/CK2: 6.2 lbs","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460,1.3,16.7,0,59682,68,59493,462,2038,163,61722,152,6.2150840799999996,1060,null,null,6.0096667000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MF7, 100% charge CK1 and CK2, 110% airflow (450 cfm/ton), 30% condenser coil blockage,--2 HP fan motor, 1 turn, 5.75\" AK59 pulley (1060 rpm), adjust code tester speed to match--total static of run T2-MF7-100C1-100C2-110A-95-CCE-SPWCT-SS","With econo: both stages: 95/75 amb: 2 HP blower motor: 5.75` mtr. pulley: 1 turn open: AX 35 belt: 100% inlet-outlet Meriam: condenser coil blocked 25.25\" of 62\" coil",75.004000000000005,1.4E-2,62.008000000000003,2.1000000000000001E-2,95.004999999999995,4.3999999999999997E-2,75,2.1000000000000001E-2,75.010000000000005,0.12,59.16,0.02,61.85,0.01,0.26,4.0000000000000001E-3,2.4350000000000001,3.2000000000000002E-3,59682,68,2038,163,6.2149999999999999,1.7999999999999999E-2,null,null,null,null,null,null,460,2.5,461.6,2.5,459.9,2.5,16.7,0,14.5,0,14.5,0,7641.5,49.5,3302.7,57.8,2289.9,37.799999999999997,460,null,460,null,460,null,3.7,null,3.7,null,3.6,null,0.65,460,null,460,null,460,null,5.5,null,5.3,null,4.8,null,3560,null,0.85,460,460,460,5.3,5.0999999999999996,4.8,3410,0.84,458.9,null,1.6,null,672.3,null,85,null,9927.2999999999993,null,null,null,null,null,null,null,null,null,null,null,null,null,null,247.99,0.15,115.62,0.05,116.45,0.04,0.84,0.03,280.52,0.16,189,0.06,125.6,0.04,63.4,0.06,239.3,0.05,112.89,0.05,113.87,0.05,0.97333333300000002,0.05,78.66,0.03,53.2,0.22,46.46,0.02,6.74,0.22,78.010000000000005,0.03,60.34,7.0000000000000007E-2,46.04,0.02,14.3,7.0000000000000007E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,286.2,0.18,187.08,0.28000000000000003,127.12,0.05,59.96,0.3,269.43,0.38,122.57,0.11,15.67,0.12,257.3,0.05,101.79,0.05,119.51,0.05,17.696666666999999,0.05,80.75,0.2,47.77,0.12,3.3,1.1200000000000001,80.39,0.15,61.84,0.06,47.55,0.09,14.3,0.11,107.55,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.24,0.06,115.1,0.05,107.55,0.09,107.98,0.09,58.65,0.03,59.29,0.03,59.18,0.03,59.04,0.03,59.02,0.03,null,null,115.77,0.05,110.07,0.06,54.81,0.27,61.09,0.08,187.26,0.34,107.37,0.09,100.66,0.04,51.84,1.04,62.02,0.7,112.89,0.05,101.79,0.05,93.1,0.22,115.53,0.04,115.51,0.05,109.83,0.05,110.12,7.0000000000000007E-2,115.1,0.05,107.98,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115.62,0.05,106.91,0.1,115.24,0.06,107.55,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,51.06,1.02,null,null,null,null,null,null,null,null,null,null,null,null,190.14,0.08,94.06,0.12,93.55,0.12,75.349999999999994,0.06,75.59,0.05,75.099999999999994,0.06,75.86,0.06,75.739999999999995,0.06,75.78,7.0000000000000007E-2,75.569999999999993,0.06,79.81,0.11,76.78,0.06,76.84,7.0000000000000007E-2,78.16,0.09,78.2,0.08,77.430000000000007,7.0000000000000007E-2,76.86,0.06,75.8,7.0000000000000007E-2,75.489999999999995,7.0000000000000007E-2,75.8,0.08,75.150000000000006,7.0000000000000007E-2,75.31,0.08,75.260000000000005,0.08,75.25,7.0000000000000007E-2,75.650000000000006,0.06,75.44,7.0000000000000007E-2,75.349999999999994,0.05,76.319999999999993,0.06,76.36,0.06,null,null,75.17,0.06,75.45,0.05,75.59,7.0000000000000007E-2,75.41,7.0000000000000007E-2,75.48,null,75.22,7.0000000000000007E-2,null,null,81.69,0.08,78.73,0.08,75.540000000000006,7.0000000000000007E-2,75.31,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-TRN-110A-55-CE-DM-2",75.004000000000005,1.4E-2,62.008000000000003,2.1000000000000001E-2,59.112000000000002,8.0000000000000002E-3,56.008000000000003,1.4E-2,95.004999999999995,4.3999999999999997E-2,75,2.1000000000000001E-2,3449.7,2.2999999999999998,3374.5,2.2000000000000002,0.85399999999999998,3.0000000000000001E-3,-0.376,2E-3,0.26,4.0000000000000001E-3,2.4350000000000001,3.2000000000000002E-3,29.263999999999999,2E-3,9931,17,2200,null,0,0,13.029,0.34499999999999997,1.6810136129878437,15742.58989403269,338.5574737007874,0,0,15742.58989403269,8.7849558850225055E-3,27.614352827061779,57.430986387012155,14.100030309218248,13.147900148148914,1.3919580961934684E-2,38.15703422705684,8.7849558850225037E-3,27.614352827061779,8.8086480966476227E-3,23.764045012535458,75.004000000000005,62.008009081552807,23.354027234349431,67068.55862112224,66394.739162765138,7731,0.39341687882479931,60715.455278863024,60041.635820505922,6.1137302667267166,0.17489703892176242,-4.2603255927123485,-17.57301361298785,53.706035452613598,67068.55862112224,60613.816889877155,6454.7417312450934,0,67068.558621122254,1.0000000000000002]
[2,"T2-TRN-55-T2FER-DM","75T0104","T2-TRN-55-T2FER-DM","2 finger","off","off","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/13/2014","10:30:36","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,461,1.4,3.7,0,13640,32,13867,115,8004,86,21651,103,12.225296443,949,1660,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 2F-pen, tape around damper perimeter inside/outside frame gaps, no compressor--55/51 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm), unsealed cab, 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-TRN-55-T","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6: .;2F Open: Jade Control set to 6.9V",74.971999999999994,1.0999999999999999E-2,62.009,2.5999999999999999E-2,55.017000000000003,1.9E-2,51.002000000000002,1.9E-2,74.989999999999995,0.04,70.87,0.02,71.56,0,0.186,4.0000000000000001E-3,1.3105,2.5000000000000001E-3,13640,32,8004,86,12.228,0.114,null,null,null,null,null,null,461,2.4,460.5,2.4,459.2,2.4,3.7,0,3.3,0,3.4,0,1633.5,20.5,1089.5,23.2,137.30000000000001,16.600000000000001,460,null,460,null,459,null,3.2,null,3.2,null,3.2,null,0.57999999999999996,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.5,null,0,null,0,null,85,null,1745,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102.89,0.03,59.49,0.02,60.55,0.01,1.07,0.03,101.7,0.02,60.27,0.03,59.91,0.02,-0.35,0.04,null,null,72.91,0.02,null,null,null,null,101.91,0.03,69.819999999999993,0.02,60.03,0.02,9.7899999999999991,0.03,101.02,0.03,59.52,0.02,59.55,0.01,-0.03,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103,0.04,60.09,0.02,60.6,0.02,-0.51,0.02,103.3,0.03,60.77,0.02,0.45,0.03,null,null,70.8,0.02,null,null,null,null,102.91,0.02,60.56,0.01,9.1199999999999992,0.09,102.86,0.02,60.69,7.0000000000000007E-2,60.53,0.01,0.15,7.0000000000000007E-2,59.99,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60.06,0.03,59.99,0.02,60.16,0.02,60.32,0.02,70.72,0.03,70.87,0.03,null,null,70.989999999999995,0.03,71.42,0.02,71.2,0.02,59.22,0.02,73.3,0.01,70.23,0.02,59.67,0.02,60.63,0.02,60.46,0.02,71.430000000000007,0.01,70.239999999999995,0.14000000000000001,60.81,0.02,72.91,0.02,70.8,0.02,55.3,0.03,60.53,0.01,59.91,0.02,60.93,0.02,61.59,0.01,60.16,0.02,60.32,0.02,null,null,null,null,null,null,null,null,null,null,null,null,59.49,0.02,71.2,0.02,null,null,60.32,0.03,60.06,0.03,59.99,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69.680000000000007,0.08,null,null,null,null,null,null,null,null,null,null,null,null,59.86,0.02,61.03,0.31,56.32,0.16,75.510000000000005,0.03,75.41,0.03,75.099999999999994,0.02,75.84,0.03,75.84,0.03,75.81,0.04,75.61,0.04,62.82,0.15,63.85,0.16,62.96,0.18,72.069999999999993,0.1,66.05,0.12,64.63,0.18,62.21,0.14000000000000001,68.48,0.16,67.88,0.09,67.73,0.13,72.31,0.13,74.75,0.03,71.56,0.09,69.34,7.0000000000000007E-2,69.930000000000007,7.0000000000000007E-2,74.89,0.03,73.75,0.05,71.010000000000005,0.06,70.39,0.05,null,null,75.209999999999994,0.03,75.83,0.02,75.62,0.03,75.44,0.03,75.31,null,75.12,0.03,null,null,61.83,0.09,63.82,0.11,74.819999999999993,0.03,74.8,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.971999999999994,1.0999999999999999E-2,62.009,2.5999999999999999E-2,70.921000000000006,6.0000000000000001E-3,59.72,2.4E-2,55.017000000000003,1.9E-2,51.002000000000002,1.9E-2,3088.1,2.9,2987.1,2.9,0.58099999999999996,2E-3,-0.13600000000000001,2E-3,0.186,4.0000000000000001E-3,1.3105,2.5000000000000001E-3,29.459,1E-3,1771,14,1660,null,0.127837634678025,381.86379854672845,13.03,0.13600000000000001,1.5019090715374823,13783.166899400612,203.8876857637795,381.86247015213075,1758.3965937649143,12024.770305635699,8.5616562572157703E-3,26.74332080274942,69.419090928462523,13.029909344894346,13.442919276270066,6.9784105902595704E-3,20.778639095922678,8.7931761712854856E-3,27.615543367471542,8.2749430184658659E-3,26.061323594405088,72.433568048780842,60.732320257250748,25.695347291114356]
[2,"T2-CAN-55-CE-DM","75T0123","T2-CAN-55-CE-DM","closed","off","off","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/6/2014","22:33:40","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.9,1,3.7,0,null,null,null,null,null,null,null,null,null,952,1570,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo closed, no compressor, 55/51 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm),--100% inlet/outlet Meriam, adjust code tester speed to match total static of run T2-CAN-55-CE-DM-SPWCT-SS","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.001000000000005,1.0999999999999999E-2,61.994,4.2999999999999997E-2,54.982999999999997,3.5000000000000003E-2,51.081000000000003,4.4999999999999998E-2,74.900000000000006,0.03,70,0.12,71.64,0.01,0.217,3.0000000000000001E-3,1.1073999999999999,2.3999999999999998E-3,null,null,null,null,null,null,null,null,null,null,null,null,460.9,2.2000000000000002,460.3,2.2000000000000002,459.1,2.2000000000000002,3.7,0,3.2,0,3.4,0,1591.6,18.7,1088.4000000000001,20.5,115.1,14.9,460,null,460,null,460,null,3.2,null,3.1,null,3.1,null,0.55000000000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,null,1655,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64.34,0.02,62.56,0.03,65.17,0.01,64.09,0.02,71.040000000000006,0.02,70.8,0.02,70.41,0.02,71.36,0.02,71.260000000000005,0.02,71.13,0.02,62.19,0.02,67.739999999999995,0.02,69.52,0.01,63.07,0.01,64.599999999999994,0.03,61.83,0.02,70.349999999999994,0.04,69.06,0.02,62.7,0.02,68.040000000000006,0.02,69.709999999999994,0.04,54.75,0.04,65.44,0.01,64.27,0.01,65.16,0.04,66.72,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,71.13,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.5,0.02,54.33,0.36,54.59,0.31,75.5,0.03,75.290000000000006,0.05,74.92,7.0000000000000007E-2,74.489999999999995,0.11,75.91,0.03,75.83,0.03,75.53,0.05,71.39,0.06,71.25,0.09,72.69,0.04,74.12,0.03,74.260000000000005,0.03,73.67,0.04,72.77,0.05,73.239999999999995,0.05,73.7,7.0000000000000007E-2,73.47,7.0000000000000007E-2,73.52,0.04,72.2,0.05,72.41,0.05,70.64,0.24,72.58,0.04,62.97,0.09,66.59,0.13,59.72,0.26,57.28,0.09,null,null,74.42,0.15,75.8,0.03,75.58,0.03,75.400000000000006,0.03,75.209999999999994,null,75.16,0.03,null,null,null,null,74.47,0.03,72.67,0.04,72.38,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75.001000000000005,1.0999999999999999E-2,61.994,4.2999999999999997E-2,70.834000000000003,1.2E-2,59.615000000000002,4.5999999999999999E-2,54.982999999999997,3.5000000000000003E-2,51.081000000000003,4.4999999999999998E-2,2846.4,3.1,2735,3,0.51900000000000002,2E-3,-0.16,3.0000000000000001E-3,0.217,3.0000000000000001E-3,1.1073999999999999,2.3999999999999998E-3,29.265999999999998,1E-3,1707,13,1570,null,0.12973324008392448,354.82041162953345,13.029,0.16,1.569977501743461,12706.81060822731,166.75919527559057,354.82636768477448,1633.9601919146662,11072.850416312644,8.5516562622191331E-3,26.732504202629521,69.264022498256537,13.029437416182976,13.440351419845832,7.0284124762557219E-3,20.824646419520114,8.7764330464497678E-3,27.604294579466256,8.2294632924967727E-3,25.990439609809233,72.434039750578819,60.71692861701284,25.607908497324836]
[2,"T2-CAN-95-1ER-DM","75T0138","T2-CAN-95-1ER-DM","10% open","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","22:31:40","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,461.2,1.3,15.4,0,47478,73,47252,512,51,30,47492,82,5.5663384899999997,952,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 10%-open, both stages, 95/75 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm),--unsealed cab, 100% inlet/outlet Meriam, adjust code tester speed to match total static--of run T2-CAN-95-1E-DM-SPWCT-SSR","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.043999999999997,2.5000000000000001E-2,61.985999999999997,1.4999999999999999E-2,95.066999999999993,1.0999999999999999E-2,74.995999999999995,1.6E-2,75.17,0.17,59.35,0.03,61.9,0.03,0.184,4.0000000000000001E-3,1.0523,2.3999999999999998E-3,47478,73,51,30,5.5659999999999998,1.7000000000000001E-2,null,null,null,null,null,null,461.2,2.6,461.8,2.6,458.7,2.6,15.4,0.1,13,0,12.6,0.1,6998,56.6,3084.7,62.8,1533.8,42.2,460,null,460,null,460,null,3.2,null,3.1,null,3.1,null,0.56000000000000005,460,null,460,null,460,null,4.5999999999999996,null,4.8,null,4.5,null,3150,null,0.85,460,460,460,5,4.5999999999999996,4.4000000000000004,3010,0.81,460.2,null,1.6,null,696.2,null,85,null,8481.2000000000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,215.54,0.24,106.06,0.16,106.44,0.08,0.39,0.12,243.53,0.28000000000000003,172.78,0.09,115.13,0.08,-57.65,0.11,206.73,0.05,100.03,0.09,103.55,0.05,3.58,0.05,75.08,0.06,48.55,0.35,44.13,0.03,4.42,0.37,74.5,0.05,56.08,0.19,43.75,0.03,12.33,0.19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,247.26,0.27,167.57,0.23,116.23,0.08,51.34,0.23,227.91,0.4,110.37,0.12,10.4,0.17,215.7,0.05,99.15,0.11,106.49,0.05,7.36,0.05,81.290000000000006,0.08,48.08,0.05,2.96,0.39,80.849999999999994,0.09,58.96,0.43,47.81,0.06,11.16,0.46,105.02,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105.47,0.09,105.02,0.11,100.24,0.12,100.58,0.11,59.38,0.03,58.97,0.03,58.5,0.04,59.6,0.03,59.16,0.05,59.28,0.02,105.61,0.11,101.37,0.1,49.78,0.61,55.87,0.28000000000000003,167.21,0.26,100.78,0.11,99.55,0.11,51.33,0.11,60.46,0.64,100.03,0.09,99.15,0.11,94.11,0.08,106.17,0.1,105.95,0.14000000000000001,100.95,0.08,100.76,0.09,100.24,0.12,100.58,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.28,0.02,null,null,99.97,0.17,105.47,0.09,105.02,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,51.04,0.35,null,null,null,null,null,null,null,null,null,null,null,null,173.36,0.11,94.44,0.23,93.94,0.19,75.88,0.1,75.760000000000005,0.1,75.62,0.1,77.22,0.09,76.23,0.1,76.16,0.1,76.03,0.1,79.45,0.11,79.540000000000006,0.11,78.319999999999993,0.1,76.34,0.11,76.430000000000007,0.12,76.849999999999994,0.1,77.14,0.11,77.02,0.11,76.25,0.1,76.36,0.11,76.260000000000005,0.09,77.22,0.1,77.16,0.11,77.680000000000007,0.18,76.83,0.1,83.03,0.15,80.180000000000007,0.1,84.3,0.21,88.94,0.33,null,null,76.05,0.12,76.209999999999994,0.1,75.900000000000006,0.1,75.67,0.11,75.540000000000006,null,75.400000000000006,0.1,null,null,null,null,76.14,0.12,77.08,0.09,77.13,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-1ER-DM",75.043999999999997,2.5000000000000001E-2,61.985999999999997,1.4999999999999999E-2,59.15,8.9999999999999993E-3,56.231999999999999,1.2E-2,95.066999999999993,1.0999999999999999E-2,74.995999999999995,1.6E-2,2753.9,3.2,2684.9,3.2,0.48599999999999999,2E-3,-0.156,4.0000000000000001E-3,0.184,4.0000000000000001E-3,1.0523,2.3999999999999998E-3,29.181999999999999,0,8532,23,1540,null,0.1491979675201755,405.19184019129267,13.028,0.151,1.5689249217656818,12565.493075239818,153.29552825196851,428.47708333819935,1823.118651923457,10742.37442331636,9.5067926584528444E-3,29.129189331778722,57.581075078234313,14.101454654730464,13.149822216335625,1.3901231133813472E-2,38.152053696024112,8.7610001145092212E-3,27.597893580205678,8.9314381240403161E-3,23.906818636483194,77.972332757026393,64.119332752385432,23.524054991657586,{"$f":"(XZ542-YL542)*XT542","v":70431.276736581043},{"$f":"0.24*(YJ542-YA542)*XT542","v":61494.289717990228},{"$f":"XK542-XM542","v":6992},{"$f":"YO542*3.413/YM542","v":0.33882242528773471},{"$f":"YM542-(XM542-XU542)*3.413","v":65698.454374505018},{"$f":"YN542-(XM542-XU542)*3.413","v":56761.467355914196},{"$f":"YQ542/XK542","v":7.7002407846349064},{"$f":"(YA542-YW542)/(YJ542-YW542)","v":0.15885008917271889},{"$f":"-XZ542+YL542","v":-5.6051343401211362},{"$f":"-YJ542+YA542","v":-20.39125767879208},{"$f":"(-(-0.0182984848494437-(YU542/YV542))+SQRT((-0.0182984848494437-(YU542/YV542))^2-4*0.00577826340327261*(6.76723916086377-XZ542+(YU542/YV542)*YJ542)))/(2*0.00577826340327261)","v":53.730212040711947},{"$f":"XT542*(XZ542-YL542)","v":70431.276736581043},{"$f":"XT542*(YG542-YI542)","v":46380.17664553607},{"$f":"XT542*(YI542-YL542)","v":4809.6139285097388},{"$f":"XW542*(YE542-YG542)","v":19241.486162535221},{"$f":"SUM(YY542:ZA542)","v":70431.276736581029},{"$f":"ZB542/YX542","v":0.99999999999999978}]
[2,"T2-CAN-95-2ER-DM","75T0139","T2-CAN-95-2ER-DM","20% open","on","on","3 turns","unsealed","unsealed",null,5.75,null,0,0,"CUST 6","8/7/2014","21:13:27","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,461.1,1.2,15.3,0,47292,64,47480,549,918,171,48211,176,5.6625557904627675,null,null,null,5.5546159270000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,".","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.003,0.02,62.006,2.3E-2,95.206999999999994,0.04,74.991,1.9E-2,75.05,0.17,58.92,0.04,61.51,0.02,0.182,4.0000000000000001E-3,1.0217000000000001,2.3999999999999998E-3,47292,64,918,171,5.6630000000000003,2.5999999999999999E-2,null,null,null,null,null,null,461.1,2.5,461.4,2.5,458.9,2.4,15.3,0.1,13,0,12.6,0.1,6947.5,53.9,3123.9,61.3,1565.8,41.7,460,null,460,null,460,null,3.1,null,3.2,null,3,null,0.56000000000000005,460,null,460,null,460,null,4.5999999999999996,null,4.8,null,4.4000000000000004,null,3130,null,0.86,460,460,460,5,4.5,4.4000000000000004,3000,0.81,460.2,null,1.6,null,696.1,null,85,null,8451.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,215.66,0.31,105.9,0.18,106.48,0.1,0.57999999999999996,0.14000000000000001,243.29,0.34,172.97,0.14000000000000001,115.05,0.1,-57.92,0.16,209.8,0.05,99.75,0.11,104.53,0.05,4.93,0.05,74.34,0.08,47.83,0.42,43.64,0.05,4.1900000000000004,0.43,73.77,0.08,55.38,0.33,43.26,0.05,12.12,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,247.57,0.32,167.62,0.14000000000000001,116.32,0.09,51.3,0.12,227.86,0.42,110.35,0.13,10.119999999999999,0.1,215.8,0.05,99.23,0.1,106.62,0.05,7.4,0.05,81.75,0.04,48.36,0.03,2.77,0.25,81.400000000000006,0.05,59.06,0.2,48.14,0.03,10.92,0.2,105.04,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105.48,0.12,105.04,0.13,100.3,0.12,100.59,0.11,59.13,0.04,58.75,0.04,58.26,0.03,59.34,0.04,58.72,0.05,59.01,0.03,105.54,0.13,101.35,0.13,48.97,0.68,55.16,0.43,167.39,0.17,100.83,0.11,99.6,0.1,51.49,0.09,60.71,0.3,99.75,0.11,99.23,0.1,94.18,0.05,106.21,0.12,106.03,0.13,101.14,7.0000000000000007E-2,100.69,0.12,100.3,0.12,100.59,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.01,0.03,null,null,100.24,0.13,105.48,0.12,105.04,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,51.13,0.24,null,null,null,null,null,null,null,null,null,null,null,null,173.53,0.17,94.52,0.25,93.96,0.2,75.739999999999995,0.1,75.59,0.09,75.400000000000006,0.09,76.87,0.08,76.099999999999994,0.1,76.040000000000006,0.09,75.88,0.09,82.21,0.16,82.69,0.14000000000000001,79.39,0.11,76.55,0.1,77.42,0.1,77.37,0.09,77.2,0.1,76.81,0.1,76.37,0.09,76.31,0.09,76.099999999999994,0.09,76.8,0.09,76.66,0.1,77.27,0.27,76.53,0.1,80.37,0.28000000000000003,79.48,0.1,81.64,0.16,84.37,1.3,null,null,75.760000000000005,0.1,76.069999999999993,0.09,75.78,0.11,75.540000000000006,0.11,75.39,null,75.28,0.11,null,null,null,null,76.86,0.11,76.66,0.08,76.73,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-2ER-DM",75.003,0.02,62.006,2.3E-2,58.942,1.4E-2,56.03,1.4999999999999999E-2,95.206999999999994,0.04,74.991,1.9E-2,2713.3,3.2,2645.4,3.1,0.46800000000000003,2E-3,-0.14099999999999999,4.0000000000000001E-3,0.182,4.0000000000000001E-3,1.0217000000000001,2.3999999999999998E-3,29.158000000000001,0,8514,23,1540,null,0.18207831325301196,488.55253012048166,13.032999999999999,0.13300000000000001,1.6007066984138976,12385.721193337271,145.446174992126,523.30481671642838,2226.0869728148696,10159.634220522401,9.6968051823338695E-3,29.505802529537242,57.341293301586106,14.104700034825148,13.144006510301148,1.386333387970233E-2,38.144706820700229,8.7838731757527988E-3,27.612924116345358,8.8617770849080488E-3,23.780340391120198,78.661763867063186,64.628842516602148,23.389872596463654,{"$f":"(XZ543-YL543)*XT543","v":75750.20298903533},{"$f":"0.24*(YJ543-YA543)*XT543","v":63376.656992340701},{"$f":"XK543-XM543","v":6974},{"$f":"YO543*3.413/YM543","v":0.31422043850424164},{"$f":"YM543-(XM543-XU543)*3.413","v":70990.590784283457},{"$f":"YN543-(XM543-XU543)*3.413","v":58617.044787588828},{"$f":"YQ543/XK543","v":8.3381008673107182},{"$f":"(YA543-YW543)/(YJ543-YW543)","v":0.15686164631559099},{"$f":"-XZ543+YL543","v":-6.1159299330735877},{"$f":"-YJ543+YA543","v":-21.320470565477081},{"$f":"(-(-0.0182984848494437-(YU543/YV543))+SQRT((-0.0182984848494437-(YU543/YV543))^2-4*0.00577826340327261*(6.76723916086377-XZ543+(YU543/YV543)*YJ543)))/(2*0.00577826340327261)","v":53.374727080859245},{"$f":"XT543*(XZ543-YL543)","v":75750.20298903533},{"$f":"XT543*(YG543-YI543)","v":47469.313470760768},{"$f":"XT543*(YI543-YL543)","v":4836.2252395932255},{"$f":"XW543*(YE543-YG543)","v":23444.664278681335},{"$f":"SUM(YY543:ZA543)","v":75750.20298903533},{"$f":"ZB543/YX543","v":1}]
[2,"T2-CAN-95-3ER-DM","75T0140","T2-CAN-95-3ER-DM","30% open","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","23:32:52","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,461.1,1.2,15.4,0,44651,123,43958,570,0,0,44649,123,5.2472675989999997,952,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 30%-open, both stages, 95/75 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm),--unsealed cab, 100% inlet/outlet Meriam, adjust code tester speed to match total static of run--T2-CAN-95-3E-DM-SPWCT-SSR","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.061999999999998,4.5999999999999999E-2,62.034999999999997,2.7E-2,94.983000000000004,1.2E-2,75.010000000000005,0.02,75.02,0.19,59.88,0.02,62.43,0.03,0.14899999999999999,4.0000000000000001E-3,0.99860000000000004,2.5000000000000001E-3,44651,123,0,0,5.2480000000000002,0.02,null,null,null,null,null,null,461.1,2.4,461.9,2.4,458.6,2.4,15.4,0.1,12.9,0,12.6,0.1,6996.9,51.4,3074.1,59.1,1511.8,39.1,460,null,460,null,460,null,3.2,null,3.1,null,3,null,0.56000000000000005,460,null,460,null,460,null,4.5999999999999996,null,4.8,null,4.4000000000000004,null,3140,null,0.85,460,460,460,5.0999999999999996,4.5999999999999996,4.4000000000000004,3000,0.81,460.2,null,1.6,null,696.5,null,85,null,8461.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,215.47,0.23,105.84,0.17,106.42,7.0000000000000007E-2,0.59,0.13,243.12,0.28000000000000003,172.6,0.19,115.01,0.08,-57.6,0.18,210.07,0.05,99.73,0.08,104.64,0.05,4.8499999999999996,0.05,74.27,0.08,47.63,0.24,43.6,0.05,4.03,0.24,73.7,0.08,55.34,0.23,43.23,0.05,12.11,0.21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,248.53,0.27,166.37,0.14000000000000001,116.6,0.08,49.76,0.13,226.66,0.37,109.99,0.12,9.09,0.13,216.4,0.05,100.06,0.1,106.71,0.05,6.66,0.05,85.46,0.04,50.63,0.02,3,0.33,84.89,0.05,61.18,0.25,50.28,0.03,10.9,0.24,105.07,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105.51,0.08,105.07,0.11,101.06,0.11,101.36,0.1,59.88,0.04,59.51,0.05,59.02,0.04,60.07,0.03,59.71,0.04,59.73,0.03,105.38,0.12,101.22,0.1,48.8,0.45,55.11,0.3,166.24,0.17,101.39,0.14000000000000001,100.45,0.11,53.69,0.1,63.11,0.34,99.73,0.08,100.06,0.1,94.29,0.06,106.21,0.12,105.91,0.12,101.78,0.06,101.3,0.09,101.06,0.11,101.36,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.73,0.03,null,null,100.89,0.14000000000000001,105.51,0.08,105.07,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,53.64,0.33,null,null,null,null,null,null,null,null,null,null,null,null,173.54,0.12,94.39,0.23,93.79,0.19,75.790000000000006,0.14000000000000001,75.569999999999993,0.13,75.38,0.13,76.56,0.09,76.150000000000006,0.14000000000000001,76.040000000000006,0.13,75.84,0.13,91.75,0.18,87.86,0.12,88.19,0.16,78.14,0.15,87.94,0.16,78.08,0.15,77.86,0.14000000000000001,76.55,0.14000000000000001,78.73,0.15,77.069999999999993,0.15,77.53,0.14000000000000001,76.7,0.13,76.81,0.13,76.48,0.14000000000000001,76.75,0.15,76.8,0.13,81.02,0.21,81.88,0.21,86.21,0.17,null,null,75.569999999999993,0.12,76.099999999999994,0.15,75.81,0.16,75.55,0.15,75.44,null,75.27,0.15,null,null,null,null,84.15,0.13,77.28,0.12,76.53,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-3ER-DM",75.061999999999998,4.5999999999999999E-2,62.034999999999997,2.7E-2,59.688000000000002,1.4E-2,56.777999999999999,2.3E-2,94.983000000000004,1.2E-2,75.010000000000005,0.02,2683.4,3.4,2613.1,3.3,0.42799999999999999,2E-3,-0.109,4.0000000000000001E-3,0.14899999999999999,4.0000000000000001E-3,0.99860000000000004,2.5000000000000001E-3,29.189,1E-3,8509,22,1540,null,0.28428778271506283,755.523211343551,13.029,9.0999999999999998E-2,1.6374659635236715,12229.706232739478,131.39078311811022,860.17738236836226,3660.4364867448453,8569.2697459946321,1.0328863507032524E-2,30.785925449712032,58.050534036476328,14.099587065366096,13.164993249713962,1.3933614026102253E-2,38.167099150396815,8.7890636504831705E-3,27.632994298067903,9.1278471147504883E-3,24.251667173482108,81.06351148718943,66.321093292765738,23.852039078933458,{"$f":"(XZ544-YL544)*XT544","v":84799.393365818032},{"$f":"0.24*(YJ544-YA544)*XT544","v":67546.068903090985},{"$f":"XK544-XM544","v":6969},{"$f":"YO544*3.413/YM544","v":0.28048782020636043},{"$f":"YM544-(XM544-XU544)*3.413","v":79991.810108600141},{"$f":"YN544-(XM544-XU544)*3.413","v":62738.485645873094},{"$f":"YQ544/XK544","v":9.4008473508755603},{"$f":"(YA544-YW544)/(YJ544-YW544)","v":0.14935158688833836},{"$f":"-XZ544+YL544","v":-6.9338863707785734},{"$f":"-YJ544+YA544","v":-23.012977450713102},{"$f":"(-(-0.0182984848494437-(YU544/YV544))+SQRT((-0.0182984848494437-(YU544/YV544))^2-4*0.00577826340327261*(6.76723916086377-XZ544+(YU544/YV544)*YJ544)))/(2*0.00577826340327261)","v":54.010057797042748},{"$f":"XT544*(XZ544-YL544)","v":84799.393365818032},{"$f":"XT544*(YG544-YI544)","v":41352.637410477953},{"$f":"XT544*(YI544-YL544)","v":4887.3341986794221},{"$f":"XW544*(YE544-YG544)","v":38559.421756660675},{"$f":"SUM(YY544:ZA544)","v":84799.393365818047},{"$f":"ZB544/YX544","v":1.0000000000000002}]
[2,"T2-CAN-95-CE-DM","75T0141","T2-CAN-95-CE-DM","closed","on","on","3 turns","unsealed","unsealed",null,5.75,null,0,0,"CUST 6","8/7/2014","18:41:07","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,461.1,1.2,15.1,0,48955,97,48988,523,1233,162,50189,123,5.9164210769999999,952,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,".","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.021000000000001,3.3000000000000002E-2,61.997999999999998,1.4E-2,94.918999999999997,1.7000000000000001E-2,75.006,1.4999999999999999E-2,75.16,0.18,58.87,0.03,61.33,0.01,0.20699999999999999,3.0000000000000001E-3,1.0653999999999999,2.3E-3,48955,97,1233,162,5.9160000000000004,0.02,null,null,null,null,null,null,461.1,2.5,460.5,2.5,459.2,2.5,15.1,0.1,13.1,0,12.6,0.1,6858.2,58.9,3189.1,64.900000000000006,1625.1,47.7,460,null,460,null,460,null,3.2,null,3.1,null,3.1,null,0.55000000000000004,460,null,460,null,460,null,4.5999999999999996,null,4.8,null,4.4000000000000004,null,3120,null,0.85,460,460,460,4.9000000000000004,4.5,4.4000000000000004,2990,0.81,460.1,null,1.6,null,696.6,null,85,null,8441.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,213.2,0.22,105.28,0.14000000000000001,105.68,7.0000000000000007E-2,0.39,0.11,241.5,0.24,171.68,0.09,114.51,7.0000000000000007E-2,-57.17,0.1,207.03,0.05,99.17,7.0000000000000007E-2,103.64,0.05,4.51,0.05,75.13,0.05,48.65,0.33,44.15,0.03,4.5,0.35,74.55,0.05,55.96,0.17,43.77,0.03,12.19,0.17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,245.23,0.24,166.84,0.31,115.62,7.0000000000000007E-2,51.22,0.33,226.13,0.35,109.81,0.11,10.39,0.16,215.17,0.05,98.72,0.12,106.31,0.05,7.68,0.05,80.67,0.1,47.68,0.06,2.83,0.44,80.2,0.12,58.39,0.63,47.39,0.08,11.01,0.67,104.21,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.59,0.09,104.21,0.1,99.76,0.13,100.04,0.12,58.91,0.04,58.53,0.03,58.13,0.04,59.17,0.03,58.62,0.04,58.87,0.03,104.83,0.09,100.51,0.08,49.94,0.56999999999999995,55.88,0.25,166.59,0.32,100.28,0.12,99.1,0.12,50.96,0.12,59.91,0.88,99.17,7.0000000000000007E-2,98.72,0.12,93.19,0.04,105.32,0.09,105.26,0.09,100.46,0.08,100.04,0.09,99.76,0.13,100.04,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.87,0.03,null,null,99.41,0.16,104.59,0.09,104.21,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50.52,0.4,null,null,null,null,null,null,null,null,null,null,null,null,172.37,0.11,92.24,0.16,94.47,0.18,75.86,0.1,75.77,0.1,75.58,0.1,77.28,0.1,76.209999999999994,0.1,76.16,0.1,76.040000000000006,0.1,79.12,0.11,79.31,0.1,77.33,0.1,76.239999999999995,0.1,76.09,0.11,76.45,0.11,77.13,0.1,77.16,0.1,76.27,0.11,76.47,0.11,76.17,0.11,77.23,0.09,77.03,0.1,78.260000000000005,0.17,76.989999999999995,0.09,83.54,7.0000000000000007E-2,81.17,0.1,86.66,0.19,89,0.12,null,null,76.11,0.12,76.2,0.1,75.900000000000006,0.11,75.67,0.11,75.55,null,75.400000000000006,0.11,null,null,null,null,76.010000000000005,0.11,77.13,0.09,77.13,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-CE-DM",75.021000000000001,3.3000000000000002E-2,61.997999999999998,1.4E-2,58.741999999999997,5.0000000000000001E-3,55.901000000000003,7.0000000000000001E-3,94.918999999999997,1.7000000000000001E-2,75.006,1.4999999999999999E-2,2771.6,3,2701.3,3,0.51600000000000001,3.0000000000000001E-3,-0.16600000000000001,3.0000000000000001E-3,0.20699999999999999,3.0000000000000001E-3,1.0653999999999999,2.3E-3,29.137,0,8483,22,1550,null,0.12973324008392448,354.82041162953345,13.029,0.16,1.5570757003961455,12656.944243287851,163.75238059842522,375.94710935420159,1599.9953207934491,11056.948922494403,9.4280348791031792E-3,28.941486158330562,57.18492429960385,14.098057830610408,13.138716328642202,1.3945432208396653E-2,38.164380370135078,8.7743450918301262E-3,27.606887645983342,8.8334255559396387E-3,23.700733044151065,77.557015835079312,63.861853990249386,23.320927961401711,{"$f":"(XZ545-YL545)*XT545","v":71139.09171468296},{"$f":"0.24*(YJ545-YA545)*XT545","v":61883.622404080626},{"$f":"XK545-XM545","v":6933},{"$f":"YO545*3.413/YM545","v":0.33262062291858224},{"$f":"YM545-(XM545-XU545)*3.413","v":66407.828589665383},{"$f":"YN545-(XM545-XU545)*3.413","v":57152.35927906305},{"$f":"YQ545/XK545","v":7.8283424012336891},{"$f":"(YA545-YW545)/(YJ545-YW545)","v":0.15565009675622585},{"$f":"-XZ545+YL545","v":-5.6205581969288509},{"$f":"-YJ545+YA545","v":-20.372091535475462},{"$f":"(-(-0.0182984848494437-(YU545/YV545))+SQRT((-0.0182984848494437-(YU545/YV545))^2-4*0.00577826340327261*(6.76723916086377-XZ545+(YU545/YV545)*YJ545)))/(2*0.00577826340327261)","v":53.429469355579343},{"$f":"XT545*(XZ545-YL545)","v":71139.09171468296},{"$f":"XT545*(YG545-YI545)","v":49439.981001053391},{"$f":"XT545*(YI545-YL545)","v":4807.1717556758931},{"$f":"XW545*(YE545-YG545)","v":16891.938957953662},{"$f":"SUM(YY545:ZA545)","v":71139.091714682945},{"$f":"ZB545/YX545","v":0.99999999999999978}]
[2,"T2-CAN-95-OER-DM","75T0142","T2-CAN-95-OER-DM","open","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/8/2014","0:52:06","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,461.1,1.3,15.5,0,32547,80,32052,354,0,0,32530,80,3.7576527670000002,952,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo fully open, both stages, 95/75 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm),--unsealed cab, 100% inlet/outlet Meriam, adjust code tester speed to match total static of run--T2-CAN-95-OE-DM-SPWCT-SSR","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",74.706999999999994,1.4E-2,62.115000000000002,1.2999999999999999E-2,94.885999999999996,4.1000000000000002E-2,75.001000000000005,3.5000000000000003E-2,74.66,0.12,63.33,0.02,65.22,0.02,0.115,5.0000000000000001E-3,0.98350000000000004,2.3999999999999998E-3,32547,80,0,0,3.758,1.4E-2,null,null,null,null,null,null,461.1,2.9,461.7,2.9,459,2.9,15.5,0.1,13.1,0,12.8,0.1,7037.5,74.3,3125.7,79.2,1619.8,61.5,460,null,460,null,460,null,3.2,null,3.1,null,3,null,0.56000000000000005,460,null,460,null,460,null,4.7,null,4.9000000000000004,null,4.5,null,3220,null,0.86,460,460,460,5.0999999999999996,4.5999999999999996,4.5,3080,0.81,460.1,null,1.6,null,695.4,null,85,null,8610.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,218.63,0.22,107.44,0.08,107.44,7.0000000000000007E-2,0.01,0.05,252.61,0.25,175.07,0.09,117.79,7.0000000000000007E-2,57.28,0.1,210.93,0.05,99.99,0.06,104.94,0.05,4.96,0.05,84.26,0.08,59.9,0.48,49.91,0.05,9.99,0.46,83.61,0.08,64.45,0.2,49.51,0.05,14.94,0.19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,255.06,0.25,167.39,0.26,118.5,7.0000000000000007E-2,48.89,0.28000000000000003,231.4,0.35,111.46,0.11,8.6999999999999993,0.13,220.93,0.05,101.79,0.12,108.18,0.05,6.36,0.05,89.29,7.0000000000000007E-2,52.9,0.04,4.82,1.1399999999999999,88.74,0.1,63.43,0.51,52.58,0.05,10.85,0.53,105.58,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106.02,0.08,105.58,0.08,102.61,0.12,102.91,0.11,63.31,0.05,63.07,0.04,62.71,0.05,63.49,0.05,63.09,0.06,63.3,0.04,106.45,7.0000000000000007E-2,101.17,7.0000000000000007E-2,61.1,0.45,64.67,0.22,167.23,0.28000000000000003,103.04,0.11,102.21,0.11,56.86,0.51,65.73,0.61,99.99,0.06,101.79,0.12,93.66,0.12,106.81,0.09,106.57,0.08,102.95,0.08,102.53,0.08,102.61,0.12,102.91,0.11,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.3,0.04,null,null,102.76,0.12,106.02,0.08,105.58,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.7,1.1399999999999999,null,null,null,null,null,null,null,null,null,null,null,null,175.63,0.09,95.73,0.2,94.99,0.15,75.23,0.08,75.06,0.08,74.790000000000006,0.08,75.64,7.0000000000000007E-2,75.61,7.0000000000000007E-2,75.52,0.08,75.3,7.0000000000000007E-2,89,0.37,86.64,0.36,88.41,0.73,92.51,0.28999999999999998,85.41,0.79,83.18,0.55000000000000004,87.56,0.35,85.83,0.23,85,0.6,85.17,0.14000000000000001,86.98,0.4,89.54,0.31,85.02,0.37,85.46,0.16,85.26,0.13,77.400000000000006,0.09,75.459999999999994,7.0000000000000007E-2,75.3,7.0000000000000007E-2,76.239999999999995,0.11,null,null,74.89,7.0000000000000007E-2,75.58,0.09,75.319999999999993,0.09,75.09,0.08,74.98,null,74.849999999999994,0.09,null,null,null,null,88.73,0.43,91.07,0.34,87.17,0.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-OER-DM",74.706999999999994,1.4E-2,62.115000000000002,1.2999999999999999E-2,63.201999999999998,0.01,60.317999999999998,2.5999999999999999E-2,94.885999999999996,4.1000000000000002E-2,75.001000000000005,3.5000000000000003E-2,2670.6,3.3,2581.8000000000002,3.2,0.379,2E-3,-4.3999999999999997E-2,5.0000000000000001E-3,0.115,5.0000000000000001E-3,0.98350000000000004,2.3999999999999998E-3,29.199000000000002,0,8657,23,1530,null,0.58782060896955146,1628.2630868456577,13.03,4.3999999999999997E-2,1.665351949886507,12079.864971820749,114.9547466456693,1693.6339079206889,7208.3596917292016,4871.5052800915473,1.1923242501885183E-2,33.940225272594688,61.536648050113492,14.097248031592656,13.264717807176638,1.3948951414824126E-2,38.160138181680864,8.9258037974912774E-3,27.696025919927081,1.048335638587785E-2,26.585501801509711,86.792469241240781,70.237986513779759,26.178065769305579,{"$f":"(XZ546-YL546)*XT546","v":93765.838689467651},{"$f":"0.24*(YJ546-YA546)*XT546","v":73220.858337904006},{"$f":"XK546-XM546","v":7127},{"$f":"YO546*3.413/YM546","v":0.25941698319957829},{"$f":"YM546-(XM546-XU546)*3.413","v":88936.289239769321},{"$f":"YN546-(XM546-XU546)*3.413","v":68391.308888205676},{"$f":"YQ546/XK546","v":10.273338251099609},{"$f":"(YA546-YW546)/(YJ546-YW546)","v":0.12749559466317273},{"$f":"-XZ546+YL546","v":-7.7621595032891086},{"$f":"-YJ546+YA546","v":-25.255821191127289},{"$f":"(-(-0.0182984848494437-(YU546/YV546))+SQRT((-0.0182984848494437-(YU546/YV546))^2-4*0.00577826340327261*(6.76723916086377-XZ546+(YU546/YV546)*YJ546)))/(2*0.00577826340327261)","v":57.84611546165457},{"$f":"XT546*(XZ546-YL546)","v":93765.838689467651},{"$f":"XT546*(YG546-YI546)","v":13414.981398432104},{"$f":"XT546*(YI546-YL546)","v":4921.7722536803185},{"$f":"XW546*(YE546-YG546)","v":75429.085037355253},{"$f":"SUM(YY546:ZA546)","v":93765.838689467681},{"$f":"ZB546/YX546","v":1.0000000000000002}]
[2,"T2-CAN-55-T1ER-DM","75T0125","T2-CAN-55-T1ER-DM","10% open","off","off","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","2:20:10","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.9,0.5,3.6,0,null,null,null,null,null,null,null,null,null,952,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 10%-open, tape around damper perimeter inside/outside frame gaps, no compressor, 55/51 ambient,--2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm), unsealed cab, 100% inlet/outlet Meriam, adjust code tester speed","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.004000000000005,1.2E-2,62.005000000000003,4.9000000000000002E-2,54.853999999999999,2.3E-2,50.993000000000002,4.1000000000000002E-2,74.989999999999995,0.04,72.150000000000006,0.12,73.489999999999995,0.01,0.19700000000000001,3.0000000000000001E-3,1.0018,2.2000000000000001E-3,null,null,null,null,null,null,null,null,null,null,null,null,460.9,2.1,460.2,2.1,459.1,2.1,3.6,0,3.2,0,3.3,0,1558.4,16.7,1089.5999999999999,19.5,86.4,12.6,460,null,460,null,460,null,3.2,null,3.1,null,3.1,null,0.54,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.5,null,0,null,0,null,85,null,1595,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.72,0.02,61.51,0.02,61.88,0.05,61.56,0.06,73.09,0.01,72.930000000000007,0.02,72.67,0.02,73.42,0.02,73.44,0.02,73.33,0.02,60.36,0.03,71.430000000000007,0.01,71.760000000000005,0.02,61.11,0.01,62.38,0.05,60.86,0.06,72.61,0.05,71.739999999999995,0.01,61.45,0.03,71.44,0.01,71.959999999999994,7.0000000000000007E-2,55.48,0.02,63.23,0.02,62.24,0.02,64.099999999999994,0.05,65.41,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,73.33,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.72,0.04,54.09,0.32,54.29,0.28000000000000003,75.510000000000005,0.04,75.33,0.05,74.959999999999994,0.06,74.819999999999993,0.12,75.91,0.04,75.849999999999994,0.03,75.56,0.05,72.319999999999993,0.06,72.459999999999994,0.05,72.75,0.04,74.28,0.04,74.239999999999995,0.04,73.849999999999994,0.04,73.150000000000006,0.04,73.45,0.04,73.959999999999994,0.04,73.760000000000005,0.05,73.73,0.04,72.62,0.04,72.62,0.06,71.989999999999995,0.11,72.87,0.04,70.680000000000007,0.06,70.53,0.04,69.41,0.05,69.459999999999994,0.06,null,null,74.55,0.13,75.819999999999993,0.03,75.599999999999994,0.04,75.44,0.04,75.23,null,75.16,0.05,null,null,null,null,74.489999999999995,0.04,73.16,0.04,72.86,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75.004000000000005,1.2E-2,62.005000000000003,4.9000000000000002E-2,72.977999999999994,8.0000000000000002E-3,60.771000000000001,4.4999999999999998E-2,54.853999999999999,2.3E-2,50.993000000000002,4.1000000000000002E-2,2711.7,2.9,2594.6999999999998,2.9,0.51500000000000001,3.0000000000000001E-3,-0.192,2E-3,0.19700000000000001,3.0000000000000001E-3,1.0018,2.2000000000000001E-3,29.257999999999999,1E-3,1645,13,1510,null,2.1141439205955844E-2,54.855692307693623,13.026,0.192,1.5956169267918168,12055.121824176977,156.98547921259842,54.855783804476424,252.6743473563493,11802.447476820627,8.7458565826080744E-3,27.468889356199909,71.382383073208175,13.026043453579257,13.496504006595382,7.0119371788299233E-3,20.775402310829893,8.7829774386490433E-3,27.612187809681579,8.4579789416410738E-3,26.762693052999346,74.582990879675549,61.797446711320291,26.373752902270926]
[2,"T2-CAN-55-T2ER-DM","75T0126","T2-CAN-55-T2ER-DM","20% open","off","off","3 turns","unsealed","unsealed",null,5.75,null,0,0,"CUST 6","8/7/2014","3:42:08","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.9,0.8,3.6,0,null,null,null,null,null,null,null,null,null,953,1490,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,".","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",74.998999999999995,1.2999999999999999E-2,62.000999999999998,0.06,55.003,0.02,50.987000000000002,3.2000000000000001E-2,75.010000000000005,0.04,71.56,0.12,72.930000000000007,0.01,0.18099999999999999,3.0000000000000001E-3,0.96160000000000001,1.9E-3,null,null,null,null,null,null,null,null,null,null,null,null,460.9,2.2000000000000002,460.2,2.2000000000000002,459,2.1,3.6,0,3.1,0,3.3,0,1550.7,17.899999999999999,1087.8,19.5,75.099999999999994,13.6,460,null,460,null,460,null,3.1,null,3,null,3,null,0.53,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,null,1575,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63.28,0.03,61.87,0.03,63.34,0.05,62.05,0.05,72.41,0.03,72.260000000000005,0.02,72.03,0.02,72.7,0.02,72.75,0.02,72.64,0.02,60.87,0.03,72.209999999999994,0.01,72.14,0.01,61.6,0.02,63.68,0.02,60.8,0.02,72.290000000000006,0.03,71.7,0.02,61.96,0.01,72.25,0.01,71.489999999999995,0.04,55.29,0.03,63.93,0.02,62.91,0.02,63.7,0.02,65.11,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72.64,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.2,0.04,54.38,0.38,54.56,0.3,75.5,0.04,75.41,0.04,74.98,0.04,74.91,7.0000000000000007E-2,75.91,0.04,75.87,0.03,75.599999999999994,0.03,69.44,7.0000000000000007E-2,69.48,7.0000000000000007E-2,71.209999999999994,0.04,74.010000000000005,0.04,73.02,0.05,73.17,0.04,72.849999999999994,0.05,73.66,0.03,73.81,0.03,73.81,0.04,73.7,0.03,72.73,0.03,72.91,7.0000000000000007E-2,72.989999999999995,0.04,73.17,0.03,72.260000000000005,0.06,70.52,0.04,70.19,0.05,69.760000000000005,0.09,null,null,74.72,0.08,75.819999999999993,0.03,75.61,0.04,75.459999999999994,0.05,75.319999999999993,null,75.17,0.04,null,null,null,null,74.03,0.04,73.400000000000006,0.03,72.95,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.998999999999995,1.2999999999999999E-2,62.000999999999998,0.06,72.295000000000002,5.0000000000000001E-3,60.389000000000003,0.05,55.003,0.02,50.987000000000002,3.2000000000000001E-2,2655.1,2.6,2543,2.6,0.48199999999999998,3.0000000000000001E-3,-0.16800000000000001,2E-3,0.18099999999999999,3.0000000000000001E-3,0.96160000000000001,1.9E-3,29.251999999999999,1E-3,1626,13,1490,null,5.4210842168433374E-2,137.85817163432606,13.03,0.16800000000000001,1.6190253245575053,11819.242020700249,143.99867653543305,137.85562461990327,634.81528179189911,11184.426738908349,8.6844240952971691E-3,27.242038013520936,70.67597467544249,13.029518529936164,13.478529310169899,6.9737315268586812E-3,20.770156962893342,8.7815210507553067E-3,27.609374586846183,8.3745752586615908E-3,26.505039673176221,73.928353626918963,61.467278270029475,26.110453554937191]
[2,"T2-CAN-55-T3ER-DM","75T0127","T2-CAN-55-T3ER-DM","30% open","off","off","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","5:07:29","10 Ton","0:15:00","75/62  55/51","ENG 1","TECH 4","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.9,0.8,3.6,0,13083,23,14804,312,7644,135,20735,142,12.799382716,952,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 30%-open, tape around damper perimeter inside/outside frame gaps, no compressor, 55/51 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm),--unsealed cab, 100% inlet/outlet Meriam, adjust code tester speed to match total static of run T2-CAN-55","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75,8.9999999999999993E-3,61.994999999999997,4.9000000000000002E-2,54.972000000000001,2.8000000000000001E-2,51.037999999999997,3.3000000000000002E-2,74.94,0.04,69.709999999999994,0.12,71.33,0.01,0.17100000000000001,3.0000000000000001E-3,0.93659999999999999,2.3E-3,13083,23,7644,135,12.8,0.14000000000000001,null,null,null,null,null,null,460.9,2.1,460.2,2.1,459.3,2.1,3.6,0,3.1,0,3.3,0,1542.8,17.600000000000001,1094.7,19.100000000000001,77.2,13.5,460,null,460,null,460,null,3,null,3.1,null,3,null,0.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,null,1575,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64.06,0.03,62.22,0.02,64.599999999999994,0.03,63.21,0.04,70.41,0.03,70.260000000000005,0.02,70.11,0.02,70.760000000000005,0.02,70.81,0.02,70.739999999999995,0.03,61.89,0.02,72.099999999999994,0.02,71.86,0.02,62.48,0.03,64.540000000000006,0.02,61.27,0.03,71.95,0.05,70.790000000000006,0.02,62.41,0.02,72.150000000000006,0.01,71.16,7.0000000000000007E-2,54.76,7.0000000000000007E-2,65.099999999999994,0.02,63.97,0.03,64.37,0.03,65.8,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70.739999999999995,0.03,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.99,0.03,54.25,0.3,54.49,0.27,75.44,0.04,75.34,0.03,74.98,0.03,75.27,0.09,75.87,0.03,75.78,0.04,75.56,0.03,57.56,7.0000000000000007E-2,58.62,0.06,65.72,0.08,72.22,0.06,62.61,0.15,71.239999999999995,7.0000000000000007E-2,71.88,0.05,73.64,0.04,71.28,0.08,72.67,0.04,72.06,0.05,73.209999999999994,0.04,72.55,0.06,72.97,0.03,72.680000000000007,0.04,73.430000000000007,0.05,69.02,0.04,69.22,0.04,68.95,0.09,null,null,74.97,7.0000000000000007E-2,75.75,0.04,75.53,0.04,75.37,0.04,75.23,null,75.09,0.04,null,null,null,null,65.77,0.09,72.58,0.06,72.709999999999994,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75,8.9999999999999993E-3,61.994999999999997,4.9000000000000002E-2,70.388999999999996,8.0000000000000002E-3,59.387,3.7999999999999999E-2,54.972000000000001,2.8000000000000001E-2,51.037999999999997,3.3000000000000002E-2,2616.1999999999998,3.2,2514,3.1,0.437,2E-3,-0.126,1E-3,0.17100000000000001,3.0000000000000001E-3,0.93659999999999999,2.3E-3,29.253,1E-3,1620,13,1490,null,0.14734371879368904,370.42210904733423,13.029,0.126,1.6551945470011971,11689.227244968799,129.06598866141732,370.4221255463022,1705.8351026864707,9983.3921422823278,8.519144416446708E-3,26.611949935485267,68.733805452998794,13.029001160649175,13.428774777867618,7.0081225450451881E-3,20.799949247863466,8.7773286200148598E-3,27.605030708882261,8.191597300297334E-3,25.840654399628029,72.085312526206877,60.537799403314452,25.43738765123863]
[2,"T2-CAN-55-TCE-DM","75T0128","T2-CAN-55-TCE-DM","closed","off","off","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","0:26:49","10 Ton","0:15:00","75/62 55/51","ENG 1","TECH 3","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,460.7,1.1000000000000001,3.6,0,null,null,null,null,null,null,null,null,null,952,1520,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo closed, tape around damper perimeter frame gaps, no compressor, 55/51 ambient,--2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm), 100% inlet/outlet Meriam, adjust code tester speed--to match total static of run T2-CAN-55-TCE-DM-SPWCT-SS","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",74.988,1.9E-2,61.997,4.7E-2,54.941000000000003,0.02,51.16,4.5999999999999999E-2,74.98,0.04,72.34,0.12,73.7,0.01,0.21099999999999999,5.0000000000000001E-3,1.012,2.8E-3,null,null,null,null,5.577,6.3E-2,null,null,null,null,null,null,460.7,2.2999999999999998,460.4,2.2999999999999998,459,2.2000000000000002,3.6,0,3.1,0,3.3,0,1564.9,18.100000000000001,1087,20.6,87.2,13.3,460,null,460,null,460,null,3.1,null,3.1,null,3,null,0.55000000000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,null,1605,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.01,0.03,61.18,0.02,60.5,0.05,60.34,0.03,73.37,0.03,73.23,0.02,73,0.02,73.67,0.02,73.709999999999994,0.03,73.59,0.02,59.96,0.01,70.97,0.02,71.44,0.02,61.21,0.01,57.46,0.03,58.08,0.06,72.48,0.01,71.400000000000006,0.01,60.76,0.02,70.97,0.01,71.900000000000006,0.01,55.43,0.03,62.59,0.02,61.76,0.02,61.96,0.19,63.4,0.22,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,73.59,0.02,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58.84,0.02,54.21,0.41,54.38,0.33,75.459999999999994,0.04,75.290000000000006,0.05,74.95,0.06,74.72,0.09,75.84,0.04,75.8,0.04,75.510000000000005,0.05,72.849999999999994,0.05,73.150000000000006,0.05,73.290000000000006,0.05,74.39,0.03,74.44,0.04,74.13,0.04,73.27,0.04,73.3,0.05,74,0.04,73.650000000000006,0.06,73.83,0.04,72.7,0.05,72.78,0.06,71.150000000000006,0.13,72.73,0.04,70.61,7.0000000000000007E-2,70.3,0.05,69.22,0.06,69.41,0.08,null,null,74.53,0.11,75.760000000000005,0.04,75.56,0.04,75.400000000000006,0.04,75.23,null,75.14,0.05,null,null,null,null,74.599999999999994,0.04,73.17,0.03,72.989999999999995,0.04,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",74.988,1.9E-2,61.997,4.7E-2,73.230999999999995,1.4E-2,60.917999999999999,4.3999999999999997E-2,54.941000000000003,0.02,51.16,4.5999999999999999E-2,2725,3.8,2608.3000000000002,3.6,0.52100000000000002,3.0000000000000001E-3,-0.2,2E-3,0.21099999999999999,5.0000000000000001E-3,1.012,2.8E-3,29.279,0,1652,13,1520,null,7.8315957499877752E-3,20.427151194693117,13.029,0.2,1.5972328261533035,12108.245521875315,159.64685477165355,20.426977179582522,94.0701137982322,12014.175408077082,8.7682663379210317E-3,27.554318224068965,71.633767173846692,13.028778017678805,13.503194967810437,7.0803645920664675E-3,20.870823858289931,8.7814824850072498E-3,27.606649495604753,8.4928950752458932E-3,26.862544455305258,74.8327315212983,61.921268684798584,26.47318565895182]
[2,"T2-CAN-55-TOER-DM","75T0129","T2-CAN-55-TOER-DM","open","off","off","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","6:41:54","10 Ton","0:15:00","75/62  55/51","ENG 1","TECH 4","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,55,51,6.4,6.2,6.4,6.2,461,1.1000000000000001,3.7,0,40355,72,39128,286,22767,394,63143,411,36.775189284,950,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo fully open, tape around damper perimeter inside/outside frame gaps, no compressor, 55/51 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm),--unsealed cab, 100% inlet/outlet Meriam, adjust code tester speed to match total static of run T2-CAN-","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.016999999999996,0.02,61.991,8.3000000000000004E-2,55.040999999999997,4.3999999999999997E-2,51.006999999999998,9.4E-2,74.7,0.09,61.86,0.06,64.040000000000006,0.02,0.2,3.0000000000000001E-3,1.0606,2.3E-3,40355,72,22767,394,36.780999999999999,0.38600000000000001,null,null,null,null,null,null,461,2.4,460.4,2.5,459,2.4,3.7,0,3.2,0,3.4,0,1601.9,21.5,1087.0999999999999,23.4,114.9,16.2,460,null,460,null,460,null,3.1,null,3.2,null,3.1,null,0.55000000000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,null,1655,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64.28,0.02,63.73,0.03,63.02,7.0000000000000007E-2,63.88,0.03,61.9,0.06,61.59,0.05,61.29,0.05,62.19,0.06,62.11,0.06,62.06,0.06,63.16,0.01,62.9,0.03,62.44,0.03,65.760000000000005,0.01,59.02,7.0000000000000007E-2,61.52,0.17,63.96,0.02,58.86,7.0000000000000007E-2,64.63,0.02,62.87,0.02,63.31,0.02,55.94,0.08,65.819999999999993,0.02,64.77,0.02,61.77,0.05,61.37,0.05,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62.06,0.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59.91,0.08,55.7,1.04,55.96,0.78,75.39,0.09,75.260000000000005,0.09,74.98,0.08,75.819999999999993,7.0000000000000007E-2,75.819999999999993,0.08,75.739999999999995,0.09,75.52,0.09,57.77,0.33,59.94,0.34,55.78,0.42,57.27,0.28000000000000003,65.52,0.22,60.62,0.4,57.19,0.14000000000000001,60.52,0.12,63.38,0.16,59.63,0.19,62.25,0.15,58.97,0.18,61.63,0.11,59.82,0.16,60.05,0.19,71.56,0.12,72.47,0.09,70.209999999999994,0.1,70.03,0.04,null,null,75.099999999999994,0.08,75.61,0.09,75.39,0.09,75.209999999999994,0.09,75.09,null,74.930000000000007,0.09,45.52,1.17,null,null,58.54,0.22,57.88,0.22,60.77,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Economizer test",75.016999999999996,0.02,61.991,8.3000000000000004E-2,61.765999999999998,1.4E-2,54.186,5.7000000000000002E-2,55.040999999999997,4.3999999999999997E-2,51.006999999999998,9.4E-2,2764.7,3.1,2700.2,3,0.38500000000000001,2E-3,-3.1E-2,1E-3,0.2,3.0000000000000001E-3,1.0606,2.3E-3,29.268999999999998,1E-3,1717,14,1570,null,0.58124749699639555,1569.4844913896673,13.03,3.1E-2,1.6382034565683499,12564.915214184215,122.12983338582677,1569.5142264511996,7226.9597400988969,5337.9554740853182,7.73810275838568E-3,23.678857908550057,60.12779654343165,13.030493730934124,13.201999151792128,6.9754272995311093E-3,20.781235280135615,8.770675034917812E-3,27.601895891765725,7.1346599655840778E-3,22.589375880385521,63.54339056255175,55.966228447666573,22.191017567879143]
[2,"T2-CAN-95-T1ER-DM","75T0143","T2-CAN-95-T1ER-DM","10% open","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","15:28:05","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460.6,1.5,15,0,51701,97,51903,750,7918,352,59627,337,7.0782288698955362,953,null,null,6.1373456790000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 10%-open, tape around damper perimeter inside/outside frame gaps, both stages--95/75 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm), unsealed cab, 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-CAN-95-T","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",74.992999999999995,5.6000000000000001E-2,62.000999999999998,3.2000000000000001E-2,94.902000000000001,1.0999999999999999E-2,75.006,1.2E-2,74.89,0.26,56.99,0.05,60.09,0.03,0.20499999999999999,3.0000000000000001E-3,0.97770000000000001,2E-3,51701,97,7918,352,7.0789999999999997,4.4999999999999998E-2,null,null,null,null,null,null,460.6,2.8,460.2,2.8,459,2.8,15,0.1,13,0,12.6,0.1,6809.1,65,3196.2,74.3,1614.9,52.5,460,null,459,null,460,null,3.1,null,3.1,null,3,null,0.54,460,null,459,null,460,null,4.5,null,4.8,null,4.4000000000000004,null,3120,null,0.85,460,460,459,4.9000000000000004,4.5,4.4000000000000004,2990,0.81,459.7,null,1.6,null,696.5,null,85,null,8421.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,213,0.19,105.27,0.13,105.62,0.06,0.35,0.1,240.54,0.23,171.89,0.16,114.23,7.0000000000000007E-2,-57.65,0.17,207,0.05,98.82,0.06,103.64,0.05,4.83,0.05,73.89,0.08,47.48,0.37,43.35,0.05,4.13,0.38,73.319999999999993,0.08,55.09,0.31,42.98,0.05,12.11,0.31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243.38,0.21,166.83,0.37,115.08,0.06,51.75,0.37,225.42,0.33,109.59,0.1,9.7899999999999991,0.13,215,0.05,98.75,0.09,106.27,0.05,7.52,0.04,77.56,7.0000000000000007E-2,45.74,0.05,2.62,0.22,77.09,0.1,55.55,0.71,45.43,0.06,10.119999999999999,0.73,104.25,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.64,0.09,104.25,0.09,99.85,0.09,100.18,0.08,57.37,0.06,57.01,0.05,56.51,0.05,57.48,0.03,57.09,7.0000000000000007E-2,57.15,0.04,104.79,0.08,100.27,7.0000000000000007E-2,48.49,0.59,54.86,0.4,166.63,0.35,100.32,0.09,99.07,0.09,48.75,0.08,56.89,0.98,98.82,0.06,98.75,0.09,92.95,0.03,105.33,0.08,105.27,0.09,100.58,0.06,100.09,0.14000000000000001,99.85,0.09,100.18,0.08,null,null,null,null,null,null,null,null,null,null,null,null,105.27,0.13,57.15,0.04,null,null,99.79,0.11,104.64,0.09,104.25,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48.37,0.2,null,null,null,null,null,null,null,null,null,null,null,null,172.52,0.18,94.29,0.17,94.33,0.17,75.709999999999994,0.17,75.52,0.17,75.39,0.15,76.959999999999994,0.13,76.040000000000006,0.17,75.92,0.17,75.790000000000006,0.17,77.94,0.17,77.84,0.17,77.290000000000006,0.16,76.06,0.18,76.150000000000006,0.19,76.36,0.19,76.739999999999995,0.18,76.819999999999993,0.17,76.02,0.17,76.11,0.18,75.92,0.16,76.75,0.15,76.58,0.17,76.959999999999994,0.18,76.599999999999994,0.16,78.25,0.1,78.41,0.12,79.39,0.12,79.290000000000006,0.13,null,null,75.86,0.16,76.010000000000005,0.15,75.72,0.18,75.47,0.19,75.36,null,75.17,0.19,null,null,null,null,75.900000000000006,0.19,76.7,0.14000000000000001,76.62,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-T1ER-DM",74.992999999999995,5.6000000000000001E-2,62.000999999999998,3.2000000000000001E-2,57.164000000000001,0.02,54.35,2.4E-2,94.902000000000001,1.0999999999999999E-2,75.006,1.2E-2,2648.2,2.7,2594.5,2.7,0.51,3.0000000000000001E-3,-0.19500000000000001,2E-3,0.20499999999999999,3.0000000000000001E-3,0.97770000000000001,2E-3,29.193000000000001,1E-3,8424,24,1530,null,2.1141439205955844E-2,54.855692307693623,13.026,0.192,1.6104631741783004,12134.104338761541,155.44936535433069,57.511720576041284,244.77135924553502,11889.332979516006,8.8871595361820072E-3,27.822384362360335,55.553536825821702,14.097659322555822,13.094662412983437,1.3949502956391345E-2,38.164685700659163,8.7829386617168728E-3,27.60946248014341,8.3117901319343414E-3,22.749129345951577,75.398308323201036,62.303344729761399,22.356674874776758,{"$f":"(XZ552-YL552)*XT552","v":66321.489207698003},{"$f":"0.24*(YJ552-YA552)*XT552","v":57791.646702739657},{"$f":"XK552-XM552","v":6894},{"$f":"YO552*3.413/YM552","v":0.35477523621814178},{"$f":"YM552-(XM552-XU552)*3.413","v":61630.147891652334},{"$f":"YN552-(XM552-XU552)*3.413","v":53100.305386693988},{"$f":"YQ552/XK552","v":7.3160194553243514},{"$f":"(YA552-YW552)/(YJ552-YW552)","v":0.15917424064040742},{"$f":"-XZ552+YL552","v":-5.4657094875835774},{"$f":"-YJ552+YA552","v":-19.844771497379334},{"$f":"(-(-0.0182984848494437-(YU552/YV552))+SQRT((-0.0182984848494437-(YU552/YV552))^2-4*0.00577826340327261*(6.76723916086377-XZ552+(YU552/YV552)*YJ552)))/(2*0.00577826340327261)","v":51.79678175663399},{"$f":"XT552*(XZ552-YL552)","v":66321.489207698003},{"$f":"XT552*(YG552-YI552)","v":58975.789371423605},{"$f":"XT552*(YI552-YL552)","v":4762.0835014487375},{"$f":"XW552*(YE552-YG552)","v":2583.6163348256746},{"$f":"SUM(YY552:ZA552)","v":66321.489207698018},{"$f":"ZB552/YX552","v":1.0000000000000002}]
[2,"T2-CAN-95-T2ER-DM","75T0144","T2-CAN-95-T2ER-DM","20% open","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","13:49:15","10 Ton","0:15:00","75/62  95/75","ENG 1","TECH 2","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460.8,1.4,15,0,50215,63,47935,310,6330,76,56550,103,6.7185458001663303,952,null,null,5.9659023409999996,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 20%-open, tape around damper perimeter inside/outside frame gaps, both stages, 95/75 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm),--unsealed cab, 100% inlet/outlet Meriam, adjust code tester speed to match total static of run T2-CAN-95-T","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.001999999999995,1.2999999999999999E-2,61.997999999999998,1.2E-2,94.906999999999996,7.0000000000000001E-3,75.003,1.2999999999999999E-2,74.2,0.12,57.4,0.04,60.32,0.02,0.20499999999999999,3.0000000000000001E-3,0.94699999999999995,2.2000000000000001E-3,50215,63,6330,76,6.7190000000000003,2.3E-2,null,null,null,null,null,null,460.8,2.8,460.2,2.8,459.3,2.8,15,0.1,13.1,0,12.6,0.1,6791.3,68.3,3214.6,76.3,1626,56.3,460,null,460,null,460,null,3.1,null,3,null,3,null,0.54,460,null,460,null,460,null,4.5,null,4.8,null,4.4000000000000004,null,3120,null,0.86,460,460,460,4.9000000000000004,4.5,4.5,2970,0.8,459.8,null,1.6,null,696.9,null,85,null,8371.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,213.23,0.2,105.35,0.12,105.7,0.06,0.35,0.09,240.64,0.24,172.02,0.11,114.27,7.0000000000000007E-2,-57.75,0.1,207,0.01,98.82,7.0000000000000007E-2,103.64,0.03,4.82,0.05,73.59,0.05,47.16,0.22,43.17,0.03,3.99,0.24,73.03,0.04,54.8,0.13,42.8,0.03,12,0.13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,244.24,0.23,166.25,0.1,115.34,7.0000000000000007E-2,50.91,0.11,225.07,0.31,109.49,0.1,9.18,0.09,214,null,99.23,0.1,105.95,null,6.71,null,79.67,0.04,47.08,0.03,2.5099999999999998,0.15,79.040000000000006,0.04,56.71,0.23,46.69,0.03,10.02,0.23,104.3,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.71,0.09,104.3,0.1,100.34,0.09,100.68,0.08,57.6,0.03,57.23,0.03,56.71,0.03,57.65,0.03,57.39,0.05,57.3,0.03,104.83,0.09,100.2,0.08,48.12,0.43,54.46,0.19,165.86,0.12,100.73,0.09,99.53,0.09,49.85,0.08,58.18,0.33,98.82,7.0000000000000007E-2,99.23,0.1,93.17,0.04,105.36,0.08,105.18,0.14000000000000001,100.82,0.08,100.61,0.08,100.34,0.09,100.68,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.3,0.03,null,null,100.31,0.1,104.71,0.09,104.3,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,49.59,0.14000000000000001,null,null,null,null,null,null,null,null,null,null,null,null,172.58,0.11,94.38,0.18,94.44,0.17,75.099999999999994,0.1,74.930000000000007,0.1,74.77,0.09,76.260000000000005,0.09,75.44,0.09,75.37,0.08,75.209999999999994,0.08,80.45,0.11,80.53,0.12,78.63,0.08,75.64,0.09,77.31,0.1,76.45,0.09,76.569999999999993,0.09,76.13,0.09,75.69,0.08,75.55,0.08,75.36,0.08,76.150000000000006,0.08,75.7,0.09,75.92,0.09,75.77,0.09,76.72,0.06,78.02,0.06,78.45,7.0000000000000007E-2,79.040000000000006,0.1,null,null,75.12,0.09,75.39,0.1,75.12,0.1,74.88,0.1,74.78,null,74.540000000000006,0.09,null,null,null,null,75.900000000000006,0.1,76.010000000000005,7.0000000000000007E-2,76.03,0.08,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-T2ER-DM",75.001999999999995,1.2999999999999999E-2,61.997999999999998,1.2E-2,57.4,7.0000000000000001E-3,54.637999999999998,8.9999999999999993E-3,94.906999999999996,7.0000000000000001E-3,75.003,1.2999999999999999E-2,2604.4,3,2554.4,3,0.46600000000000003,2E-3,-0.16900000000000001,2E-3,0.20499999999999999,3.0000000000000001E-3,0.94699999999999995,2.2000000000000001E-3,29.242999999999999,1E-3,8417,23,1500,null,5.4210842168433374E-2,137.85817163432606,13.03,0.16800000000000001,1.6212444744482946,11927.197091968672,139.84273990551182,143.82155967843107,612.1041049112531,11315.092987057418,9.043996577510283E-3,28.148824691551226,55.778755525551702,14.097754796068548,13.101485520451602,1.3945675914001792E-2,38.161694909958655,8.778834104143339E-3,27.607165955768739,8.4200791711067178E-3,22.924294770267384,76.032636046382322,62.763407808431673,22.529135049367017,{"$f":"(XZ553-YL553)*XT553","v":67027.145958025969},{"$f":"0.24*(YJ553-YA553)*XT553","v":57977.285963791648},{"$f":"XK553-XM553","v":6917},{"$f":"YO553*3.413/YM553","v":0.35221134157769046},{"$f":"YM553-(XM553-XU553)*3.413","v":62384.929229323483},{"$f":"YN553-(XM553-XU553)*3.413","v":53335.069235089162},{"$f":"YQ553/XK553","v":7.4117772637903627},{"$f":"(YA553-YW553)/(YJ553-YW553)","v":0.1525629563788983},{"$f":"-XZ553+YL553","v":-5.6196896421842091},{"$f":"-YJ553+YA553","v":-20.25388052083062},{"$f":"(-(-0.0182984848494437-(YU553/YV553))+SQRT((-0.0182984848494437-(YU553/YV553))^2-4*0.00577826340327261*(6.76723916086377-XZ553+(YU553/YV553)*YJ553)))/(2*0.00577826340327261)","v":52.132476532130134},{"$f":"XT553*(XZ553-YL553)","v":67027.145958025969},{"$f":"XT553*(YG553-YI553)","v":55853.52758577565},{"$f":"XT553*(YI553-YL553)","v":4713.147873986004},{"$f":"XW553*(YE553-YG553)","v":6460.4704982643225},{"$f":"SUM(YY553:ZA553)","v":67027.145958025969},{"$f":"ZB553/YX553","v":1}]
[2,"T2-CAN-95-T3ER-DM","75T0145","T2-CAN-95-T3ER-DM","30% open","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","11:58:22","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460.6,1.5,15,0,45515,86,44027,392,1343,155,46860,175,5.5606977572089713,953,null,null,5.401091729,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo 30%-open, tape around damper perimeter inside/outside frame gaps, both stages--95/75 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm), unsealed cab, 100% inlet/outlet Meriam,--adjust code tester speed to match total static of run T2-CAN-95-T","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",74.981999999999999,2.8000000000000001E-2,61.991,2.7E-2,94.893000000000001,2.1000000000000001E-2,75.010000000000005,2.4E-2,74.36,0.14000000000000001,58.54,0.05,61.49,0.02,0.17799999999999999,4.0000000000000001E-3,0.9083,2.3999999999999998E-3,45515,86,1343,155,5.5609999999999999,2.5999999999999999E-2,null,null,null,null,null,null,460.6,2.6,460.2,2.6,459.3,2.5,15,0.1,13,0,12.6,0.1,6792.8,67.2,3216.8,71.3,1634.2,55.8,460,null,460,null,459,null,3,null,3,null,3,null,0.53,460,null,459,null,459,null,4.5,null,4.8,null,4.4000000000000004,null,3100,null,0.85,459,459,459,4.9000000000000004,4.5999999999999996,4.4000000000000004,3020,0.82,459.7,null,1.6,null,697.6,null,85,null,8412.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,213.61,0.24,105.63,0.13,105.83,0.08,0.21,0.09,241.51,0.27,171.66,0.1,114.54,0.08,-57.12,0.13,208,7.0000000000000007E-2,98.53,7.0000000000000007E-2,103.98,0.06,5.46,0.04,74.099999999999994,0.05,47.15,0.15,43.52,0.03,3.63,0.15,73.55,0.05,54.81,0.21,43.16,0.03,11.65,0.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,246.12,0.25,164.62,0.16,115.91,7.0000000000000007E-2,48.71,0.17,224.28,0.33,109.25,0.1,8.2200000000000006,0.25,213,0.2,100.45,0.15,105.6,0.05,5.18,0.06,83.6,0.04,49.53,0.02,3.17,0.32,83.09,0.04,59.06,0.24,49.22,0.03,9.84,0.24,104.42,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.83,0.1,104.42,0.1,101.47,0.13,101.85,0.12,58.8,0.03,58.48,0.03,57.97,0.05,58.83,0.03,58.52,0.05,58.5,0.03,104.94,0.09,100,0.08,47.96,0.28000000000000003,54.38,0.27,164.12,0.13,101.92,0.12,100.77,0.12,52.58,0.15,60.89,0.32,98.53,7.0000000000000007E-2,100.45,0.12,93.39,0.05,105.51,0.09,105.42,0.09,101.98,0.08,101.63,7.0000000000000007E-2,101.47,0.13,101.85,0.12,null,null,null,null,null,null,null,null,null,null,null,null,105.63,0.13,58.5,0.03,null,null,101.02,0.23,104.83,0.1,104.42,0.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,52.7,0.32,null,null,null,null,null,null,null,null,null,null,null,null,172.15,0.13,94.46,0.2,94.56,0.2,75.150000000000006,0.09,74.95,0.08,74.77,0.08,75.91,7.0000000000000007E-2,75.459999999999994,0.09,75.38,0.08,75.2,0.08,90.88,0.21,88.16,0.17,83.75,0.16,77.92,0.1,88.19,0.18,77.88,0.1,77.33,0.1,76.19,0.09,78.45,0.1,76.73,0.09,77.78,0.12,76.260000000000005,0.08,76.12,0.09,76.09,0.08,76.459999999999994,0.08,75.34,0.08,79.23,7.0000000000000007E-2,79.23,0.06,79.84,0.12,null,null,74.94,0.08,75.430000000000007,0.09,75.150000000000006,0.09,74.91,0.09,74.81,null,74.599999999999994,0.09,null,null,null,null,84.57,0.12,77.52,0.1,76.75,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-T3ER-DM",74.981999999999999,2.8000000000000001E-2,61.991,2.7E-2,58.633000000000003,1.4E-2,55.813000000000002,1.9E-2,94.893000000000001,2.1000000000000001E-2,75.010000000000005,2.4E-2,2551.8000000000002,3.3,2498.5,3.2,0.42099999999999999,2E-3,-0.123,3.0000000000000001E-3,0.17799999999999999,4.0000000000000001E-3,0.9083,2.3999999999999998E-3,29.277999999999999,1E-3,8427,22,1510,null,0.14734371879368904,370.42210904733423,13.029,0.126,1.6910311895782568,11655.821996708446,123.57384267716536,380.69690286827773,1620.2767090791317,10035.545287629315,9.49849103986233E-3,29.071231675871008,56.941968810421749,14.09747732847347,13.135753106322063,1.3955164753169205E-2,38.168715670434111,8.778944227937957E-3,27.602408507310237,8.8077038557288333E-3,23.646185203405082,77.772255887366825,64.038535897268503,23.23372473665,{"$f":"(XZ554-YL554)*XT554","v":68040.941788110416},{"$f":"0.24*(YJ554-YA554)*XT554","v":58270.588394209939},{"$f":"XK554-XM554","v":6917},{"$f":"YO554*3.413/YM554","v":0.34696346610718504},{"$f":"YM554-(XM554-XU554)*3.413","v":63309.06931316758},{"$f":"YN554-(XM554-XU554)*3.413","v":53538.715919267102},{"$f":"YQ554/XK554","v":7.5126461745778546},{"$f":"(YA554-YW554)/(YJ554-YW554)","v":0.14818956581049825},{"$f":"-XZ554+YL554","v":-5.8375069392210079},{"$f":"-YJ554+YA554","v":-20.830287076945076},{"$f":"(-(-0.0182984848494437-(YU554/YV554))+SQRT((-0.0182984848494437-(YU554/YV554))^2-4*0.00577826340327261*(6.76723916086377-XZ554+(YU554/YV554)*YJ554)))/(2*0.00577826340327261)","v":53.318121210365469},{"$f":"XT554*(XZ554-YL554)","v":68040.941788110416},{"$f":"XT554*(YG554-YI554)","v":46113.034609548267},{"$f":"XT554*(YI554-YL554)","v":4807.5657811765168},{"$f":"XW554*(YE554-YG554)","v":17120.341397385608},{"$f":"SUM(YY554:ZA554)","v":68040.941788110387},{"$f":"ZB554/YX554","v":0.99999999999999956}]
[2,"T2-CAN-95-TCE-DM","75T0146","T2-CAN-95-TCE-DM","closed","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","16:42:46","10 Ton","0:15:00","75/62  95/75","ENG 1","TECH 4","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,461,1.5,15,0,52104,97,53279,701,8612,180,60724,183,7.2050308495491215,952,null,null,6.1822496439999997,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo closed, tape around damper perimeter frame gaps, both stages, 95/75 ambient, 2 HP fan motor, 5.75\" pulley,--3 turns (939 rpm), 100% inlet/outlet Meriam, adjust code tester speed to match total static of run T2-CAN-95-TCE-DM-SPWCT-SS","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",75.003,1.7999999999999999E-2,61.999000000000002,2.4E-2,94.911000000000001,1.2999999999999999E-2,74.998000000000005,1.7999999999999999E-2,75.12,0.22,56.79,7.0000000000000007E-2,60.01,0.03,0.19600000000000001,4.0000000000000001E-3,0.98240000000000005,3.2000000000000002E-3,52104,97,8612,180,7.2050000000000001,3.1E-2,null,null,null,null,null,null,461,2.8,460.5,2.8,459.3,2.8,15,0.1,13,0,12.6,0.1,6820.2,64.2,3197.4,72.7,1607.8,50.4,460,null,460,null,460,null,3.1,null,3.1,null,3.2,null,0.53,460,null,460,null,460,null,4.5,null,4.8,null,4.4000000000000004,null,3110,null,0.86,460,460,460,4.9000000000000004,4.5,4.4000000000000004,2960,0.81,460,null,1.6,null,696.6,null,85,null,8276.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,213.09,0.2,105.28,0.13,105.64,0.06,0.37,0.1,240.67,0.23,171.81,0.13,114.27,7.0000000000000007E-2,-57.54,0.15,207,null,98.88,0.06,103.64,null,4.76,null,74.11,0.06,47.59,0.37,43.49,0.04,4.0999999999999996,0.37,73.540000000000006,0.05,55.15,0.28000000000000003,43.11,0.04,12.03,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243.2,0.23,167.3,0.28999999999999998,115.03,7.0000000000000007E-2,52.28,0.3,225.54,0.33,109.63,0.1,10.29,0.12,214,null,98.8,0.1,105.95,null,7.14,null,77.13,7.0000000000000007E-2,45.46,0.05,2.4700000000000002,0.23,76.53,0.09,55.25,0.65,45.06,0.06,10.19,0.67,104.24,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104.64,0.09,104.24,0.09,99.82,0.1,100.1,0.09,57.25,0.04,56.87,0.04,56.43,0.04,57.39,0.05,56.86,0.1,57.07,0.05,104.84,0.08,100.22,0.08,48.66,0.57999999999999996,55.04,0.35,166.89,0.28999999999999998,100.26,0.1,99.11,0.09,48.45,0.1,56.54,0.94,98.88,0.06,98.8,0.1,92.91,0.04,105.29,0.08,105.17,0.12,100.39,7.0000000000000007E-2,99.83,0.19,99.82,0.1,100.1,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.07,0.05,null,null,99.34,0.12,104.64,0.09,104.24,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,47.93,0.21,null,null,null,null,null,null,null,null,null,null,null,null,172.47,0.15,94.25,0.17,94.29,0.18,75.88,0.13,75.760000000000005,0.13,75.569999999999993,0.12,77.150000000000006,0.11,76.23,0.13,76.16,0.13,76.040000000000006,0.13,77.59,0.12,77.489999999999995,0.12,76.959999999999994,0.13,76.14,0.13,76.11,0.15,76.290000000000006,0.14000000000000001,76.84,0.13,77.12,0.13,76.180000000000007,0.13,76.37,0.14000000000000001,76.06,0.12,76.98,0.12,76.930000000000007,0.13,77.75,0.15,76.87,0.12,78.59,7.0000000000000007E-2,78.819999999999993,0.08,79.89,0.09,79.569999999999993,0.09,null,null,76.06,0.13,76.180000000000007,0.11,75.88,0.13,75.63,0.14000000000000001,75.53,null,75.39,0.13,null,null,null,null,76.010000000000005,0.14000000000000001,76.91,0.11,76.81,0.12,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-TCE-DM",75.003,1.7999999999999999E-2,61.999000000000002,2.4E-2,57.078000000000003,1.2E-2,54.222000000000001,0.02,94.911000000000001,1.2999999999999999E-2,74.998000000000005,1.7999999999999999E-2,2655.6,4.3,2600,4.2,0.52500000000000002,3.0000000000000001E-3,-0.20200000000000001,2E-3,0.19600000000000001,4.0000000000000001E-3,0.98240000000000005,3.2000000000000002E-3,29.167000000000002,1E-3,8428,23,1510,null,7.8315957499877752E-3,20.427151194693117,13.029,0.2,1.5765586617278702,12170.414910911419,160.36062992125983,21.354470679617329,90.884188966016168,12079.530721945403,8.8177982427807312E-3,27.686648281522597,55.50144133827213,14.09781234067168,13.092076249359986,1.39403355992907E-2,38.156788560123971,8.7792572047378607E-3,27.607872853115236,8.2594988449171906E-3,22.671365714188301,75.153051877793914,62.111097669920916,22.287210051879814,{"$f":"(XZ555-YL555)*XT555","v":65713.403540589672},{"$f":"0.24*(YJ555-YA555)*XT555","v":57400.380944068776},{"$f":"XK555-XM555","v":6918},{"$f":"YO555*3.413/YM555","v":0.3593046886609052},{"$f":"YM555-(XM555-XU555)*3.413","v":61107.084370510929},{"$f":"YN555-(XM555-XU555)*3.413","v":52794.061773990034},{"$f":"YQ555/XK555","v":7.2504846191873433},{"$f":"(YA555-YW555)/(YJ555-YW555)","v":0.16479778787264096},{"$f":"-XZ555+YL555","v":-5.399438229642783},{"$f":"-YJ555+YA555","v":-19.651610539521783},{"$f":"(-(-0.0182984848494437-(YU555/YV555))+SQRT((-0.0182984848494437-(YU555/YV555))^2-4*0.00577826340327261*(6.76723916086377-XZ555+(YU555/YV555)*YJ555)))/(2*0.00577826340327261)","v":51.623887019062515},{"$f":"XT555*(XZ555-YL555)","v":65713.403540589672},{"$f":"XT555*(YG555-YI555)","v":60079.340091417034},{"$f":"XT555*(YI555-YL555)","v":4675.3338006702616},{"$f":"XW555*(YE555-YG555)","v":958.72964850235792},{"$f":"SUM(YY555:ZA555)","v":65713.403540589657},{"$f":"ZB555/YX555","v":0.99999999999999978}]
[2,"T2-CAN-95-TOER-DM","75T0147","T2-CAN-95-TOER-DM","open","on","on","3 turns","unsealed","unsealed",939,5.75,null,0,0,"CUST 6","8/7/2014","10:15:20","10 Ton","0:15:00","75/62 95/75","ENG 1","TECH 2","RTU2","RTU2","7.5","R22","PSC Air Handler","CK1- 6.40 lbs/CK2- 6.20","460/460/3","TU4","AHRI 340/360",75,62,95,75,6.4,6.2,6.4,6.2,460.2,1.5,14.9,0,31615,46,31917,315,0,0,31593,45,3.706358517128109,953,null,null,3.7089394649999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Econo fully open, tape around damper perimeter inside/outside frame gaps, both--stages, 95/75 ambient, 2 HP fan motor, 5.75\" pulley, 3 turns (939 rpm), unsealed cab,--100% inlet/outlet Meriam, adjust code tester speed to match total static of run T2-CAN-9","Installed:SG:FD:LSV on 2 circuits: Unsealed cab: dampers on S/R: AX35 belt: 5.75 BP: ID Blw 2 HP GE: Mtr Pulley 3 T/O: With econo: Supply Meriam @100% Return Meriam @100%: Horiz Air Disch: Max Mtr Amp 3.6",74.998999999999995,8.0000000000000002E-3,62.066000000000003,1.2E-2,94.930999999999997,1.6E-2,74.695999999999998,8.0000000000000002E-3,74.72,0.1,63.4,7.0000000000000007E-2,65.650000000000006,0.01,0.184,3.0000000000000001E-3,0.98540000000000005,2.0999999999999999E-3,31615,46,0,0,3.706,1.0999999999999999E-2,null,null,null,null,null,null,460.2,2.5,460,2.5,459.8,2.5,14.9,0.1,13.1,0,12.8,0.1,6784.7,66.599999999999994,3268.8,71.7,1739.6,55.7,460,null,459,null,459,null,3.1,null,3.1,null,3.1,null,0.54,460,null,460,null,459,null,4.5,null,4.9000000000000004,null,4.5,null,3130,null,0.86,460,459,459,4.9000000000000004,4.5999999999999996,4.5,3000,0.82,459.2,null,1.6,null,697.2,null,85,null,8422.2000000000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,211.82,0.21,105.18,0.09,105.25,7.0000000000000007E-2,7.0000000000000007E-2,0.05,246.97,0.23,172.92,0.1,116.16,7.0000000000000007E-2,56.76,0.1,203,0.06,97.66,7.0000000000000007E-2,102.31,0.06,4.6500000000000004,0.05,84.69,7.0000000000000007E-2,61.73,0.38,50.19,0.04,11.54,0.39,84.04,0.06,65.06,0.16,49.8,0.04,15.26,0.16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,249.73,0.24,164.27,0.2,116.97,7.0000000000000007E-2,47.3,0.2,224.19,0.33,109.22,0.1,7.28,0.11,212,0.1,100.97,0.12,105.3,null,4.33,null,90.92,7.0000000000000007E-2,53.87,0.04,7.77,0.84,90.39,0.06,64.66,0.38,53.56,0.03,11.1,0.37,103.24,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103.76,0.08,103.24,0.09,101.77,0.12,102.17,0.11,63.85,0.03,63.57,0.03,63.17,0.03,64.010000000000005,0.04,63.78,0.05,63.79,0.03,104.03,7.0000000000000007E-2,99.1,7.0000000000000007E-2,62.55,0.37,65.37,0.18,163.78,0.22,102.2,0.12,101.39,0.12,60.77,1.34,66.709999999999994,0.39,97.66,7.0000000000000007E-2,100.97,0.12,87.44,0.2,104.52,0.09,104.46,0.08,102.18,0.08,101.83,0.08,101.77,0.12,102.17,0.11,null,null,null,null,null,null,null,null,null,null,null,null,105.18,0.09,63.79,0.03,null,null,101.95,0.12,103.76,0.08,103.24,0.09,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61.62,0.87,null,null,null,null,null,null,null,null,null,null,null,null,173.47,0.12,94.54,0.2,95.1,0.19,75.33,0.06,75.16,0.06,74.92,0.05,75.72,0.05,75.69,0.05,75.63,0.05,75.42,0.05,90.38,0.32,88.79,0.36,90.73,0.39,88.47,0.32,83.39,0.35,85.22,0.43,89.32,0.18,87.29,0.14000000000000001,84.53,0.26,86.9,0.2,85.77,0.23,87.31,0.24,85.29,0.16,87.16,0.2,86.53,0.19,77.319999999999993,0.09,76.28,7.0000000000000007E-2,78.430000000000007,0.12,78.5,0.04,null,null,75.03,0.05,75.55,7.0000000000000007E-2,75.349999999999994,0.06,75.150000000000006,0.06,75.02,null,74.819999999999993,7.0000000000000007E-2,null,null,null,null,88.96,0.35,88.27,0.28999999999999998,86.72,0.21,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T2-CAN-55-TOER-DM",74.998999999999995,8.0000000000000002E-3,62.066000000000003,1.2E-2,63.786000000000001,1.0999999999999999E-2,60.93,1.6E-2,94.930999999999997,1.6E-2,74.695999999999998,8.0000000000000002E-3,2670.6,2.9,2586.3000000000002,2.8,0.36499999999999999,2E-3,-3.5999999999999997E-2,4.0000000000000001E-3,0.184,3.0000000000000001E-3,0.98540000000000005,2.0999999999999999E-3,29.280999999999999,0,8524,22,1510,null,0.58124749699639555,1569.4844913896673,13.03,3.1E-2,1.6486733349615819,12064.560393511654,110.90135858267716,1759.1574886832752,7487.8472693666245,4576.7131241450297,1.1832944599932425E-2,33.992622284021593,62.137326665038422,14.096100724811476,13.281544853153147,1.3671815647764729E-2,37.865494736556904,8.8244131100325279E-3,27.656311348269174,1.073951746703313E-2,27.007421734873716,87.410941923127467,70.310369537935756,26.603878689984192,{"$f":"(XZ556-YL556)*XT556","v":89141.943322436578},{"$f":"0.24*(YJ556-YA556)*XT556","v":73179.613834462303},{"$f":"XK556-XM556","v":7014},{"$f":"YO556*3.413/YM556","v":0.26854678177040292},{"$f":"YM556-(XM556-XU556)*3.413","v":84366.819659279252},{"$f":"YN556-(XM556-XU556)*3.413","v":68404.490171304977},{"$f":"YQ556/XK556","v":9.8975621374095795},{"$f":"(YA556-YW556)/(YJ556-YW556)","v":0.12007583237242006},{"$f":"-XZ556+YL556","v":-7.3887435940374004},{"$f":"-YJ556+YA556","v":-25.273615258089045},{"$f":"(-(-0.0182984848494437-(YU556/YV556))+SQRT((-0.0182984848494437-(YU556/YV556))^2-4*0.00577826340327261*(6.76723916086377-XZ556+(YU556/YV556)*YJ556)))/(2*0.00577826340327261)","v":58.688449476726248},{"$f":"XT556*(XZ556-YL556)","v":89141.943322436578},{"$f":"XT556*(YG556-YI556)","v":7828.5679295319269},{"$f":"XT556*(YI556-YL556)","v":4868.5694364512474},{"$f":"XW556*(YE556-YG556)","v":76444.805956453391},{"$f":"SUM(YY556:ZA556)","v":89141.943322436564},{"$f":"ZB556/YX556","v":0.99999999999999989}]